Department of Parks and Recreation		Mono Lake ADA Boardwalk Materials
		BU 3790 Event ID 0000039497

Attachment 2 – Technical Requirements/Statement of Work
Contractor to provide materials for the replacement of the Mono Lake ADA boardwalk
trail. Boardwalk materials to be composed of fiber reinforced polymer (FRP) composite
materials and manufactured using continuous ECR glass fiber and vinyl ester resin. All
structural members will have non-woven polyester veil applied during the manufacturing
process. Due to strict scenic corridor constraints and high-alkaline and UV exposure
environment, FRP materials must be painted in a two-part fluoropolymer coating such
as Vitreflon or approved equal and must be RAL 080-30-26 (Smoked Oak) in color.

The boardwalk required is 740 lineal feet and 6 feet width outside to outside. Decking
required is to be 38mm mini-mesh decking with anti-slip surface and in panels 4 feet by
6 feet by 1.5 inches thick. Bull rail edging to attach flush with outside of decking for total
of 6-foot-wide decking surface.

Hardware and brackets to be stainless steel and provided in full to connect all
boardwalk materials directly to concrete Diamond Pier foundation, provided by Parks,
and construct entire boardwalk structure.

Due to sensitive wetland environment, spans between Diamond Pier foundations need
to be 20 foot and engineered for 100 psi live load.
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