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[bookmark: _Toc120526612]INTRODUCTION AND SUMMARY OF THE BID SOLICITATION
This Bid Solicitation is issued by the Department of Treasury, Division of Purchase and Property (Division), Procurement Bureau, on behalf of the Department of Transportation and the State of New Jersey. Quotes submitted in response to this Bid Solicitation shall be through the State of New Jersey’s eProcurement system, NJSTART.  Bidders are advised to thoroughly read all sections of this Bid Solicitation and follow all instructions.  

Bidders are strongly encouraged to visit the NJSTART Vendor Support Page, which contains Quick Reference Guides (QRGs), supporting videos, a glossary of NJSTART terms, and helpdesk contact information.  Bidders should utilize the QRGs before attempting to submit a Quote through NJSTART.   It is the Bidder’s responsibility to ensure that the Quote and attachments have been properly submitted.  Inquiries concerning the use of NJSTART may be directed to njstart@treas.nj.gov. The Division will not respond to substantive questions related to the Bid Solicitation or any other Contract via this email address.

[bookmark: _Toc400531467][bookmark: _Toc428533937][bookmark: _Toc32310614][bookmark: _Toc120526613]PURPOSE AND INTENT
The purpose of this Bid Solicitation is to solicit Quotes for fencing services including, but not limited to, repair, installation, and preventative maintenance for chain link fencing, correctional facility security fencing, ornamental metal fencing, and various other fences.

It is the intent of the State to award Contracts to those responsible Bidders whose Quotes, conforming to this Bid Solicitation are most advantageous to the State of New Jersey (State), price and other factors considered.  The State may award any or all price lines.  The State, however, reserves the right to separately procure individual requirements that are the subject of the Contract during the Contract term, when deemed by the Director of the Division (Director) to be in the State’s best interest.

The State intends to award to multiple Contractors per Category, with one (1) award set-aside for a Small Business Enterprise (SBE) for each Category for each Region. Should an SBE business not bid or be responsive within a Category, the State may award to the next qualifying Bidder, including non-SBE classified Bidders.

The awarded Contractors will be selected to perform services via a Mini-Bid process based on the following considerations, and in accordance with Section 4.3, Method of Engagement:

A. The most cost-effective quote received; 
B. Quoted timeframe for the repair; and
C. The Contractor’s current backlog of pending and/or unfinished repair jobs.

Quotes will be evaluated in accordance with Bid Solicitation Section 8.9, Quote Evaluation. The State intends to award multiple Blanket P.O.s for each Category for each Region. The Bidder must submit pricing for all Price Lines in a Category to be considered for an award for that Region’s Category. Failure to submit pricing for all Price Lines in a Category will result in the Bidder being deemed nonresponsive for that Region’s Category. Each Region is as follows:

A. North Region;
B. Central Region; and
C. South Region.

The Categories and Types, applicable to all Regions, are listed below:
A. Category I – Standard chain link fencing:
1. Type I – Aluminum-coated and vinyl-clad chain link fence and installation; and
2. Type II – Specialty fencing and installation.

B. Category II – Additional fencing: 
1. Type I – Ornamental metal fence;
2. Type II – Vinyl fence including plastic snow and PVC type;
3. Type III – Wooden fence;
4. Type IV – Motorized automatic fence gates; and
5. Type V – Steel barricade.

C. Category III – Emergency repairs to security fencing:
1. Type I – Standard fabric;
2. Type II – Anti-climb security fencing fabric;
3. Type III – Framing; 
4. Type IV – Fitting and accessories; and
5. Type V – Barbed tape (razor ribbon).

D. Category IV – Preventive Maintenance

The State of New Jersey Standard Terms and Conditions (SSTCs) included with this Bid Solicitation will apply to all Contracts made with the State.  These terms are in addition to the terms and conditions set forth in this Bid Solicitation and should be read in conjunction with them unless the Bid Solicitation specifically indicates otherwise.  

[bookmark: _Toc400531468][bookmark: _Toc428533938][bookmark: _Toc32310615][bookmark: _Toc120526614]BACKGROUND 
This is a reprocurement of the services under T0640 - Fence: Chain Link, Rock Fall, Wooden, Vinyl, and Ornamental (Install & Replace).  Bidders interested in reviewing the current Contract/Master Blanket Purchase Order specifications and pricing information may do so by following the instruction below.  Bidders should not rely upon or use data or information from the contract when preparing a response to this Bid Solicitation as this Bid Solicitation addresses the State’s current requirements. 
· Go to: www.njstart.gov 
· Select “Active Blankets”
· In the search bar, select “Blankets” from the drop down menu
· Enter the T0640 and click “[image: ]”
· The current Contract list will appear under “Results”

[bookmark: _Toc120526615]CONTRACT AMOUNT
The estimated amount of the Contract, if stated, shall not be construed as either the maximum or minimum amount which the State shall be obliged to order.

[bookmark: _Toc400531506][bookmark: _Toc428533977][bookmark: _Toc32310702][bookmark: _Toc120526616]ORDER OF PRECEDENCE OF CONTRACTUAL TERMS
The Contract awarded, and the entire agreement between the parties, as a result of this Bid Solicitation shall consist of:  (1) the final Bid Solicitation, (2) the State of New Jersey Standard Terms and Conditions, (3) the Quote, and if applicable (4) any Bidder responses to clarifications; (5) a Bidder’s Best and Final Offer, (6) other negotiated document, and/or (7) third party document.  In the event of a conflict in the terms and conditions among the documents comprising this Contract, the order of precedence, for purposes of interpretation thereof, listed from highest ranking to lowest ranking as noted above. 

Any other terms or conditions, not included with the Bidder’s Quote and accepted by the State, shall not be incorporated into the Contract awarded.  Any references to external documentation, includinged those documents referenced by a URL, including without limitation, technical reference manuals, technical support policies, copyright notices, additional license terms, etc., are subject to the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Conditions.  In the event of any conflict between the terms of a document incorporated by reference the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Conditions shall prevail.

[bookmark: _Toc120526617]INTRASTATE COOPERATIVE PURCHASING
The State intends to extend the Contracts awarded to the State's Intrastate Cooperative Purchasing Participants.  Although the State is making the use of any Contract resulting from this Bid Solicitation available to Intrastate Cooperative Purchasing Participants, the State makes no representation as to the acceptability of the Bid Solicitation’s terms and conditions to any Intrastate Cooperative Purchasing Participants.















If a Contractor makes any sales to Intrastate Cooperative Purchasing Participants pursuant to the awarded Contract, the Contractor agrees to the remit the Supplier Convenience Fee in the amount of one percent (1%) of all Net Purchases made by Intrastate Cooperative Purchasing Participants to the Division’s eProcurement administrator, Periscope Holdings, Inc. (Periscope).  
A. Supplier Convenience Fee - For all purchases made by Intrastate Cooperative Purchasing Participants under the Contract, the Vendor shall remit the Supplier Convenience Fee in the amount of one percent (1%) of all Net Purchases to Periscope Holdings, Inc. (Periscope). 
B. Remittance of the Supplier Convenience Fee - On a quarterly basis, the Vendor shall remit the Supplier Convenience Fee via Automated Clearing House (ACH) transactions directly to Periscope using the NJSTART Reconciler module. The remittance shall be made no later than thirty (30) calendar days after the end of each calendar quarter.  The calendar quarters will end March 31, June 30, September 30, and December 31.  Failure to remit the Supplier Convenience Fee timely and accurately may result in Vendor’s goods and services being made ineligible for purchase through the NJSTART Marketplace module by Intrastate Cooperative Purchasing Participants.
C. Catalog Enablement - The Vendor shall cooperate with the State and/or Periscope as requested to upload catalog items and pricing consistent with the awarded Contract to the NJSTART Marketplace module. Vendor shall only upload a catalog containing items awarded.
D. Quarterly Sales Reporting - The Vendor shall submit a Sales Report documenting all sales made to Intrastate Cooperative Purchasing Participants. The Sales Report shall be submitted directly to Periscope using the NJSTART Reconciler module no later than thirty (30) calendar days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31. The Sales Report must contain the following information:  
· Complete and accurate details of all sales, credits, returns, refunds, and the like for the reporting quarter;
· Purchasing entity;
· Total of Supplier Convenience Fee amount due for the reporting quarter;
· Such other information as the State may reasonably request; and
· If no sales were made to State during the reporting quarter, then a report shall be submitted showing zero sales and zero Supplier Convenience Fee due.
E. Retention and Inspection of Records and Audit - The Vendor shall keep records of sales made to Intrastate Cooperative Purchasing Participants in sufficient detail to enable the State to determine the Supplier Convenience Fee payable by the Vendor. The State and/or Periscope may examine and audit, at its own expense, Vendor’s sales records and Sales Reports for completeness and accuracy. If such examination reveals underpayment of the Supplier Convenience Fee, the Vendor shall immediately pay to Periscope the amount of deficiency. If the examination reveals an underpayment of 5% or more, then the Vendor shall reimburse the State and/or Periscope for the cost of the audit.


[bookmark: _Toc120526629]PRE-QUOTE SUBMISSION INFORMATION
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote and for reviewing the Quote submission requirements and the Scope of Work requirements.  

[bookmark: _ELECTRONIC_QUESTION_AND][bookmark: _Toc428533940][bookmark: _Toc32310617][bookmark: _Toc120526630]ELECTRONIC QUESTION AND ANSWER PERIOD
The Division will electronically accept questions and inquiries from all potential Bidders via the “Q&A” Tab of the Bid Solicitation in NJSTART.  Questions should be directly tied to a Bid Solicitation Section, the Price Sheet, Form or Attachment; and should reference the specific Bid Solicitation Section or document to which it relates.

The cut-off date for electronic questions and inquiries relating to this Bid Solicitation is indicated on the Bid Solicitation cover page.  In the event that questions are posed by Bidders, answers to such questions will be issued by Bid Amendment.  
[bookmark: _1.3.3__Mandatory_Pre-Bid_Conference][bookmark: _1.3.5__SUBMISSION_OF_BID_PROPOSAL][bookmark: _1.3.2_SUBMISSION_OF_BID_PROPOSAL]
A Bidder shall not contact the Using Agency and/or the Procurement Specialist directly, in person, by telephone or by e-mail, concerning this Bid Solicitation, prior to Contract award.

[bookmark: _Toc120526631]EXCEPTIONS TO THE STATE OF NJ STANDARD TERMS AND CONDITIONS (SSTC)
Questions regarding the State of New Jersey Standard Terms and Conditions and exceptions to mandatory requirements MUST be posed during the Electronic Question and Answer period and shall contain the Bidder’s suggested changes and the reason(s) for the suggested change(s).

[bookmark: _Toc120526632]BID AMENDMENTS
In the event that it becomes necessary to clarify or revise this Bid Solicitation, such clarification or revision will be by Bid Amendment.  Any Bid Amendment will become part of this Bid Solicitation and part of any Contract awarded. Bid Amendments will be posted as a file attachment on the “Summary” page of the Bid Solicitation in NJSTART after the cut-off date.  

There are no designated dates for release of Bid Amendments.  Those Bidders who are on the bid holder list either through commodity code registration in NJSTART or by acknowledging the bid in NJSTART should receive notification of any Bid Amendment(s). If a Bidder is not on the bid holder list, Bid Amendments are still viewable on the “Summary” page of the Bid Solicitation in NJSTART.

It is the sole responsibility of the Bidder to be knowledgeable of all Bid Amendments related to this procurement. An interested Bidder should check the NJSTART “Open Bids” Tab on a daily basis to ensure review of the most updated information.

[bookmark: _1.3.4_MANDATORY/OPTIONAL_SITE][bookmark: _1.3.45_MANDATORY/OPTIONAL_SITE][bookmark: _MANDATORY/OPTIONAL_SITE_VISIT][bookmark: _Toc224543885][bookmark: _Toc238623352][bookmark: _Toc400531474][bookmark: _Toc428533944][bookmark: _Toc32310620][bookmark: _Toc120526633]MANDATORY/OPTIONAL SITE VISIT
Not applicable to this procurement.

[bookmark: _1.3.5__MANDATORY/OPTIONAL][bookmark: _1.3.6__MANDATORY/OPTIONAL][bookmark: _OPTIONAL_PRE-QUOTE_CONFERENCE][bookmark: _Toc224543888][bookmark: _Toc238623354][bookmark: _Toc428533945][bookmark: _Toc32310621][bookmark: _Toc120526634]OPTIONAL PRE-QUOTE CONFERENCE
The date and time of the Optional Pre-Quote Conference is indicated on the Bid Solicitation cover sheet.  Attendees may attend the Optional Pre-Quote Conference from their computer, tablet, or smartphone. Click the following link to join the Optional Pre-Quote Conference:

https://teams.microsoft.com/l/meetup-join/19%3ameeting_ODZjNDBlOTItM2ZjNi00ZjRlLWJiOWUtNjQwMGZlMGExZjM3%40thread.v2/0?context=%7b%22Tid%22%3a%225076c3d1-3802-4b9f-b36a-e0a41bd642a7%22%2c%22Oid%22%3a%224d28d3d5-8037-403a-aa66-89adb85ab228%22%7d
To call in, audio only, to the optional Pre-Quote Conference:

United States: +1 856-338-7074
Phone Conference ID: 122 111 484#

The Optional Pre-Quote Conference may be recorded.

The purpose of the Optional Pre-Quote Conference is to address procedural questions regarding the Bid Solicitation and Bidder Quote Submission Requirements only.  No substantive questions regarding the Bid Solicitation Scope of Work will be accepted or answered during the pre-Quote conference.  All questions are to be submitted during the Electronic Question and Answer Period.  

[bookmark: _Toc95619434][bookmark: _Toc109701220][bookmark: _Toc225321579][bookmark: _Toc400531476][bookmark: _Toc428533946][bookmark: _Toc32310622][bookmark: _Toc120526635][bookmark: _Toc94946029][bookmark: _Toc72744593]PRE-QUOTE DOCUMENT REVIEW 
The following are publicly available documents that a Bidder needs to review in order to prepare and submit accurate and comprehensive Quotes:
A. The Vendor shall refer to the following for all references to the Standard Construction Details 2016: https://www.state.nj.us/transportation/eng/CADD/v8/pdf/StandConstDetails.pdf;
B. For needed drawings and plans and references to the Standard Specifications for Road and Bridge Construction 2019, the Vendor shall refer to the following: https://www.state.nj.us/transportation/eng/specs/2019/pdf/StandSpecRoadBridge201920200114.pdf; 
C. The Vendor shall refer to the following link for other drawings and plans https://www.state.nj.us/transportation/eng/CADD/v8/stdconsdtls.shtml; and
D. The Vendor shall ensure that all safety set-ups conform to NJDOT’s Manual on Uniform Traffic Control Devices (MUTCD) as located at the following link:  https://mutcd.fhwa.dot.gov/pdfs/2009r1r2/mutcd2009r1r2edition.pdf. Throughout this Bid Solicitation, safety will refer to safety-related set-up for lane closures.



[bookmark: _QUOTE_SUBMISSION_REQUIREMENTS][bookmark: _Toc120526636]QUOTE SUBMISSION REQUIREMENTS

[bookmark: _Toc120526637]QUOTE SUBMISSION 
In order to be considered for award, the Quote must be received electronically by the Division’s Proposal Review Unit, through NJSTART, by the required date and time. 

The date and time of the Quote opening are indicated on the Bid Solicitation cover sheet and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  If the Quote opening deadline has been revised, the new Quote opening deadline will be shown on the posted Bid Amendment and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  Quotes not received prior to the Quote opening deadline shall be rejected.

Quotes will be publicly opened and announced by telephone conference on the date and time of the quote opening. 
(Dial-in phone number: 888-204-5984 / Access code: 2602305)

When submitting a Quote through NJSTART, do not use any symbols (i.e., #, @, $, &, *) in the filename as this may prevent the Quote from being properly uploaded.  Uploaded files must be compatible with Microsoft Office and/or Adobe software applications. DO NOT UPLOAD files with extensions such as .zip, .numbers, or .pages.

When uploading the documents to NJSTART, the Bidder should select the “Confidential” option in NJSTART for attachments on the “Attachments” Tab to request that the documents not be displayed publicly through NJSTART. Marking an attachment as "Confidential" in NJSTART shall not constitute the Bidder's designation of the attachment as exempt from public disclosure under the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know.

[bookmark: _Toc120526638]BIDDER RESPONSIBILITY
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote in response to this Bid Solicitation.  No special consideration will be given after Quotes are opened because of a Bidder’s failure to be knowledgeable as to all of the requirements of this Bid Solicitation.  The State assumes no responsibility and bears no liability for costs incurred by a Bidder in the preparation and submittal of a Quote in response to this Bid Solicitation or any pre-contract award costs incurred.

[bookmark: _Toc120526639]ANNOUNCEMENT OF QUOTE INFORMATION
On the date and time Quotes are due under the Bid Solicitation, all information concerning the Quotes submitted may be publicly announced and shall be available for inspection and copying except otherwise noted:  
A. Information appropriately designated as proprietary and/or confidential in a Bidder’s Quote shall not be available for inspection and copying; and
B. Where negotiation is contemplated, only the names and addresses of the Bidders submitting Quotes will be announced, and the contents of the Quotes shall not be available for inspection and copying until the Notice of Intent to Award is issued by the Director. 

[bookmark: _Toc120526640]QUOTE ERRORS
In accordance with N.J.A.C. 17:12-2.11 “Proposal errors,” a Bidder may withdraw its Quote as described below.

[bookmark: _Toc120526641]QUOTE WITHDRAWAL PRIOR TO QUOTE OPENING
A Bidder may withdraw its Quote submission in NJSTART prior to the Quote opening; however, Bidders should note that while withdrawn NJSTART Quotes remain viewable by the Bidder on its Vendor Profile Homepage, they are removed from the Division’s view and cannot be considered for Contract award. The Bidder may submit a revised Quote as long as the Quote is received prior to the announced date and time for Quote submission. Bidders may refer to the QRG “Submit a Quote” for additional instructions.

[bookmark: _Toc120526642]QUOTE WITHDRAWAL AFTER QUOTE OPENING, BUT PRIOR TO CONTRACT AWARD
If, after the Quote opening, but before Contract award, a Bidder discovers an error in its Quote, the Bidder may make a written request to the Procurement Bureau to withdraw its Quote, or a portion thereof, from consideration for award.  If the Bidder’s request to withdraw is made in good faith, and the State will not be significantly prejudiced by granting the withdrawal of the Quote beyond the loss of the benefit of the bargain to the State of the withdrawing Bidder’s offer, the request shall be granted.  Evidence of the Bidder’s good faith in making this request can be demonstrated by one (1) or more of the following factors: A mistake is so significant that to enforce the Contract resulting from the Quote would be unconscionable; that the mistake relates to a material feature or term of the Contract; and that the mistake occurred notwithstanding the Bidder’s exercise of reasonable care.  After Quote opening, while pursuant to the provisions of this section a Bidder may request to withdraw its Quote and the Director may in his/her discretion allow said Bidder to withdraw it, the Division also may take notice of repeated or unusual requests to withdraw by a Bidder and take those prior requests to withdraw into consideration when evaluating the Bidder’s future Quotes.

The Quote withdrawal request must include the Bid Solicitation Number, Bid Solicitation Title, and the Quote submission date and should be sent to Procurement.Bureau@treas.nj.gov.

If, during a Quote evaluation process, an obvious pricing error made by a potential Contract awardee is found, the Director or his/her designee shall issue written notice to the Bidder.  The Bidder will have up to five (5) business days after receipt of the notice to confirm its pricing.  If the Bidder fails to respond, its Quote shall be considered withdrawn, and no further consideration shall be given to it.

[bookmark: _Toc120526643]JOINT VENTURE
If a Joint Venture is submitting a Quote, the agreement between the parties relating to such Joint Venture should be submitted with the Joint Venture’s Quote.  Authorized signatories from each party comprising the Joint Venture must sign the Offer and Acceptance Page.  Each party to the Joint Venture must individually complete and comply with all the forms and certification requirements in Bid Solicitation Section 3 – Quote Submission Requirements. 

[bookmark: _Toc120526644]SMALL BUSINESS SET-ASIDE CONTRACTS
Pursuant to the provisions of N.J.S.A. 52:32-17 et seq. and N.J.A.C. 17:13 et seq. this is a partial Set-Aside Contract for Category I, II, or III for Small Businesses.  

The State intends to award to multiple Contractors per Category, with two (2)one (1) awards set-aside for Small Business Enterprises (SBE) for each Category for each Region. Should an SBE business not bid or be responsive within a Category, the State may award to the next qualifying Bidder, including non-SBE classified Bidders.

To be considered as a Small Business Enterprise, the Bidder must be registered as a qualified small business with the Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit, by the date the Quote is received and opened.   

A Bidder should verify its Small, Minority, Veteran, and Women Owned Business Certification status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Bidder’s Small, Minority, Veteran, and Women Owned Business Certification status, NJSTART provides a link to take corrective action.

If the Bidder has previously registered or been certified as a Small Business Enterprise, the Bidder should ensure it is currently registered and that its registration is active with the Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit, prior to the quote opening date, to be eligible for award.  The Bidder should ensure that it has completed the annual verification, if required.

Information, registration requirements and application are available at https://www.nj.gov/treasury/revenue/ucs.shtml.

[bookmark: _Toc120526645]DISABLED VETERANS’ BUSINESS SET-ASIDE CONTRACT 
Not applicable to this procurement.

[bookmark: _Toc120526646]BID SECURITY
Not applicable to this procurement.

[bookmark: _Toc120526647]BIDDER ADDITIONAL TERMS SUBMITTED WITH THE QUOTE
A Bidder may submit additional terms as part of its Quote.  Additional terms are Bidder-proposed terms or conditions that do not conflict with the scope of work required in this Bid Solicitation, the terms and conditions of this Bid Solicitation, or the State of New Jersey Standard Terms and Conditions.  Bidder proposed terms or conditions that conflict with those contained in the State of New Jersey Standard Terms and Conditions will render a Quote non-responsive.  It is incumbent upon the Bidder to identify and remove its conflicting proposed terms and conditions prior to Quote submission.  

Quotes including Bidder proposed additional terms may be accepted, rejected, or negotiated, in whole or in part, at the State’s sole discretion. 

If Bidder intends to propose terms and conditions that conflict with the State of New Jersey Standard Terms and Conditions, those Bidder proposed terms and conditions shall only be considered if submitted and agreed to pursuant to the electronic question and answer procedure.  Bidders shall not submit exceptions or modifications as part of the Quote or on the “Terms and Conditions” Tab through NJSTART. 

[bookmark: _Toc120526648]QUOTE CONTENT
The Quote should be submitted with the attachments organized in following manner:
· Forms
· Technical Quote
· State-Supplied Price Sheet

A Bidder should not password protect any submitted documents. Use of URLs in a Quote should be kept to a minimum and shall not be used to satisfy any material term of a Bid Solicitation. If a preprinted or other document included as part of the Quote contains a URL, a printed copy of the information should be provided and will be considered as part of the Quote. 

[bookmark: _Toc120526649]FORMS, REGISTRATIONS AND CERTIFICATIONS TO BE SUBMITTED WITH QUOTE 
A Bidder is required to complete and submit the following forms.  As an alternative to uploading certain forms with the submitted Quote, a Bidder may complete the appropriate several certifications electronically in NJSTART on the “Terms and Categories” Tab within the Vendor Profile.  Those forms that may be completed on the NJSTART “Terms and Categories” Tab are noted below. Additionally, a Bidder may attach completed forms to the Vendor Profile.  Refer to QRGs “Vendor Forms” and “Attaching Files” for additional instructions.  VENDOR QUICK REFERENCE GUIDES

OFFER AND ACCEPTANCE PAGE 
The Bidder should complete and submit the Offer and Acceptance Page with the Quote.  The Offer and Acceptance Page must be signed by an authorized representative of the Bidder.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.    

OWNERSHIP DISCLOSURE FORM 
Pursuant to N.J.S.A. 52:25-24.2, in the event the Bidder is a corporation, partnership or limited liability company, the Bidder must disclose all 10% or greater owners by (a) completing and submitting the Ownership Disclosure Form with the Quote; (b) if the Bidder has submitted a signed and accurate Ownership Disclosure Form dated and received no more than six (6) months prior to the Quote submission deadline for this procurement, the Division may rely upon that form; however, if there has been a change in ownership within the last six (6) months, a new Ownership Disclosure Form must be completed, signed and submitted with the Quote; or, (c) a Bidder with any direct or indirect parent entity which is publicly traded may submit the name and address of each publicly traded entity and the name and address of each person that holds a 10 percent or greater beneficial interest in the publicly traded entity as of the last annual filing with the federal Securities and Exchange Commission or the foreign equivalent, and, if there is any person that holds a 10 percent or greater beneficial interest, also shall submit links to the websites containing the last annual filings with the federal Securities and Exchange Commission or the foreign equivalent and the relevant page numbers of the filings that contain the information on each person that holds a 10 percent or greater beneficial interest. N.J.S.A. 52:25-24.2.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab. 

A Bidder’s failure to submit the information required by N.J.S.A. 52:25-24.2 will result in the rejection of the Quote as non-responsive and preclude the award of a Contract to said Bidder.

  DISCLOSURE OF INVESTMENT ACTIVITIES IN IRAN FORM
The Bidder should submit Disclosure of Investment Activities in Iran form to certify that, pursuant to N.J.S.A. 52:32-58, neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates (as defined in N.J.S.A. 52:32-56(e)(3)), is listed on the Department of the Treasury’s List of Persons or Entities Engaging in Prohibited Investment Activities in Iran and that neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates, is involved in any of the investment activities set forth in N.J.S.A. 52:32-56(f).  If the Bidder is unable to so certify, the Bidder shall provide a detailed and precise description of such activities as directed on the form.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab. 

DISCLOSURE OF INVESTIGATIONS AND OTHER ACTIONS INVOLVING BIDDER FORM
The Bidder should submit the Disclosure of Investigations and Other Actions Involving Bidder Form,  with its Quote, to provide a detailed description of any investigation, litigation, including administrative complaints or other administrative proceedings, involving any public sector clients during the past five (5) years, including the nature and status of the investigation, and, for any litigation, the caption of the action, a brief description of the action, the date of inception, current status, and, if applicable, disposition.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab. 

MACBRIDE PRINCIPLES FORM
The Bidder should submit the MacBride Principles Form.  Pursuant to N.J.S.A. 52:34-12.2, a Bidder is required to certify  that it either has no ongoing business activities in Northern Ireland and does not maintain a physical presence therein or that it will take lawful steps in good faith to conduct any business operations it has in Northern Ireland in accordance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of their compliance with those principles.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab.

SERVICE PERFORMANCE WITHIN THE UNITED STATES
The Bidder should submit a completed Source Disclosure Form. Pursuant to N.J.S.A. 52:34-13.2, all Contracts primarily for services shall be performed within the United States. If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive. 

CONFIDENTIALITY/COMMITMENT TO DEFEND
Pursuant to the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know, Quotes can be released to the public in accordance with N.J.A.C. 17:12-1.2(b) and (c).  

The Bidder should submit a completed and signed Confidentiality /Commitment to Defend Form with the Quote.  In the event that the Bidder does not submit the Confidentiality form with the Quote, the State reserves the right to request that the Bidder submit the form after Quote submission.

After the opening of sealed Quotes, all information submitted by a Bidder in response to a Bid Solicitation is considered public information notwithstanding any disclaimers to the contrary submitted by a Bidder.  Proprietary, financial, security and confidential information may be exempt from public disclosure by OPRA and/or the common law when the Bidder has a good faith, legal/factual basis for such assertion. 

When the Bid Solicitation contains a negotiation component, the Quote will not be subject to public disclosure until a notice of intent to award a Contract is announced. 

As part of its Quote, a Bidder may request that portions of the Quote be exempt from public disclosure under OPRA and/or the common law. The Bidder must provide a detailed statement clearly identifying those sections of the Quote that it claims are exempt from production, and the legal and factual basis that supports said exemption(s) as a matter of law.  The State will not honor any attempts by a Bidder to designate its price sheet, price list/catalog, and/or the entire Quote as proprietary and/or confidential, and/or to claim copyright protection for its entire Quote.  If the State does not agree with a Bidder’s designation of proprietary and/or confidential information, the State will use commercially reasonable efforts to advise the Bidder. Copyright law does not prohibit access to a record which is otherwise available under OPRA.

The State reserves the right to make the determination as to what to disclose in response to an OPRA request.  Any information that the State determines to be exempt from disclosure under OPRA will be redacted.  

In the event of any challenge to the Bidder’s assertion of confidentiality that is contrary to the State’s determination of confidentiality, the Bidder shall be solely responsible for defending its designation, but in doing so, all costs and expenses associated therewith shall be the responsibility of the Bidder. The State assumes no such responsibility or liability.  

In order not to delay consideration of the Quote or the State’s response to a request for documents, the State requires that Bidder respond to any request regarding confidentiality markings within the timeframe designated in the State’s correspondence regarding confidentiality.  If no response is received by the designated date and time, the State will be permitted to release a copy of the Quote with the State making the determination regarding what may be proprietary or confidential.

SUBCONTRACTOR UTILIZATION PLAN
Bidders intending to use Subcontractor(s) shall list all subcontractors on the Subcontractor Utilization Plan form or may list the Subcontractor(s) on the “Subcontractor” Tab in NJSTART. 

For a Quote that does NOT include the use of any Subcontractors, the Bidder is automatically certifying that, if selected for an award, the Bidder will be performing all work required by the Contract. 

If it becomes necessary for the Contractor to substitute a Subcontractor, add a Subcontractor, or substitute its own staff for a Subcontractor, the Contractor will identify the proposed new Subcontractor or staff member(s) and the work to be performed.  The Contractor shall forward a written request to substitute or add a Subcontractor or to substitute its own staff for a Subcontractor to the State Contract Manager for consideration.    The Contractor must provide a completed Subcontractor Utilization Plan, a detailed justification documenting the necessity for the substitution or addition, and resumes of its proposed replacement staff or of the proposed Subcontractor’s management, supervisory, and other key personnel that demonstrate knowledge, ability and experience relevant to that part of the work which the Subcontractor is to undertake. The qualifications and experience of the replacement(s) must equal or exceed those of similar personnel proposed by the Contractor in its Quote.  The State Contract Manager will forward the request to the Director for approval.  

NOTE: No substituted or additional Subcontractors are authorized to begin work until the Contractor has received written approval from the Director.

SMALL BUSINESS AND/OR DISABLED VETERANS’ BUSINESS SUBCONTRACTING SET-ASIDE CONTRACT 
Not applicable to this procurement.

[bookmark: _Toc120526658]PAY TO PLAY PROHIBITIONS
Pursuant to N.J.S.A. 19:44A-20.13 et seq. (P.L. 2005, c. 51), the State shall not enter into a Contract to procure services or any material, supplies or equipment, or to acquire, sell, or lease any land or building from any Business Entity, where the value of the transaction exceeds $17,500, if that Business Entity has solicited or made any contribution of money, or pledge of contribution, including in-kind contributions, to a candidate committee and/or election fund of any candidate for or holder of the public office of Governor or Lieutenant Governor, to any State, county, municipal political party committee, or to any legislative leadership committee during certain specified time periods.  

Prior to awarding any Contract or agreement to any Business Entity, the Business Entity proposed as the intended Contractor of the Contract shall submit the Two-Year Chapter 51/Executive Order 117 Vendor Certification and Disclosure of Political Contributions form, available on the Division’s website Forms page, certifying that no contributions prohibited by either Chapter 51 or Executive Order No. 117 have been made by the Business Entity and reporting all qualifying contributions made by the Business Entity or any person or entity whose contributions are attributable to the Business Entity.  Failure to submit the required forms will preclude award of a Contract under this Bid Solicitation.

Further, the Contractor is required, on a continuing basis, to report any contributions it makes during the term of the Contract, and any extension(s) thereof, at the time any such contribution is made. 

AFFIRMATIVE ACTION
The intended Contractor and its named Subcontractor(s) must submit a copy of a New Jersey Certificate of Employee Information Report, or a copy of Federal Letter of Approval verifying it is operating under a federally approved or sanctioned Affirmative Action program.  If the Contractor and/or its named Subcontractor(s) are not in possession of either a New Jersey Certificate of Employee Information Report or a Federal Letter of Approval, it/they must complete and submit the Affirmative Action Employee Information Report (AA-302).  Information, instruction and the application are available at https://www.state.nj.us/treasury/contract_compliance/index.shtml.

[bookmark: _Toc120526660]STATE OF NEW JERSEY SECURITY DUE DILIGENCE THIRD-PARTY INFORMATION SECURITY QUESTIONNAIRE 
The Bidder shall complete and submit the State of New Jersey Security Due Diligence Third-Party Information Security Questionnaire (Questionnaire) with its Quote. This Questionnaire is designed to provide the State with an overview of the Bidder’s security and privacy controls to ensure that the Bidder will (1) meet the State of New Jersey’s objectives as outlined and documented in the Statewide Information Security Manual; and (2) comply with the State’s security requirements as outlined in Section 6 – Data Security Requirements – Contractor Responsibility.  

The State has executed a Confidentiality/Non-Disclosure Agreement which is attached to the Questionnaire.  The Bidder must countersign the Confidentiality/Non-Disclosure Agreement and include it with its submitted Questionnaire.  No amendments to Confidentiality/Non-Disclosure Agreement are permitted.  

To the extent permissible under OPRA, the New Jersey common law right to know, and any other lawful document request or subpoena, the completed Questionnaire and supplemental documentation provided by the Bidder will be kept confidential and not shared with the public or other Bidders.Not applicable to this procurement.

BUSINESS REGISTRATION
[bookmark: OLE_LINK1]In accordance with N.J.S.A. 52:32-44(b), a Bidder and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Contract.  A Bidder should verify its Business Registration Certification Active status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Bidder’s Business Registration Certification Active status, NJSTART provides a link to take corrective action. 

[bookmark: _Toc120526662][bookmark: _Toc99544656]3.13.14	Certification of Non-Involvement in Prohibited Activities in Russia or Belarus Pursuant to P.L.2022, c3CERTIFICATON REGARDING PROHIBITED ACTIVITIES WITH RUSSIA OR BELARUS
The Bidder should submit Certification of Non-Involvement in Prohibited Activities in Russia or Belarus Pursuant to P.L.2022, c.3 (Attachment 2).  Pursuant to P.L.2022, c.3, a person or entity seeking to enter into or renew a contract for the provision of goods or services shall certify that it is not Engaging in Prohibited Activities in Russia or Belarus as defined by P.L.2022, c.3, sec. 1(c).  If the Contractor is unable to so certify, the Contractor shall provide a detailed and precise description of such activities. 

If you certify that the Bidder is engaged in activities prohibited by P.L.2022, c.3, the Bidder shall have 90 days to cease engaging in any prohibited activities and on or before the 90th day after this certification, shall provide an updated certification.  If the Bidder does not provide the updated certification or at that time cannot certify on behalf of the entity that it is not engaged in prohibited activities, the State shall not award the business entity any contracts, renew any contracts, and shall be required to terminate any contract(s) the business entity holds with the State that were issued on or after the effective date of P.L.2022, c.3. 
The Bidder should submit the Disclosure of Prohibited Activities in Russia / Belarus Form.  Pursuant to P.L.2022, c. 3, a person or entity seeking to enter into or renew a contract for the provision of goods or services shall certify that it is not Engaging in Prohibited Activities in Russia or Belarus as defined by P.L.2002, c. 3, sec. 1(e).    If the Contractor is unable to so certify, the Contractor shall provide a detailed and precise description of such activities. 

If you certify that the bidder is engaged in activities prohibited by P.L. 2022, c. 3, the bidder shall have 90 days to cease engaging in any prohibited activities and on or before the 90th day after this certification, shall provide an updated certification.  If the bidder does not provide the updated certification or at that time cannot certify on behalf of the entity that it is not engaged in prohibited activities, the State shall not award the business entity any contracts, renew any contracts, and shall be required to terminate any contract(s) the business entity holds with the State that were issued on or after the effective date of P.L. 2022, c. 3. 

[bookmark: _Toc120526663]TECHNICAL QUOTE 
The Bidder shall describe its approach and plans for accomplishing the work outlined in the Scope of Work.  The Bidder must set forth its understanding of the requirements of this Bid Solicitation and its approach to successfully complete the Contract. 

[bookmark: _Toc120526664]BIDDER QUOTE OVERVIEW FORM
The Bidder should submit the Bidder Quote Overview Form with its Quote. The Bidder should complete all of the information requested on the form, so that the State is able to evaluate the Bidder’s ability to complete the Scope of Work.  The Bidder’s responses to the questions on the form should demonstrate to the State that the Bidder’s plans and approach to complete the Scope of Work are realistic, attainable, appropriate, and that the Bidder’s Quote will lead to the successful completion of the tasks required.

[bookmark: _Toc120526665]BIDDER DATA SHEET/FORM
The Bidder should submit the Bidder Data Sheet with its Quote.  The Bidder Data Sheet will be used to evaluate the Bidder’s ability to complete the Scope of Work.  

The Bidder should provide in its response to Part I of the Bidder Data Sheet all relevant information regarding its experience in successfully completing contracts of a similar size and scope to the work required by this Bid Solicitation.  

The Bidder must provide, in Part II of the Bidder Data Sheet, details of any negative actions taken by other contracting entities against it in the course of performing these projects including, but not limited to, receipt of letters of potential default, default, cure notices, termination of services for cause, or other similar notifications/processes.  Additionally, the Bidder should provide details, including any negative audits, reports, or findings by any governmental agency for which the Bidder is/was the contractor on any contracts of similar scope.  In the event a Bidder neglects to include this information in its Quote, the Bidder’s omission of necessary disclosure information may be cause for rejection of the Bidder’s Quote by the State.

If proposing to use a Subcontractor, the Bidder should provide as an attachment to the Bidder Data Sheet documented experience to demonstrate that each Subcontractor has successfully performed work on contracts of a similar size and scope to the work that the Subcontractor is designated to perform in the Bidder’s Quote.  The Bidder must provide a detailed description of services to be provided by each Subcontractor.  

[bookmark: _Toc120526666]FINANCIAL CAPABILITY OF THE BIDDER
The Bidder should provide sufficient financial information to enable the State to assess the financial strength and creditworthiness of the Bidder and its ability to undertake and successfully complete the Contract.  In order to provide the State with the ability to evaluate the Bidder’s financial capacity and capability to undertake and successfully complete the Contract, the Bidder should submit the following:
A. For publicly traded companies the Bidder should provide copies or the electronic location of the annual reports filed for the two most recent years; or
B. For privately held companies the Bidder should provide the certified financial statement (audited or reviewed) in accordance with applicable standards by an independent Certified Public Accountant which include aincluding a balance sheet, income statement, and statement of cash flow, and all applicable notes for the most recent calendar year or the Bidder’s most recent fiscal year. 

If the information is not supplied with the Quote, the State may still require the Bidder to submit it.  If the Bidder fails to comply with the request within seven (7) business days, the State may deem the Quote non-responsive.

A Bidder may designate specific financial information as not subject to disclosure when the Bidder has a good faith legal/factual basis for such assertion.  The State reserves the right to make the determination to accept the assertion and will so advise the Bidder.A Bidder may designate specific financial information as not subject to disclosure when the Bidder has a good faith legal/factual basis for such assertion.  The State reserves the right to make the determination to accept the assertion and shall so advise the Bidder.

[bookmark: _Toc112919790][bookmark: _Toc120526667]PUBLIC WORKS CONTRACTOR REGISTRATION
At the time of the Quote due date, the Bidder and Subcontractors performing public work as defined in N.J.S.A. 34:11-56.26 must be registered in accordance with the Public Works Contractor Registration Act (PWCRA), N.J.S.A. 34:11-56.48 et seq.  This registration is required for all trade categories required to perform work as listed herein.

Questions regarding Public Works Contractor Registration should be addressed to:

Contractor Registration
New Jersey Department of Labor and Workforce Development Division of Wage and Hour Compliance
PO Bo 369 Trenton, NJ 08625-0389
Tel. 609-292-9464
Fax: 609-633-8591

For additional information, please reference the following web site:  https://www.nj.gov/labor/wagehour/regperm/pw_cont_reg.html.

NOTE:	 All Bidders and Subcontractors performing public work must be registered at the time of Bid Opening. The Bidder should provide proof of registration ON THE DATE OF BID OPENING.

[bookmark: _Toc120526668]STATE-SUPPLIED PRICE SHEET INSTRUCTIONS
Bidders must submit their pricing using the State-Supplied Price Sheet(s) accompanying this Bid Solicitation, and located on the “Attachments Tab.” This Bid Solicitation includes the following three (3) State-Supplied Price Sheets:
A. North Region;
B. Central Region; and 
C. South Region.

Any changes or alterations to the State-Supplied Price Sheet may result in the Bidder’s Quote being deemed non-responsive.

The Bidder may submit pricing for one (1) or multiple Categories in addition to Category IV – Preventative Maintenance, but must submit pricing for all Price Lines in a Category to be considered for an award in that Category. Failure to submit pricing for all Price Lines in a Category will result in the Bidder’s Quote deemed non-responsive for that Category only. The Bidder may submit pricing for multiple Categories and Regions. The Bidder must submit pricing for all Price Lines for at least one (1) Category to be considered an award.

All Categories and Types are listed below. All Regions contain the same Categories and Types:
A. Category I – Standard chain link fencing:
1. Type I – Aluminum-coated and vinyl-clad chain link fence and installation; and
2. Type II – Specialty fencing and installation.

B. Category II – Additional fencing: 
1. Type I – Ornamental metal fence;
2. Type II – Vinyl fence including plastic snow and PVC type;
3. Type III – Wooden fence;
4. Type IV – Motorized automatic fence gates; and
5. Type V – Steel barricade.

C. Category III – Emergency repairs to security fencing:
1. Type I – Standard fabric;
2. Type II – Anti-climb security fencing fabric;
3. Type III – Framing; 
4. Type IV – Fitting and accessories; and
5. Type V – Barbed tape (razor ribbon).

D. Category IV – Preventive Maintenance

The Bidder must provide pricing for Category IV - Preventive Maintenance Services on the Region(s) it intends to service. Failure to submit pricing for all Price Lines for Category IV – Preventative Maintenance may result in the Bidder’s Quote being deemed non-responsive. The Bidder cannot bid solely on Category IV – Preventative Maintenance. Preventative Maintenance will apply to all Categories, including its Types, and each Category’s respective Region. See Section 4.10, Preventative Maintenance, for more details. 

There are no all-inclusive Price Lines within this Bid Solicitation or Price Sheets.
The cost of installation services shall be included with the cost of both material and installation for Categories I, II, and III.
Lane closures and aAdditional roadway lane closures applies to all Types in Category I and Category II. The Bidder must submit pricing for lane closures and additional lane closures to be considered for an award for Category I and Category II. Lane closures shall be inclusive of safety-related set-up. 
Lane closures inclusive of safety-related set-up are found in the Price Lines below:
Additional Lane closures are found in the Price Lines below:
A. North Region – Price Lines #11, 2, 111, and 112;
B. Central Region – Price Line #208188, 189, 298, and 299; and
C. South Region – Price Line #415375, 376, 485, and 486.

Under Category I, Type I, site clearing shall be included with fence construction. 
Under Category I, Type I, Aluminum Coated Chain Link Fence, the Bidder’s unit price submitted shall be for the entire finished width of the gate (single leaf or double leafs). 
Gate items for the below Price Lines shall be inclusive of materials and installation:
A. North Region – Price Lines #3250 to -81#63; 
B. Central Region – Price Lines #219 to 57-288#250; and
C. South Region – Price Lines #406 to 64#-495437.

Under Category I, the removal of any existing fence shall be included in the cost for fabric-only items. Fabric items are found in the Price Lines below: 
A. North Region – Price Lines #1421 to #3621; 
B. Central Region – Price Lines #20128 to #243208; and 
C. South Region – Price Lines #435 388 to #450395.

The cost of both materials and installation shall be included in barbed wire installation items. Barbed wire installation items are found in the Price Lines below: 
A. North Region – Price Lines #88 and #8969 and #70;
B. Central Region – Price Lines #295 and #296256 and #257; and
C. South Region – Price Lines #502 and #503443 and #444.

The cost of removal and disposal shall be included in barbed wire removal item. Barbed wire removal items are found in the Price Lines below: 
A. North Region – Price Lines #90 and #9171 and #72; 
B. Central Region – Price Lines #297 and #298258 and #259; and
C. South Region – Price Lines #504 and #505445 and #446.

The cost of non-NJDOC emergency services shall be on a per site basis, per occurrence. Non-NJDOC emergency service requests are found in the Price Lines below:
A. North Region – Price Lines #2 and 1303 and #113; 
B. Central Region – Price Lines #209 and 337190 and #300; and
C. South Region – Price Lines #416 and 544377 and #487.

Under Category I, the percentage markup for privacy slats shall not exceed 8%. Privacy slats are found in the Price Lines below:
A. North Region – Price Line #83;
B. Central Region – Price Line #270; and
C. South Region – Price Line #457.
Under Categories II and IVand IV, mark-ups on parts cost shall not exceed the awarded markup percentage, which shall not exceed 8%. Price Lines in Categories II and IV and IVwhere markup shall not exceed 8% are found below:
A. North Region – Price Lines #131, #132, #135, #136, #139, #140, #144, #146, and #207114, 115, 117, 118, 120, 121, 124, 126, and 187.  
B. Central Region – Price Lines #338, #339, #342, #343, #346, #347, #351, #353, and #414301, 302, 304, 305, 307, 308, 311, 313, and 374; and 
C. South Region – Price Lines #545, #546, #549, #550, #552, #553, #557, #559, and #620488, 489, 491, 492, 494, 495, 498, 500, and 561. 

Where the State-Supplied Price Sheet includes an estimate quantity column, Bidders are advised that estimated quantities may vary throughout the Contract term resulting from this Bid Solicitation.  There is no guaranteed minimum or maximum volume for these price lines. 

[bookmark: _Toc120526669]USE OF “NO BID” VERSUS “NO CHARGE” ON THE STATE-SUPPLIED PRICE SHEET
All price lines must be filled out in accordance with the instructions above.  If the Bidder is not submitting a price for an item on a price line, the Bidder must indicate “No Bid” on the State-Supplied Price Sheet accompanying this Bid Solicitation. If the Bidder will supply an item on a price line free of charge, the Bidder must indicate “No Charge” on the State-Supplied Price Sheet accompanying this Bid Solicitation.  The use of any other identifier may result in the Bidder’s Quote being deemed non-responsive.

[bookmark: _Toc120526670]ORAL PRESENTATIONS
Not applicable to this procurement.


[bookmark: _Toc120526671]SCOPE OF WORK
[bookmark: _Toc400531507][bookmark: _Toc428533978][bookmark: _Toc32310703]The Contractor shall be responsible for providing all services related to fencing construction for chain link, security, emergency, and various additional fencings, including but not limited to the following functions:

A. Installation of fencing;
B. Removal of fencing; 
C. Safety-related set-ups for lane closures;
D. Preventative maintenance;
E. Site clearing; and
F. Providing emergency repairs.

The Contractor shall perform all services in accordance with the fencing specifications set forth within this Bid Solicitation.

[bookmark: _Toc112919795][bookmark: _Toc120526672]NJDOT STANDARD CONSTRUCTION DETAILS
All materials and construction / installation shall comply with the NJDOT Standard Specifications for Road and Bridge Construction 2019 and the NJDOT Standard Construction Details 2016 unless otherwise stated in this Bid Solicitation. 
Any references to the Standard Construction Details 2016 and Standard Specifications for Road and Bridge Construction 2019 are additional requirements that Contractors must comply with as part of these specifications.
The Contractor shall refer to the following for all references to the Standard Construction Details 2016: 
https://www.state.nj.us/transportation/eng/CADD/v8/pdf/StandConstDetails.pdf. 
For needed drawings and plans and references to the Standard Specifications for Road and Bridge Construction 2019, the Contractor  shall refer to the following: https://www.state.nj.us/transportation/eng/specs/2019/pdf/StandSpecRoadBridge201920200114.pdf. 
The Contractor  shall refer to the following link for other drawings and plans https://www.state.nj.us/transportation/eng/CADD/v8/stdconsdtls.shtml.
[bookmark: _Toc112919796][bookmark: _Toc120526673]REGIONS TO BE SERVED
The State has been divided into the following three (3) regions. The breakdown of the three (3) regions, and counties included in each region, are as follows:
	North Region
	Central Region
	South Region

	Bergen
	Hunterdon
	Atlantic

	Essex
	Mercer
	Burlington

	Hudson
	Middlesex
	Camden

	Sussex
	Monmouth
	Cape May

	Morris
	Ocean
	Cumberland

	Passaic
	Somerset
	Gloucester

	Union
	Warren (south of Route 57)
	Salem

	Warren (north of Route 57)
	
	



[bookmark: _Toc109830335][bookmark: _Toc112919797][bookmark: _Toc120526674]METHOD OF ENGAGEMENT
Using Agencies will obtain written price quotations from all awarded Contractors in the Region of service, for the installation and/or repair service that best meets the Using Agency’s needs. 
Using Agencies will consider the following when selecting the Contractor:
D. The most cost-effective quote received; 
E. Quoted timeframe for the repair; and
F. The Contractor’s current backlog of pending and/or unfinished repair jobs.

All price quotations shall be received within five (5) business days of the Using Agency’s request, with exception to emergencies, which shall be provided within 48 hours. Emergency calls are those service calls where the work consists of correcting failures that constitute an immediate danger to public safety and property. Please see Sections 4.9.2, Emergency Services – NJDOC, and Section 4.11, Emergency Services – Non-NJDOC, for more details.
All price quotes will reflect the total hours, if applicable, and the cost for labor per hour, if applicable. The quote shall be a “Not-to-Exceed” estimate with an option for the Using Agency to reduce the final amount due to the actual hours worked.  A Not-to-Exceed estimate is a quoted estimate where the amount to be paid cannot surpass the quoted estimate. No additional work shall be performed or paid for without the prior written approval of the designated Using Agency main point of contact.
The Contractor shall begin a project within ten (10) business days after request of a job by the NJDOT or any other Using Agency. In the event the Contractor is unable to begin the job within ten (10) business days after notification, the requesting Using Agency will consider the following when selecting the Contractor:
G. The next most cost-effective quote received; 
H. Quoted timeframe for the repair; and
I. The Contractor’s current backlog of pending and/or unfinished repair jobs.

After award, inquiries regarding the technical aspects of any NJDOT purchases shall be directed to the SCM. Inquiries regarding the technical aspect of non-NJDOT purchases shall be directed to the respective Using Agency’s main point of contact, which will be determined by the Using Agency.
[bookmark: _Toc112919798][bookmark: _Toc120526675]NJDOT SITES AND COMMUNICATION
[bookmark: _Hlk39152871][bookmark: _Hlk39152925]All Blanket P.O. design, supervision, and inspection for NJDOT site(s) will be assigned to the NJDOT Regional Engineer. For non-DOT projects, Blanket P.O. design, supervision, and inspection for the respective Using Agency locations will be determined by the Using Agency’s main point of contact. The Contractor shall direct all inquiries and correspondence to the designated representative having responsibility for a specific region or project as listed in this Bid Solicitation.
Unless otherwise directed, the Contractor shall forward all inquiries and correspondence with NJDOT to the DOT Regional Engineer. The Contractor shall forward inquiries and correspondence with non-NJDOT Using Agencies to the respective Using Agency’s main point of contact. A clear copy of each communication shall be sent to the DOT Regional Engineer or each respective Using Agency’s main point of contact.
All inspections and certifications of materials and procedures affecting materials will be reviewed by the NJDOT Regional Engineer or Using Agency main point of contact.
[bookmark: _Toc112919799][bookmark: _Toc120526676]DESCRIPTION OF CATEGORIES I, II, III, AND IV
Each Region consists of four (4) separate Categories: 
E. Category I – Standard chain link fencing:
1. Type I – Aluminum-coated and vinyl-clad chain link fence and installation; and
2. Type II – Specialty fencing and installation.

F. Category II – Additional fencing: 
1. Type I – Ornamental metal fence;
2. Type II – Vinyl fence including plastic snow and PVC type;
3. Type III – Wooden fence;
4. Type IV – Motorized automatic fence gates; and
5. Type V – Steel barricade.

G. Category III – Emergency repairs to security fencing:
1. Type I – Standard fabric;
2. Type II – Anti-climb security fencing fabric;
3. Type III – Framing; 
4. Type IV – Fitting and accessories; and
5. Type V – Barbed tape (razor ribbon).

H. Category IV – Preventive Maintenance

[bookmark: _Toc112919800][bookmark: _Toc120526677]CATEGORY I – STANDARD CHAIN LINK FENCING 
Under Category I, the Contractor shall provide or perform services to aluminum-coated roadway fencing and vinyl-coated chain link fencing including, but not limited to: 
A. Material;
B. Replacement and installation of fencing;
C. Installation of galvanized and vinyl-coated line, corner, and gate fence posts;
D. Resetting of galvanized and vinyl-coated line, corner, and gate fence posts;
E. Drive anchors;
F. Barbed wire installation and removal; and
G. Drilling through solid rock and fabric fasteners for projects less than 500 feet, and projects 500 feet and over.

Under Category I, the cost of fencing removal shall not be included in the cost, with exception to Fabric Only Fence Chain Link Items, specified in Section 4.5.6.1, Fence and Chain Link Install and Replace – Fabric Only. 
The cost of lane closures and additional lane closures, inclusive of safety-related set-up, shall apply to all types in Category I.
Under Category I, the cost of installation services shall include the cost of both materials and installation, unless otherwise specified. Under Category I, Type I, the cost of site clearing shall be included with the cost of fence construction. 

[bookmark: _Toc109830341][bookmark: _Toc112919801][bookmark: _Toc120526678]MATERIALS
Materials for chain link fence for Category I – Type I and II must conform to the current requirements specified in the American Association of State Highway and Transportation Officials (AASHTO) Designation M181.
[bookmark: _Toc112919802][bookmark: _Toc120526679]ALUMINUM FOR COATING
Both Types I & II Fencing for Category I must conform to the requirements specified in American Society for Testing and Materials (ASTM) Specification A491-63T. Weight of coating shall be determined in accordance with current ASTM Specification A428. The American Standard Test Method is included and part of ASTM specifications. 
[bookmark: _Toc112919803][bookmark: _Toc120526680]CARRIAGE BOLTS WITH ELASTIC NUTS
Steel bolts shall conform to ASTM A307. Nuts and washers shall conform to ASTM A194 or ASTM A563.
[bookmark: _Toc112919804][bookmark: _Toc120526681]MEDIAN BARRIER CHAIN LINK FENCE
Median barrier chain link fence end assembly with breakaway posts shall be constructed per Attachment 4 - Exhibit 2 - Chain Link Fence Standard Detail. All median barrier components shall conform to the General notes in Attachment 4 - Exhibit 2 - Chain Link Fence Standard Detail. Median Barrier Chain Link Fence Items for square and round posts shall follow their respective details in Attachment 4 - Exhibit 2 - Chain Link Fence Standard Detail. 
[bookmark: _Toc112919805][bookmark: _Toc120526682]NON-VEGETATIVE SURFACE
All non-vegetative surface, polyester matting shall be U-Teck “WeedEnder” or an approved equal by a Regional Engineer, including all anchor pins, fence post templates, and adhesives. Non-vegetative asphalt surfaces 4’’ thick shall be excavated, constructed, and delivered according to Section 608.03.01 of the NJDOT Standard Specifications for Road and Bridge Construction 2019. The Contractor shall also provide weed control for non-vegetative asphalt surfaces 4’’ thick, as specified in Section 608.03.06 of the NJDOT Standard Specifications for Road and Bridge Construction 2019. 
If requested by the Using Agency, the Contractor shall provide the brand and model number for Non-Vegetative items.
[bookmark: _Toc112919806][bookmark: _Toc120526683]FENCE, CHAIN LINK, MATERIAL, AND INSTALLATION
[bookmark: _Hlk92878350]Under Category I, the Contractor shall provide or perform services to aluminum-coated and vinyl-coated fencing including, but not limited to:
A. Installation;
B. Providing all incidental hardware including, but not limited to, tension wires, stretcher bars, ring ties, and fabric;
C. Line posts and end posts in the installation; and 
D. Corner and gateposts shall be separate.

FENCE AND CHAIN LINK INSTALL AND REPLACE – FABRIC ONLY
[bookmark: _Hlk92879447]Under Category I, the Contractor shall service aluminum-coated and vinyl-coated fencing, including, but not limited to, installation, fabric, and all incidental hardware, tension wires, stretcher bars, and ring ties. The removal of any existing fence shall be included in the cost for fabric-only items. Fabric items are found in the Price Lines below: 
A. North Region – Price Lines #21 to #3614 to 21;
B. Central Region – Price Lines #228 to #243201 to 208; and 
C. South Region – Price Lines #435 to #450388 to 395.

BARBED WIRE
[bookmark: _Hlk92880836][bookmark: _Hlk92881164][bookmark: _Hlk92880999]Under Category I, the Contractor shall provide installation and service wire, brackets, angled masts, and all hardware to complete the installation of barbed wire. The installation of barbed wire shall include, but not be limited to, installation, the wire, brackets, angled masts, and all hardware needed to complete the installation. The removal of barbed wire shall include the removal and disposal of barbed wire fences and all of its components. Barbed wire will be measured by the actual number of linear feet of wire installed. 
The cost of both materials and installation shall be included in barbed wire installation items. Barbed wire installation items are found in the Price Lines below: 
A. North Region – Price Lines #88 and #8969 and 70; 
B. Central Region – Price Lines #295 and #296256 and 257; and
C. South Region – Price Lines #502 and #503443 and 444.

The cost of removal and disposal shall be included in barbed wire removal item. Barbed wire removal items are found in the Price Lines below: 
A. North Region – Price Lines #90 and #9171 and 72; 
B. Central Region – Price Lines #297 and #298258 and 259; and
C. South Region – Price Lines ##505 and #505445 and 446.

[bookmark: _Toc112919807][bookmark: _Toc120526684]CATEGORY I – TYPE I STANDARD NJDOT SPECIFICATIONS FOR CHAIN LINK
The Contractor shall perform all services and work under Category I – Type I in accordance with NJDOT’s specifications for chain link. Category I – Type I will be open to all Using Agencies.
[bookmark: _Toc112919808][bookmark: _Toc120526685]SPECIFICATIONS FOR VINYL AND CLAD CHAIN LINK FENCE
A. Materials:
1. Base metal: The base metal of the fabric shall be a good commercial quality steel wire capable of meeting the requirements for Category I – Type I;  
2. Galvanizing Zinc Coating: must conform to Section 912.02.01 of the NJDOT Standard Specifications for Road and Bridge Construction 2019;
3. Plasticized polyvinylchloride (PVC) with suitable non-migratory low temperature plasticizer. Colors shall be stabilized and shall withstand a minimum weather-o-meter exposure test of 1,000 hours without visible fading or discoloration for Category I – Type I;
4. Vinyl-covered wires shall withstand an accelerated aging test of a minimum of 2,000 hours at 145 degrees F. (63 degrees C), without any cracking or peeling, and shall exhibit a maximum shrinkage of 1/16 inch per 12 inches. The vinyl clad chain link fabric wire shall withstand a mandrel bend test (10 X O.D. on wire at minus 50 degrees C) without cracking for Category I – Type I; and
5. Vinyl coating shall have a self-extinguishing character, an average tensile strength of 3300 pounds per square inch (PSI), an elongation of 275%, and have high abrasion resistance. Vinyl coating shall have a maximum deformation of 15% at 120 degrees C (UL laboratory) for Category I – Type I.

B. Manufacture: Vinyl clad galvanized steel fabric shall have zinc coating applied by the hot-dipped method to steel wires before vinyl coating operations;

C. Tensile strength: The wire constituting the fabric shall meet a minimum tensile strength of 100,000 PSI (690 Mega Pascal MPa) uncoated wire diameter. Specimens to establish conformance to this requirement shall be taken from the straight (under-formed) section of the fabric mesh.

D. Height of fabric: Chain link fabric shall be furnished in the standard heights shown in Table 1, shown below. The height of the fabric shall be the overall dimension from ends to barbs or knuckles. Permissible variation in height shall be plus or minus one inch.

E. Size of wire: Chain link fabric shall be fabricated from the wire diameter as necessary to conform to size as shown in Table 1 below. The diameter of the coated wire shall be determined as the average of two readings taken at right angles to each other on the straight portion of the parallel sides of the mesh and measured to the nearest 0.001 inch. The permissible variation in diameter of the coated wire shall be plus or minus 0.005 inch.







TABLE 1
	Normal Diameter of Coated Wire- Inches
	
Permissible Variations of Diameter Coated Wire +/- Inches
	Size Coated Wire Gauge
	Size of Mesh Inches
Tolerance +/- 1/8 Inch
	Height of Fence Fabric Inches Tolerance +/- 1 Inch

	0.148
	       0.005
	9
	2
	36, 48, 60, 72, 96



F. Vinyl coating: 
1. Vinyl shall be bonded to standard galvanized steel wire by the molten extrusion process under minimum pressure of 5,000 lbs. PSI; and
2. Wire shall be vinyl clad before weaving and free and flexible at all joints.

G. Size of mesh: 
1. The maximum size of mesh openings shall be two (2) inches on parallel wires for nine (9) gauge fabrics. The permissible variation in sizes of mesh shall be plus or minus .125 inches; and
2. The size of mesh shall be determined by measuring the minimum clear distance between the wires forming the parallel sides of the mesh, measured in either direction.

H. Standard length of rolls:
1. The standard length of rolls shall be 100 feet except as otherwise agreed upon at the time of purchase. The permissible variation in length shall be plus or minus 1%; and
2. The length of rolls shall to be determined by unrolling a roll of fabric on a flat surface and hand stretching to remove all slack.

I. Selvage: Fabric in all gauges shall be delivered with one (1) or both selvages, either knuckles or barbed at the agency’s option;

J. Workmanship: Chain link fence fabric shall be produced by methods recognized as Good Industry Practice. Roughness, blisters, spots, bruises, and discoloration shall be noted. These and other obvious defects, if present to any considerable extent, shall provide a basis for rejection. Good Industry practice is hereby defined as standards, practices, methods and procedures conforming to the law and the degree of skill and care, diligence, prudence and foresight which would reasonably and ordinarily be expected from a skilled and experienced person or body engaged in a similar type of undertaking under the same or similar circumstances;

K. Number of tests: 
1. One (1) roll from every 50 rolls or fraction thereof shall be taken at random as a sample for test purposes but in no case shall be less than three (3) samples;
2. To determine compliance with the requirements of these specifications, one (1) test specimen for each of the tests specified shall be taken from the outside end of sample rolls representing the lot; and
3. If any specimen tested fails to meet the requirements of these specifications, two additional specimens shall be taken from the sample roll and tested, both of which shall meet the requirements in every respect, otherwise the lot represented by the samples may be rejected.

L. Inspection: The Contractor shall afford the Agency Inspectors, or the person designated by Using Agency to do inspection of the work, all reasonable quantities of materials, without charge, to ensure that the materials are being furnished in accordance with the specifications of each Price Line. All tests and inspections shall be made prior to shipment and shall be so conducted as not to interfere unnecessarily with operations.

Prior to construction, the Contractor shall submit, to DOT’s Regional Engineer or the ordering Using Agency’s main point of contact, certifications of compliance for all materials stating that such materials or assemblies fully comply with the requirements of this Bid Solicitation. The form of certificates shall be approved by the NJDOT Resident Engineer or Using Agency main point of contact. Materials or assemblies used on the basis of certificates or compliance may be sampled and tested at any time and if found not to be in conformity with the requirements of this Blanket P.O., will be subject to rejection whether in place or not.

M. Pipe framework: Line, corner and terminal post, top and/or bottom rail, shall be resin-clad steel with EMPVC (epoxy modified polyvinyl chloride), and continuously chemically bonded to heated standard weight ASTM A-53 schedule 40, diameter as specified, by the electrostatically applied powder dispersion process. Pipes shall be ten (10) to ten (10) mils (0.25 to 0.25 MM) in thickness according to pipe diameter. Each length of pipe shall include two J4 polyethylene seals to prevent internal corrosion. Painted pipe will not be accepted;

N. Top Rail: Top rails shall be 1 5/8 inches O.D. and an EMPVC resin-coated steel pipe, weighing at 2.30 lbs. per ft. of 21 ft. lengths joined by six (6) inches long outside sleeves. Top rails shall be resin-clad and run continuously along the top of the fence. Bottom and intermediate rails, if required, shall conform to the same specifications as top rails and joined at line posts with resin-clad boulevard clamps;

O. Line Posts: Line posts shall be 2 ½” O.D. and be EMPVC resin-coated by the Fusion-Bond Method. The Fusion-Bond Method is the fusion bond epoxy process where the surface of a pipe is cleaned and exposed to heat, an epoxy powder is applied onto the surface of the pipe electrostatically, and the powder undergoes melting onto the pipe surface and dries quickly in controlled and uniformed thickness;

P. Corner and Terminal Posts: Corner and terminal posts shall be three (3) inches O.D. and nominally weigh at 5.85 lbs. per ft. Corner and terminal posts shall be EMPVC resin-coated by the Fusion-Bond Method;

Q. Gates: 
1. Gate frames shall be made of 2 ½” O.D. EMPVC resin-coated steel pipe. Gates shall be welded at the corners. Frames shall be filled with vinyl-clad chain link fabric of the same gauge and color as used for the fence and fastened with resin-clad fittings;
2. Gate posts for 3 ft. to 20 ft. gates shall be three (3) inches O.D. with a nominal weight of 5.85 lbs. per ft. and EMPVC resin coated. The Contractor shall construct gate keepers or gate hold backs on each gate;
3. Gate posts for gates greater than 20 ft. with 10 ft. leafs shall be made of four (4) inches O.D. EMPVC resin-coated steel pipe;
4. Gate posts for gates greater than 20 ft. with heights greater than 6 ft., shall be made of 6 5/8 inches O.D. EMPVC resin coated steel pipe;
5. Each ten (10) foot leaf shall be constructed of 2 ½ inches O.D. pipe and shall have a 2 ½ inch O.D. pipe brace placed vertically at the center frame. Truss rods of 3/8 inch diameter steel with turnbuckles shall be constructed in both diagonal directions on each gate;
6. All gates shall have 180-degree offset type hinges with “hold backs” capable of locking gates in the opened position. Center locking latches shall be of the “drop rod” type and center stops shall be of the depressed channel type set in concrete;
7. The Contractor’s unit price submitted shall be for the entire finished width of gate (single leaf or double leafs); and
8. All framework for sliding gates shall be galvanized steel.

R. Fittings: All fittings and other appurtenances shall be pressed steel or malleable iron as specified in Section 4.6.1, Item W, Fittings and Appurtenances, of the Bid Solicitation. Fittings shall be epoxy-phenolic primed and coated with matching vinyl (PVC) by the fusion-bond method. Painted fittings are not acceptable;

S. Tension Wire: Tension wire of six (6) gauge O.D. vinyl-clad galvanized wire shall be stretched along the bottom of the fence and securely fastened to the fabric with nine (9) gauge O.D. vinyl-clad hog rings at intervals of two (2) feet;

T. Color: Vinyl coated fabric shall be available in color choices of green, gray and brown;

U. Bottom Hinges: To be ball and socket type designed to carry the weight of the gate on the rest footing. Upper hinge(s) to be wrap adjustable type. Equip all gates with a positive type-latching device with provisions for padlocking. No padlocks provided under this Blanket P.O.;

V. Truss and Brace Rods: 3/8 inch diameter (std.) and be equipped with a turnbuckle;

W. [bookmark: _Hlk39154000]Fittings and Appurtenances: All fittings and appurtenances shall be pressed steel or malleable iron coated with matching vinyl (PVC) by the thermal-fusion bond process. Painted fittings are not acceptable.

Fitting specifications include, but are not limited to:
1. Tension wire for bottom of fence: six (6) gauge;
2. Hog ring fastener wire: nine (9) gauge;
3. Wire fabric ties: nine (9) gauge;
4. Flat bond fabric ties, ½ inches wide by 0.60 inches thick strip;
5. Stretcher bars ½ inches x ¾ inches flat bars, with square edges (std.);
6. Turnbuckles wrought parts;
7. Gate hinges: offset type of wrought aluminum;
8. Locking devices, center stops and keepers for gates: galvanized malleable iron except plunger bars, either tubular or bar steel;
9. Post tops: Post tops shall be permanent mold castings ASTM B108 (p.mold) alloy no. “f” (356-f), sand castings ASTM B26 sand alloy “f” (356-f), or die castings ASTM B85 (die) alloy SG100d (360). Posts not equipped with extension arms shall be fitted with post tops;
10. Stretcher bar bands and brace bonds: Stretcher bar bands and brace bonds shall be 0.125 inches by one (1) inch side complete with bolts and nuts. Aluminum alloy (2042-T4) carriage bolts with 205 aluminite finish shall be made from rod conforming to ASTM Specification B211-56T alloy CC42A;
11. Bolt heads: Bolt heads shall conform to American Standard Regular Hexagon ASA Specification B18.2;
12. Finished bolts shall be supplied to T4 temper and given as anodic coating at least 0.0002 inches in thickness and chromate sealed;
13. Nuts: Nuts shall be made from 6061-T6 rod conforming to ASTM Specifications B211 Alloy RS 11A-T6. Nuts shall conform to American Standard Regular Hexagon ASA B28.2;
14. Threads: Threads shall conform to standards of Class 2, 2a or 2b of the Unified Thread Standard, a standard thread form and series for bolts, nuts, screws, and other thread fasteners; 
15. Expansion sleeves: Expansion sleeves shall conform to ASTM B210 alloy MIA-H18 (3003-h18) and be 1.695 inches Interior Diameter (I.D.) x 0.078 inches wall drawn tube 6” long: self-centering type; and
16. Rail and brace ends: Rail and brace end shall be made of permanent mold castings conforming to ASTM B108 (permanent mold) alloy SG70A- T6 (356-T6) or die castings conforming to ASTM B85 (die) SG100B (360).

X. Wire coating: Wire coating shall be plasticized, unfilled, melt-mixed polyvinyl chloride (PVC) with non-migratory low temperature plasticizer, and shall not support fire combustion, and be insulated for 12,000 volts. Pigment systems shall be stabilized and subjected to a weather-o-meter 2000-hour test without visible deterioration. The vinyl-covered wire shall withstand an accelerated aging test of 2000 hours at 145 degrees F (63 Degrees C.) without cracking or peeling, have a specific gravity of no less than 1.30, and a hardness of no less than durometer A-90. The minimum tensile strength shall be 3000 PSI, with an elongation at 200% and maximum deformation of 15% at 120 degrees C. in an Underwriters Laboratories (U.L.) test under 500 gram load, and compression cut-through of 1800 PSI.

Vinyl coating shall be melt extruded (not sprayed or powder coated) over Type I A.I.S.I. galvanized steel wire by the thermal extrusion process under pressure to 5000 PSI. The protective resin coating thickness shall be 14 to 22 mils over the galvanized steel wire. Type IV with a permissible diameter variation of plus or minus.005 mils.

Mesh size shall be measured by the distance between the wires forming parallel sides of the mesh, with permissible variation of plus or minus ¼ inch.

The height of the fabric, measured from the ends of the barbs or knuckles, shall have a permissible variation of plus or minus on inch;

Y. Pipe resin: Pipe resin shall have:
1. A specific gravity of 1.35 to 1.40;
2. Tensile strength of 1500 PSI;
3. A minimum elongation of 170%;
4. Tear strength at 15 mils-.36 lbs. mil hardness;
5. A coating of 80+ 5 shore a durometer;
6. A dielectric strength of 1000 volts per mil;
7. Volume resistivity of2.0 x10 ohm/cm; 
8. Brittle temperature of minus 20 degrees C (film); and
9. Water absorption of 77 degrees F – one week 0.70% maximum at 212 degrees F – two hours 0.95% maximum.

Z. Pipe resin criteria: The resin formulation shall meet the standard ASTM-#42-64 (d) minimum hour weather-o-meter requirement without cracking, blistering, or loss of adhesion;

AA. Sure-Loc fabric fasteners: Category I & II: The Sure-Loc washer shall be made from 304 stainless steel, .078” thick, shaped as a concave washer with scalloped edge, and designed to be positioned over the strand of chain link fabric and other wire products like tension wire or barbed wire. The washer shall be secured to a steel or aluminum frame with a special plated ramset/redhead drive pin that can withstand over 500 hours in a salt spray chamber with no signs of rust. A nylon sleeve over the pin stem shall provide additional protection to the stem and the material it has penetrated; 

AB. Barbed wire shall conform to ASTM A-121. Barbed wire shall be measured by the actual number of linear feet installed;

AC. Construction.
1. Preliminary work: Before beginning construction or placing of fences, site clearing shall be done as directed by NJDOT’s Resident Engineer or the Using Agency’s point of contact. Any rock protruding above the ground surface and in the line of fence shall be removed to ground surface as directed by the Resident Engineer. Site cleaning shall be done for the preparation of access to fence and work locations;
2. Setting posts and backfilling: Fence and gates shall be erected in accordance with the Standard Construction Details 2016 and Standard Specifications for Road and Bridge Construction 2019, or any revisions construction practices as recommended by the manufacturer. The Contractor shall adhere to the following procedures:

a. Terminal posts shall be set at the beginning and end of each continuous length of fence and at abrupt changes in vertical and horizontal alignment, and on each side of gate locations. Aluminum surfaces to be placed in contact with concrete shall be given a coat of zinc chromate primer;

b. Posts to be set in concrete shall be installed in dug or drilled holes. Posts not requiring concrete foundation may be driven to the required depth if ground conditions permit or they shall be installed in holes dug or drilled as will allow sufficient room for proper backfilling. When solid rock is encountered, any posts not required to be set in concrete shall be installed by drilling the rock to the required depth and grouting the post therein with grout composed of one part cement to two parts sand;
[bookmark: _Hlk92801024]
c. Post holes for posts not requiring concrete foundations shall be backfilled with a suitable material approved by the Bureau of Materials, for DOT projects. All backfilling shall be performed in layers not exceeding four (4) inches and each layer shall be thoroughly tamped. When backfilling and tamping is completed, the posts and anchors shall be held securely in their proper positions;

d. The drilling through solid rock, in Category I, Type I, will be paid per each hole. The cost of drilling in the asphalt for posts shall be included in the fence item;

e. Pull and setting of fabric shall not be applied to posts set in concrete foundations until the concrete has cured for a minimum of 72 hours; and

f. Fence fabric shall face away from the roadway.

3. [bookmark: _Hlk92879838][bookmark: _Hlk92880070]Removal and Reset Fence: Removal and Resent Fence: Resetting of chain link fence 4 ft to 8 ft high shall include the removal and reinstallation of existing fence on one project site. Materials damaged or rendered unusable by the Contractor shall be disposed of and replaced with new materials of the same or equivalent type without additional compensation.

[bookmark: _Hlk92880016][bookmark: _Hlk92879876]Removal of chain link fence shall include the disassembly and removal of the fence and all its components. It is the responsibility of the Contractor to dispose of all material removed and to fill in all holes with suitable material at no additional cost to the State.

a. The Contractor will be paid for the removal of chain link fence when:
1. The fence is removed and not replaced; and
2. Existing fencing is removed and replaced with new chain link fence.

b. The removal of chain link fence is not a pay item when:
1. Existing fence is being reset or repaired; 
2. The removal of fence is included in the cost of the reset chain link fence, new fence post or install chain link fence fabric; and
3. The cost or removal of chain link fencing shall be included with the resetting or reparations of chain link fencing.

4. [bookmark: _Hlk92881261]Removal of barbed wire: Removal of barbed wire shall include the disassembly and removal of the barbed wire and all its components. The Contractor shall dispose of all removed material at no additional cost to the State.

The removal of the barbed wire will be a pay item when barbed wire is removed and not replaced, and when existing barbed wire is removed and replaced with new barbed wire.

[bookmark: _Toc112919809][bookmark: _Toc120526686]SPECIFICATIONS FOR ALUMINUM COATED CHAIN LINK FENCE
All specifications under Aluminum Coated Chain Link Fence Category I are under Type I, unless stated otherwise. The Contractor shall follow the specifications below: 
A. Chain link fence fabric: Aluminum-coated chain link fence fabric shall consist of a 2” (50 MM) mesh or as otherwise specified and fabricated of 9 gauge wire helically wound and interwoven at various heights specified throughout the Bid Solicitation. Aluminum-coated chain link fence fabric shall conform to Attachment 3 - Exhibit 1 - Aluminum-Coated Chain Link Fence. 

[bookmark: _Hlk92801641]Fence fabric shall be delivered in individual rolls of one hundred (100) feet, each tightly rolled with the ends securely fastened. The State reserves the right to order fence fabric delivered in rolls less than 100 feet at no additional unit cost;
B. Pipe: All new pipes and pipes used for the replacement of chain link fence pipe items, shall be fabricated in conformance with the following requirements:
1. Aluminum pipe shall conform to the current requirements of American Standard Test Method (ASTM) Designation B429/B429M;
2. Steel pipe shall conform to the current requirements of ASTM Designation A53, Schedule 40, plain end. Steel pipe shall be hot dipped galvanized after fabrication in accordance with the current requirements of ASTM Designation A123;
3. Terminal post pipe 3 inches O.D. at the various lengths specified in the Bid Solicitation;
4. Corner post pipe 3 inches O.D. at the various lengths specified in the Bid Solicitation (Category I Price Lines; and
5. Line post pipe 2 ½ inches O.D. at the various lengths specified in the Bid Solicitation.

C.    Post cap: Post caps shall be three (3) inches in diameter and shall conform to the detail included in Attachment 3 - Exhibit 1 - Aluminum-Coated Chain Link Fence Fabric and to the current requirements specified in the AASHO Designation M 181-60;
D. Stretcher bar: Stretcher bars shall be ¼ inches x ¾ inches at various lengths specified throughout the Bid Solicitation and conforming to Attachment 3 - Exhibit 1 - Aluminum-Coated Chain Link Fence Fabric;

E. Brace band: Brace bands shall be 1 inch x 1/8 inch and conform to Attachment 3 - Exhibit 1. Each brace band shall include a 5/16 inch carriage bolt, 1 ¼ inches long with the elastic stop hex nut;

F. Diagonal brace rod: Diagonal brace rods shall be 3/8 inch diameter with turnbuckles conforming to Attachment 3 - Exhibit 1 - Aluminum-Coated Chain Link Fence Fabric;

G. Standard spring coupling: Standard spring coupling shall have a 1.695 inch I.D., be six (6) inches long, and shall be self-centering. Both aluminum and steel sleeves shall contain a hot-dipped galvanized spring which shall not exceed 1 ½ inches, fully compressed;

H. Fabric ties: Fabric ties shall be 9-gauge wire conforming to Attachment 3 - Exhibit 1 - Aluminum-Coated Chain Link Fence Fabric;

I. Hog ring fasteners: Hog ring fastener shall be 9-gauge wire conforming to the details in Attachment 3 - Exhibit 1 - Aluminum-Coated Chain Link Fence Fabric;

J. Spring coil tension wire: Spring coil tension wire shall be a 7-gauge wire conforming to the details in the Standard Construction Details 2016;

K. Gates:
1. Pricing for gates shall be inclusive of installation and materials; 
2. Gate frames shall be made of 2 ½ inches diameter pipe. Gates shall be welded at the corners to form a rigid panel. Gate fabric shall be the same material used in the fence. Gate locking devices, stops and keepers may be galvanized malleable iron or steel except plunger bars may be tubular or bar steel;
3. Gate posts for 3 ft. to 20 ft. gates shall be 3 inches O.D. Construct “gate keepers” or gate “hold backs” on each gate;
4. Gate posts for 20 ft. gate, with 10 ft. leafs, shall be made of 4 inches O.D.;
5. Gate posts for gates greater than 20 ft. with heights greater than 6 ft. shall be made of 6 5/8 inches O.D.;
6. Each 10 ft. leaf shall be constructed of 2 ½ inches O.D. pipe and shall be made of 2 ½ in O.D. pipe brace placed vertically at the center frame. Truss rods of 3/8 inch diameter steel with turnbuckles shall be constructed in both diagonal directions on each gate;
7. [bookmark: _Hlk92801495]The Contractor’s unit price submitted shall be for the entire finished width of gate (single leaf or double leafs). Gate items for Price Lines #50-8132-63  for the North Region, #256-287 219-250 for the Central Region, and #463-494406-437 for the South Region, shall be inclusive of materials and installation; and
8. All framework for sliding gates must be galvanized steel.

L. Sure-Loc fabric fastener: Category I & II: The Sure-Loc fabric fastener is a power driven fastener in accordance with ASTM Designation F-626 6.1.4. See Section 4.6.1, Item AA, Sure-Loc Fabric Fasteners, of the Bid Solicitation. 

[bookmark: _Toc89784913][bookmark: _Toc112919810][bookmark: _Toc120526687]CATEGORY I – TYPE II – SPECIALTY FENCING AND INSTALLATION
Category I, Type II shall include, but not be limited to:
A. Special fencing and miscellaneous items: Chain link fencing on bridges and median barriers shall be measured by linear foot. Chain link fencing and caging shall be measured by square foot;
B. Median barrier chain link fence end assembly with breakaway post for the approach and trailing ends per unit;
C. Intermediate median barrier breakaway fence post to be single post of the end treatment detail with cable guide per unit;
D. Median barrier chain link fence, aluminum coated 6’ high, 1” mesh or 2’’ mesh, per linear foot;
E. Non-Vegetative surface, polyester matting - Includes anchor pins, fence post templates and adhesive (per square yard); 
F. Non-Vegetative asphalt surfacing, 4” thick (per square yards). Non-Vegetative asphalt surfacing shall follow Section 608.03.05 of the NJDOT Standard Specifications for Road and Bridge Construction 2019;
G. Sure-Loc fabric fasteners per unit;
H. Bridge type caging, aluminum, chain link fence 4’ – 6’ high per linear foot; 
I. Lane Closure: The Contractor shall provide lane closures inclusive of safety-related set-up for both sides of a barrier fence when safety-related set-up is required. This item will be paid on a per hour basis. Throughout this Bid Solicitation, safety will refer to safety-related set-up for lane closures. See Section 4.17.2, Lane Closures, for more details;
J. Additional Lane Closure: The Contractor shall provide additional lane closure for when additional safety-related set-ups beyond both sides of a barrier fence are required. This item will be paid on a per hour basis for each Lane Closure. Throughout this Bid Solicitation, safety will refer to safety-related set-up for lane closures. See Section 4.17.2, Lane Closures, for more details; and
K. [bookmark: _Hlk92801540]If deemed necessary and at the request of the Resident Engineer or Using Agency point of contact, the Contractor shall provide privacy slats. Privacy slats will be paid an additional markup of corresponding Chain Fence Link installation prices. Mark-up percentage shall not exceed 8%.

[bookmark: _Toc112919811][bookmark: _Toc120526688]SPECIFICATION FOR CHAIN LINK FENCE AND MEDIAN BARRIER
ALUMINUM BRIDGE AND MEDIAN BARRIER
The Contractor shall be responsible for furnishing and erecting aluminum fencing and removing the railing and fencing on bridges, including median barriers. The Contractor shall conform to all Category II specifications listed below:
A. Anchorage: In the event the existing parapet is steel beam, the Contractor shall, as determined and directed by the engineer, attach bolts by welding or drill holes into the top flange to allow for bolts, nuts and washers;

B. Drilling: All holes whether in concrete or steel shall be made using the core drill;

C. Method of measurement: Fencing shall be 6’3” high and fence curved top shall be measured by linear foot. Fence (caging) shall be measured by square foot along the contour of the fence; 

D. [bookmark: _Hlk92967539]Removal: Bridge rail and bridge fencing shall be measured by the linear foot and shall include the cutting off of any existing bolts where necessary;

E. Basis of payment: 

	Pay Item
	Unit

	Chain Link Fence Aluminum, Bridge 6 ft., 3 in. high
	Linear Foot

	Chain Link Fence Curved Top
	Linear Foot

	Bridge Chain Link Fence (Caging)
	Square Foot

	Bridge Chain Link Fence (Caging) with Safety
	Linear Foot

	Chain Link Fence Median Barrier
	Linear Foot

	Removal Bridge Rail
	Linear Foot

	Removal Bridge Fence
	Linear Foot

	Non Vegetative Surface, Polyester Matting
	Square Yard

	Sure-Loc Fabric Fastener
	Each 



F. Conformity: Chain link fence shall conform to the American Association of State Highway Transportation Officials (AASHTO) M 181. Posts, rails, wire fabric ties, stretcher bars, railing, and post sleeves for chain link fencing on bridges shall be alloy 6061 T6, conforming to Section 908 of the Standard Specifications for Road and Bridge Construction 2019;

G. Aluminum-pigmented alkaline-resistant paint: The Contractor shall use aluminum paint conforming to AASHTO M 69, Type II and submit certifications of compliance as specified in 106.07 of the Standard Specifications for Road and Bridge Construction 2019; 

H. Bolts and bolting material: Corrosion-resistant steel bolts shall be of an alloy steel, containing approximately 18% chromium and 8% nickel, conforming to ASTM A 276, Type 302; 

I. [bookmark: _Hlk60739986]Non-vegetative surface, polyester matting: Non-vegetative surface, polyester matting shall control the growth of unwanted vegetation without herbicides or poisons, and shall not add to water runoff problems. They shall be installed according to Section 608.03.05 of the NJDOT Standard Specifications for Road and Bridge Construction 2019. The Contractor shall install anchor pins stakes, 316 stainless steel, fence post templates and adhesive (per sq. yard), and U-Teck’s “WeedEnder” or an approved equal; 

J. Non-vegetative Asphalt surface 4’’ thick shall be excavated, constructed and delivered according to 608.03.01 of the NJDOT Standard Specifications for Road and Bridge Construction 2019. Non-vegetative Asphalt surface 4’’ thick shall also provide weed control as specified in 608.03.06; and  

K. [bookmark: _Hlk92801731]Inspection and payment for bridge fence: After notice of a mini-bid project award and prior to shipment, the Contractor shall contact NJDOT’s Manager of Bureau of Materials, Thiokol Building, 930 Lower Ferry Road, Trenton, New Jersey, 08625, at telephone number (609) 530-2307, to arrange for inspection and testing of the material. For non-NJDOT projects, the Contractor shall contact the respective Using Agency’s main point of contact. Failure to comply shall be a cause for rejection of the material upon delivery at Contractor’s expense. All shipments shall be accompanied by two (2) copies of a notarized certification listing test results for above criteria.

The State reserves the right to reject any material not complying with the requirements set forth in this Blanket P.O. If the material fails to comply with the requirements, it shall be removed and replaced by the Contractor at no additional cost to the State.

Prior to construction, the Contractor shall submit, to DOT’s Regional Engineer or the ordering Using Agency’s main point of contact, certifications of compliance for all materials stating that such materials or assemblies fully comply with the requirements of the Blanket P.O. The form of certificates shall be approved by the NJDOT Resident Engineer or Using Agency main point of contact. Materials or assemblies used on the basis of certificates of compliance may be sampled and tested at any time and if found not to be in conformity with Blanket P.O. requirements will be subject to rejections whether in place or not.

[bookmark: _Toc112919812][bookmark: _Toc120526689]CATEOGRY II – ADDITIONAL TYPES OF FENCING (ORNAMENTAL, VINYL, WOODEN, ETC.)
Category II consists of various other types of fence for use including, but not limited to, ornamental, vinyl, wooden, motorized automatic fencing, and steel barricade fencing. The Contractor shall be responsible for the installation of all Category II fencing and the reparations of motorized automatic fence gates. Materials and parts incorporated on the installation of ornamental, vinyl, wooden, and motorized automatic fencing will be paid by a percentage (%) markup by invoice.  Mark-ups on parts costs shall not exceed the awarded markup percentage, which shall not exceed 8%. 
Under Category II, the cost of installation services shall include the cost of both materials and installation, unless otherwise specified.
If requested by the Using Agency, the Contractor shall provide the fence manufacturer, catalog number and date for Category II fencing.




[bookmark: _Toc112919813][bookmark: _Toc120526690]TYPE I – ORNAMENTAL FENCE
Ornamental fencing shall include all wrought iron fencing, aluminum fencing, and steel fencing of all styles and colors. The Contractor   shall provide and complete the installation of ornamental fencing installation and supply all varieties of ornamental fencing available within its published catalog.
[bookmark: _Toc112919814][bookmark: _Toc120526691]TYPE II – VINYL FENCE
Vinyl fencing shall include all types of vinyl picket fencing, vinyl privacy fencing, vinyl railings, and vinyl snow fencing. The Contractor shall provide and complete the installation of all vinyl fencing, and supply all varieties of vinyl fencing available within its published catalog.
[bookmark: _Toc112919815][bookmark: _Toc120526692]TYPE III – WOODEN FENCE
Wooden fencing shall include all types of wooden fence such as post and rail, stockade, and picket fencing. The Contractor shall provide and complete the installation of wooden fencing and supply all varieties of wooden fencing available within its published catalog.
[bookmark: _Toc89784919][bookmark: _Toc112919816][bookmark: _Toc120526693]4.8.4    TYPE IV – INSTALLATION and repair of MOTORIZED AUTOMATIC FENCE GATES
New installations shall include motorized automated gates and parts such as motors, hardware, posts, chains, sensors, controls, photo eyes, and locks. The Contractor shall complete installations and furnish all parts, manuals, and accessories for the proper operation of motorized automatic sliding gates.
Materials and parts incorporated in the final installation or repair of motorized automated gates will be paid as a percentage markup by invoice. The Contractor shall furnish all warranties and manuals to the Using Agency. 
[bookmark: _Hlk92974096]The labor associated with performing installation or repairs on motorized automatic gates will be paid on an hourly rate per approved worker for work completed on site.
0. [bookmark: _Toc112919817][bookmark: _Toc120526694]TYPE IV – STEEL BARRICADE
The Contractor shall adhere to the following specifications:
A. Material: Barricades shall be made of 18-gauge steel and hot-dipped galvanized after assembly;
B. Barricades shall be fabricated with interlocking features to attach to adjacent barricades and shall have removable feet;
C. Four (4) barricade feet must be provided with each barricade. Two (bridge) and two (smooth) must be provided for use on uneven and smooth surfaces;
D. Barricades must weigh between 30-45 lbs.;
E. Delivery: The Contractor shall be responsible, but not be limited to, delivering to the Region’s designated location or, if requested by the RE, to a different location within ten (10) miles of the designated location. NJDOT’s designated locations for delivery for each Region are as follows:

1. [bookmark: _Hlk94184353][bookmark: _Hlk94184442]North Region - NJDOT Rockaway Maintenance Yard on 200 NJ-15, Dover, NJ 07801;
2. Central Region - NJDOT Hamilton Maintenance Yard on 2779 Kuser Rd, Hamilton Township, NJ 08691; and
3. Region South - One Executive Campus on Route 70, West Cherry Hill, NJ 08002.

Other Using Agencies will determine its designated delivery location at the time of order.
Deliveries for steel barricades will be a minimum of ten (10) Steel Barricades.
Shipments shall be delivered within 15 calendar days after the ordering Using Agency has issued a purchase order. Material stockpiles shall be created as soon as practical whenever product shortages occur. Stockpiles shall remain in place until such product shortages no longer exist.
Deliveries must be scheduled on a business day, Monday to Friday, not including State holidays, between the hours of 8:00 am and 3:00 pm. No deliveries will be accepted after 3:00 pm unless previously agreed upon by the Contractor and the Using Agency. 
[bookmark: _Toc95129320][bookmark: _Toc95129840][bookmark: _Toc95486633][bookmark: _Toc89784923][bookmark: _Toc112919818][bookmark: _Toc120526695]CATEGORY III – NJDOC EMERGENCY REPAIRS
The Contractor shall perform emergency repairs to security fencing at all NJDOC facilities. Installation of new equipment, unless associated with a repair, is prohibited under Category III.
Category III does not include hourly rates.
Under Category III, the cost of installation services shall include the cost of both materials and installation, unless otherwise specified.
Attachment 5 - Exhibit 3 – NJDOC Fencing Configurations contains a listing of several NJDOC Facilities, including addresses and descriptions of fence configurations at each facility. The Contractor shall service, but not be limited to servicing, the NJDOC locations listed within Attachment 5 - Exhibit 3 - NJDOC Fencing Configurations. 
[bookmark: _Toc89784924][bookmark: _Toc112919819][bookmark: _Toc120526696]REQUIREMENTS
[bookmark: _Hlk76120077]Category III will be purchased on an as-needed basis only and is exclusive to NJDOC emergency repairs to security fencing. The State makes no guarantee of any minimum or maximum number of hours to be used.
[bookmark: _Toc89784925][bookmark: _Toc112919820][bookmark: _Toc120526697]EMERGENCY SERVICES - NJDOC
The Contractor shall establish an emergency telephone contact within twenty (20) days after notice of award. The line shall be operational and provided to NJDOC’s main point of contact within thirty (30) days after notice of award. The Contractor shall maintain this emergency telephone contact, which shall be available 24 hours per day, seven (7) days a week, and 365 days a year. 
Emergency calls are those service calls where the work consists of correcting failures that constitute an immediate danger to public safety and property. Any work considered by the NJDOC’s main point of contact or designee to be of an emergency nature shall be classified as an emergency service request. The callback response time is one (1) hour from time of notification. The Contractor shall physically respond to emergency service requests within two (2) hours. 
Emergency services shall be conducted during any time of the day or night which may include both overtime and normal business hours. Normal business hours are Monday through Friday from 8:00 am to 4:30pm. 
The Contractor shall remain on the job until the emergency has been resolved and all work has been approved by the facility. 
MATERIALS FOR EMERGENCIES 
The Contractor shall ensure that materials are kept in stock. In an event where the Contractor’s primary supplier is unable to provide the Contractor with adequate stock, the Contractor shall acquire its stock from various other suppliers at no increased cost to the State without prior approval from the Division of Purchase and Property. The Contractor shall have enough materials sufficient to replace a minimum of 100 feet of security fencing and barbed tape, or must give assurance that they have access to such materials within a three (3) hours of being contacted by the Using Agency.
[bookmark: _Hlk92974542]The Contractor must supply all tools and equipment to perform the work required. It shall be the responsibility of the Contractor to safeguard its own materials, tools, and equipment. The State assumes no responsibility for vandalism or theft of materials, tools, and equipment.
[bookmark: _Toc89784926][bookmark: _Toc112919821][bookmark: _Toc120526698]DESCRIPTION OF CATEGORY III – TYPES I, II, III, IV, AND V
This section consists of one (1) Type of standard fencing fabric, one (1) Type of anti-climb fencing fabric, one (1) Type of framing, one (1) Type of fittings and accessories, and one (1) Type of barbed tape as described below. Fence heights range from 8’ to 16’. Installation services shall include the cost of both the delivery of materials and installation, unless otherwise specified. Lane closures and safety-related set-up will not be paid-for items in Type III unless approved by NJDOCT’s Resident Engineermain point of contact or the Using Agency main point of contact.
Installation shall be included for all items under Category III with exception to bottom tension wire, Price Line #202182 for the North Region, #409 369 for the Central Region, and #615556 for the South Region, which shall only include material and delivery. 
Under Category III, repairs and replacements shall include the removal of damaged posts. 
TYPE I - Standard Fabric
All steel, welded wires, and fence fabric shall be in accordance with ASTM A853, Grade American Iron and Steel Institute (AISI) 1006, and be of 70,000 PSI minimum tensile strength. Type I fences shall be of low carbon steel wire, electronically control welded at all wire intersections, 7”-3” wide, and conform to heights as indicated on Attachment 3 - Exhibit 3. In addition, some fencing will require 24” high sheets for buried fabric.
The Contractor shall use 2” mesh and 9-gauge wire.
Coating shall be of 1.2 oz. zinc coating per square foot per side conforming to ASTM F1043, and applied after fabrication.
TYPE ii – anti-climb security fencing fabric
All steel, welded wire, and fence fabric shall be in accordance with ASTM A853, Grade AISI 1006, and be of 70,000 PSI minimum tensile strength. Type II fences shall be of low carbon steel wire and electronically control welded at all wire intersections, 7”-3” wide, with heights as indicated in Attachment 3 - Exhibit 3.  The Contractor shall provide 24” high sheets for buried fabric.
All mesh used shall be 3/8”. All wires shall be 11-gauge wires.
Coating shall be of 1.2 oz. zinc coating per square foot per side conforming to ASTM F1043, and applied after fabrication.
All polymer-coated fabric shall be finished with ASTM F 668, [Class 1] [Class 2a] [Class 2b] over [aluminum] [zinc] [Zn-5-AL-MM-aloy]-coated steel wire. All finish shall be black or green, as required to match existing fences at the facilities.


type iii – framing 
The Contractor shall adhere to the specifications below:
A. Standard framing and fittings must be galvanized steel;
B. Galvanized steel pipe diameter shall be 1-1/2” – 4”, varying by facility location, Using Agency direction, and application;
C. Standard upright posts shall be 2 ½” with 1 ½” cross members. Gate posts shall be 4”;
D. Galvanized steel ties shall be used. Aluminum ties are not permitted;
E. The use of aluminum on NJDOC security fencing is not permitted;
F. Type I Round Posts: Type I Round Posts shall be standard weight, schedule 40, and of a galvanized steel pipe conforming to ASTM F1083 in accordance with heavy industrial requirements of ASTM F699, Group IA. Type I Round Posts shall have a minimum yield strength of 25,000 psi, and a minimum of 1.8 oz. of zinc per sq. ft. Type A coating both inside and outside. Type A coating shall be in accordance with ASTM F1234, as determined by ASTM A90.
G. Type II Round Posts: Type II Round Posts shall be cold formed, electric-welded, and of a steel pipe, conforming to the heavy industrial requirements of ASTM F669, Group IC. Type II Round Posts shall have a minimum yield strength of 50,000 psi and either of the protective coating systems below, in accordance with ASTM F1234:
1. Type B coating outside with a minimum 0.9 oz. zinc per sq. ft. after welding, a chromate conversion coating and clear polymer over coat, and Type B coating inside with a minimum 0.9 oz. of zinc per sq. ft; or
2. Type D coating inside with a minimum 0.3 mil thickness and 81% zinc-pigmented coating.

H. Roll Formed Steel: Roll form steel shapes, C section, shall be made from a structural quality steel conforming to ASTM A570, Grade 45, or ASTM A446, Grade D, galvanized. These roll form steel shapes shall conform to heavy industrial requirements of ASTM F669, with a minimum yield strength of 60,000 psi. The protective coating system shall conform to ASTM F1043, Type A, galvanized, with a minimum of 4.0 oz. of zinc per sq. ft. in accordance with ASTM A525.
Roll formed steel shapes shall comply with the specifications below:
4. Posts: Posts shall have a 3.250” x 2.500” x 0.150” wall thickness, with punched-in 14” on-center (O.C.). fastener holes; and
5. Rails: Rails shall have a 1.650” x 1.50” x 0.080” wall thickness.

I. Tubing: Cold-formed steel structural tubing shall conform to ASTM A500, Grade B, with a minimum yield strength of 42,000 psi and a minimum 1.8 oz. zinc per sq. ft., Type A coating inside and outside. This Type A coating shall be in accordance with ASTM A123, as determined by ASTM A90.



TYPE IV – FITTINGS AND ACCESSORIES 
The Contractor shall adhere to the following:
A. Material: Materials used for fencing shall comply with ASTM F626 and be of a galvanized iron or steel, to suit manufacturer’s standards. Dipped galvanize pressed steel fence and cast-iron fence fittings and accessories shall have a minimum 1.2 oz. zinc per sq. ft. as determined by ASTM A90;
B. End, corner, intermediate, and gatepost caps: Weather-tight closure caps for fencing shall be used for each post;
C. Line Post Caps: The Contractor shall provide top caps for each fencing post with loops to receive a top rail; and
D. Post-Brace Assembly: The Contractor shall perform post-brace assembly in accordance with manufacturer’s standard. Adjustable brace shall match existing braces at each facility. The Contractor shall provide manufacturer’s standard galvanized steel or cast-iron cap for each end of the post-brace.

TYPE V – BARBED TAPE (RAZOR RIBBON)
The Contractor shall provide:
A. Supporting Arms: Provide manufacturer’s standard supporting arms conforming to ASTM F626. Supporting arms shall be metal and finished to match fence frameworks, with provisions for anchorage to posts and three (3) rows of barbed wire attached to each arm. Supporting arms may be attached either to posts or to integral with post top weather caps and shall be capable of withstanding a 250 lbs. downward pull at outermost ends. The Contractor shall provide V type with two (2) arms at 45 degrees to vertical, one (1) for each post; and
B. Barbed Tape: Provide continuous helical coils of barbed tape in accordance with ASTM F1379.1.
1. Tape; ANSI 430 stainless steel hardened to Rockwell (30N) 40-45, 0.025” thick x 1” wide prior to fabrication with 4, needle sharp barbs minimum 1.25” long in clusters on 4” centers and permanently cold clenched to minimum of 230 degrees around core wire;
2. Core wire; 0.098” diameter, high tensile, zinc coated steel conforming to ASTM A764 or stainless steel conforming to ASTM A478.Clips; 0.065”thick x 0.375” wide, stainless steel clips capable of withstanding minimum 150 lbs. pull load to limit extension of coil, resulting in concertina effect when deployed; and
3. Size and type:
a. 	Double maze concertina; 24” diameter inner coil, 30” diameter outer coil; and
b. Single maze concertina; 24” diameter.

[bookmark: _Toc112919822][bookmark: _Toc120526699]CATEGORY IV – PREVENTIVE MAINTENANCE AND EMERGENCY SERVICE REQUESTS
Preventative Maintenance and emergency service requests shall apply to Categories I, II, and and III.
[bookmark: _Toc112919823][bookmark: _Toc120526700]PREVENTATIVE MAINTENANCE
The Contractor shall provide Preventive Maintenance services at the request of the Using Agency. Preventative Maintenance shall include, but not be limited to, periodic inspection, testing, cleaning, lubrication, adjustment, parts replacement, and repairs to keep the systems and equipment in optimum operating condition. Manufacturers' recommended Preventive Maintenance shall be the minimum accepted level. Preventative Maintenance is hereby defined as maintenance that is regularly performed on systems and/or equipment to lessen the likelihood of failure. Preventative Maintenance shall include, but not be limited to, periodic inspection, testing, cleaning, lubrication, adjustment, parts replacement, and repairs to keep the systems and equipment in optimum operating condition.
Materials and parts incorporated for preventive maintenance services will be paid as a percentage markup by invoice. Mark-ups on parts costs shall not exceed the awarded markup percentage, which shall not exceed 8%. Upon request of the Using Agency, the Contractor shall furnish all warranties and manuals.
The labor associated with performing preventive maintenance services will be paid on an hourly rate per approved worker for work completed on site. These Preventative Maintenance are found in the Price Lines are listed below:
A. North Region – Price Lines #206 and #207186 and 187; 
B. Central Region – Price Lines #413 and #414373 and 374; and
C. South Region – Price Lines #619 and #620560 and 561.

The Contractor shall provide the Using Agency with a detailed work schedule of all activities completed under Preventive Maintenance items to the ordering Using Agency’s main point of contact within the day of service, by end of business day. This detailed work schedule shall be written and sent to the Using Agency’s main point of contact, or sent by email, as determined by the Using Agency’s main point of contact. 
The Contractor shall be responsible for Preventative Maintenance for the Category or Categories it is awarded. 
[bookmark: _Toc109830365][bookmark: _Toc109830366][bookmark: _Toc109830367][bookmark: _Toc109830368][bookmark: _Toc109830369][bookmark: _Toc109830370][bookmark: _Toc109830371][bookmark: _Toc109830372][bookmark: _Toc109830373][bookmark: _Toc109830374][bookmark: _Toc109830375][bookmark: _Toc109830376][bookmark: _Toc109830377][bookmark: _Toc109830378][bookmark: _Toc109830379][bookmark: _Toc109830380][bookmark: _Toc109830381][bookmark: _Toc109830382][bookmark: _Toc109830383][bookmark: _Toc109830384][bookmark: _Toc109830385][bookmark: _Toc89784928][bookmark: _Toc112919824][bookmark: _Toc120526701]EMERGENCY SERVICES – NON-NJDOC
Emergencies service requests are service requests when the work consists of correcting failures that constitute an immediate danger to public safety and property. Any work considered by the SCM or Using Agency main point of contact, to be of an emergency nature, shall be classified as an emergency service request. 
For all non-NJDOC emergency service requests, the Contractor shall respond to and begin a project within two (2) business days after notification by the NJDOT Resident Engineer or the respective Using Agency main point of contact. The Contractor will be paid on a per site basis, per occurrence. 
The Contractor shall remain on the job until the emergency has been resolved and all work has been approved by the facility.
For NJDOC emergency services, see Section 4.9.2, Emergency Services – NJDOC. 
[bookmark: _Toc112919825][bookmark: _Toc120526702]DELIVERY
The Contractor shall be responsible for delivering, but not be limited to delivering, top rails, fabric, fence line posts, and tension wires to the Region’s designated location or, if requested by the Resident Engineer, to a different location within ten (10) miles of the designated location. Delivery locations will be determined by the Using Agency. 
NJDOT’s designated delivery locations for each Region are as follows:
A. North Region - NJDOT Rockaway Maintenance Yard on 200 NJ-15, Dover, NJ 07801;
B. Central Region - NJDOT Hamilton Maintenance Yard on 2779 Kuser Rd, Hamilton Township, NJ 08691; and
C. Region South - One Executive Campus on Route 70, West Cherry Hill, NJ 08002.

Delivery locations for other Using Agencies will be determined at the time the order and reflected on the Purchase Order.
The Contractor shall deliver the items, but shall not provide installation services for, the specified Price Lines below:
A. North Region – Price Lines #94 to #10175 to 82, #121102, #124 to #129105 to 110, #147127, and #202182; 
B. Central Region – Price Lines ##301 262 to #308269, #328289, #331 to #336292 to 297, #354314, and #409369; and 
C. South Region – Price Lines #508449 to #515456, #535476, #538 479 to #543484, #560501, and #615556. 

The Contractor shall comply with the established minimum delivery amounts for the following items:
A. Top Rail – 100 FT minimum – Price Line #94 75 for the North Region, #301 262 for the Central Region, and #508 449 for the South Region; 
B. Fabric – 500 FT minimum – Price Line #95 76 for the North Region, #302 263 for the Central Region, and #509 450 for the South Region; and 
C. Tension Wire – 200 FT minimum – Price Line #202 182 for the North Region, #409 369 for the Central Region, and #615 556 for the South Region. 

All deliveries shall be made within 15 calendar days of receipt of a purchase order. Material stockpiles shall be created as soon as practical whenever product shortages occur. Stockpiles shall remain in place until such product shortages no longer exist.
Deliveries must be made on a business day, Monday to Friday, between the hours of 8:00 am and 3:00 pm. No deliveries will be accepted after 3:00 pm unless previously agreed upon by the Contractor and the SCM.

[bookmark: _Toc95129328][bookmark: _Toc95129848][bookmark: _Toc95486641][bookmark: _Toc89784929][bookmark: _Toc112919826][bookmark: _Toc120526703]MINIMUM CALL-OUT ORDER
The minimum call-out will be $500.00 per location for one or a combination of items listed in the Bid Solicitation.  The location will include areas within the same site property.
[bookmark: _Toc89784930][bookmark: _Toc112919827][bookmark: _Toc120526704]GUARANTEE
The Contractor shall fully guarantee its products for a period of one (1) year against all defects in materials, installation, and workmanship. If any failures or defects occur, the Contractor shall replace the item within 15 calendar days of notification at no additional cost to the State.
[bookmark: _Toc89784931][bookmark: _Toc112919828][bookmark: _Toc120526705]PRICE QUOTATIONS 
The Contractor shall provide written price quotations within five (5) days of being contacted, with exception to emergency requests, which shall be within 48 hours.
[bookmark: _Toc95129332][bookmark: _Toc95129852][bookmark: _Toc95486645][bookmark: _Toc89784932][bookmark: _Toc112919829][bookmark: _Toc120526706]CONSTRUCTION, STAKES, LINES, AND MARKERS
The construction layout, including, but not limited to, lines, marks, and grade, is the responsibility of the Contractor. The cost of this phase shall be included in the unit cost of fence being constructed.
The Contractor shall be responsible for clearing the site required to gain access to the fence construction site. This may require, but not be limited to, clearing brush, weeds, debris, and other material, vegetation, and growth.
[bookmark: _Toc89784933][bookmark: _Toc112919830][bookmark: _Toc120526707]MAINTENANCE AND PROTECTION OF TRAFFIC
There will be no provisions for payment for the maintenance and protection of traffic for fence operations that do not interfere with the existing flow of traffic. The State will not be responsible for any cost associated for the protection of Contractor personnel and traffic safety. All safety set-ups shall conform to NJDOT’s Manual on Uniform Traffic Control Devices (MUTCD) as located at the following link: https://mutcd.fhwa.dot.gov/pdfs/2009r1r2/mutcd2009r1r2edition.pdf. MUTCD’s website can be accessed at the following link: https://mutcd.fhwa.dot.gov/. NJDOT and Using Agencies have the right to adjust or restrict the hours of work, if operations create a lane restriction or result in a highway closure during peak traffic hours. 
[bookmark: _Toc89784934][bookmark: _Toc112919831][bookmark: _Toc120526708]TRAFFIC CONTROL DEVICES
The State will not purchase or provide, in any way, maintenance of traffic control devices as required by the MUTCD. The Contractor shall be responsible for providing maintenance of traffic control devices at no additional cost to the State. 
[bookmark: _Toc89784935][bookmark: _Hlk92975361][bookmark: _Toc112919832][bookmark: _Toc120526709]ROADWAY LANE CLOSURE
The cost for roadway Lane Closures will be paid in accordance with the provisions specified below. The Contractor shall be responsible for, but not limited to, providing signs, barricades, traffic control trucks with mounted crash cushions, cones, and flashing arrow boards, all in in accordance with the number, configuration, and placement as shown on the Standard Construction Details and in compliance with the MUTCD, located at the following link: https://mutcd.fhwa.dot.gov/pdfs/2009r1r2/mutcd2009r1r2edition.pdf. For lane closures on State Highways, the Contractor must follow the 2016 Traffic Control Details at the following link https://www.state.nj.us/transportation/eng/CADD/v8/pdf/StandConstDetails.pdf.
The cost, on an hourly basis, for roadway lane closure on both sides of a barrier fence shall be included in the costfence inclusive of safety-related set-up are, found in the Price Lines below:
A. North Region – Price Lines #108 to #1161 and 111; 
B. Central Region – Price Lines #316 to #323188 and 298; and 
C. South Region – Price Lines #375 and #523 to #530485.

The cost, on an hourly basis, for lane closures when additional safety beyond both sides of a barrier fence, inclusive of safety-related set-up, is required, are found in the Price Lines below:

A. North Region – Price Lines #2 and #112; 
B. Central Region – Price Lines #189 and 299; and 
C. South Region – Price Lines #376 and 486.

The Contractor will be paid for additional roadway lane closure on an hourly basis for each lane closure required, with a minimum of four (4) hours per day, when approved by NJDOT’s Resident Engineer or the Using Agency main point of contact. The Contractor shall provide additional lane closure for when additional safety-related set-ups beyond both sides of a barrier fence are required. 


[bookmark: _Toc89784937][bookmark: _Toc112919833][bookmark: _Toc120526710]WORKPLACE SAFETY AND HEALTH
The Contractor shall comply with all applicable Occupational Safety and Health Administration (OSHA) standards and applicable federal, State, and local regulations, including but not limited to personnel qualifications. 
In accordance with OSHA standards, the Contractor and its personnel shall, at a minimum:
A. Conform to safety and health practices for the protection of all personnel and property;
B. Establish, implement, and maintain a safety program within ten (10) business days of Blanket P.O. award and prior to the commencement of an engagement, to be submitted and approved by the Using Agency main point of contact or SCM. At a minimum, the program shall consist of an Emergency Response Plan that includes but is not limited to:
1. Reporting emergencies to local authorities;
2. Protective actions for life;
3. Incident stabilization, and
4. Any additional topic deemed necessary by the Using Agency main point of contact, SCM, and/or Contractor.
C. Meet all applicable fire and workplace safety and health regulatory requirements (OSHA, Department of Community Affairs, Division of Fire Safety, etc.); 
D. Report emergencies immediately to the local emergency response agency through 911 in accordance with the Contractor’s own emergency plan, as part of its safety program. The Contractor shall take corrective action and report workplace injuries per the OSHA guidelines; and
E. Report emergencies via in person or by phone to the Using Agency main point of contact/SCM within two (2) hours of an occurrence on State or local property.   
[bookmark: _Toc89784938][bookmark: _Toc112919834][bookmark: _Toc120526711]SAFETY EQUIPMENT AND WORK ATTIRE
While on a project site, the Contractor shall wear, at a minimum, the safety equipment and work attire listed below:
A. Head protection (hard hats);
B. Eye protection (safety glasses);
C. Hearing Protection (headphones/earplugs);
D. Appropriate clothing for the task being performed. Long pants and a short-sleeve shirt is a minimum;
E. The appropriate footwear based on an assessment by the Foreman (crew Leader) of hazards that may exist while performing work (e.g. closed toed, slip resistant, puncture resistant sole footwear, crush resistant toes, or toe/metatarsal guards when warranted); 
F. High visibility safety apparel, while exposed to road operations, vehicular Traffic or working on the Right-Of-Way.  Apparel shall meet the current ANSI 107 Standard. The performance class shall be chosen based on the ANSI Guidelines, however, Class-1 apparel shall not be considered acceptable for these work locations; and
G. Use and maintain safety and Personal Protective Equipment (PPE) for all Contractor employees. PPE must meet current ANSI standards at a minimum:
1. Life lines, harnesses, and fall protection systems;
2. First aid kit; and
3. Protective helmets, hearing protection, and other protective attire and equipment.
[bookmark: _Toc89784939][bookmark: _Toc112919835][bookmark: _Toc120526712][bookmark: _Toc453765996][bookmark: _Toc454790661][bookmark: _Toc508883620][bookmark: _Toc2672500][bookmark: _Toc4059048]PUBLIC WORKS CONTRACTOR REGISTRATION ACT 
This act specifies that no Contractor or Subcontractor shall engage in, any Blanket P.O. (or part thereof) for public work which is subject to the provisions of N.J.S.A 34:11-56.48, et seq. for the construction, reconstruction, demolition, alteration, custom fabrication, repair work, or maintenance work done under contract and paid for in whole or in part out of the funds of a public body or if the property or premises are owned by the public body, unless the Contractors and named Subcontractors maintain a valid public works certificate issued by the Department of Labor and Workforce Development during the duration of the Blanket P.O. period.  All Contractors and named Subcontractors must maintain a valid public works certificate issued by the Department of Labor and Workforce Development during the duration of the Blanket P.O. period.

[bookmark: _Toc4059049][bookmark: _Toc89784940][bookmark: _Toc112919836][bookmark: _Toc120526713]PREVAILING WAGE
The NJ State Prevailing Wage Act, N.J.S.A. 34:11-56.25 et seq. applies to public work and building services performed under this procurement.  This Act establishes wage standards for all workers performing public work and building services for properties or premises owned or leased by the State, requiring the payment of the State Prevailing Wage rate to all employees performing those duties. See N.J.S.A. 34:11-56.25 to -56.47; N.J.S.A. 34:11-56.58 to -56.70. Prevailing wages amounts are listed by county.  It is the responsibility of the Contractor to comply with the requirements of the State Prevailing Wage Act as well as adhere to the requirements of the Fair Labor Standards Act (FLSA) during the duration of this Contract and any extensions exercised.  Prevailing wages by county can be found on the wage determinations website at https://www.nj.gov/labor/wagehour/wagerate/CurrentWageRates.html.  If it is found that any worker employed by the Contractor or any subcontractor under the Blanket P.O. has been paid a rate of wages less than the prevailing wage required to be paid under the Blanket P.O., the State may terminate the Contractor’s  and/or subcontractor’s right to proceed with the work, or such part of the work as to which there has been a failure to pay required wages and may prosecute the work to completion.
[bookmark: _Toc454790662][bookmark: _Toc89784941][bookmark: _Toc112919837][bookmark: _Toc120526714]CERTIFIED PAYROLL RECORDS
N.J.A.C. 12:60-5.1 of the New Jersey Prevailing Wage Act and N.J.S.A. 34:11-56.25 et seq. requires that certified payroll records must be submitted to the public body, by all Contractors and Subcontractors, for each employee on the project within ten (10) days of the payment of wages. The Using Agency shall receive, file and make these records available for inspection during normal business hours.





[bookmark: _Toc120526715]GENERAL CONTRACT TERMS
The Contractor shall have sole responsibility for the complete effort specified in this Contract.  Payment will be made only to the Contractor or to the authorized dealers/distributors, if applicable.  The Contractor is responsible for the professional quality, technical accuracy and timely completion and submission of all deliverables, services or commodities required to be provided under this Contract.  The Contractor shall, without additional compensation, correct or revise any errors, omissions, or other deficiencies in its deliverables and other services.  The approval of deliverables furnished under this Contract shall not in any way relieve the Contractor of responsibility for the technical adequacy of its work.  The review, approval, acceptance or payment for any of the deliverables, goods or services, shall not be construed as a waiver of any rights that the State may have arising out of the Contractor’s performance of this Contract.

[bookmark: _Toc120526716]CONTRACT TERM AND EXTENSION OPTION
The base term of this Contract shall be for a period of three (3) years.  The anticipated Contract effective date is provided on the “Summary” page the Bid Solicitation in NJSTART.  If delays in the procurement process result in a change to the anticipated Contract effective date, the Contractor agrees to accept a Contract for the full term of this Contract 

This Contract may be extended up to two (2) years with no single extension exceeding one (1) year, by the mutual written consent of the Contractor and the Director at the same terms, conditions, and pricing at the rates in effect in the last year of this Contract or rates more favorable to the State.  

[bookmark: _Toc400531508][bookmark: _Toc428533979][bookmark: _Toc32310704][bookmark: _Toc120526717]CONTRACT TRANSITION
In the event that a new Contract has not been awarded prior to the expiration date for this Contract, including any extensions exercised, and the State exercises this Contract transition, the Contractor shall continue this Contract under the same terms, conditions, and pricing until a new Contract can be completely operational.  At no time shall this transition period extend more than 180 days calendar days beyond the expiration date of this Contract, including any extensions exercised.

[bookmark: _Toc118513795][bookmark: _Toc400531563][bookmark: _Toc428534035][bookmark: _Toc32310758][bookmark: _Toc120526718][bookmark: OLE_LINK3][bookmark: OLE_LINK4]PERFORMANCE SECURITY
Not applicable to this procurement.

[bookmark: _Toc400531513][bookmark: _Toc428533984][bookmark: _Toc32310709][bookmark: _Toc120526719]OWNERSHIP OF MATERIAL
Not applicable to this procurement.

[bookmark: _Toc120526720]SUBSTITUTION OF STAFF
If a Contractor needs to substitute any management, supervisory or key personnel, the Contractor shall identify the substitute personnel and the work to be performed.  The Contractor must provide detailed justification documenting the necessity for the substitution.  Resumes must be submitted for the individual(s) proposed as substitute(s) whom must have qualifications and experience equal to or better than the individual(s) originally proposed or currently assigned.

The Contractor shall forward a request to substitute staff to the State Contract Manager for consideration and approval.  No substitute personnel are authorized to begin work until the Contractor has received written approval to proceed from the State Contract Manager.

[bookmark: _Toc120526721]DELIVERY TIME AND COSTS
Unless otherwise noted in this Bid Solicitation or on the State-Supplied Price Sheet, all delivery times are thirty (30) calendar days after receipt of order (ARO) and prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination (30 calendar days ARO/F.O.B.).  The Contractor shall assume all costs, liability and responsibility for the delivery of merchandise in good condition to the State's Using Agency or designated purchaser.  Thirty calendar days ARO/F.O.B. does not cover "spotting" but does include delivery on the receiving platform of the Using Agency at any destination in the State of New Jersey unless otherwise specified.  No additional charges will be allowed for any additional transportation costs resulting from partial shipments made at the Contractor’s convenience when a single shipment is ordered.  The weights and measures of the State's Using Agency receiving the shipment shall govern.  Collect on Delivery (C.O.D.) Terms are not permitted.
All delivery times are thirty (30) calendar days after receipt of order (ARO) and prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination (30 calendar days ARO/F.O.B.).  The Contractor shall assume all costs, liability and responsibility for the delivery of merchandise in good condition to the State's Using Agency or designated purchaser.  Thirty calendar days ARO/F.O.B. does not cover "spotting" but does include delivery on the receiving platform of the Using Agency at any destination in the State of New Jersey unless otherwise specified.  No additional charges will be allowed for any additional transportation costs resulting from partial shipments made at the Contractor’s convenience when a single shipment is ordered.  The weights and measures of the State's Using Agency receiving the shipment shall govern.  Collect on Delivery (C.O.D.) Terms are not permitted.

[bookmark: _Toc120526722]AUTHORIZED DEALER AND/OR DISTRIBUTORS
Not applicable to this procurement.

[bookmark: _Toc400531525][bookmark: _Toc428533996][bookmark: _Toc32310718][bookmark: _Toc120526723]LIQUIDATED DAMAGES
[bookmark: _Toc400531531][bookmark: _Toc428534002][bookmark: _Toc32310724]Not applicable to this procurement. 

[bookmark: _Toc120526724]RETAINAGE
Not applicable to this procurement. 

[bookmark: _Toc120526725]ELECTRONIC PAYMENTS
With the award of this Contract, the successful Contractor(s) will be required to receive its payment(s) electronically.  In order to receive your payments via automatic deposit from the State of New Jersey, you must complete the EFT information within your NJSTART Vendor Profile.  Please refer to the QRG entitled “Vendor Profile Management – Company Information and User Access” for instructions. 

CONTRACT ACTIVITY REPORT REPORTING AND SUPPLIER CONVENIENCE FEE
A. Quarterly Sales Reporting - The Contractor shall submit a Sales Report documenting all sales made under the Contract.  The Sales Report shall be submitted directly to Periscope using the NJSTART system no later than thirty (30) calendar days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31. The Sales Report must contain the following information:  
· Complete and accurate details of all sales, credits, returns, refunds, and the like for the reporting quarter;
· Purchasing entity;
· Total of Supplier Convenience Fee amount due for the reporting quarter;
· Such other information as the State may reasonably request; and
· If no sales were made to the State during the reporting quarter, then a report shall be submitted showing zero sales and zero Supplier Convenience Fee due.
Quarterly Sales Reporting and remittance of the Supplier Convenience Fee shall begin on the first calendar quarter starting after the effective date of the Contract.
B. Supplier Convenience Fee - For all purchases made under the Contract, the Contractor shall remit the Supplier Convenience Fee in the amount of one percent (1%) of all Purchases to Periscope Holdings, Inc. (Periscope). 
C. Remittance of the Supplier Convenience Fee - On a quarterly basis, the Contractor shall remit the Supplier Convenience Fee directly to Periscope no later than thirty (30) days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31.  Failure to remit the Supplier Convenience Fee timely and accurately may result in Contractor’s goods and/or services being made ineligible for purchase through the NJSTART Marketplace.
D. Retention and Inspection of Records and Audit - The Contractor shall keep records of all sales made to Using Agencies and Intrastate Cooperative Purchasing Participants in sufficient detail to enable the State to determine the Supplier Convenience Fee payable by the Contractor. The State and/or Periscope may examine and audit, at its own expense, Contractor’s sales records and Sales Reports for completeness and accuracy. If such examination reveals underpayment of the Supplier Convenience Fee, the Contractor shall immediately pay to Periscope the amount of deficiency. If the examination reveals an underpayment of 5% or more, then the Contractor shall reimburse the State and/or Periscope for the cost of the audit.
E. Catalog Enablement - The Contractor shall cooperate with the State and/or Periscope as requested to upload catalog items and pricing consistent with the awarded Contract to the NJSTART Marketplace module within thirty days (30) of the Contract award.
The Contractor must provide, on a quarterly basis, a record of all purchases made under this Contract.  The calendar quarters will end March 31, June 30, September 30, and December 31 with the required reports due no later than thirty (30) days after the calendar quarter.  The Contractor must submit the required information in Microsoft Excel format to NJSupplierReports@treas.nj.gov. 

This reporting requirement includes sales to State Using Agencies, political sub-divisions thereof and, if permitted under the terms of this Contract, sales to counties, municipalities, school districts, volunteer fire departments, first aid squads and rescue squads, independent institutions of higher education, state and county colleges and quasi-State entities.  Quasi-State entities include any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member.

This information must be provided in Microsoft Excel such that an analysis can be made to determine the following:
A. Contractor’s total sales volume, with line item detail, to each purchaser under this Contract;
B. Subtotals by product, including, if applicable, catalog number and description, price list with appropriate page reference, and/or Contract, discount applied; and
C. Total dollars paid to Subcontractors.

Submission of purchase orders, confirmations, and/or invoices do not fulfill this Contract requirement for information.  Failure to report this mandated information may be a factor in future award decisions.


[bookmark: _Toc120526727]DATA SECURITY REQUIREMENTS – CONTRACTOR RESPONSIBILITY 

Not applicable to this procurement.



[bookmark: _4.4.1.1_Ownership_Disclosure][bookmark: _4.4.1.1_Signatory_page][bookmark: _4.4.2.3_Contract_Schedule][bookmark: _4.4.2.4_mobilization_and][bookmark: _Toc120526728]MODIFICATIONS TO THE STATE OF NEW JERSEY STANDARD TERMS AND CONDITIONS

Not applicable to this procurement.























































[bookmark: _Toc120526729]QUOTE EVALUATION AND AWARD

[bookmark: _Toc400531542][bookmark: _Toc428534014][bookmark: _Toc32310736][bookmark: _Toc120526730]RIGHT TO WAIVE
Pursuant to N.J.A.C. 17:12-2.7(d) the Director may waive minor irregularities or omissions in a Quote.  The Director reserves the right to waive a requirement provided that the requirement does not materially affect the procurement or the State's interests associated with the procurement.
[bookmark: _Toc400531543][bookmark: _Toc428534015][bookmark: _Toc32310737]
[bookmark: _Toc120526731]DIRECTOR’S RIGHT TO ACCEPT OR REJECT A QUOTE
The Director reserves the right to reject any or all Quotes, or to award in whole or in part if deemed to be in the best interest of the State to do so. The Director shall have authority to award Contracts in accordance with N.J.S.A. 52:34-12. 

[bookmark: _Toc120526732]RECIPROCITY FOR JURISDICTIONAL BIDDER PREFERENCE
In accordance with N.J.S.A. 52:32-1.4 and N.J.A.C. 17:12-2.13, the State of New Jersey will invoke reciprocal action against an out-of-State Bidder whose state or locality maintains a preference practice for its in-state Bidders.  The State of New Jersey will use the annual surveys compiled by the Council of State Governments, National Association of State Procurement Officials, or the National Institute of Governmental Purchasing or a State’s statutes and regulations to identify States having preference laws, regulations, or practices and to invoke reciprocal actions. The State of New Jersey may obtain additional information as it deems appropriate to supplement the stated survey information.

A Bidder may submit information related to preference practices enacted for a State or Local entity outside the State of New Jersey. This information may be submitted in writing as part of the Quote response, including name of the locality having the preference practice, as well as identification of the county and state, and should include a copy of the appropriate documentation, i.e., resolution, regulation, law, notice to Bidder, etc.  It is the responsibility of the Bidder to provide documentation with the Quote or submit it to the Director within five (5) business days after the deadline for Quote submission.  Written evidence for a specific procurement that is not provided to the Director within five (5) business days of the public Quote submission date may not be considered in the evaluation of that procurement, but may be retained and considered in the evaluation of subsequent procurements.

[bookmark: _Toc400531545][bookmark: _Toc428534017][bookmark: _Toc32310739][bookmark: _Toc120526733]CLARIFICATION OF QUOTE
After the Quote Opening Date, unless requested by the State as noted below, Bidder contact with the Procurement Bureau regarding this Bid Solicitation and the submitted Quote is not permitted. 

After the Quotes are reviewed, one (1), some or all of the Bidders may be asked to clarify certain aspects of its Quote.  A request for clarification may be made in order to resolve minor ambiguities, irregularities, informalities or clerical errors.  Clarifications cannot correct any deficiencies, material omissions, or used to revise or modify a Quote.

The Director reserves the right to request that a Bidder to explain, in detail, how the Quote price was determined.

[bookmark: _Toc32310741][bookmark: _Toc120526734][bookmark: _Toc118513837][bookmark: _Toc400531547][bookmark: _Toc428534019]ORAL PRESENTATION 
Not applicable to this procurement.

[bookmark: _Toc120526735]TIE QUOTES
Tie Quotes will be awarded by the Director in accordance with N.J.A.C. 17:12-2.10. 

[bookmark: _Toc120526736]STATE'S RIGHT TO INSPECT BIDDER’S FACILITIES
The State reserves the right to inspect the Bidder’s establishment before making an award, for the purposes of ascertaining whether the Bidder has the necessary facilities for performing the Contract.

[bookmark: _Toc120526737]STATE'S RIGHT TO CHECK REFERENCES
The State may also consult with clients of the Bidder during the evaluation of Quotes. Such consultation is intended to assist the State in making a Contract award that is most advantageous to the State.

[bookmark: _Toc120526738]EVALUATION CRITERIA
The following evaluation criteria categories, not necessarily listed in order of significance, will be used to evaluate Quotes received in response to this Bid Solicitation.  The evaluation criteria categories may be used to develop more detailed evaluation criteria to be used in the evaluation process.

[bookmark: _Toc118513839][bookmark: _Toc400531549][bookmark: _Toc428534021][bookmark: _Toc32310743][bookmark: _Toc120526739]TECHNICAL EVALUATION CRITERIA
The following criteria will be used to evaluate and score Quotes received in response to this Bid Solicitation:  
A. The Bidder’s demonstration in the Quote that the Bidder understands and is able to complete the requirements of the Scope of Work as sought.

[bookmark: _Toc118513840][bookmark: _Toc400531550][bookmark: _Toc428534022][bookmark: _Toc32310744][bookmark: _Toc120526740]PRICE EVALUATION
For evaluation purposes, Bidders will be ranked in each Category award grouping from lowest to highest according to the total Category grouping price located on the State-Supplied Price Sheets accompanying this Bid Solicitation. 

Price Lines #2, 102, 130, 131, 132, 135, 136, 139, 140, 144, 146, 206, and 207 3, 83, 113, 114, 115, 117, 118, 120, 121, 124, 126, 186, 187 for the North Region will be evaluated for reasonableness. Price Lines #209, 309, 337, 338, 339, 342, 343, 346, 347, 351, 353, 413, and 414 190, 270, 300, 301, 302, 304, 305, 307, 308, 311, 313, 373, and 374 for the Central Region will be evaluated for reasonableness. Price Lines #416, 516, 544, 545, 546, 549, 550, 552, 553, 557, 559, 619, and 620377, 457, 487, 488, 489, 491, 492, 494, 495, 498, 500, 560, and 561 for the South Region will be evaluated for reasonableness.

[bookmark: _Toc118513841][bookmark: _Toc400531551][bookmark: _Toc428534023][bookmark: _Toc32310745][bookmark: _Toc120526741]QUOTE DISCREPANCIES
In evaluating Quotes, discrepancies between words and figures will be resolved in favor of words.  Discrepancies between Unit Prices and totals of Unit Prices will be resolved in favor of Unit Prices.  Discrepancies in the multiplication of units of work and Unit Prices will be resolved in favor of the Unit Prices.  Discrepancies between the indicated total of multiplied Unit Prices and units of work and the actual total will be resolved in favor of the actual total.  Discrepancies between the indicated sum of any column of figures and the correct sum thereof will be resolved in favor of the correct sum of the column of figures.

[bookmark: _Toc118513842][bookmark: _Toc400531553][bookmark: _Toc428534025][bookmark: _Toc32310747][bookmark: _Toc120526742]NEGOTIATION
In accordance with N.J.S.A. 52:34-12(f) and N.J.A.C. 17:12-2-7, after evaluating Quotes, the Procurement Bureau may establish a competitive range and enter into negotiations with one (1) Bidder or multiple Bidders within this competitive range.  The primary purpose of negotiations is to maximize the State’s ability to obtain the best value based on the mandatory requirements, evaluation criteria, and cost.  Multiple rounds of negotiations may be conducted with one (1) Bidder or multiple Bidders.  Negotiations will be structured by the Procurement Bureau to safeguard information and ensure that all Bidders are treated fairly.

Negotiations will be conducted only in those circumstances where it is deemed by the Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Bidder is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Contract award based on the content of the initial submission.  

If the Procurement Bureau contemplates negotiation, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Bidder will be publicly announced at the Quote opening.

[bookmark: _Toc120526743]BEST AND FINAL OFFER (BAFO) 
The Procurement Bureau may invite one (1) Bidder or multiple Bidders to submit a Best and Final Offer (BAFO). Said invitation will establish the time and place for submission of the BAFO. Any BAFO that does not result in more advantageous pricing to the State will not be considered, and the State will evaluate the Bidder’s most advantageous previously submitted pricing.

The Division may conduct more than one (1) round of BAFO in order to attain the best value for the State. 

BAFOs will be conducted only in those circumstances where it is deemed by the Procurement Bureau or Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Bidder is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Contract award based on the content of the initial submission 

If the Procurement Bureau contemplates BAFOs, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Bidder will be publicly announced at the Quote opening.

[bookmark: _Toc32310748][bookmark: _Toc120526744]“REQUEST FOR REVISION” WITHIN NJSTART
The State may request a revision of the Bidder’s Quote within NJSTART. The Bidder shall respond to the “Request for Revision” only for the reason(s) identified by the State. Any changes made by a Bidder to the Quote other than as requested by the State shall be considered null and void. 

[bookmark: _Toc400531554][bookmark: _Toc428534026][bookmark: _Toc32310749][bookmark: _Toc120526745]POOR PERFORMANCE
A Bidder with a history of performance problems may be bypassed for consideration of an award issued as a result of this Bid Solicitation. The following materials may be reviewed to determine Bidder performance:  
A. Contract cancellations for cause pursuant to State of New Jersey Standard Terms and Conditions Section 5.7(B); 
B. Iinformation contained in Vendor performance records; 
C. Iinformation obtained from audits or investigations conducted by a local, state or federal agency of the Bidder’s work experience; 
D. Ccurrent licensure, registration, and/or certification status and relevant history thereof; or 
E. Bidder’s status or rating with established business/financial reporting services, as applicable.  

Bidders should note that this list is not exhaustive.

[bookmark: _Toc120526746]RECOMMENDATION FOR AWARD 
After the evaluation of the submitted Quotes is complete, the Procurement Bureau will recommend to the Director for award, the responsible Bidder(s) whose Quote, conforming to this Bid Solicitation, is most advantageous to the State, price and other factors considered.  The Director may accept, reject or modify the recommendation of the Procurement Bureau.

[bookmark: _Toc400531561][bookmark: _Toc428534033][bookmark: _Toc32310756][bookmark: _Toc120526747]CONTRACT AWARD
Contract award(s) will be made with reasonable promptness by written notice to those responsible Bidder(s), whose Quote(s), conforming to this Bid Solicitation, is(are) most advantageous to the State, price, and other factors considered.  Any or all Quotes may be rejected when the State Treasurer or the Director determines that it is in the public interest to do so.

The State intends to make multiple Blanket P.O. awards in accordance with Section 3.8, Small Business Set-Aside Contracts, with two (2) one (1) awards set-aside for Small Business Enterprises (SBE) for each Category for each Region. Should an SBE business not bid or be responsive within a Category, the State may award to the next qualifying Bidder, including non-SBE classified Bidders.



[bookmark: _Toc120526748]GLOSSARY

[bookmark: _Toc120526749]CROSSWALK
[bookmark: _CROSSWALK]
	NJSTART Term
	Equivalent Statutory, Regulatory and/or Legacy Term

	Bid/Bid Solicitation 
	Request For Proposal (RFP)/Solicitation

	Bid Amendment 
	Addendum

	Change Order 
	Contract Amendment

	Master Blanket Purchase Order (Blanket/Blanket P.O.) 
	Contract

	Offer and Acceptance Page
	Signatory Page

	Quote
	Proposal

	Vendor 
	Bidder/Contractor



[bookmark: _Toc114734106][bookmark: _Toc120526750]DEFINITIONS
Unless otherwise specified in the Bid Solicitation, the following definitions will be part of any Contract awarded, or order placed, as a result of this Bid Solicitation.  Note that not all definitions included here apply to all Bid Solicitations..
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AASHTO – American Association of State Highway and Transportation Officials.  

Acceptance – The written confirmation by the Using Agency that Contractor has completed a Deliverable according to the specified requirements.

Agency Inspector – The person designated by the Using Agency to do inspection of the work.

AISI – American Iron and Steel Institute. 

All-Inclusive Hourly Rate – An hourly rate comprised of all direct and indirect costs including, but not limited to: labor costs, overhead, fee or profit, clerical support, travel expenses, per diem, safety equipment, materials, supplies, managerial support and all documents, forms, and reproductions thereof.  This rate also includes portal-to-portal expenses as well as per diem expenses such as food.

Apparel - means any clothing, headwear, linens or fabric.  

Apparel Contracts - include all purchases, rentals or other acquisition of apparel products by the State of New Jersey, including authorizations by the State of New Jersey for vendors to sell apparel products through cash allowances or vouchers issued by the State of New Jersey, and license agreements with a public body.

Apparel Production - includes the cutting and manufacturing of apparel products performed by the vendor or by any subcontractors, but not including the production of supplies or sundries such as buttons, zippers, and thread.

Approved Products – Those products that have been identified in Bid Solicitation as meeting Using Agency needs and confirmed as meeting product specifications.

ASTM – American Society for Testing and Materials. The American Standard Test Method is included and part of the American Society for testing and Materials. 

AWS – American Welding Society. 

Best and Final Offer or BAFO – Pricing timely submitted by a Bidder upon invitation by the Procurement Bureau after Quote opening, with or without prior discussion or negotiation.

Bid or Bid Solicitation – The documents which establish the bidding and Contract requirements and solicits Quotes to meet the needs of the Using Agencies as identified herein, and includes the Bid Solicitation, State of New Jersey Standard Terms and Conditions (SSTC), State-Supplied Price Sheet, Attachments, and Bid Amendments.

Bid Amendment – Written clarification or revision to this Bid Solicitation issued by the Division. Bid Amendments, if any, will be issued prior to Quote opening.

Bid Opening Date – The date Quotes will be opened for evaluation and closed to further Quote submissions.

Bid Security - means a guarantee, in a form acceptable to the Division, that the bidder, if selected, will accept the contract as bid; otherwise, the bidder or, as applicable, its guarantor will be liable for the amount of the loss suffered by the State, which loss may be partially or completely recovered by the State in exercising its rights against the instrument of bid security.

Bidder – An entity offering a Quote in response to the Division’s Bid Solicitation.

Breach of Security – as defined by N.J.S.A. 56:8-161, means unauthorized access to electronic files, media, or data containing Personal Data that compromises the security, confidentiality, or integrity of Personal Data when access to the Personal Data has not been secured by encryption or by any other method or technology that renders the Personal Data unreadable or unusable.  Good faith acquisition of Personal Data by an employee or agent of the Provider for a legitimate business purpose is not a Breach of Security, provided that the Personal Data is not used for a purposes unrelated to the business or subject to further unauthorized disclosure.  

Business Day – Any weekday, excluding Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Calendar Day – Any day, including Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Change Order – An amendment, alteration, or modification of the terms of a Contract between the State and the Contractor(s). A Change Order is not effective until it is signed and approved in writing by the Director or Deputy Director, Division of Purchase and Property.

Commercial off the Shelf Software or COTS - Software provided by Provider that is commercially available and that can be used with little or no modification.

Customized Software - COTS that is adapted or configured by Provider to meet specific requirements of the Authorized Purchaser that differ from the standard requirements of the base product. For the avoidance of doubt, “Customized Software” is not permitted to be sold to the State under the scope of this Contract.

Contract – The Contract consists of the State of NJ Standard Terms and Conditions (SSTC), the Bid Solicitation, the responsive Quote submitted by a responsible Bidder as accepted by the State, the notice of award, any Best and Final Offer, any subsequent written document memorializing the agreement, any modifications to any of these documents approved by the State and any attachments, Bid Amendment or other supporting documents, or post-award documents including Change Orders agreed to by the State and the Contractor, in writing.

Contractor – The Bidder awarded a Contract resulting from this Bid Solicitation.

Cooperative Purchasing Program – The Division’s intrastate program that provides procurement-related assistance to New Jersey local governmental entities and boards of education, State and county colleges and other public entities having statutory authority to utilize select State Contract s issued by the Division, pursuant to the provisions of N.J.S.A. 52:25-16.1 et seq.

Cooperative Purchasing Participants - These participants include quasi-State entities, counties, municipalities, school districts, volunteer fire departments, first aid squads, independent institutions of higher learning, County colleges, and State colleges

Days After Receipt of Order (ARO) – The number of calendar days ‘After Receipt of Order’ in which the Using Agency will receive the ordered materials and/or services.

Dealer/Distributor – A Company authorized by a Bidder or Contractor as having the contractual ability to accept and fulfill orders and receive payments directly on behalf of the Contractor that is awarded a Contract.  Any authorized Dealer/Distributor must agree to all terms and conditions contained within the Bid Solicitation and must agree to provide all products and services in accordance with the Contract specifications, terms, conditions and pricing.  

Deliverable – Goods, products, Services and Work Product that Contractor is required to deliver to the State under the Contract.

Director – Director, Division of Purchase and Property, Department of the Treasury, who by statutory authority is the Chief Contracting Officer for the State of New Jersey; or the Director’s designee.

Disabled Veterans’ Business - means a business which has its principal place of business in the State, is independently owned and operated and at least 51% of which is owned and controlled by persons who are disabled veterans or a business which has its principal place of business in this State and has been officially verified by the United States Department of Veterans Affairs as a service disabled veteran-owned business for the purposes of department contracts pursuant to federal law.  N.J.S.A. 52:32-31.2.

Disabled Veterans’ Business Set-Aside Contract - means a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from disabled veterans’ businesses, or a portion of a Contract when that portion has been so designated.  N.J.S.A. 52:32-31.2.

Discount – The standard price reduction applied by the Bidder to all items.

Division – The Division of Purchase and Property.

EMPVC – Epoxy Modified Polyvinyl Chloride. 
Equivalent Products – Products offered other than those identified as an Approved Product in this Bid Solicitation that meet the specifications herein. Equivalent Products will be evaluated to ensure that they meet all technical, nutritional, and packaging specifications herein as part of the Quote evaluation process.

Evaluation Committee – A group of individuals or a Division staff member assigned by the Director to review and evaluate Quotes submitted in response to this Bid Solicitation and recommend a Contract award to the Director.

Firm Fixed Price – A price that is all-inclusive of direct cost and indirect costs, including, but not limited to, direct labor costs, overhead, fee or profit, clerical support, equipment, materials, supplies, managerial (administrative) support, all documents, reports, forms, travel, reproduction and any other costs.

Fusion-Bond Method – Fusion bond epoxy process where the surface of a pipe is cleaned and exposed to heat, an epoxy powder is applied onto the surface of the pipe electrostatically, and the powder undergoes melting onto the pipe surface and dries quickly in controlled and uniformed thickness.

Good Industry Practice – Standards, practices, methods and procedures conforming to the law and the degree of skill and care, diligence, prudence and foresight which would reasonably and ordinarily be expected from a skilled and experienced person or body engaged in a similar type of undertaking under the same or similar circumstances.

Hardware – Includes computer equipment and any Software provided with the Hardware that is necessary for the Hardware to operate.

I.D. – Interior Diameter. 

Internet of Things (IoT) - the network of physical devices, vehicles, home appliances and other items embedded with electronics, software, sensors, actuators, and network connectivity which enables these objects to connect and exchange data.

Intrastate cooperative purchasing participants - refers to political subdivisions, volunteer fire departments and first aid squads, and independent institutions of higher education and school districts pursuant to N.J.S.A. 52:25-16.1 et seq., State and county colleges pursuant to N.J.S.A. 18A:64-60 and 18A:64A-25.9, quasi-State agencies and independent authorities pursuant to N.J.S.A. 52:27B-56.1, and other New Jersey public entities having statutory authority to utilize select State contracts issued by the Division

Lane Closure – In order to accommodate the maintenance and protection of traffic on those project sites that require the closing of a normally traveled lane, the item “lane closure” will be included in this Blanket P.O. Lane closure will consist of the signs, barricades, traffic control trucks with mounted crash cushions and a flashing arrow board in accordance with the number, configuration, and placement as show on the Standard Construction Details and in accordance with the “Manual on Uniform Traffic Control Devices.” 

Joint Venture – A business undertaking by two (2) or more entities to share risk and responsibility for a specific project.

Life cycle assessment – The comprehensive examination of a product’s environmental and economic aspects and potential impacts throughout its lifetime, including raw material extraction, transportation, manufacturing, use and disposal.

Life cycle cost – The amortized total cost of a product, including capital costs, installation costs, operating costs, maintenance costs, and disposal costs discounted over the lifetime of the product.

Master Blanket Purchase Order (Blanket/Blanket P.O.) – A Term Contract that allows repeated purchases from an awarded contract.

Materials in Solid Waste – Material found in the various components of the solid waste stream. General, solid waste has several components, such as municipal solid waste (MSW), construction and demolition debris (C&D), and nonhazardous industrial waste.  Under RCRA Section 6002, EPA considers materials recovered from any component of the solid waste stream when designating items containing Recovered Materials.

May – Denotes that which is permissible or recommended, not mandatory.

Mobile Device - means any device used by Provider that can move or transmit data, including but not limited to laptops, hard drives, and flash drives.

Must – Denotes that which is a mandatory requirement.  

MUTCD – Manual or Uniform Traffic Control Devices. 

Net Purchases - means the total gross purchases, less credits, taxes, regulatory fees and separately stated shipping charges not included in unit prices, made by Intrastate Cooperative Purchasing Participants, regardless of whether or not NJSTART is used as part of the purchase process.

NJDEP – New Jersey Department of Environmental protection.

NJDOT – New Jersey Department of Transportation.

No Bid – The Bidder is not submitting a price Quote for an item on a price line.

No Charge – The Bidder will supply an item on a price line free of charge.

Non-Public Data - means data, other than Personal Data, that is not subject to distribution to the public as public information. Non-Public Data is data that is identified by the State as non-public information or otherwise deemed to be sensitive and confidential by the State because it contains information that is exempt by statute, ordinance or administrative rule from access by the general public as public information.

O.C. – On-center. A unit of measurement indicating the distance from the center of one framing member to the center of the next framing member.

OSHA – Occupational Safety and Health Administration. 

Percentage Discount or Markup - The percentage bid applied as a Markup or a Discount to a firm, fixed price contained within a price list/catalog. 

Performance Security - means a guarantee, executed subsequent to award, in a form acceptable to the Division, that the successful bidder will complete the contract as agreed and that the State will be protected from loss in the event the contractor fails to complete the contract as agreed.

Personal Data means – 
“Personal Information” as defined in N.J.S.A. 56:8-161, means an individual’s first name or first initial and last name linked with any one or more of the following data elements: (1) Social Security number, (2) driver’s license number or State identification card number or (3) account number or credit or debit card number, in combination with any required security code, access code, or password that would permit access to an individual’s financial account.  Dissociated data that, if linked would constitute Personal Information is Personal Information if the means to link the dissociated were accessed in connection with access to the dissociated data.  Personal Information shall not include publicly available information that is lawfully made available to the general public from federal, state or local government records, or widely distributed media; and/or 

Data, either alone or in combination with other data, that includes information relating to an individual that identifies the person or entity by name, identifying number, mark or description that can be readily associated with a particular individual and which is not a public record, including but not limited to, Personally Identifiable Information (PII); government-issued identification numbers (e.g., Social Security, driver’s license, passport); Protected Health Information (PHI) as that term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and defined below; and Education Records, as that term is defined in the Family Educational Rights and Privacy Act (FERPA), 20 U.S.C. § 1232g.

Personally Identifiable Information or PII - as defined by the U.S. Department of Commerce, National Institute of Standards and Technology, means any information about an individual maintained by an agency, including (1) any information that can be used to distinguish or trace an individual’s identity, such as name, social security number, date and place of birth, mother’s maiden name, or biometric records; and (2) any other information that is linked or linkable to an individual, such as medical, educational, financial, and employment information.

Post-Consumer Material – Material or finished product that has served its intended use and has been diverted or recovered from waste destined for disposal, having completed its life as a consumer item.  Post-Consumer Materials are part of the broader category of Recovered Materials.

PPE – Personal Protective Equipment. 

Pre-Consumer Material – Materials generated in manufacturing and converting processes, such as manufacturing scrap and trimmings/cuttings.

Preventative Maintenance – Maintenance that is regularly performed on systems and/or equipment to lessen the likelihood of failure. Preventative Maintenance includes, but not be limited to, periodic inspection, testing, cleaning, lubrication, adjustment, parts replacement, and repairs to keep the systems and equipment in optimum operating condition.

Price List/Catalog – A document published by a manufacturer, resellers, Dealers, or Distributors that typically contains product descriptions, a list of products with fixed prices to which a Bidder’s percentage discount or markup bid is applied. 

Primary Form – An electronic form contained within a Vendor’s NJSTART profile designated by the Vendor as the primary or principal version of the required form.

Procurement Bureau (Bureau) – The Division unit responsible for the preparation, advertisement, and issuance of Bid Solicitations, for the tabulation of Quotes and for recommending award(s) of Contract(s) to the Director and the Deputy Director.

Project – The undertakings or services that are the subject of this Bid Solicitation.

Project Manager – A Using Agency’s primary contact for projects, separate from NJDOT. 

Protected Health Information or PHI - has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 means Individually Identifiable Health Information (as defined below) transmitted by electronic media, maintained in electronic media, or transmitted or maintained in any other form or medium. PHI excludes education records covered by the Family Educational Rights and Privacy Act (FERPA), as amended, 20 U.S.C. 1232g, records described at 20 U.S.C. 1232g(a)(4)(B)(iv) and employment records held by a covered entity in its role as employer. The term “Individually Identifiable Health Information” has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and means information that is a subset of Protected Health Information, including demographic information collected from an individual, and (1) is created or received by a health care provider, health plan, employer or health care clearinghouse; and (2) relates to the past, present or future physical or mental health or condition of an individual; the provision of health care to an individual; or the past, present or future payment for the provision of health care to an individual; and (a) that identifies the individual; or (b) with respect to which there is a reasonable basis to believe the information can be used to identify the individual.

Purchases – Means the total gross purchases, less credits, taxes, regulatory fees and separately stated shipping charges not included in unit prices, made regardless of whether or not NJSTART is used as part of the purchase process.  

P.V.C. – Polyvinyl Chloride. 

Quasi-State Agency - is any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member, as defined in N.J.S.A. 52:27B-56.1, provided that any sale to any such bi-state governmental entity is for use solely within the State of New Jersey.

Quick Reference Guides (QRGs) – Informational documents which provide Vendors with step-by-step instructions to navigate the NJSTART eProcurement System. QRGs are available on the NJSTART Vendor Support Page.

Quote – Bidder’s timely response to the Bid Solicitation including, but not limited to, technical Quote, price Quote including Best and Final Offer, any licenses, forms, certifications, clarifications, negotiated documents, and/or other documentation required by the Bid Solicitation.

Quote Opening Date - The date Quotes will be opened for evaluation and closed to further Quote submissions.

Recovered Material – Waste material and byproduct that have been recovered or diverted from solid waste, but does not include materials and byproducts generated from, and commonly reused within, an original manufacturing process.

Recycling – The series of activities, including collection, separation, and processing, by which products or other materials are recovered from the solid waste stream for use in the form of raw materials in the manufacture of new products other than fuel for producing heat or power by combustion.

Recyclability – The ability of a product or material to be recovered from, or otherwise diverted from, the solid waste stream for the purpose of recycling.

Regional Engineer – NJDOT’s designated project engineer responsible for a specific region or project, specific to NJDOT.

Resident Engineer – NJDOT’s engineer who supervises crews from site but is not specific to a region. Duties include supervision of and issuing of instructions to the Contractor and to report regularly to the designer and/or client.

Retainage – The amount withheld from the Contractor payment that is retained and subsequently released upon satisfactory completion of performance milestones by the Contractor.

Revision – A response to a BAFO request or a requested clarification of the Bidder’s Quote. 

RMAN – Recovered Materials Advisory Notices provide purchasing guidance and recommendations for Recovered and Post-Consumer Material content levels for designated items. 

R.O.W. – Right of Way. 

Security Incident - means the potential access by non-authorized person(s) to Personal Data or Non-Public Data that the Provider believes could reasonably result in the use, disclosure, or access or theft of State’s unencrypted Personal Data or Non-Public Data within the possession or control of the Provider. A Security Incident may or may not turn into a Breach of Security.

Services – Includes, without limitation (i) Information Technology (IT) professional services, (ii) Software and Hardware-related services, including without limitation, installation, configuration, and training, and (iii) Software and Hardware maintenance and support and/or Software and Hardware technical support services. 

Shall – Denotes that which is a mandatory requirement.  

Should – Denotes that which is permissible or recommended, not mandatory.

Small Business – Pursuant to N.J.S.A. 52:32-19, N.J.A.C. 17:13-1.2, and N.J.A.C. 17:13-2.1, “small business” means a business that meets the requirements and definitions of “small business” and has applied for and been approved by the New Jersey Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit as (i) independently owned and operated, (ii) incorporated or registered in and has its principal place of business in the State of New Jersey; (iii)  has 100 or fewer full-time employees; and has gross revenues falling in one (1) of the six (6) following categories:  
For goods and services - (A) 0 to $500,000 (Category I); (B) $500,001 to $5,000,000 (Category II); and (C) $5,000,001 to $12,000,000, or the applicable federal revenue standards established at 13 CFR 121.201, whichever is higher (Category III). 
For construction services: (A) 0 to $3,000,000 (Category IV); (B) gross revenues that do not exceed 50 percent of the applicable annual revenue standards established at 13 CFR 121.201 (Category V); and (C) gross revenues that do not exceed the applicable annual revenue standards established at CFR 121.201, (Category VI).

Small Business Set-Aside Contract – means (1) a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from small businesses, or (2) a portion of a Contract when that portion has been so designated.”  N.J.S.A. 52:32-19.

Software - means, without limitation, computer programs, source codes, routines, or subroutines supplied by Provider, including operating software, programming aids, application programs, application programming interfaces and software products, and includes COTS, unless the context indicates otherwise.  

Software as a Service or SaaS - means the capability provided to a purchaser to use the Provider’s applications running on a cloud infrastructure. The applications are accessible from various client devices through a thin client interface such as a Web browser (e.g., Web-based email) or a program interface. The purchaser does not manage or control the underlying cloud infrastructure, including network, servers, operating systems, storage or even individual application capabilities, with the possible exception of limited user-specific application configuration settings.

State – The State of New Jersey.

State Confidential Information - shall consist of State Data and State Intellectual Property  supplied by the State, any information or data gathered by the Contractor in fulfillment of the Contract and any analysis thereof (whether in fulfillment of the Contract or not);

State Contract Manager or SCM – The individual, responsible for the approval of all deliverables, i.e., tasks, sub-tasks or other work elements in the Scope of Work.  The SCM cannot direct or approve a Change Order.

State Data - means all data and metadata created or in any way originating with the State, and all data that is the output of computer processing of or other electronic manipulation of any data that was created by or in any way originated with the State, whether such data or output is stored on the State’s hardware, the Provider’s hardware or exists in any system owned, maintained or otherwise controlled by the State or by the Provider.  State Data includes Personal Data and Non-Public Data.

State Intellectual Property – Any intellectual property that is owned by the State.  State Intellectual Property includes any derivative works and compilations of any State Intellectual Property.

State Price Sheet or State-Supplied Price Sheet – the bidding document created by the State and attached to this Bid Solicitation on which the Bidder submits its Quote pricing as is referenced and described in the Bid Solicitation.   

Subtasks – Detailed activities that comprise the actual performance of a task.

Subcontractor – An entity having an arrangement with a Contractor, whereby the Contractor uses the products and/or services of that entity to fulfill some of its obligations under its State Contract, while retaining full responsibility for the performance of all  Contractor's obligations under the Contract, including payment to the Subcontractor.  The Subcontractor has no legal relationship with the State, only with the Contractor.

Task – A discrete unit of work to be performed.

Third Party Intellectual Property – Any intellectual property owned by parties other than the State or Contractor and contained in or necessary for the use of the Deliverables.  Third Party Intellectual Property includes COTS owned by Third Parties, and derivative works and compilations of any Third Party Intellectual Property. 

U.L. – Underwriters Laboratories. An independent safety science company which tests and certifies products in respect of their safety.

Unified Thread Standard – A standard thread form and series for bolts, nuts, screws, and other thread fasteners.

Unit Cost or Unit Price – All-inclusive, firm fixed price charged by the Bidder for a single unit identified on a price line.

US CERT – United States Computer Emergency Readiness Team.


USEPA – United States Environmental Protection Agency

Using Agency[ies] – A State department or agency, a quasi-State governmental entity, or an Intrastate Cooperative Purchasing participant, authorized to purchase products and/or services under a Contract procured by the Division. 

Vendor – Either the Bidder or the Contractor.

Vendor Intellectual Property – Any intellectual property that is owned by Contractor and contained in or necessary for the use of the Deliverables or which the Contractor makes available for the State to use as part of the work under the Contract Vendor Intellectual Property includes COTS or Customized Software owned by Contractor, Contractor’s technical documentation, and derivative works and compilations of any Vendor Intellectual Property.

Work Product – Every invention, modification, discovery, design, development, customization, configuration, improvement, process, Software program, work of authorship, documentation, formula, datum, technique, know how, secret, or intellectual property right whatsoever or any interest therein (whether patentable or not patentable or registerable under copyright or similar statutes or subject to analogous protection) that is specifically made, conceived, discovered, or reduced to practice by Contractor or Contractor’s subcontractors or a third party engaged by Contractor or its subcontractor pursuant to the Contract Notwithstanding anything to the contrary in the preceding sentence, Work Product does not include State Intellectual Property, Vendor  Intellectual Property or Third Party Intellectual Property. 
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Agency Inspector – The person designated by the Using Agency to do inspection of the work.

AASHTO – American Association of State Highway and Transportation Officials.  

AISI – American Iron and Steel Institute. 

ASTM – American Society for Testing and Materials. The American Standard Test Method is included and part of the American Society for testing and Materials. 

AWS – American Welding Society. 

EMPVC – Epoxy Modified Polyvinyl Chloride. 

Fusion-Bond Method – Fusion bond epoxy process where the surface of a pipe is cleaned and exposed to heat, an epoxy powder is applied onto the surface of the pipe electrostatically, and the powder undergoes melting onto the pipe surface and dries quickly in controlled and uniformed thickness.

Good Industry Practice – Standards, practices, methods and procedures conforming to the law and the degree of skill and care, diligence, prudence and foresight which would reasonably and ordinarily be expected from a skilled and experienced person or body engaged in a similar type of undertaking under the same or similar circumstances.

I.D. – Interior Diameter. 
Lane Closure – In order to accommodate the maintenance and protection of traffic on those project sites that require the closing of a normally traveled lane, the item “lane closure” will be included in this Blanket P.O. Lane closure will consist of the signs, barricades, traffic control trucks with mounted crash cushions and a flashing arrow board in accordance with the number, configuration, and placement as show on the Standard Construction Details and in accordance with the “Manual on Uniform Traffic Control Devices.” 

NJDEP – New Jersey Department of Environmental protection.

NJDOT – New Jersey Department of Transportation.

O.C. – On-center. A unit of measurement indicating the distance from the center of one framing member to the center of the next framing member.

OSHA – Occupational Safety and Health Administration. 

PPE – Personal Protective Equipment. 

Preventative Maintenance – Maintenance that is regularly performed on systems and/or equipment to lessen the likelihood of failure. Preventative Maintenance includes, but not be limited to, periodic inspection, testing, cleaning, lubrication, adjustment, parts replacement, and repairs to keep the systems and equipment in optimum operating condition.

Project Manager – A Using Agency’s primary contact for projects, separate from NJDOT. 

P.V.C. – Polyvinyl Chloride. 

Regional Engineer – NJDOT’s designated project engineer responsible for a specific region or project.

Resident Engineer – NJDOT’s engineer who supervises crews from site but is not specific to a region. Duties include supervision of and issuing of instructions to the Contractor and to report regularly to the designer and/or client.

R.O.W. – Right of Way. 

U.L. – Underwriters Laboratories. An independent safety science company which tests and certifies products in respect of their safety.

Unified Thread Standard – A standard thread form and series for bolts, nuts, screws, and other thread fasteners.
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