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Bid Solicitation #	21DPP00583
	For:
	[bookmark: _Hlk54607358]T1495 – Customized Snow Plows and Related Components, NJDOT and  Authorities – Statewide



	Event
	Date
	Time

	Vendor’s {Bidder’s} Electronic Question Due Date
(Refer to Bid Solicitation Section 1.3.1 for more information.)
	November 17, 2020
	2:00 PM

	Mandatory/Optional Pre-Quote Conference 
(Refer to Bid Solicitation Section 1.3.5 for more information.)
	Not Applicable 


	Mandatory/Optional Site Visit
(Refer to Bid Solicitation Section 1.3.4 for more information.)
	Not Applicable 


	Quote Submission Date
(Refer to Bid Solicitation Section 1.3.2 for more information.)
	December 18, 2020
	2:00 PM



Dates are subject to change.  All times contained in the Bid Solicitation refer to Eastern Time. All changes will be reflected in Bid Amendments to the Bid Solicitation posted on www.njstart.gov.

	☐  Small Business Set-Aside Category
For Goods and Services:
☐  I          ☐  II          ☐  III
For Construction:
☐  IV          ☐  V          ☐  VI

	[bookmark: _GoBack]Status

☒  Not Applicable

☐  Entire Blanket P.O. 

☐  Partial Blanket P.O. 

☐  Subcontracting Only

	☐  Disabled Veteran-Owned Business Set-Aside
	



	Bid Solicitation Issued By:
State of New Jersey
Department of the Treasury
Division of Purchase and Property
Trenton, New Jersey 08625‑0230
	Using Agency/Agencies:
State of New Jersey
Cooperative Purchasing Program Participants



Date:  10/31/2020 
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[bookmark: _Toc428533936][bookmark: _Toc54703884]INFORMATION FOR VENDORS {BIDDERS}

NOTICE: This Bid Solicitation is part of the NJSTART Procurement Program. The Vendor {Bidder} is advised to thoroughly read all sections, as many have been revised, and follow all instructions contained in this Bid Solicitation, including the instructions on the Bid Solicitation’s Offer and Acceptance Page  and read through all Quick Reference Guides (QRGs) located on the NJSTART Vendor Support Page , before preparing and submitting its Quote.

[bookmark: _Toc400531467][bookmark: _Toc428533937][bookmark: _Toc54703885]PURPOSE AND INTENT

This Bid Solicitation is issued by the Procurement Bureau, Division of Purchase and Property (Division), Department of the Treasury on behalf of the New Jersey Department of Transportation (NJDOT), the New Jersey Turnpike Authority and the South Jersey Transportation Authority (SJTA), other State Using Agencies and the Cooperative Purchasing participants.  The purpose of this Bid Solicitation is to solicit Quotes for customized snow plows and related components.

The intent of this Bid Solicitation is to award Master Blanket Purchase Orders (Blanket P.O.s) to those responsible Vendors {Bidders} whose Quotes, conforming to this Bid Solicitation are most advantageous to the State, price and other factors considered.  The State may award any and all price lines.  The State, however, reserves the right to separately procure individual requirements that are the subject of the Blanket P.O. during the Blanket P.O. term, when deemed by the Director of the Division of Purchase and Property (Director) to be in the State’s best interest.

[bookmark: _Hlk49247350]There are twenty-three (23) price lines, which are grouped and itemized as follows:

	Group Number
	Price Line Number
	Description

	Group 1
(Price lines 1 – 7)
	1
	NJDOT Specific Heavy-Duty Manual Reversible (Straight) Snow Plow, 11 Foot Wide, 36 Inches High (M.R. 11-36-MOD-J)

	
	2
	NJDOT Specific Heavy-Duty One-Way (Funnel), 12 Foot Wide (MODEL O.R.12.75 -53-1HD)

	
	3
	NJDOT Specific Heavy-Duty Power Reversible Snow Plow, 11 Foot Wide, 36 Inches High (Worm Gear Type)

	
	4
	N NJDOT Specific High Power Reversible Torsion Trip Edge Plow, 11 Foot Wide, 36 Inches High

	
	5
	One Additional Set Of Parts Service And O&M Manuals 

	
	6
	Technical Support (Hourly Rate) – Operators And Mechanics Training

	
	7
	Special Monotone Paint Color in Lieu of Manufacturer’s Standard Paint Color

	

	Group 2
(Price Lines 8 – 21)
	8
	NJTA Specific Manual Reversible One-Way Snow Plow, 11 Foot Long, 47 Inches High

	
	9
	NJTA Specific Manual Reversible Snow Plow, 11 Foot Long, 42 Inches High (J-STYLE)

	
	10
	NJTA Specific Power Reversible Expressway Snow Plow 11 Foot Long, 50 Inches High

	
	11
	NJTA Specific Power Reversible Snow Plow, 11 Foot Long, 42 Inches High,

	
	12
	NJTA Specific Snow Plow Blade: Option A

	
	13
	NJTA Specific Snow Plow Blade: Option B

	
	14
	NJTA Specific Snow Plow Blade: Option C

	
	15
	NJTA Specific Ceramic Combination Plow Blades - Blades Only

	
	16
	NJTA Specific Flexible Carbide Combination Plow Blades - Blades Only

	
	17
	Hourly Rate For Installation, Maintenance And Repair of   Snow Plow

	
	18
	One Additional Set Of Parts Service And O&M Manuals

	
	19
	Technical Support (Hourly Rate) – Operators And Mechanics Training

	
	20
	Special Monotone Paint Color in Lieu of Manufacturer’s Standard Paint Color 

	
	21
	Special Two Color Paint in Lieu of Manufacturer’s Standard Paint Color 

	

	Group 3
(Price Lines 22 and 23
	22
	SJTA Specific  Reversible Snow Plow (J STYLE), 11 Foot Wide, 36 Inches High

	
	23
	Special Monotone Paint Color in Lieu of Manufacturer’s Standard Paint Color

	



The State intends to make one (1) Blanket P.O. award per group (Groups 1, Group 2, and Group 3), in accordance with Section 7.2 of this Bid Solicitation. Vendors {Bidders} may bid on one Group, two Groups or all Groups.

For Group 1 Vendors {Bidders} must bid on all price lines (Price Lines 1 - 7) within the Group in order for its Quote to be considered for an award for the Group.  If a Vendor {Bidder} does not bid on all price lines within the Group, its Quote will be considered non-responsive for the Group.

For Group 2 Vendors {Bidders} must bid on Price Lines (Price Line 8 - 21) within the Group in order for its Quote to be considered for an award for the Group. If a Vendor {Bidder} does not bid on all price lines within the Group, its Quote will be considered non-responsive for the Group.

For Group 3 Vendors {Bidders} must bid on both price lines (Price Lines 22 and 23) within the Group in order for its Quote to be considered for an award for the Group.  If a Vendor {Bidder} does not bid on all price lines within the Group, its Quote will be considered non-responsive for the Group.

Price line items are grouped for Quote evaluation purposes only.  Upon Blanket P.O. award, Using Agencies will be able to order any price lines within the group individually.

The State makes no representation and provides no guarantee as to the minimum, average or maximum volume of purchases to be made under this Blanket P.O. 

This procurement is not a Small Business or Disabled Veteran-Owned Business set aside procurement.

The State of NJ Standard Terms and Conditions (SSTCs) accompanying this Bid Solicitation will apply to all Blanket P.O.s made with the State of New Jersey.  These terms are in addition to the terms and conditions set forth in this Bid Solicitation and should be read in conjunction with them unless the Bid Solicitation specifically indicates otherwise.  

The State of New Jersey (State) intends to extend the Blanket P.O.s awarded to the Division's Cooperative Purchasing Program participants.  These participants include quasi-State entities, counties, municipalities, school districts, volunteer fire departments, first aid squads, independent institutions of higher learning, County colleges, and State colleges.  In order for the State Blanket P.O. to be extended to Cooperative Purchasing Program participants, the Vendor {Bidder} must agree to the extension by executing the Cooperative Purchase Form.  Also refer to Section 4.4.3.2 of this Bid Solicitation. Although the State, with the consent of the Vendor(s) {Bidder(s)}, is making the use of any Blanket P.O. resulting from this Bid Solicitation available to non-State Agencies, the State makes no representation as to the acceptability of any State Bid Solicitation terms and conditions under the Local Public Contracts Law or any other enabling statute or regulation.

[bookmark: _Toc400531468][bookmark: _Toc428533938][bookmark: _Toc54703886]BACKGROUND 

This is a reprocurement of the product under T1495 – Snow Plow, D.O.T. and Authorities, presently due to expire on February 28, 2021.  Vendors {Bidders} interested in the current Blanket P.O. specifications and pricing information may review the current Blanket P.O. T1495 at www.njstart.gov by following these steps: 

Go to: www.njstart.gov 
Select “Contract & Bid Search”
Select “Contracts/Blankets”
Under “Contract/Blanket Description” type in T1495, Click “Find It”
The current Blanket P.O.s will appear under “Results”.

Vendors {Bidders} are cautioned that this new Bid Solicitation addresses current requirements.  Vendors {Bidders} should not rely upon or use data from the prior Blanket P.O.

[bookmark: _Toc37223603][bookmark: _Toc53748345][bookmark: _Toc54703887]Notable Change Since The Last Bid Solicitation 

This Bid Solicitation has been revised since the last reprocurement of this commodity.  Please thoroughly read the entire Bid Solicitation including all sub-sections.

Notable changes include, but are not limited to:

SECTION 4.4.3 SUBMITTALS 

The Vendor {Bidder} shall submit with its Quote a Vendor’s {Bidder’s} certification in the form of the attachment titled “Specification Conformance Certification”, confirming that all items offered in response to this Bid Solicitation conform to the requirements set forth in Section 3.0 of this Bid Solicitation.  Please refer to the Attachments tab of the Bid Solicitation in NJSTART for the Specification Conformance Certification. 

Please see the attachment entitled “Specification Conformance Certification”.

[bookmark: _Toc428533939][bookmark: _Toc54703888]Key Events

[bookmark: _1.3.1_ELECTRONIC_QUESTION_AND_ANSWE][bookmark: _Toc428533940][bookmark: _Toc54703889]ELECTRONIC QUESTION AND ANSWER PERIOD

The Division will electronically accept questions and inquiries from all potential Vendors {Bidders} via the “Q&A” Tab of the Bid Solicitation in NJSTART. 

A. Questions should be directly tied to the Bid Solicitation and asked in consecutive order, from beginning to end, following the organization of the Bid Solicitation; and  

B. Each question should begin by referencing the Bid Solicitation page number and section number to which it relates.

Vendors {Bidders} may refer to the QRG “Submit a Quote” for additional instruction. QRGs are located on the NJSTART Vendor Support Page.  

A Vendor {Bidder} shall not contact the Using Agency and/or the Procurement Specialist directly, in person, by telephone or by email, concerning this Bid Solicitation, prior to the final award of the Blanket P.O.

The cut-off date for electronic questions and inquiries relating to this Bid Solicitation is indicated on the Bid Solicitation cover sheet.  In the event that questions are posed by Vendors {Bidders}, answers to such questions will be issued by Bid Amendment.  Any Bid Amendment to this Bid Solicitation will become part of this Bid Solicitation and part of any Blanket P.O. awarded as a result of this Bid Solicitation. Bid Amendments to this Bid Solicitation, if any, will be posted as a File Attachment on the “Summary” page of the Bid Solicitation in NJSTART after the cut-off date.  (See Bid Solicitation Section 1.4.1 for further information.)
[bookmark: _1.3.3__Mandatory_Pre-Bid_Conference][bookmark: _1.3.5__SUBMISSION_OF_BID_PROPOSAL][bookmark: _1.3.2_SUBMISSION_OF_BID_PROPOSAL]
EXCEPTIONS TO THE STATE OF NJ STANDARD TERMS AND CONDITIONS (SSTC)

Questions regarding the State of New Jersey Standard Terms and Conditions (SSTC) and exceptions to mandatory requirements must be posed during this Electronic Question and Answer period and shall contain the Vendor’s {Bidder’s} suggested changes and the reason(s) for the suggested changes.

[bookmark: _SUBMISSION_OF_QUOTES][bookmark: _Toc428533941][bookmark: _Toc54703890]SUBMISSION OF QUOTES

In order to be considered for award, the Quote must be received by the Procurement Bureau of the Division at the appropriate location by the required time.  

Vendors {Bidders} shall submit a Quote electronically through NJSTART. 

QUOTES NOT RECEIVED PRIOR TO THE QUOTE OPENING DEADLINE SHALL BE REJECTED.  THE DATE AND TIME OF THE QUOTE OPENING ARE INDICATED ON THE BID SOLICITATION COVER SHEET AND ON THE “SUMMARY” TAB OF THE BID SOLICITATION WEBPAGE WITHIN NJSTART.  

IF THE QUOTE OPENING DEADLINE HAS BEEN REVISED, THE NEW QUOTE OPENING DEADLINE SHALL BE SHOWN ON THE POSTED BID AMENDMENT AND ON THE “SUMMARY” TAB OF THE BID SOLICITATION WEBPAGE WITHIN NJSTART. 

Inquiries concerning the use of NJSTART may be directed to njstart@treas.nj.gov.  
  
The Division will not respond to substantive questions related to the Bid Solicitation or any other Blanket P.O. via this email address. For inquiries related to substantive questions refer to Section 1.3.1 (Electronic Question and Answer Period).

[bookmark: _Toc54703891]VENDOR {BIDDER} SUPPORT

Vendors {Bidders} are strongly encouraged to visit the NJSTART Vendor Support Page, which contains Quick Reference Guides (QRGs), supporting videos, a glossary of NJSTART terms, and helpdesk contact information.  

The Vendor {Bidder} should utilize the QRGs before attempting to submit its Quote using the NJSTART process.   It is the Vendor’s {Bidder’s} responsibility to ensure that the NJSTART Quote and attachments have been properly submitted.

[bookmark: _1.3.4_MANDATORY/OPTIONAL_SITE][bookmark: _1.3.45_MANDATORY/OPTIONAL_SITE][bookmark: _MANDATORY/OPTIONAL_SITE_VISIT][bookmark: _Toc224543885][bookmark: _Toc238623352][bookmark: _Toc400531474][bookmark: _Toc428533944][bookmark: _Toc54703892]MANDATORY/OPTIONAL SITE VISIT

Not applicable to this procurement.

[bookmark: _1.3.5__MANDATORY/OPTIONAL][bookmark: _1.3.6__MANDATORY/OPTIONAL][bookmark: _MANDATORY/OPTIONAL_PRE-QUOTE_CONFER][bookmark: _Toc224543888][bookmark: _Toc238623354][bookmark: _Toc428533945][bookmark: _Toc54703893]MANDATORY/OPTIONAL PRE-QUOTE CONFERENCE

[bookmark: _Toc95619434][bookmark: _Toc109701220][bookmark: _Toc225321579][bookmark: _Toc94946029][bookmark: _Toc72744593]Not applicable to this procurement.

[bookmark: _Toc400531476][bookmark: _Toc428533946][bookmark: _Toc54703894]PRE-QUOTE DOCUMENT REVIEW 

Not applicable to this procurement.

[bookmark: _Toc428533947][bookmark: _Toc54703895]ADDITIONAL Information

[bookmark: _Toc428533948][bookmark: _Toc54703896]BID AMENDMENTS: Revisions to this BID SOLICITATION

In the event that it becomes necessary to clarify or revise this Bid Solicitation, such clarification or revision will be by Bid Amendment.  Any Bid Amendment to this Bid Solicitation will become part of this Bid Solicitation and part of any Blanket P.O. awarded as a result of this Bid Solicitation.

There are no designated dates for release of Bid Amendments.  Those Vendors {Bidders} who are on the bid holder list either through commodity code registration in NJSTART or by acknowledging the bid in NJSTART should receive notification of any Bid Amendment(s). If a Vendor {Bidder} is not on the bid holder list to receive notifications related to a Bid Solicitation, Bid Amendments are still viewable on the “Summary” page of the Bid Solicitation in NJSTART.

BID AMENDMENTS WILL BE ISSUED AS FILE ATTACHMENTS, AND ARE VIEWABLE ON THE “SUMMARY” PAGE OF THE BID SOLICITATION IN NJSTART.  Vendors {Bidders} may refer to the QRG “Submit a Quote” for additional instructions. QRGs are located on the NJSTART Vendor Support Page.  

It is the sole responsibility of the Vendor {Bidder} to be knowledgeable of all Bid Amendments related to this procurement. An interested Vendor {Bidder} should check the NJSTART “Open Bids” Tab on a daily basis to ensure review of the most updated information.

[bookmark: _Toc400531479][bookmark: _Toc428533949][bookmark: _Toc54703897]VENDOR {BIDDER} Responsibility

The Vendor {Bidder} assumes sole responsibility for the complete effort required in submitting a Quote in response to this Bid Solicitation.  No special consideration will be given after Quotes are opened because of a Vendor’s {Bidder’s} failure to be knowledgeable as to all of the requirements of this Bid Solicitation.

[bookmark: _Toc400531480][bookmark: _Toc428533950][bookmark: _Toc54703898]COST Liability

The State assumes no responsibility and bears no liability for costs incurred by a Vendor {Bidder} in the preparation and submittal of a Quote in response to this Bid Solicitation.

[bookmark: _Toc54703899][bookmark: _Toc400531481][bookmark: _Toc428533951]CONTENTS of QUOTE 

Quotes can be released to the public pursuant to N.J.A.C. 17:12-1.2(b) and (c), or under the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know.  

After the opening of sealed Quotes, all information submitted by a Vendor {Bidder} in response to a Bid Solicitation is considered public information notwithstanding any disclaimers to the contrary submitted by a Vendor {Bidder}. Proprietary, financial, security and confidential information may be exempt from public disclosure by OPRA and/or the common law when the Vendor {Bidder} has a good faith, legal/factual basis for such assertion. 

When the Bid Solicitation contains a negotiation component, the Quote will not be subject to public disclosure until a notice of intent to award a Blanket P.O. is announced. 

As part of its Quote, a Vendor {Bidder} may designate any data or materials it asserts are exempt from public disclosure under OPRA and/or the common law, explaining the basis for such assertion. Vendor {Bidder} must provide a detailed statement clearly identifying those sections of the Quote that it claims are exempt from production, and the legal and factual basis that supports said exemption(s) as a matter of law.  The State will not honor any attempts by a Vendor {Bidder} to designate its entire Quote as proprietary, confidential and/or to claim copyright protection for its entire Quote.

The State reserves the right to make the determination as to what is proprietary or confidential, and will advise the Vendor {Bidder} accordingly.  Any proprietary and/or confidential information in a Quote will be redacted by the State.  Copyright law does not prohibit access to a record which is otherwise available under OPRA.

In the event of any challenge to the Vendor’s {Bidder’s} assertion of confidentiality with which the State does not concur, the Vendor {Bidder} shall be solely responsible for defending its designation, but in doing so, all costs and expenses associated therewith shall be the responsibility of the Vendor {Bidder}. The State assumes no such responsibility or liability.  

A Vendor {Bidder} shall not designate any price lists and/or catalogs submitted as exempt from public disclosure as the same must be accessible to State Using Agencies and Cooperative Purchasing Program participants (if the Bid Solicitation has been extended to these participants) and thus must be made public to allow all eligible purchasing entities access to the pricing information.

In order not to delay consideration of the Quote or the State’s response to a request for documents, the State requires that Vendor {Bidder} respond to any request regarding confidentiality markings within the timeframe designated in the State’s correspondence regarding confidentiality.  If no response is received by the designated date and time, the State will be permitted to release a copy of the Quote with the State making the determination regarding what may be proprietary or confidential.  

See Bid Solicitation Section 4.4.2.4 Confidentiality/Commitment to Defend for additional information.

[bookmark: _Toc400531482][bookmark: _Toc428533952][bookmark: _Toc54703900] ANNOUNCEMENT OF QUOTE INFORMATION

On the date and time Quotes are due under the Bid Solicitation, all information concerning the Quotes submitted may be publicly announced and shall be available for inspection and copying except as noted below:

A. Information appropriately designated as proprietary and/or confidential shall not be available for inspection and copying; and
B. Where negotiation is contemplated, only the names and addresses of the 
Vendors {Bidders} submitting Quotes will be announced, and the contents of the Quotes shall not be available for inspection and copying until the Notice of Intent to Award is issued by the Director. 

[bookmark: _Toc400531483][bookmark: _Toc428533953][bookmark: _Toc54703901]PRICE Alteration In QUOTES

Any price changes including hand written revisions or "white-outs" must be initialed.  Failure to initial price changes may preclude a Blanket P.O. award from being made to the Vendor {Bidder} pursuant to N.J.A.C. 17:12-2.2(a)(8).

[bookmark: _Toc400531484][bookmark: _Toc428533954][bookmark: _Toc54703902]QUOTE ERRORS

In accordance with N.J.A.C. 17:12-2.11 “Proposal errors,” a Vendor {Bidder} may withdraw its Quote as described below.

QUOTE WITHDRAWAL PRIOR TO QUOTE OPENING

A Vendor {Bidder} may withdraw its Quote submission in NJSTART prior to the Quote opening; however, Vendors {Bidders} should note that while withdrawn NJSTART Quotes remain viewable by the Vendor {Bidder} on its Vendor Profile Homepage, they are removed from the Division’s view and cannot be considered for Blanket P.O. award. The Vendor {Bidder} may submit a revised Quote as long as the Quote is received prior to the announced date and time for Quote submission. Vendors {Bidders} may refer to the QRG “Submit a Quote” for additional instruction. QRGs are located on the NJSTART Vendor Support Page.  


QUOTE WITHDRAWAL AFTER QUOTE OPENING, BUT PRIOR TO BLANKET P.O. AWARD

If, after the Quote opening, but before Blanket P.O. award, a Vendor {Bidder} discovers an error in its Quote, the Vendor {Bidder} may make a written request to the Procurement Bureau to withdraw its Quote, or a portion thereof, from consideration for award.  If the Vendor’s {Bidder’s} request to withdraw is made in good faith, and the State will not be significantly prejudiced by granting the withdrawal of the Quote beyond the loss of the benefit of the bargain to the State of the withdrawing Vendor’s {Bidder’s} offer, the request shall be granted.   Evidence of the Vendor’s {Bidder’s} good faith in making this request can be demonstrated by one (1) or more of the following factors: A mistake is so significant that to enforce the Blanket P.O. resulting from the Quote would be unconscionable; that the mistake relates to a material feature or term of the Blanket P.O.; and that the mistake occurred notwithstanding the Vendor’s {Bidder’s} exercise of reasonable care.  After Quote opening, while pursuant to the provisions of this section a Vendor {Bidder} may request to withdraw its Quote and the Director may in his/her discretion allow said Vendor {Bidder} to withdraw it, the Division also may take notice of repeated or unusual requests to withdraw by a Vendor {Bidder} and take those prior requests to withdraw into consideration when evaluating the Vendor’s {Bidder’s} future Quotes.

The Quote withdrawal request must include the Bid Solicitation Number, Bid Solicitation Title, the Quote submission date and should be sent to Procurement.Bureau@treas.nj.gov.

If during a Quote evaluation process, an obvious pricing error made by a potential Blanket P.O. awardee is found, the Director or his/her designee shall issue written notice to the Vendor {Bidder}.  The Vendor {Bidder} will have up to five (5) business days after receipt of the notice to confirm its pricing.  If the Vendor {Bidder} fails to respond, its Quote shall be considered withdrawn, and no further consideration shall be given to it.

[bookmark: _Toc400531485][bookmark: _Toc428533955][bookmark: _Toc54703903]JOINT Venture

If a Joint Venture is submitting a Quote, the agreement between the parties relating to such Joint Venture should be submitted with the Joint Venture’s Quote.  Authorized signatories from each party comprising the Joint Venture must sign the Offer and Acceptance Page.  Each party to the Joint Venture must individually comply with all the forms and certification requirements in Sections 4.4.1 and 4.4.2 of this Bid Solicitation. 
 
[bookmark: _Toc400531486][bookmark: _Toc428533956][bookmark: _Toc54703904]Reciprocity for Jurisdictional Vendor Preference

In accordance with N.J.S.A. 52:32-1.4 and N.J.A.C. 17:12-2.13, the State of New Jersey will invoke reciprocal action against an out-of-State Vendor {Bidder} whose state or locality maintains a preference practice for its in-state Vendors {Bidders}.  The State of New Jersey will use the annual surveys compiled by the Council of State Governments, National Association of State Procurement Officials, or the National Institute of Governmental Purchasing or a State’s statutes and regulations to identify States having preference laws, regulations, or practices and to invoke reciprocal actions. The State of New Jersey may obtain additional information as it deems appropriate to supplement the stated survey information.

A Vendor {Bidder} may submit information related to preference practices enacted for a State or Local entity outside the State of New Jersey. This information may be submitted in writing as part of the Quote response, including name of the locality having the preference practice, as well as identification of the county and state, and should include a copy of the appropriate documentation, i.e., resolution, regulation, law, notice to Vendor {Bidder}, etc.  It is the responsibility of the Vendor {Bidder} to provide documentation with the Quote or submit it to the Director within five (5) business days after the deadline for Quote submission.  Written evidence for a specific procurement that is not provided to the Director within five (5) business days of the public Quote submission date may not be considered in the evaluation of that procurement, but may be retained and considered in the evaluation of subsequent procurements.

[bookmark: _Toc294607267][bookmark: _Toc294680428][bookmark: _Toc400531487][bookmark: _Toc428533957][bookmark: _Toc54703905]QUOTE ACCEPTANCES AND REJECTIONS 
 
N.J.A.C. 17:12-2.7(d), the Director’s right to waive minor irregularities or omissions in a Quote and N.J.A.C. 17:12-2.2 which defines causes for Quote rejection, apply to all Quotes.  

[bookmark: _Toc54703906]ELECTRONIC SIGNATURES

Vendors {Bidders} submitting Quotes through NJSTART may sign the forms listed in Section 4.4.1 (Forms, Registrations and Certifications Required with Quote) and Section 4.4.2 (Forms, Registrations and Certifications Required Before Blanket P.O. Award and That Should Be Submitted with the Quote) of this Bid Solicitation electronically by typing the name of the authorized signatory in the “Signature” block as an alternative to downloading, physically signing the form, scanning the form, and uploading the form to NJSTART. 



[bookmark: _DEFINITIONS][bookmark: _Toc400531488][bookmark: _Toc428533958][bookmark: _Toc54703907] DEFINITIONS

[bookmark: _CROSSWALK][bookmark: _Toc428533959][bookmark: _Toc54703908]CROSSWALK

	NJSTART Term
	Equivalent Statutory, Regulatory and/or Legacy Term

	Bid/Bid Solicitation 
	Request For Proposal (RFP)/Solicitation

	Bid Amendment 
	Addendum

	Change Order 
	Contract Amendment

	Master Blanket Purchase Order (Blanket P.O.) 
	Contract

	Offer and Acceptance Page
	Signatory Page

	Quote
	Proposal

	Vendor 
	Bidder/Contractor



[bookmark: _Toc428533960][bookmark: _Toc54703909]General Definitions

The following definitions will be part of any Blanket P.O. awarded or order placed as a result of this Bid Solicitation.

All-Inclusive Hourly Rate – An hourly rate comprised of all direct and indirect costs including, but not limited to:  labor costs, overhead, fee or profit, clerical support, travel expenses, per diem, safety equipment, materials, supplies, managerial support and all documents, forms, and reproductions thereof.  This rate also includes portal-to-portal expenses as well as per diem expenses such as food.

Best and Final Offer or BAFO – Pricing timely submitted by a Vendor {Bidder} upon invitation by the Bureau after Quote opening, with or without prior discussion or negotiation.

Bid or Bid Solicitation – This series of documents, which establish the bidding and Blanket P.O. requirements and solicits Quotes to meet the needs of the Using Agencies as identified herein, and includes the Bid Solicitation, State of NJ Standard Terms and Conditions (SSTC), State-Supplied Price Sheet, attachments, and Bid Amendments.
  
Bid Amendment – Written clarification or revision to this Bid Solicitation issued by the Division. Bid Amendments, if any, will be issued prior to Quote opening.

Business Day – Any weekday, excluding Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Calendar Day – Any day, including Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Change Order – An amendment, alteration, or modification of the terms of a Blanket P.O. between the State and the Vendor(s) {Contractor(s)}.  A Change Order is not effective until it is signed and approved in writing by the Director or Deputy Director, Division of Purchase and Property.

Cooperative Purchasing Program – The Division’s intrastate program that provides procurement-related assistance to New Jersey local governmental entities and boards of education, State and county colleges and other public entities having statutory authority to utilize select State Blanket P.O.s issued by the Division, pursuant to the provisions of N.J.S.A. 52:25-16.1 et seq.

Days After Receipt of Order (ARO) – The number of calendar days ‘After Receipt of Order’ in which the Using Agency will receive the ordered materials and/or services.

Director – Director, Division of Purchase and Property, Department of the Treasury, who by statutory authority is the Chief Contracting Officer for the State of New Jersey.

Disabled veterans’ business - means a business which has its principal place of business in the State, is independently owned and operated and at least 51% of which is owned and controlled by persons who are disabled veterans or a business which has its principal place of business in this State and has been officially verified by the United States Department of Veterans Affairs as a service disabled veteran-owned business for the purposes of department contracts pursuant to federal law.  N.J.S.A. 52:32-31.2.

Disabled veterans’ business set-aside contract - means a contract for goods, equipment, construction or services which is designated as a contract with respect to which bids are invited and accepted only from disabled veterans’ businesses, or a portion of a contract when that portion has been so designated.  N.J.S.A. 52:32-31.2.

Discount – The price reduction applied by the Vendor {Bidder} to all items.

Division – The Division of Purchase and Property.

Evaluation Committee – A committee established or Division staff member assigned by the Director to review and evaluate Quotes submitted in response to this Bid Solicitation and recommend a Blanket P.O. award to the Director.

Firm Fixed Price – A price that is all-inclusive of direct cost and indirect costs, including, but not limited to, direct labor costs, overhead, fee or profit, clerical support, equipment, materials, supplies, managerial (administrative) support, all documents, reports, forms, travel, reproduction and any other costs.

Joint Venture – A business undertaking by two (2) or more entities to share risk and responsibility for a specific project.

Master Blanket Purchase Order (Blanket P.O.) – The Blanket P.O. consists of the State of NJ Standard Terms and Conditions (SSTC), the Bid Solicitation, the responsive Quote submitted by a responsible Vendor {Bidder} as accepted by the State, the notice of award, any Best and Final Offer, any subsequent written document memorializing the agreement, any modifications to any of these documents approved by the State and any attachments, Bid Amendment or other supporting documents, or post-award documents including Change Orders agreed to by the State and the Vendor {Contractor}, in writing.

May – Denotes that which is permissible or recommended, not mandatory.

Must – Denotes that which is a mandatory requirement.  

No Bid – The Vendor {Bidder} is not submitting a price Quote for an item on a price line.

No Charge – The Vendor {Bidder} will supply an item on a price line free of charge.

Primary Form – An electronic form contained within a Vendor’s {Bidder’s} NJSTART profile designated by the Vendor {Bidder} as the primary or principal version of the required form.

Procurement Bureau (Bureau) – The Division unit responsible for the preparation, advertisement, and issuance of Bid Solicitations, for the tabulation of Quotes and for recommending award(s) of Blanket P.O.(s) to the Director and the Deputy Director.

Project – The undertakings or services that are the subject of this Bid Solicitation.

QRGs – Quick Reference Guides.

Quote – Vendor’s {Bidder’s} timely response to the Bid Solicitation including, but not limited to, technical Quote, price Quote, and any licenses, forms, certifications, or other documentation required by the Bid Solicitation.

Retainage – The amount withheld from the Vendor {Contractor} payment that is retained and subsequently released upon satisfactory completion of performance milestones by the Vendor {Contractor}.

Revision – A response to a BAFO request or a requested clarification of the Vendors {Bidders} Quote. 

Shall – Denotes that which is a mandatory requirement.  

Should – Denotes that which is permissible or recommended, not mandatory.

Small Business – Pursuant to N.J.S.A. 52:32-19, N.J.A.C. 17:13-1.2, and, N.J.A.C. 17:13-2.1, “small business” means a business that meets the requirements and definitions of “small business” and has applied for and been approved by the New Jersey Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit as (i) independently owned and operated, (ii) incorporated or registered in and has its principal place of business in the State of New Jersey; (iii)  has 100 or fewer full-time employees; and has gross revenues falling in one (1) of the three (3) following categories:  
· For goods and services - (A) 0 to $500,000 (Category I); (B) $500,001 to $5,000,000 (Category II); and (C) $5,000,001 to $12,000,000, or the applicable federal revenue standards established at 13 CFR 121.201, whichever is higher (Category III). 
· For construction services: (A) 0 to $3,000,000 (Category IV); (B) gross revenues that do not exceed 50 percent of the applicable annual revenue standards established at 13 CFR 121.201 (Category V); and (C) gross revenues that do not exceed the applicable annual revenue standards established at CFR 121.201, (Category VI).

Small business set-aside contract – “means (1) a contract for goods, equipment, construction or services which is designated as a contract with respect to which bids are invited and accepted only from small businesses, or (2) a portion of a contract when that portion has been so designated.”  N.J.S.A. 52:32-19.

State – State of New Jersey.

State Contract Manager or SCM – The individual, as set forth in Section 8.0, responsible for the approval of all deliverables, i.e., tasks, sub-tasks or other work elements in the Scope of Work.  The SCM cannot direct or approve a Change Order.

State-Supplied Price Sheet – The bidding document created by the State and attached to this Bid Solicitation on which the Vendor {Bidder} submits its Quote pricing as is referenced and described in Bid Solicitation Section 4.4.5.  

Subtasks – Detailed activities that comprise the actual performance of a task.

Subcontractor – An entity having an arrangement with a Vendor {Contractor}, whereby the Vendor {Contractor} uses the products and/or services of that entity to fulfill some of its obligations under its State Blanket P.O., while retaining full responsibility for the performance of all [the Vendor’s {Contractor's}] obligations under the Blanket P.O., including payment to the Subcontractor.  The Subcontractor has no legal relationship with the State, only with the Vendor {Contractor}.

Task – A discrete unit of work to be performed.

Unit Cost or Unit Price – All-inclusive, firm fixed price charged by the Vendor {Bidder} for a single unit identified on a price line.
  
Using Agency[ies] – A State department or agency, a quasi-State governmental entity, or a Cooperative Purchasing Program participant, authorized to purchase products and/or services under a Blanket P.O. procured by the Division. 

Vendor {Bidder} – An entity offering a Quote in response to the Division’s Bid Solicitation.

Vendor {Contractor} – The Vendor {Bidder} awarded a Blanket P.O. resulting from this Bid Solicitation.

[bookmark: _Toc355709006][bookmark: _Toc400531490][bookmark: _Toc428533961][bookmark: _Toc54703910]BLANKET P.O. specific definitions/ACRONYMS

AASHTO – American Association of State Highway and Transportation Officials

Aftermarket Component - Any component - utility body, snow plow, crane, liftgate or the like - installed on the vehicle chassis (prime unit) by manufacturer or installer (aftermarket installer) other than the chassis manufacturer (prime unit manufacturer).

Aftermarket Installer – An entity modifying a unit with or without installation of an accessory equipment after the vehicle is manufactured by the original vehicle manufacturer (primary unit manufacturer), where the Vendor {Contractor} uses the products and/or services of that entity to fulfill some of its obligations under its Blanket P.O., while retaining full responsibility for the performance of all of its (Vendor’s {Contractor’s}) obligations under the Blanket P.O., including payment to the aftermarket installer and prime unit manufacturer.  The aftermarket installer and prime unit manufacturer have no legal relationship with the State, only with the Vendor {Contractor}.

AISI -  American Iron and Steel Institute

ANSI – American National Standards Institute (http://www.ansi.org/).

Approved Products – Those products that have been identified in Bid Solicitation as meeting Using Agency needs and confirmed as meeting product specifications.

ASTM - American Society for Testing Materials (http://www.astm.org/). 

AWS - American Welding Society 

BBC – Bumper-to-back-of-cab, the distance from the front-most edge of the front bumper to the back of cab.

BL - Body length, overall length minus BBC.

Brinell Hardness - the hardness of a metal or alloy measured by hydraulically pressing a hard ball under a standard load into the specimen

CA - Cab-to-axle, the distance from the back of cab to the centerline of rear axle.

Dealer/Distributor – A Company authorized by a Vendor {Bidder/Contractor} as having the contractual ability to accept and fulfill orders and receive payments directly on behalf of the Vendor {Contractor} that is awarded a Blanket P.O.  Any authorized Dealer/Distributor must agree to all terms and conditions contained within the Bid Solicitation and must agree to provide all products and services in accordance with the Blanket P.O. specifications, terms, conditions and pricing.  A Dealer/Distributor must provide all forms required of a Vendor {Contractor}.

DRW – Dual Rear Wheel.

Dry Weight - Curb weight or tare weight of a vehicle - weight of an empty vehicle, without any payload, driver and passenger, with fluids filled to half capacity.

FHWA - Federal Highway Administration

GAWR - Gross Axle Weight Rating; the maximum legal weight carrying capacity of axle components, including their own dry weights, as published by the vehicle/chassis manufacturer.  GAWR shall not exceed the capacity of the least rated axle component.

GVWR – Gross Vehicle Weight Rating

JIC -  Joint Industry Council

NJMVC or NJDMV - New Jersey Motor Vehicle Commission, formerly known as Division of Motor Vehicles (http://www.state.nj.us/ /).

Pre-Consumer Material – Materials generated in manufacturing and converting processes, such as manufacturing scrap and trimmings/cuttings.

Post-Consumer Material – Material or finished product that has served its intended use and has been diverted or recovered from waste destined for disposal, having completed its life as a consumer item.  Post-Consumer Materials are part of the broader category of Recovered Materials.

Recovered Material – Waste material and byproduct that have been recovered or diverted from solid waste, but does not include materials and byproducts generated from, and commonly reused within, an original manufacturing process.

Materials in Solid Waste – Material found in the various components of the solid waste stream. General, solid waste has several components, such as municipal solid waste (MSW), construction and demolition debris (C&D), and nonhazardous industrial waste.  Under RCRA Section 6002, EPA considers materials recovered from any component of the solid waste stream when designating items containing Recovered Materials. 

Outside Diameter (OD) – A measure of the distance of a straight line from one point on the outer wall of the tubing, through its center, to an opposite point also on the outside. Specified in inches or fraction of an inch and is always larger than the inside.

Recycling – The series of activities, including collection, separation, and processing, by which products or other materials are recovered from the solid waste stream for use in the form of raw materials in the manufacture of new products other than fuel for producing heat or power by combustion.

Recyclability – The ability of a product or material to be recovered from, or otherwise diverted from, the solid waste stream for the purpose of recycling.

RMAN – Recovered Materials Advisory Notices provide purchasing guidance and recommendations for Recovered and Post-Consumer Material content levels for designated items. 

SAE – Society of Automotive Engineers (https://www.sae.org/).

Unit -  ("snow plow”, “plow”, "product", "commodity" or "item"),  as specified herein, made available for outright purchase as a new, unused unit under a Blanket P.O. established as a result of this Bid Solicitation. 

USEPA – United States Environmental Protection Agency.
	
WB - Wheelbase, the distance between the centerlines of front and rear axles.

[bookmark: _2.2_contract_specific][bookmark: _3.0_Scope_of][bookmark: _Ref37485783][bookmark: _Toc400531491][bookmark: _Toc428533962][bookmark: _Toc53748369][bookmark: _Toc54703911]
SCOPE OF WORK – REQUIREMENTS OF THE VENDOR {CONTRACTOR}

[bookmark: _Toc18397128][bookmark: _Toc9499247][bookmark: _Toc493254935][bookmark: _Toc482353331][bookmark: _Toc475965611][bookmark: _Toc455130499][bookmark: _Toc424044871][bookmark: _Toc172392759][bookmark: _Toc53748370][bookmark: _Toc54703912]BLANKET P.O. UTILIZATION

This Bid Solicitation has been developed to establish a term Blanket P.O. to procure the customized snow plows and related components for the New Jersey Department of Transportation (NJDOT), the New Jersey Turnpike Authority (NJTA), the South Jersey Transportation Authority (SJTA), other State agencies, and the Cooperative Purchasing Program participants.  

The State guarantees neither any minimum nor average or maximum quantity per order nor total quantity during Blanket P.O. term, including any extension(s) thereof.

[bookmark: _Toc18397129][bookmark: _Toc9499248][bookmark: _Toc493254936][bookmark: _Toc482353332][bookmark: _Toc475965612][bookmark: _Toc455130500][bookmark: _Toc424044872][bookmark: _Toc172392760][bookmark: _Toc53748371][bookmark: _Toc54703913]BLANKET P.O. SPECIFIC REQUIREMENTS

3.2.1 The Vendor {Contractor} must be a franchised and/or authorized factory representative, able to furnish the specified Unit. The Vendor {Contractor} may be required to submit a letter of certification from the manufacturer for the contracted product, certifying that the Vendor {Contractor} remains authorized by the manufacturer to supply the Unit awarded under the Blanket P.O. The  State reserves the right to request such certification and to require that such certification be provided within five (5) business days from the time it is requested.  The Vendor {Contractor} must notify the State of New Jersey of any changes in the status of its franchise with the manufacturer.  

3.2.2 The Vendor {Contractor} shall provide a new Unit of latest design and is current in production.  No used Unit will be accepted.

3.2.3 This Bid Solicitation is for the outright purchase of the Blanket P.O. Unit only; leasing of the Blanket P.O. Unit or trade-in against the purchase of the Blanket P.O. Unit is not permitted.

3.2.4 All components of each Unit supplied under the Blanket P.O. established shall be identical, for example, alternators, filters, distributors, etc. 

3.2.5 Aftermarket installation is permitted. The Vendor {Contractor} is responsible for assuring aftermarket installer(s)' compliance with all terms and conditions of the Bid Solicitation.  The Vendor {Contractor} will assume sole responsibility for any payments due the aftermarket installer(s).  Nothing contained in the Bid Solicitation shall be construed as creating any contractual relationship between any aftermarket installer(s) and the State. 

[bookmark: _Toc18397130][bookmark: _Toc5608562][bookmark: _Toc478734468][bookmark: _Toc475622011][bookmark: _Toc467160934][bookmark: _Toc448401100][bookmark: _Toc172392761][bookmark: _Toc53748372][bookmark: _Toc54703914]Unit SPECIFICATIONS – GENERAL PROVISIONS

3.3.1 Each Unit and its components shall be completely assembled, serviced and ready for use when delivered to the Using Agency. Unless specified otherwise; any parts, components, equipment, controls, materials, features, performances, capacities, ratings or designs which are standard and/or necessary to form an efficient and complete working Unit shall be furnished whether specifically required herein or not. The Vendor {Contractor} shall supply any item required to meet the Industry standards and practices, Federal and New Jersey Safety Standards and Regulations, and SAE and other applicable standards.

3.3.2 The Unit provided shall be manufacturer’s standard Units with the necessary options, upgrades, customization and/or accessories required to conform to the specifications set forth in Section 3.0 of this Bid Solicitation. All options, upgrades, customization and/or accessories shall be supplied and installed by the manufacturer. Dealer installation is permitted only if factory installation is not available.  Dealer installation shall be in accordance with the practices recommended by the manufacturer and shall not adversely affect manufacturer's warranty.
[bookmark: finish]
[bookmark: manuals][bookmark: VEHICLESPECIFICATIONSTECHNICALPROVION]3.3.3  Manuals:  If available, the Vendor {Contractor} shall supply one line set sheet for each Unit.  A Unit shall comprise each and every assembly system and/or component.  In addition to any line set sheet, the Vendor {Contractor} shall provide Unit operation and maintenance manuals for each and every assembly system and/or component that makes up the Unit.  The Vendor {Contractor} shall also include any other manuals that the manufacturers provide as standard manuals. 

Note:  These manuals are required as a part of the Unit purchase and are not part of the “optional manuals” specified in Section 3.4.5 and Section 3.4.18.  

[bookmark: weightchart][bookmark: guaranteewarranty]3.3.4 Training: Complete instructions on the operation and maintenance of each Unit and a demonstration of the operation of the Unit shall be given by the Vendor {Contractor}, if requested by the Using Agency. Training must include operator training with instruction on proper operation of the Unit, safety, and basic preventive maintenance. This demonstration shall be a formal training session and shall be arranged with the Vendor {Contractor}, at the convenience of the Using Agency. The training session shall be conducted at the location of delivery or at a field location within the State of New Jersey, as specified by the Using Agency.

Note:  This training is required as a part of the Unit purchase and is not part of the “technical support specified in Section 3.4.6 and Section 3.4.19.

3.3.5 Brand Names:  Brand names have been kept to a minimum in this Bid Solicitation; but if a brand name is given, the term "or comparable" is considered to follow the brand name.  Wherever a brand name is used, it is meant to denote the minimum level of quality and performance.  Any item supplied as "comparable" must be approved by the State during the proposal evaluation and prior to an award.  Specifying a brand name, components and/or equipment in response to this specification shall not relieve the Vendor {Contractor} from its responsibility to produce the Unit in accordance with all specifications and other contractual requirements.

[bookmark: _Toc53748373][bookmark: _Toc54703915][bookmark: vehiclespecstechnicalprovisions]Snow Plow Specification – TECHNICAL PROVISIONS

The following written specifications and attached drawings (Attachment A - NJDOT Specific Snow Plow Drawings and Attachment B - NJTA Specific Snow Plow Drawings) identify the technical requirements necessary to  produce a satisfactory Unit.  Please refer to the Attachments tab of the Bid Solicitation in NJSTART for Attachments A and B.  

The Units shall be built from new materials and suited for continuous work under conditions of rapid snow removal. 

NJDOT Specific Snow Plows (Sections 3.4.1, 3.4.2, 3.4.3, and 3.4.4):

Please refer to Attachment A - NJDOT Specific Snow Plow Drawings for all drawings referenced throughout Section 3.4.1, Section 3.4.2, Section 3.4.3, and Section 3.4.4.

For NJDOT- Specific Snow plows castings in lieu of weldments are acceptable. 

NJTA Specific Snow Plows (Sections 3.4.8, 3.4.9, 3.4.10 and 3.4.11): 

Please refer to Attachment B - NJTA Specific Snow Plow Drawings for the drawings referenced throughout Section 3.4.8, Section 3.4.9, Section 3.4.10, and Section 3.4.11.

SJTA Specific Snow Plows (Section 3.4.22): 

Please refer to Attachment A - NJDOT Specific Snow Plow Drawings for the drawings referenced throughout Section 3.4.22,



[bookmark: _Toc53748374][bookmark: _Toc54703916]NJDOT Specific HEAVY-DUTY Manual reversible (Straight) Snow Plow, 11 Foot Wide, 36 Inches High (M.R. 11-36-MOD-J) (Group 1, Price line 1)

It is the intent of these specifications to describe a 11 foot wide x 36 inch high heavy-duty manual reversible (straight) snow plow, built in accordance with the listed specifications and/or drawings. 

The snow plow assembly shall consist of all of the components listed in this specification, except as noted on the drawings and notes below. 

The snow plow assembly appears on Drawing No. 4-162. 

Note: Delete items 15, 16, 17 and 18 and delete L.A.C. rivet pin of item 7. In addition, snow plow shoes shall replace snow plow wheels.

MOLDBOARD

The moldboard and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing 4-213 – Moldboard

· Drawing 4-169A - Blade “Z” – Blade shall be included

·  The blade support angle shall be 4 inch x 4 inch x ¾ inch structural angle. 

· The blade used shall be blade "Z" (Please refer to drawing 4-169A)

· The moldboard shall have additional holes punched in to accommodate both 3 foot and 4 foot long carbide blades.

· A separate bolt-on snow shield shall be installed on each moldboard. It shall be constructed of 3/8 inch thick rubber belting and shall be 12 inches wide (full length of moldboard), mating to holes shown on drawing no. 4-213. 

· A ¼ inch x 2 inch steel backing plate (full length) shall be installed with seven (7) bolts to sandwich the snow shield to the mold board.

Moldboard left and Right Wrap Arounds and BUMPERS 

The moldboard shall include left and right wrap around and curb bumpers. The left and right wrap around and curb bumper shall be manufactured in accordance with the following drawings:

· Drawing 4-158 - Wrap Around - Right Side & Curb Bumper
 
· Drawing 4-159 - Wrap Around - Left Side

· Drawing 4-169A - Blade “Z” – Blade shall be included

Semicircle    

The semicircle and its accessory parts shall be manufactured in accordance with the following drawings and specification:

· Drawing 4-135 – Moldboard Hinge and Semicircle Hinge

· Drawing 4-147 – Shoe, Locking Pin, and Rivet Pin

· Note: Moldboard shoe is not applicable.

· Drawing 4-203 – Large Semicircle

caster assembly

The caster assembly and its accessory parts, which includes the caster housing, caster stem, snow plow shoe and axle and nut, shall be manufactured in accordance with the following drawings: 

· Drawing 4-146 – Caster Housing

· Drawing 4-182-1 – Caster Assembly And 4-144-4

· Drawing 4-182-2 – Caster Assembly

· Drawing 4-182-3 – Caster Assembly (Fabrication) 

· Drawing 4- 144-4 - Caster Assembly

· Drawing 4-205 – 6 inch Snow Plow Shoe with Extended Leg

· Drawing 4-219 – Axle – Pin Type 

Trip Spring

The trip spring and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing 4-143 – Trunnion Plate

· Drawing 4-160-1 – Trip Spring Assembly 

· Note: The 2-5/8 inch free height spring made of ½ inch square material shown on 4-160-1 may be replaced with a spring made of 9/16 inch round wire, 3 ¼ inch O.D., ground at both ends for a free height of 2-5/8 inches with suitable spring constant 

· Drawing 4-160-2 – Trip Spring Assembly 

· Drawing 4-160-3 – Trip Spring Assembly

Push Bar

The push bar and its accessory parts shall be manufactured in accordance with the following drawings:

· Drawing 4-132 – Large Snow Plow Push Bar 

· Drawing 4-154 – Latch Pin Swivel and Eye Bar 




Lift Chain

The lift chain and its accessory parts shall be manufactured in accordance with the following drawings: 

· Drawing 4-192-1- Snow Plow Lifting Chains (Type C)

· Drawing 4-192-2 – Snow Plow Lifting Chains 

Hardware

All nuts and bolts shall be minimum grade 5 corrosion resistant, heat treated medium carbon steel. All lock washers shall be corrosion resistant. All bolt, nut and washer combinations shall have a minimum of 2 to 3 bolt threads showing after it has passed through the nut.

[bookmark: _Toc53748375][bookmark: _Toc54703917]NJDOT SPECIFIC Heavy-Duty One-Way (Funnel) SNOW PLOW, 12 FOOT WIDE (MODEL O.R.12.75-53-1 HD) (GROUP 1, PRICE LINE 2)

It is the intent of this specification to describe and govern the purchase of a 12 foot wide heavy duty manual one-way (funnel) snow plow, built in accordance with the listed specifications and drawings.

Moldboard

The moldboard and its accessory parts shall be manufactured in accordance with the following drawing and specifications: 

· Drawing 4-131

· The moldboard shall be 34 1/2 inches high at the nose end, 52 ¾ inches high at the discharge end and shall be overall 144 inches long
· The moldboard shall be 144 inches at the cutting edge and formed in a funnel shaped blade
· A separate bolt-on snow shield shall be installed on each moldboard. It shall be constructed of 3/8 inch thick rubber belting and shall be 12 inches  wide (full length of moldboard), mating to holes shown on Drawing No. 4-222. A 1/4 inch x 2 inch steel backing plate (full length) shall be installed, which will sandwich the snow shield to the mold board.

Moldboard’s inner and outer nose pieces, curb bumper and moldboard shoes

The moldboard shall include inner and outer nose pieces, a curb bumper and moldboard shoes, which shall be manufactured in accordance with the following drawings and specifications:

· Drawing 4 -133 – Curb Bumper Guard 

· Drawing 4 -168 – Snow Plow Blades 

· Note: Cover blade shall be included.

· Drawing 4 -186 – Inner & Outer Nose Piece

· Drawing 4 -221 – Moldboard Shoe with Tungsten Carbide Inserts 

Note: Two (2) - 3 foot and one (1) - 4 foot carbide blades shall be mounted directly to the moldboard, sandwiched between the cover blades and fastened with Grade 5 carriage bolts.

Semicircle

The semicircle and its accessory parts shall be manufactured in accordance with following drawings and specifications:

· Drawing 4 -135 – Moldboard Hinge and Semicircle Hinge

· Drawing 4 -147 – Shoe, Locking Pin, and Rivet Pin

· Note: Moldboard shoe is not applicable

· Drawing 4 -156 – Moldboard and Semicircle Hinges 

· Drawing 4 - 203 – Large Semicircle Hinges 

Caster Assembly

The caster assembly and its accessory parts, which includes the caster housing, caster stem, snow plow shoe, and axle pin, shall be manufactured in accordance with the following drawings: 

· Drawing 4-146 – Caster Housing

· Drawing 4-182-1 – Caster Assembly (Fabrication)

· Drawing 4-182-2 – Caster Assembly (Fabrication)

· Drawing 4-182-3 – Caster Assembly (Fabrication)

· Drawing 4-205 – 6 Snow Plow Shoe with Extended Leg

· Drawing 4-219 – Axle Pin Type

Trip Spring

The trip spring and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing 4-143 – Trunnion Plate 

· Drawing 4-145-1 – Trip Spring Assembly

· Drawing 4 -145-2 – Trip Spring Assembly

· Drawing 4-145-3 – Trip Spring Assembly 	

Note: The 2-5/8 inch free height spring made of ½ inch square material shown on Drawing No. 4-145-1 may be replaced with a spring made of 9/16 inch round wire, 3 ¼ inch O.D., ground at both ends for a free height of 2-5/8 inches, with suitable spring constant.

Push Bar

The push bar and its accessory parts shall be manufactured in accordance with the following drawings:

· Drawing 4 -132 – Large Snow Plow Push Bar

· Drawing 4 -154 – Latch Pin Swivel and Eye Bar 

Lift Chain Assembly (Type G)

The lift chain assembly and its accessory parts shall be manufactured in accordance with the following drawings: 

· Drawing4-192-1-Snow Plow Lifting Chains (Type G)

· Drawing4-192-2 – Snow Plow Lifting Chains 

Hardware: 

All nuts and bolts shall be minimum Grade 5 corrosion resistant, heat treated medium carbon steel. All bolt, nut and washer combinations shall have a minimum of 2 to 3 bolt threads showing after it has passed through the nut.

[bookmark: _Toc53748376][bookmark: _Toc54703918]NJDOT Specific Heavy-Duty Power reversible snow plow, 11 foot wide, 36 inches high (worm gear type) (Group 1, Price Line 3)

It is the intent of this specification to describe and govern the purchase of a 11 foot wide x 36 inches high worm gear type heavy duty power reversible snow plow, built in accordance with the listed specifications and drawings. 

Moldboard

The moldboard and its accessory parts shall be manufactured in accordance with the following specifications:

· The moldboard shall be shallow "J" type with the snow shield as an integral part of the moldboard curvature. 

· The moldboard shall be 132 inches long and 36 inches high measured from top of the skin (less ribs) to the ground (with a 6 inch blade installed) in operating position. 

· The main part of the moldboard shall have a radius of curvature of 24 inch to 28 inch. The integral snow shield to extend 6 inches beyond the most vertical point of the moldboard.

· The radius of curvature of the snow shield shall be 7-1/2 inches – 10 inches. 

· The entire perimeter of the moldboard shall be 49 inches – 52 inches long, measured from the top moldboard reinforcement at the outer edge of the snow shield to the top of the moldboard blade reinforcement.

· The angle-of-attack for the moldboard blade and the moldboard blade reinforcement shall be 35 degrees from vertical. 

· The moldboard shall not be less than 10 US standard gauge steel. It shall extend to the bottom of the moldboard blade reinforcement. This lower portion shall be tack welded only. 

· Drainage holes, ½ inch diameter shall be provided along the top section of the moldboard. (minimum 3 holes between each vertical rib, one hole between ribs pairs).

· The moldboard blade reinforcement shall be made of 4 inch x 4 inch x ¾ inch steel angle, electrically welded to the plow framework with reinforcement gussets, one gusset under each rib.

· Eight (8) reinforcing vertical ribs shall skip fillet welded on alternate sides of each rib at 7 inch intervals to the moldboard skin. 

· Hinge and trip spring hole area shall be welded on both sides of the rib. Two of the vertical ribs shall be at the ends (one each end) of the moldboard. The remaining three pairs of vertical ribs shall reinforce the moldboard and serve as mounting points for the moldboard hinges and the trip spring mount. They  shall be 2-1/2 inch x ½ inch. Hinge and trip spring hole areas  shall be reinforced with ¼ inch plate welded to the rib to give an effective thickness of  ¾ inch. The moldboard hinge points to have four (4) holes for adjustment, spaced 2 inches apart on the vertical ribs. The trip spring mount to have four (4) holes on the center vertical ribs, spaced 2 inches apart, also for adjustment. The second from the bottom hole shall be located so that the trip spring is parallel with the ground at the specified operating condition. All hinge points shall be located so that the trip spring and moldboard hinges are parallel with the ground with the moldboard at a 35 degree angle of attack.

· Horizontal rib sections (2-1/2 inches x ½ inch) shall be welded between vertical ribs (except center ribs), full width of moldboard, placed at the approximate center of the moldboard.

· The top horizontal (snow shield) reinforcement shall measure 132 inches long (2-1/2 inches x 1-1/2 inches)  and  shall be formed as a continuous part of the moldboard skin. At the point where the vertical ribs meet the top horizontal reinforcement, both sides of the ribs to have welded 2-1/4 inch x 2 inch x 3/8 inch plates.

· A separate bolt-on snow shield shall be installed on each moldboard. It shall be constructed of 3/8 inch thick rubber belting, 12 inches wide and 132 inches long. A ¼ inch x 2 inch steel backing plate (full length) shall be installed with seven (7) bolts to sandwich the snow shield to the moldboard. The moldboard shall incorporate a rigid support for installing the snow shield.

· The moldboard blade shall measure 6 inches x 132 inches, shall be made of high-tensile steel, and shall conform to the drawing for blade "Z". 

Note: The moldboard shall have additional holes to accommodate 3 foot and 4 foot long carbide blade. 

Moldboard Left and Right Wrap arounds and Bumpers 

The moldboard shall include left and right wrap around at the end of the moldboard blade. The left and right wrap arounds shall be manufactured in accordance with the following drawings:

· Drawing 4-158 - Wrap Around - Right Side & Curb Bumper 

· Drawing 4-159 - Wrap Around - Left Side

The curb bumper and its accessory parts shall be manufactured in accordance with the follow drawings:

· Drawing 4-158 - Wrap Around - Right Side & Curb Bumper
 
· Drawing 4-191


Moldboard Hinges 

The moldboard hinges and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing 4-135 –Moldboard Hinges

· Drawing 4-156 – Moldboard and Semicircle Hinges 

· A minimum of three (3) moldboard hinges shall be included to conform to drawing No. 4-135. They are to attach to the moldboard at the vertical ribs, and also to the truss frame. One hinge shall be located at mid-point of moldboard and the other two shall be located 42 inches from mid-point, for a total center-to- center distance of 84 inches.

Truss Frame:

The truss frame and the accessory parts shall be manufactured in accordance with the following specifications:

· The truss frame shall be a triangular welded assembly consisting of a main drive member and truss members.  

· The truss frame shall be constructed of 3 inch x 3 inch angle and ½ inch thick boxed where appropriate.  In lieu of the angle, the three members may be 4 inch O.D. pipe and  3/8 inch thick. For additional strength, the inside corner to have ½ inch thick webs. Additional steel angle gussets at other points within the truss frame may be required for additional strength and rigidity. 

· The "A" frame pivot pin shall be supported top and bottom by a box section capturing the "A" frame. The box section may be fabricated with 4 inch x 6 inch x ½ inch  angle and plates. 

· At the front of the truss frame, securely gusseted welded 4 inch x 6 inch x ½ inch angle shall provide attaching points for the three moldboard hinges identified previously.

· At the rear of the truss frame, bolt-on worm gear plate(s), 1 inch thick, which mate to the worm gear/motor assembly of the "A” frame shall be provided. Elastic stop nuts shall be used with the proper size bolts. Elongated holes shall be provided to allow for adjustment of the gear plate.  The worm gear plate mounting shall be rigid to provide minimum flexing under severe plowing conditions. Bolt on worm gear plate(s) shall be properly positioned and track welded.

· Mounting for the central part of the truss frame for the trip spring's trunnion plates shall be reinforced for further strength. The trunnion plate mounting shall have six (6) 15/16 inch  holes, placed 3 inches apart for adjustment.

· Two attaching points, approximately 32 inches apart, shall be provided for the lift chain identified. Alternate location point(s) may be necessary for proper leveling of plow during transport. These points will be clarified at time of initial inspection of prototype plow.

· The truss frame shall also provide mounting points for the caster assemblies identified. The caster housing, mounting plate shall have gusset extending to the top of the plate.

· All welding on truss frame components shall be fillet welds-all around.


Trip Spring Assembly:

The trip spring assembly and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing 4-160-3 - Trip Spring Assembly

· The trip spring assembly shall be cylinder type, 6 inch diameter, approximately 22 inches long. It shall have an inner and outer spring. The outer spring shall be 24 inches long, 5-1/2 inch  O.D., and 0.813 inches thick with 18 turns. The inner spring shall be 24 inches long, 3-1/4 inch O.D., and 0.594 inches thick with 18 turns. It shall mate the moldboard at one of the four holes of the center ribs. 

· Trunnion plates which mount the trip spring to the truss frame shall conform to Drawing No. 4 -143. In lieu of the designated trunnion plates, Vendor {Contractor} shall provide equally rigid plates which can adapt to the design of the trip spring, having the proper number of holes for adjustment.

Caster assemblies: 

The caster assemblies, which includes the caster housing, caster stem, snow plow shoe and axle and nut, shall be manufactured in accordance with the following drawings: 

· Drawing 4 -144-1 - Caster Assembly 

· Drawing 4 -144-2 - Caster Assembly

· Drawing 4 -144-3 - Caster Assembly

· Drawing 4 -205 - Shoe - Tungsten Carbide

· Drawing 4 -121 – Axle

“A” Frame

The “A” frame and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· The "A" frame section shall form a triangular arrangement. It shall be constructed of 3 inch x 5 inch rectangular steel tubing 3/8 inches thick, fully welded at each joint. 

· The mounting for the drive motor and worm gear assembly and oscillating drive bars shall be 1 inch thick plates, each approximately 6 inches x 6 inches tied together with a 30 inch x 12 inch x 1 inch backing plate. In addition, a bottom plate to tie the 6 inch x 6 inch plates together (welded). 

· Up and down movement of the gear plate to the gear shall be limited by a steel surface attached to this sub-frame assembly. Gear plate play shall be 1/8 inch. The gear plate shall be centered on the worm gear.

· A bolt-on stabilizer, conforming to Drawing No. 4-211,  shall mate with the truss frame to provide alignment and strength to the entire mounted assembly. The "A" frame shall be connected to the truss frame by means of a 2 -1/2 inch diameter pin with a welded washer at the top which limits up/down movement of the frame. Two ears, each 1 inches thick, shall be an integral welded part of the "A" frame, on 21 inch centers, which will mate to the truck's hitch. 

· Each ear shall have two (2) 1 - 5/16 inch diameter holes, located 15 inches from the ground. The top of the ears shall be rounded. 

· The "A" frame shall have stops to prevent override of the worm gear.

Note: The maximum distance from the center holes of the two 1 inch thick ears (for mounting to the truck hitch) to the moldboard hinges shall be approximately 48 inches. This is specified to reduce weight on the front axle of the truck, as mounted.

Power Angling

The plow shall be constructed in a manner that will permit angling of the moldboard so as to discharge either to the right or to the left. The reversing mechanism shall be actuated by means of a Char-Lynn Model D5P, or approved equal hydraulic orbit motor. The motor shaft shall be properly supported so radial load design capacity is not exceeded. The motor shall be connected to a fabricated hardened steel worm 5-1/4 inch (13.3 cm) pitch that in turn rotates a 1 inch (2.54 cm) thick, bolt on, steel gear sector mounted on the truss frame. The mechanism shall give a 100 to 1 reduction ratio and infinitely variable plowing angles up to 35 degrees left or right from the bulldozing position. The moldboard  shall lock automatically at any plowing angle desired.

Lift Chain ASSEMBLY

Power reversible chain block and its accessory parts shall be manufactured in accordance with the following drawing and specification:

· Drawing 4-230

· The chain block shall be used in conjunction with a 60 inch long lift chain.

Bolts and Fasteners

All bolts and nuts shall be Grade 5 corrosion resistant. Lock washers shall be corrosion resistant. All bolt, nut and washer combinations  shall have a minimum of two (2) to three (3) bolt threads showing after it has passed through the nut.

hydraulic 

The hydraulics and its accessory parts shall be manufactured in accordance with the following specification:

· Hydraulic lines between hydraulic motor and truck front bumper quick disconnects shall be approximately 72 inches (183 cm) in length. All hydraulic lines are to terminate with swivel ends.

· One quick disconnect shall be ½ inch (1.27 cm) Snap-Tite (part # vphn) nipple or approved equal. One quick disconnect shall be ½  inch (1.27 cm) Snap-Tite (part # vphc) coupler or approved equal. 


· Hydraulic lines shall be pressure type, working pressure rated at 2000 PSI (138 bar) and minimum burst pressure rated at 8000 PSI (552 bar).

· Hydraulic hoses from the cylinder to the cushion valve and from the cushion valve back to the truck shall be 3/8 inch SAE 100R17 hose minimum and shall be of sufficient length for the application. 

For NJDOT Only:  There shall not be hydraulic quick disconnect on the hose ends, NJDOT will supply these. Hose ends to truck or hydraulic quick disconnects shall be specified by NJDOT. Hydraulic cylinder reverse mechanisms are not acceptable.

All other Using Agencies will specify hose ends at time of order.

[bookmark: _Toc53748377][bookmark: _Toc54703919]NJDOT Specific High Power reversible torsion trip edge plow, 11 foot wide, 36 inches high (Group 1, Price Line 4)

It is the intent of these specifications to describe an 11 foot long x 36 inch high power reversible torsion trip edge plow, built in accordance with the listed specifications and drawings.  

Moldboard

The moldboard and its accessory parts shall be manufactured in accordance with the following specifications:

· The moldboard shall be smooth rolled from 10 gauge steel and shall be 11 feet long by 36 inches high. The 36 inch moldboard height shall be to the inside of the highest point of the curl with the moldboard at approx. 25 degrees angle of attack. 

· Moldboard shall have a minimum of eight (8) vertical ribs ½ inch x 3 inches at the top tapered to ½ inch x 5-1/4 inches wide at the bottom angle reinforcement. Vertical ribs shall be doubled at the two moldboard back brace locations. 

· Moldboard shall have a bottom reinforcement angle of no less than 3-1/3 inches x 3-1/2 inches x ½ inch running the entire length of the moldboard. The top of the moldboard shall project over the cutting edge a minimum of 14 inches so as to form a solid built-in style “C” style snow shield with a top angle minimum of 3 inches x 2-1/2 inches x 3/8 inches. 

· The moldboard shall have (6) hinge points spanning a minimum of 116 inches for connecting to the push beam with minimum 1-1/4 inch diameter pins. The moldboard shall be continuously welded. 

· The moldboard shall have (2) back brace bars 1 inch thick x 3 inches wide to connect to the moldboard and truss frame at various pinning locations to hold moldboard rigid at various angles of attack from 7 degrees to 29 degrees. 

· A separate bolt-on snow shield shall be installed on each moldboard. It shall be constructed of 3/8 inch thick rubber belting, 12 inches wide and 132 inches long. A ¼ inch x 2 inch steel backing plate (full length)  shall be installed with seven (7) bolts to sandwich the snow shield to the moldboard. The moldboard shall incorporate a rigid support for installing the snow shield.

· The moldboard blade shall measure 6 inches x 132 inches and shall be made of high-tensile steel. It  shall conform to the Drawing - Blade "Z". 

Note: The moldboard shall have additional holes to accommodate 3 foot. and 4 foot. long carbide blade. 



Moldboard Left and Right Wrap arounds and Bumpers: 

The moldboard shall include left and right wrap around at the end of the moldboard blade. The left and right wrap shall be manufactured in accordance with the following drawings:

· Drawing 4-158 - Wrap Around - Right Side & Curb Bumper 

· Drawing 4-159 - Wrap Around - Left Side

The curb bumper and its accessory parts shall be manufactured in accordance with the follow drawings:

· Drawing 4-158 - Wrap Around - Right Side & Curb Bumper 

· Drawing 4-191

Trip Edge Mechanism 

The trip edge mechanism and its accessory parts shall be manufactured in accordance with the following specifications:

· Trip edge shall be of a single edge design fabricated from minimum 5 inches x 5 inches x ¾ inch angle with a ½ inch gussets located between each cutting edge hole.

· Bottom trip angle shall attach to the moldboard with a 2 inch solid round cold rolled bar running the entire length of the moldboard through all vertical ribs and shall have a bolt retainer at each end. Bottom trip edge shall activate whenever the cutting edge comes into contact with an obstruction on the road surface. 

· Trip activation shall be achieved through (5) horizontal mounted torsion springs from not less than 27/32 inch round wire having 3-15/16 inch O.D. with (14) active coils each. 

· Each spring shall be pinned in place in a horizontal position and shall butt against the lower moldboard reinforcement angle and to the cutting edge reinforcement angle. 

· Spring adjustment shall be provided to alter the pre-charge of springs for varying plowing conditions. 

Drive frame & reversing frame mechanism

The drive frame, reversing frame mechanism and its accessory parts shall be manufactured in accordance with the following specifications.

· The drive frame & reversing mechanism shall consist of an “A” frame, a truss frame, and two (2) 3-1/2 inch x 16 inch single acting reversing cylinders. 

· The “A” frame shall be a triangular shaped frame with 5/8 inch top and bottom plates, a rear member of 1 inch x 7 inch plate and three (3) ½ inch x 5-5/8 inch steel plates to serve as side and front members so to form a water tight boxed in center section. 

· The rear of the A frame shall have a bolt on swivel plate minimum 1 inch thick with push lugs minimum 1 inch thick lugs on 21 inch spacing. Swivel plate bolt shall be a minimum of 1-1/4 inch diameter and shall be grade 8. A-frame shall also have an access panel for replacement of swivel bar bolt. 

· The truss frame shall include a main drive member of 4 inch square tubing 3/8 inch wall and fitted with ½ inch top and bottom gusset plates to accommodate the pivot pin bushing. 

· The truss frame shall have a minimum (12) ¾ inch thick lugs mounted to the front for connection to the moldboard at not less than (6) points spanning a minimum of 116 inches. 

· The truss frame shall also have mounting plates for caster assemblies with carbide skid shoes. 

· The caster mounting plates shall be a ½ inch thick x 6 inches wide x 11 inches tall with ten (10) 13/16 inch holes for vertical adjustment in mounting the caster housings. Ten (10) holes shall be in two (2) rows of five (5) holes.

· The caster mounting plate shall be supported by minimum two (2) ½ inch plate gussets. Moldboard and truss frame shall angle up to 37 degrees left and right and shall pivot about the “A” frame on a removable lubricated pin of not less than 2-1/2 inch diameter.

· The reversing cylinders shall have a 3-1/2 foot diameter rod, 2-1/2 inch connecting lugs and 16 inch hold valve for use on trucks with open center hydraulics. 

Caster Assembly & Skid Shoes

The caster assembly, which includes the caster housing, caster stem, carbide snow plow shoe with axle and nut, shall be manufactured in accordance with the following drawings: 

· Drawing 4-216 – Caster Housing

· Drawing 4-182-1 or 4-212 - Caster Assembly 

· Drawing 4-182-2 - Caster Assembly

· Drawing 4-182-3 - Caster Assembly

· Drawing 4-219 – Axle – Pin Type

· Drawing 4-205 – 6 inch Snow Plow Shoe with Extended Leg
	
lift chain assemblY

The lift chain shall be ½ inch thick and 90 inches long.

Hydraulic lines

The hydraulic lines and its accessory parts shall be manufactured in accordance with the following specification:

· Hydraulic lines between hydraulic motor and truck front bumper quick disconnects shall be approximately 72 inches (183 cm) in length. All hydraulic lines shall terminate with swivel ends.

· One quick disconnect should/shall be ½ inch (1.27 cm) Snap-Tite (part# vphn) nipple or approved equal. One quick disconnect shall be  ½ inch (1.27 cm) Snap-Tite (part# vphc) coupler or approved equal. 

· Hydraulic lines shall bepressure type, working pressure rated at 2000 PSI (138 bar) and minimum burst pressure rated at 8000 PSI (552 bar).

Hydraulic hoses from the cylinder to the cushion valve and from the cushion valve back to the truck shall be 3/8 inch SAE 100R17 hose minimum and shall be of sufficient length for the application. There shall not be hydraulic quick disconnect on the hose ends,

For NJDOT Only:  There shall not be hydraulic quick disconnect on the hose ends, NJDOT will supply these. Hose ends to truck or hydraulic quick disconnects shall be specified by NJDOT. Hydraulic cylinder reverse mechanisms are not acceptable.

All other Using Agencies will specify hose ends at time of order.

[bookmark: _Toc19520362][bookmark: _Toc53748378][bookmark: _Toc54703920]ONE ADDITIONAL SET OF PARTS, SERVICE AND O&M MANUALS (Group 1, Price line 5)

Optional Manuals: One set of parts, service and operation and maintenance manuals for each and every assembly system and/or component that makes up the Units specified in Sections 3.4.1, 3.4.2, 3.4.3 and 3.4.4 shall be provided as follows: 

1 - set of parts manuals (illustrations and text) bound or with binders, and on CD-ROM. 

1 - set of complete shop repair (factory service) manuals bound or with binders and on CD-ROM. 

1 - set of complete operation & routine maintenance manuals 

1 - set of electrical schematics 

1 - set of troubleshooting manuals

The manuals shall be delivered directly to the Using Agency upon delivery of the Unit. 

[bookmark: _Toc19520363][bookmark: _Toc53748379][bookmark: _Toc54703921]TECHNICAL SUPPORT (HOURLY RATE) – OPERATORS AND MECHANICS TRAINING (Group 1, PRICE LINE 6)

Operator Training:

The Vendor {Contractor}, shall provide training for the Units specified in Sections 3.4.1, 3.4.2, 3.4.3 and 3.4.4, as described below.  

The Vendor {Contractor} shall coordinate with the Using Agency to provide an operator training session for a maximum of ten (10) personnel.

Complete instructions on the operation and maintenance of each Unit and a demonstration on the operation of the Unit shall be given by the Vendor {Contractor}. 

The training shall consist of, but is not limited to, operator training with instruction on proper operation of the Unit, safety, and basic preventive maintenance. 

This demonstration shall be a formal training session and shall be arranged with the Vendor {Contractor}. 

The training session shall be conducted at a specific location or a field location, within the State of New Jersey as agreed upon between the Vendor {Contractor} and the Using Agency.



Mechanics Training:

The Vendor {Contractor}, shall provide technical training for all components of the complete Units specified in Sections 3.4.1, 3.4.2, 3.4.3 and 3.4.4.  

The Vendor {Contractor} shall coordinate with the Using Agency to provide a mechanics training session for a maximum of five (5) personnel.

Course content shall be tailored to meet the specific needs of the Using Agency mechanics, and shall not place emphasis on areas or components not specified in the Bid Solicitation. The course shall also include hands-on instruction and content to reinforce lecture content.

The training session shall be conducted at a specific location or a field location, within the State of New Jersey as agreed upon between the Vendor {Contractor} and the Using Agency.

[bookmark: _Toc53748380][bookmark: _Toc54703922]SPECIAL MONOTONE PAINT COLOR IN LIEU OF MANUFACTURER’S STANDARD PAINT COLOR (Group 1, PRice Line 7) 

NJDOT Units:

The Unit and all its components shall be cleaned and painted with one (1) coat of DuPont #1858 primer, and finished with two (2) coats of the color DuPont Centari #7744-A Lime Yellow. All paint shall be the same shade. 

All other Using Agencies: Using Agency will specify special monotone paint color at the time of ordering. 

[bookmark: _Toc53748381][bookmark: _Toc54703923]NJTA Specific MANUAL REVERSible ONE-WAY SNOW PLOW, 11 FooT Long, 47 Inches HiGH (Group 2, Price Line 8)

It is the intent of these specifications to describe an 11 foot x 47 inch high manual reversible one-way style type plow, built in accordance with the listed specifications and drawings. 

NOTE: Using Agencies will specify at time of order snow plow and snow plow blade combination/configuration. (i.e. Price Line  8 in combination with Price Line 12).
 
MOLDBOARD 

The moldboard and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-06
· The moldboard shall be 27 inches high at the nose end, 47 inches high at the discharge end and shall be overall 136 inches long
· The moldboard shall be 132 inches at the snow plow blade and formed in a funnel shaped blade 
· The radius shall be 20 inches and the last 12 inches shall have a minimum of a 6 inch radius.
MOLDBOARD SHOEs:

The moldboard shoes and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-06
· The snow plow shall be equipped with two (2) moldboard shoes.
· The moldboard shoe shall be constructed of cast steel and have a bearing wear surface of minimum 40 square inches each.
· The moldboard shoes shall be attached directly behind the snow plow blade and shall be designed to wear evenly with an 8 inch snow plow blade.  
· The moldboard shoes shall have two (2) 11/16 inch diameter bolt holes spaced on 12 inch centers for mounting to the snow plow.
· The moldboard shall be constructed with a minimum of 10-gauge steel paneled for additional strength.
CURB BUMPER 

The curb bumper and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP- 01
· Drawing SSP – 4-158
· Drawing SPP – 4-159
· Two (2) 2½ inch x 2½ inch x 8 inch cold rolled steel curb bumpers (wrap around style) shall be bolted to the lower left and right outside edge of the moldboard lower angle as part of the cutting-edge assembly.
· The bottom edge of the curb bumper shall be positioned at a height equal to the moldboard shoe.
· The curb bumper / wraparound shall bolt on as part of the plow blade attachment area.
TRIPPING MECHANISM: 

The tripping mechanism and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01 
· Drawing SSP-11
· The plow shall include a spring controlled full moldboard hinged spring mechanism.
· A minimum of six (6) heavy-duty extension springs shall be attached between the table and the moldboard.
· The spring materials shall be ASTM-A229 oil tempered ½ inch wire, 4½ inch O.D.  x twenty-four (24) active coils with the end hooks cold formed to 90 degree right angles to each other. 
· The spring force at 30.5 inch shall be a minimum of 750 pounds and allow 14 inch of stretch without deformation. 
· The springs shall maintain the vertical stability of the moldboard while plowing and facilitate a controlled trip/return action when coming in contact with any solid object while plowing.
· The trip springs shall be designed to have adjustable spring tension.
· Each spring shall be able to be adjusted individually by a threaded “J” hook or approved equal.  This will be confirmed by Using Agency at prebuilt meeting.
· A mechanical telescopic tripping post assembly constructed of a minimum of 1-¼ inch x 2 inch inside bar, ¾ inch x 2-¼ inch outside bar and reinforced with ¼ inch x 2 inch bars.
· The tripping post assembly shall be independent of the springs and must prevent the top of the moldboard from contacting the road surface.
· Two (2) 1 inch diameter pins with a minimum tensile strength of 72,000 pounds shall connect the tripping post to the moldboard and table. 
TABLE 

The table and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The table shall be a circular arc design and be constructed of a one piece solid 3-½ inch x 3-½ inch x ½ inch structural angle, a 4 inch x ¾ inch bar shall be fabricated to conform to the outside radius with eleven (11) notches 1¼ inch deep x 1⅛ inch wide at the bottom and 1-½ inch wide at the outer edge and welded in a vertical position along the underside of the 3-½ inch x 3-½ inch x ½ inch structural angle radius.  
· The notches shall be laser cut. (Flame cutting to achieve curve and notches shall not be acceptable.)
· The circular arc portion shall be welded at each end with an overlap to structural angles measuring 4 inches x 4 inches x ½ inch that continues the length of the semicircle and joins to the front square tube measuring 4 inches x 4 inches x ⅜ inch.
· The joining of the semicircle to the front tube shall be reinforced on each side by 3-½ inch x 3-½ inch x ½ inch structural angle.
· The front of the table shall be provided with a minimum of ten (10) brackets ⅝ inch thick, welded on 88 inch hinge point centers for attachment to the moldboard assembly at five (5) points with a minimum of 1 inch (72,000 pounds) tensile strength pins.
· The front center of the table shall be designed for attachment to the “A” frame with a 1-¾ inch diameter vertical pin with locked rotation to the A-frame and secured by a ⅜ inch roll pin.
LIFT CHAIN

The lift chain and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The lift chain assembly shall include a zinc plated 7/16 inch proof coil chain, repair link, two (2) ½ inch anchor shackles and a 7/16 inch grab hook clevis.
· There shall be two (2) tabs welded on the table for attachment of the lift chain.


PUSH FRAME

The push frame and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01 
· Drawing SPP- 4-132
· The push frame shall be constructed of two (2) 4 inch @ 13.8 pounds ship channels with bracing and shall be in the form of an “A”.
· The top and bottom of the push frame shall be ½ inch triangular shaped plate.
· Welded to the front of these triangular plates shall be a pair of ¾ inch x 4 inch steel brackets and between them a curved socket member shall be provided to relieve the pivot pin of thrust stress.
· The attachment pin at this point shall be a minimum of 1¾ inch diameter axle quality steel that shall engage with corresponding ears on the front tube of the semicircular frame.
· At the center of this box construction of plates and channels in the line of forward rotation shall be an assembly welded to form a continuous thrust beam.
· A latch part shall be incorporated which continues further to the rear and presses against a heavy-duty latch spring measuring 5-7/16 inch O.D. x ¾ inch diameter spring wire with 9 inches of free travel. 
· The spring shall be made of AISI 5160 hot rolled spring steel and shall be heat treated after cooling. Spring shall be closed and ground.
· The latch shall seat against a circular plate welded to the rear cross channel.
· Lubrication fittings shall be provided to allow ease of movement of slide assembly, which telescopes on the tubular member.
· The two (2) rear channels of the push frame shall be provided with a heavy-duty 1 inch thick A36 steel adjustable ear for attachment of the push frame to the travel hitch with 1¼ inch diameter bolt. Ear spacing shall be 21 inches. 
· Plow connection pins shall be 1-¼ inch diameter and tapered. Two (2) shall be supplied with chain retainers.  
MANUAL REVERSE

The manual reverse and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-06
· The latching mechanism shall operate manually and monitor the angle of the moldboard in any of eleven (11) positions from 35 degree right or left in 7 degree increments. Two (2) pins shall hold it in place.
MUSHROOM 

The mushroom and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP – 12 
· Drawing SSP - 18
· The skid shoe assemblies shall be of the hand adjustable type, enclosed and fully lubricated with replaceable chilled cast iron shoes “Mushroom” shaped of a minimum of 12 inches in diameter and 2 inches thick.  
· The design shall include an anti-flip top.
· The shoe housing shall be constructed of 3 inch square tubing x 12 inches long and the shoe post shall be constructed of 2-½ inch square tubing x 11 inches long.
· The adjustment shall be accomplished by a threaded 1-¼ inch diameter screw operated by a hand crank with rotating knob, which shall be self-locking and shall operate without the use of any tools. The adjusting screw shall be fully enclosed.
PLOW MARKERS

The plow markers accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The snow plow shall be equipped with two (2) 36 inch orange reinforced markers constructed of ¾ inch polymer reinforced with a ⅜ inch galvanized cable.
· Each plow marker shall be equipped with a crimped base 2-bolt mount installed at the upper outer most left and right corners of the moldboard and attached to a reinforced rib with bolts and nylock nuts.
RUBBER BAFFLE 

The rubber baffle and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP - 01 
· Drawing SSP - 02 
· Drawing SSP - 03
· The snow plow shall be equipped with a ½ inch thick x 12 inches wide x 11 foot long rubber belting baffle.  
· The baffle shall be bolted to top of moldboard with a ¼ inch x 2 inches x 11 foot steel keeper bar.
WELDING

The snow plows welding shall meet the following requirements:

· All welds shall be continuous.
· All welding performed in the manufacturing of the snow plow shall be done by certified welders.
· Written certification shall come from a recognized welding supply manufacturer and/or school.
[bookmark: _Toc53748382][bookmark: _Toc54703924]NJTA Specific MANUAL REVERSIBLE SNOW PLOW, 11 Foot Long, 42 inches High (J-STYLE) (Group 2, Price line 9)

It is the intent of these specifications to describe an 11 foot x 42 inch manual reversible “J” style type plow, built in accordance with the listed specifications and drawings.  

NOTE: Using Agencies will specify at time of order snow plow and snow plow blade combination/configuration. (I.e. Price Line 9 in combination with Price Line 14).

MOLDBOARD

The moldboard and its accessory parts shall be manufactured in accordance with the following drawing and specifications: 

· Drawing SSP-03
· The moldboard shall be 42 inches high and 136 inches long formed in an “J” shaped blade
· The radius shall be 20 inches and the last 12 inches shall have a minimum radius of 6 inches.
· The moldboard shall be constructed with a minimum of 10 gauge steel paneled for additional strength.
· The top shall be reinforced by a self-formed channel and the bottom with a one piece 4 inch x 4 inch x ½ inch structural angle.  
· The cutting-edge’s ⅝ inch x 4 inch steel banking plate   shall be welded and braced with a ½ inch x 2½ inch gussets welded between each cutting-edge bolt position. 
· This structural triangle shall be constructed to have the cutting-edge flush with the moldboard face to prevent snow build up on top of the snow plow blade.
· A minimum of twelve (12) full length vertical ribs shall reinforce the moldboard.
· The vertical rails shall be constructed of ½ inch x 3 inch formed steel continuously welded on both sides of edge to the moldboard sheet and secured at the top to the formed channel and to the structured angle at the bottom.  
· Two (2) horizontal braces shall also reinforce the moldboard.  
· The braces shall be constructed of ¼ inch x 2 inch x 2 inch angle or ½ inch x 3 inch flat bar continuously welded on both sides to moldboard sheets.
· The lower rear cross angle shall be provided with a minimum of ten (10) brackets ¾ inch thick welded on 88 inch hinge point centers for attachment to the table assembly at five (5) points with a minimum of 1 inch (72,000 pounds) tensile strength pins.
Moldboard Shoe

The moldboard shoe and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-03
· The snow plow shall be equipped with two (2) moldboard shoes.
· The moldboard shoe shall be constructed of cast steel and have a bearing wear surface of at least 40 square inches each.
· The moldboard shoes shall be attached directly behind the snow plow blade and be designed to wear evenly with an 8 inch snow plow blade. 
· The moldboard shoes shall have two (2) 11/16 inch diameter bolt holes spaced on 12 inch centers for mounting to the snow plow.
Curb Bumper: 

The curb bumper and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP – 01
· Drawing SPP - 4-158 
· Drawing SPP - 4 -159
· Two (2) 2½ inch x 2½ inch x 8 inch cold rolled steel curb bumpers (wrap around style) shall be bolted to the lower left and right outside edge of the moldboard lower angle as part of the cutting-edge assembly.
· The bottom edge of the curb bumper shall be positioned at a height equal to the moldboard shoe.
· The curb bumper / wraparound shall bolt on as part of the plow blade attachment area.
TRIPPING MECHANISM

The tripping mechanism and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01
· Drawing SSP-11
· The plow shall include a spring controlled full moldboard hinged spring mechanism.
· A minimum of six (6) heavy-duty extension springs shall be attached between the table and the moldboard.
· The spring materials shall be ASTM-A229 oil tempered ½ inch wire, 4-½ inch O.D. x twenty-four (24) active coils with the end hooks cold formed to 90 degree right angles to each other. 
· The spring force at 30.5 inches shall be a minimum of 750 pounds and allow 14 inches of stretch without deformation.  
· The springs shall maintain the vertical stability of the moldboard while plowing and facilitate a controlled trip/return action when coming in contact with any solid object while plowing. 
· The trip springs shall be designed to have adjustable spring tension. 
· Each spring shall be able to be adjusted individually by a threaded “J” hook or approved. This will be decided at the pre-build meeting.  
· A mechanical telescopic tripping post assembly constructed of a minimum of 1¼ inch x 2 inch inside bar, ¾ inch x 2-¼ inch outside bare and reinforced with ¼ inch x 2 inch bars.
· The tripping post assembly shall be independent of the springs and must prevent the top of the moldboard from contacting the road surface.
· Two (2) 1 inch diameter pins with a minimum tensile strength of 72,000 pounds shall connect tripping post to the moldboard and table. 
TABLE 

The table and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The table shall be a circular arc design and shall be constructed of a one piece solid 3-½ inch x 3-½ inch x ½ inch structural angle, a 4 inch x ¾ inch bar shall be fabricated to conform to the outside radius with eleven (11) notches 1-¼ inch deep x 1-⅛ inch wide at the bottom and 1-½ inch wide at the outer edge and welded in a vertical position along the underside of the 3-½ inch x 3-½ inch x ½ inch structural angle radius.   
· The notches shall be laser cut. Flame cutting to achieve curve and notches shall not be acceptable.
· Circular arc portion shall be welded at each end with an overlap to structural angles measuring 4 inches x 4 inches x ½ inch that continues the length of the semicircle and joins to the front square tube measuring 4 inches x 4 inches x ⅜ inch.
· The joining of the semicircle to the front tube shall be reinforced on each side by 3-½ inch x 3-½ inch x ½ inch structural angle.
· The front of the table shall be provided with a minimum of ten (10) brackets ⅝ inch thick welded on 88 inch hinge point centers for attachment to the moldboard assembly at five (5) points with a minimum of 1 inch (72,000 pounds) tensile strength pins.
· The front center of the table shall be designed for attachment to the “A” frame with a 1-¾ inch diameter vertical pin with locked rotation to the A-frame and secured by a ⅜ inch roll pin.
LIFT CHAIN 

The lift chain and its accessory parts shall be manufactured in accordance with the following drawing and specifications: 

· Drawing SSP-01
· The lift chain assembly shall include a zinc plated 7/16 inch proof coil chain, repair link, two (2) ½ inch anchor shackles and a 7/16 inch grab hook clevis. 
There shall be two (2) tabs welded on the table for attachment of the lift chain.
PUSH FRAME 

The push frame and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01 
· Drawing SPP- 4-132
· The push frame shall be constructed of two (2) 4 inch @ 13.8 lb. ship channels with bracing and be in the form of an “A”.
· The top and bottom of the push frame shall be ½ inch triangular shaped plate.
· Welded to the front of these triangular plates shall be a pair of ¾ inch x 4 inch steel brackets and between them a curved socket member shall be provided to relieve the pivot pin of thrust stress.
· The attachment pin at this point shall be a minimum of 1-¾ inch diameter axle quality steel that shall engage with corresponding ears on the front tube of the semicircular frame.
· At the center of this box construction of plates and channels in the line of forward rotation shall be an assembly welded to form a continuous thrust beam.
· A latch part shall be incorporated which continues further to the rear and presses against a heavy-duty latch spring measuring 5-7/16 inch O.D. x ¾ inch diameter spring wire with 9 inches of free travel. 
· The spring shall be made of AISI 5160 hot rolled spring steel and shall be heat treated after cooling.  Spring shall be closed and ground.
· The latch shall seat against a circular plate welded to the rear cross channel.
· Lubrication fittings shall be provided to allow ease of movement of slide assembly, which telescopes on the tubular member.
· The two (2) rear channels of the push frame shall be provided with a heavy-duty 1 inch thick A36 steel adjustable ear for attachment of the push frame to the travel hitch with 1¼ inch diameter bolt. Ear spacing shall be 21 inch. 
· In lieu of the push frame adjustable ear attachment above; The two (2) rear channels of the push frame shall be provided with a heavy-duty 1 inch thick A36 steel adjustable for attachment of the push frame to a Pin & Loop style travel hitch with 1¼ inch diameter bolt.  
NOTE:  Using Agencies will identify if they will require the adjustable ear or the pin & loop style attachment at the time of order.

· Plow connection pins shall be 1¼ inch diameter and tapered. Two (2) shall be supplied with chain retainers. 
MANUAL REVERSE

The manual reverse and its accessory parts shall be manufactured in accordance with the following drawing and specifications: 

· Drawing SSP-06
· The latching mechanism shall operate manually and monitor the angle of the moldboard in any of eleven (11) positions from 35 degrees right or left in 7 degree increments. Two (2) pins shall hold it in place.
MUSHROOM

The mushroom and its accessory parts shall be manufactured in accordance with the following drawing and specifications: 

· Drawing SSP – 12
· Drawing SSP - 18
· The skid shoe assemblies shall be of the hand adjustable type, enclosed and fully lubricated with replaceable chilled cast iron shoes “Mushroom” shaped of a minimum of 12 inches in diameter and 2 inches thick.    
· The design shall include an anti-flip top.
· The shoe housing shall be constructed of 3 inch x 12 inch long square tubing and the shoe post shall constructed of 2-½ inch x 11 inch long square tubing.
· The adjustment shall be accomplished by a threaded 1-¼ inch diameter screw operated by a hand crank with rotating knob, which shall be self- locking and shall operate without the use of any tools. The adjusting screw shall be fully enclosed.
Plow Markers 

The plow markers and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP – 01
· The snow plow shall be equipped with two (2) 36 inch orange reinforced markers constructed of ¾ inch polymer reinforced with a ⅜ inch galvanized cable.
· Each plow marker shall be equipped with a crimped base 2-bolt mount installed at the upper outer most left and right corners of the moldboard and attached to a reinforced rib with bolts and nylock nuts.
Rubber Baffle

The rubber baffle and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP – 01
· Drawing SSP - 02
· Drawing SSP - 03
· The snow plow shall be equipped with a ½ inch thick x 12 inch wide x 11 foot long rubber belting baffle.  
· The baffle shall be bolted to top of moldboard with a ¼ inch x 2 inch x 11 foot steel keeper bar.
Welding

The plows welding shall meet the following requirements:

· All welds shall be continuous.
· All welding performed in the manufacturing of the snow plow shall be done by certified welders.
· Written certification shall come from a recognized welding supply manufacturer and/or school at the time of delivery of the completed Unit.
[bookmark: _Toc53748383][bookmark: _Toc54703925]NJTA SPECIFIC POWER REVERSIBLE EXPRESSWAY SNOW PLOW, 11 Foot Wide, 50 inches High (Group 2, Price Line 10)

It is the intent of these specifications to describe an 11 feet x 50 inch power reversible dual tapered (expressway) style type plow, built in accordance with the listed specifications and drawings

NOTE: Using Agencies will specify at time of order snow plow and snow plow blade combination/configuration. (i.e. Price Line 10 in combination with Price Line 13).

MOLDBOARD

The moldboard and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP-04
· Drawing SSP-05
· The moldboard shall be 40 inches high in the center, 50 inches high at each discharge end and 132 inches long formed in a “J” shaped dual tapered blade. The radius shall be approximately 20 inches and the last 12 inches shall have a minimum of a 6 inch radius. The moldboard ends shall be perpendicular in a “mailbox” cut. (no bellow or flared end).
· The moldboard shall be constructed with a minimum of 10 gauge steel paneled for additional strength.
· The top shall be reinforced at the top by a self-formed channel and the bottom with a one piece 4 inch x 4 inch x ½ inch structural angle.  
· The snow plow blade’s ⅝ inch x 4 inch steel banking plate shall be welded and braced with a ½ inch x 2-½ inch gussets welded between each cutting-edge bolt position. 
· The edge shall be flush with the moldboard face to prevent snow build up on top of the cutting-edge.
· A minimum of twelve (12) full length vertical ribs shall reinforce the moldboard.
· The vertical rails shall be constructed of ½ inch x 3 inch formed steel continuously welded on both sides of edge to the moldboard sheet and secured at the top to the formed channel and to the structured angle at the bottom.
· Two (2) horizontal braces shall also reinforce the moldboard.
· The braces shall be constructed of ¼ inch x 2 inch x 2 inch angle or ½ inch x 3 inch flat bar continuously welded on both sides to moldboard sheets.
· The lower rear cross angle shall be provided with a minimum of ten (10) brackets ¾ inch thick welded on 88 inch hinge point centers for attachment to the table assembly at five (5) points with a minimum of 1 inch (72,000 pounds) tensile strength pins.
MOLDBOARD SHOE

The moldboard shoe and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP- 04
· The snow plow shall be equipped with two (2) moldboard shoes.
· The moldboard shoe shall be constructed of cast steel and have a bearing wear surface of at least 75 square inches each.
· The moldboard shoes shall be attached directly behind the snow plow blade and be designed to wear evenly with an 8 inch snow plow blade. 
· The moldboard shoes shall have two (2) 11/16 inch diameter bolt holes spaced on 12 inch centers for mounting to the snow plow.
CURB BUMPER 

The curb bumper and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP-01 
· Drawing SPP-4-158 
· Drawing SSP- 4-159
· Two (2) 2-½ inch x 2-½ inch x 8 inch cold rolled steel curb bumpers (wrap around style) shall be bolted to the lower left and right outside edge of the moldboard lower angle as part of the cutting-edge assembly.
· The bottom edge of the curb bumper shall be positioned at a height equal to the moldboard shoe.
· The curb bumper / wraparound shall bolt on as part of the plow blade attachment area.
TRIPPING MECHANISM 

The tripping mechanism and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01 
· Drawing SSP-11
· The plow shall include a spring controlled full moldboard hinged spring mechanism. A minimum of six (6) heavy-duty extension springs shall be attached between the table and the moldboard.
· The spring materials shall be ASTM-A229 oil tempered ½ inch wire, 4½ inch O.D. x 24 active coils with the end hooks cold formed to 90 degree right angles to each other.
· The spring force at 30.5 inches shall be a minimum of 1,050 pounds and allow 14 inches of stretch without deformation.
· The springs shall maintain the vertical stability of the moldboard while plowing and facilitate a controlled trip/return action when coming in contact with any solid object while plowing. 
· The trip springs shall be designed to have adjustable spring tension.
· Each spring shall be able to be adjusted individually by a threaded “J” hook or approved equal. 
· A mechanical telescopic tripping post assembly constructed of a minimum of 1-¼ inch x 2 inch inside bar, ¾ inch x 2-¼ inch outside bare and reinforced with ¼ inch x 2 inch bars.
· The tripping post assembly shall be independent of the springs and must prevent the top of the moldboard from contacting the road surface.
· Two (2) 1 inch diameter pins with a minimum tensile strength of 72,000 pounds shall connect tripping post to the moldboard and table.
TABLE 

The table and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The table shall be a circular arc design and be constructed of a one piece solid 4 inch x 4 inch x ½ inch structural angle, a 4 inch x ¾ inch bar shall be fabricated to conform to the outside radius with eleven (11) notches 1-¼ inches deep x 1-⅛ inches wide at the bottom and 1-½ Inches wide at the outer edge and welded in a vertical position along the underside of the 4 inch x 4 inch x ½ inch structural angle radius.   
· The notches shall be sheared cut. Flame cutting to achieve curve and notches shall not be acceptable.
· Circular arc portion shall be welded at each end with an overlap to structural angles measuring 4 inches x 4 inches x ½ inch that continues the length of the semicircle and joins to the front square tube measuring 4 inches x 4 inches x ⅜ inch. 
· The joining of the semicircle to the front tube shall be reinforced on each side by 3½ inch x 3-½ inch x ½ inch structural angle. 
· The front of the table shall be provided with a minimum of ten (10) brackets ⅝ inch thick welded on 88 inch hinge point centers for attachment to the moldboard assembly at five (5) points with a minimum of 1 inch 72,000 lb. tensile strength pins.
· The front center of the table shall be designed for attachment to the “A” frame with a 1-¾ inch diameter vertical pin with locked rotation to the A-frame and secured by a ⅜ inch roll pin.
LIFT CHAIN 

The lift chain and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The lift chain assembly shall include a zinc plated 7/16 inch coil proof chain, repair link, two (2) ½ inch anchor shackles and a 7/16 inch grab hook clevis. 
· There shall be two (2) tabs welded on the table for attachment of the lift chain.
PUSH FRAME

The push frame and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01
· Drawing SPP-4-132
· The push frame shall be constructed of two (2) 4 inch @ 13.8 pounds ship channels with bracing and shall be in the form of an “A”. 
· The top and bottom of the push frame shall be ½ inch triangular shaped plate.
· Welded to the front of these triangular plates shall be a pair of ¾ inch x 4 inch steel brackets and between them a curved socket member shall be provided to relieve the pivot pin of thrust stress.
· The attachment pin at this point shall be a minimum of 1¾ inch diameter axle quality steel that shall engage with corresponding ears on the front tube of the semicircular frame.  
· At the center of this box construction of plates and channels in the line of forward rotation shall be an assembly welded to form a continuous thrust beam.
· A latch part shall be incorporated which continues further to the rear and presses against a heavy-duty latch spring measuring 5-7/16 inch O.D. x ¾ inch diameter spring wire with 9 inches of free travel. 
· The spring shall be made of AISI 5160 hot rolled spring steel and shall be heat treated after cooling. Spring shall be closed and ground.
· The latch shall seat against a circular plate welded to the rear cross channel.
· Lubrication fittings shall be provided to allow ease of movement of slide assembly, which telescopes on the tubular member.
· The two (2) rear channels of the push frame shall be provided with a heavy-duty 1 inch thick cast steel adjustable ear for attachment of the push frame to the travel hitch with 1¼ inch diameter bolt.  Ear spacing shall be 21 inches. 
· In lieu of the push frame adjustable ear attachment above; The two (2) rear channels of the push frame shall be provided with a heavy-duty 1 inch thick A36 steel adjustable for attachment of the push frame to a Pin & Loop style travel hitch with 1¼ inch diameter bolt.  
NOTE:  Using Agencies will identify if they will require the adjustable ear or the pin & loop style attachment at time or order.

HYDRAULIC REVERSING CYLINDERS

The hydraulic reversing cylinders and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01 
· Drawing SPP-02
· The hydraulic reversing mechanism shall consist of two (2) hydraulic cylinders nitride piston rods and a minimum of 2½ inch diameter and 10 inch stroke.  
· The hydraulic cylinder housing shall attach to the push frame and the hydraulic cylinder piston shall attach to the front table tube with 1 inch pins secured by ¼ inch roll pins.
· Hydraulic cylinders shall be positioned to unlatch the semicircle and angle the moldboard to the desired plowing position.  
· The latching mechanism shall operate automatically and monitor the moldboard in any of eleven (11) positions from 35 degree right or left in 7 degree increments.
· High pressure hydraulic hose connections shall be made to each of the two (2) cylinders with long 90 degree JIC elbow female swivel crimp hose fittings and extend to the rear terminating in male and female brass quick disconnect couplings. This will allow the hoses to be connected during storage. All couplings shall have lanyard attached rubber cap/plug covers.
· During operation, the hoses shall connect to the corresponding connections on the Using Agency trucks.
MUSHROOM

The mushroom and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawings SSP-12
· Drawings SPP-18
· The skid shoe assemblies shall be of the hand adjustable type, enclosed and fully lubricated with replaceable chilled cast iron shoes “Mushroom” shaped of a minimum of 11 inches in diameter and 2-½ inches thick.    
· The design shall include an anti-flip top.
· The shoe housing shall be constructed of 3 inch x 12 inch long square tubing and the shoe post shall be constructed of 2-½ inch x 11 inch long square tubing.
· The adjustment shall be accomplished by a threaded 1-¼ inch diameter screw operated by a hand crank with rotating knob, which shall be self-locking and shall operate without the use of any tools. The adjusting screw shall be fully enclosed.
LEVEL-LIFT ASSEMBLY

The lift assembly and its accessory parts shall be manufactured in accordance with the following drawings and specifications

· The level-lift assembly shall provide an automatic, mechanically activated mechanical control, which will hold a raised plow moldboard an equal distance from the ground to the bottom of the snow plow blade.
· The level-lift mechanism will hold an equal elevation regardless of height raised above the road surface and regardless of moldboard plowing angle.
· The moldboard plowing angle shall be able to be changed to any desired position, maintaining equal elevation without first lowering plow, changing plowing angle and then re-lifting.
PLOW MARKERS

The plow markers accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The snow plow shall be equipped with two (2) 36 inch orange reinforced markers constructed of ¾ inch polymer reinforced with a ⅜ inch galvanized cable.  
· Each plow marker shall be equipped with a crimped base 2-bolt mount installed at the upper outer most left and right corners of the moldboard and attached to a reinforced rib with bolts and nylock nuts.
RUBBER BAFFLE

The rubber baffle and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP - 01 
· Drawing SSP - 02 
· Drawing SSP - 03
· The snow plow shall be equipped with a ½ inch thick x 12 inch wide x 11 foot long rubber belting baffle.  
· The baffle shall be bolted to the top of the moldboard with a ¼ inch x 2 inch x 11 foot steel keeper bar.
WELDING

All welding shall meet the following requirements:

· All welds shall be continuous.
· All welding performed in the manufacturing of the snow plow shall be done by AWS certified welders.
· Proof of AWS certification shall be presented at time of delivery.
[bookmark: _Toc53748384][bookmark: _Toc54703926]NJTA Specific POWER REVERSIBLE SNOW PLOW, 11 FooT Long, 42 inches high (Group 2, Price line 11)

It is the intent of these specifications to describe an 11 foot x 42 inch power reversible “J” style type plow, built in accordance with the listed specifications and drawings

NOTE Using Agencies will specify at time of order snow plow and snow plow blade combination/configuration. (I.e. Price Line 11 in combination with Price Line 12).

MOLDBOARD:

The moldboard and its accessory parts shall be manufactured in accordance with the following drawing and specifications

· Drawing SSP-03:

· The moldboard shall be 42 inches high and 132 inches long formed in a “J” shaped blade. 
· The radius shall be approximately 20 inches and the last 12 inches shall be a minimum of a 6 inch radius per Drawing: SSP-03
· The moldboard shall be constructed with a minimum of 10 gauge steel, paneled for additional strength.
· The top shall be reinforced at the top by a self-formed channel and the bottom with a one piece 4 inch x 4 inch x ½ inch structural angle.  
· The cutting-edge banking plate of ⅝ inch x 4 inch steel shall be welded and braced with a ½ inch x 2-½ inch gussets welded between each cutting-edge bolt position. 
· The edge shall be flush with the moldboard face to prevent snow build up on top of the cutting-edge.
· A minimum of twelve (12) full length vertical ribs shall reinforce the moldboard.
· The vertical rails shall be constructed of ½ inch x 3 inch formed steel continuously welded on both sides of edge to the moldboard sheet and secured at the top to the formed channel and to the structured angle at the bottom.
· Two (2) horizontal braces shall also reinforce the moldboard.  
· The braces shall be constructed of ¼ inch x 2 inch x 2 inch angle or ½ inch x 3 inch flat bar continuously welded on both sides to moldboard sheets.
· The lower rear cross angle shall be provided with a minimum of ten (10) brackets ¾ inch thick welded on 88 inch hinge point centers for attachment to the table assembly at five (5) points with a minimum of 1 inch (72,000 pounds) tensile strength pins.
MOLDBOARD SHOE:

The moldboard shoe and its accessory parts shall be manufactured in accordance with the following specifications:

· The snow plow shall be equipped with two (2) moldboard shoes.
· The moldboard shoe shall be constructed of cast steel and have a bearing wear surface of at least 75 square inches each.
· The moldboard shoes shall be attached directly behind the snow plow blade and be designed to wear evenly with an 8 inch snow plow blade.  
· The moldboard shoes shall have two (2) 11/16 inch diameter bolt holes spaced on 12 inch centers for mounting to the snow plow.
CURB BUMPER

The curb bumper and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP - 01 
· Drawing SSP – 4-158 
· Drawing SPP – 4-159
· Two (2) 2½ inch x 2½ inch x 8 inch cold rolled steel curb bumpers (wrap around style) shall be bolted to the lower left and right outside edge of the moldboard lower angle as part of the cutting-edge assembly.
· The bottom edge of the curb bumper shall be positioned at a height equal to the moldboard shoe.
· The curb bumper / wraparound shall bolt on as part of the plow blade attachment area.
TRIPPING MECHANISM

The tripping mechanism and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01 
· Drawing SSP-11
· The plow shall include a spring controlled full moldboard hinged spring mechanism. A minimum of six (6) heavy-duty extension springs shall be attached between the table and the moldboard.
· The spring materials shall be ASTM-A229 oil tempered ½ inch wire, 4-½ inch O.D. x 24 active coils with the end hooks cold formed to 90 degree right angles to each other.
· The spring force at 30.5 inches shall be a minimum of 1,050 pounds and allow 14 inches of stretch without deformation.
· The springs shall maintain the vertical stability of the moldboard while plowing and facilitate a controlled trip/return action when coming in contact with any solid object while plowing. 
· The trip springs shall be designed to have adjustable spring tension.
· Each spring shall be able to be adjusted individually by a threaded “J” hook or approved equal. 
· A mechanical telescopic tripping post assembly constructed of a minimum of 1-¼ inch x 2 inch inside bar, ¾ inch x 2-¼ inch outside bar and reinforced with ¼ inch x 2 inch bars.
· The tripping post assembly shall be independent of the springs and must prevent the top of the moldboard from contacting the road surface.
· Two (2) 1 inch diameter pins with a minimum tensile strength of 72,000 pounds shall connect tripping post to the moldboard and table.
TABLE

The table and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The table shall be a circular arc design and be constructed of a one piece solid 4 inch x 4 inch x ½ inch structural angle, a 4 inch x ¾ inch bar shall be fabricated to conform to the outside radius with eleven (11) notches 1-¼ inch deep x 1-⅛ inch wide at the bottom and 1-½ inch wide at the outer edge and welded in a vertical position along the underside of the 4 inch x 4 inch x ½ inch structural angle radius.   
· The notches shall be sheared cut. Flame cutting to achieve curve and notches shall not be acceptable.
· Circular arc portion shall be welded at each end with an overlap to structural angles measuring 4 inches x 4 inches x ½ inch that continues the length of the semicircle and joins to the front square tube measuring 4 inches x 4 inch x ⅜ inch. 
· The joining of the semicircle to the front tube shall be reinforced on each side by 3½ inch x 3½ inch x ½ inch structural angle. 
· The front of the table shall be provided with a minimum of ten (10) brackets ⅝ inch thick welded on 88 inch hinge point centers for attachment to the moldboard assembly at five (5) points with a minimum of 1 inch (72,000 pounds) tensile strength pins.
· The front center of the table shall be designed for attachment to the “A” frame with a 1¾ inch diameter vertical pin with locked rotation to the A-frame and secured by a ⅜ inch roll pin.
LIFT CHAIN

The lift chain and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The lift chain assembly shall include a zinc plated 7/16 inch coil proof chain, repair link, two (2) ½" anchor shackles and a 7/16 inch grab hook clevis.  
· There shall be two (2) tabs welded on the table for attachment of the lift chain.
PUSH FRAME

The push frame and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP-01 
· Drawing SPP- 4-132
· The push frame shall be constructed of two (2) 4 inch @ 13.8 pounds ship channels with bracing and be in the form of an “A”. 
· The top and bottom of the push frame shall be ½ inch triangular shaped plates.
· Welded to the front of these triangular plates shall be a pair of ¾ inch x 4 inch steel brackets and between them a curved socket member shall be provided to relieve the pivot pin of thrust stress.
· The attachment pin at this point shall be a minimum of 1-¾ inch diameter axle quality steel that shall engage with corresponding ears on the front tube of the semicircular frame.  
· At the center of this box construction of plates and channels in the line of forward rotation shall be an assembly welded to form a continuous thrust beam.
· A latch part shall be incorporated which continues further to the rear and presses against a heavy-duty latch spring measuring 5-7/16 inches O.D. x ¾ inch diameter spring wire with 9 inch of free travel. 
· The spring shall be made of AISI 5160 hot rolled spring steel and shall be heat treated after cooling.  The spring shall be closed and ground.
· The latch shall seat against a circular plate welded to the rear cross channel.
· Lubrication fittings shall be provided to allow ease of movement of slide assembly, which telescopes on the tubular member.
· The two (2) rear channels of the push frame shall be provided with a heavy-duty 1 inch thick cast steel adjustable ear for attachment of the push frame to the travel hitch with 1¼ inch diameter bolt.  Ear spacing shall be 21 inches. 
· In lieu of the push frame adjustable ear attachment above; The two (2) rear channels of the push frame shall be provided with a heavy-duty 1 inch thick A36 steel adjustable for attachment of the push frame to a Pin & Loop style travel hitch with 1-¼ inch diameter bolt.  
NOTE:  Using Agencies will identify if they will require the adjustable ear or the pin & loop style attachment at the time of order.

HYDRAULIC REVERSING CYLINDERS

The hydraulic reversing cylinders and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP-01 
· Drawing SSP-02
· The hydraulic reversing mechanism shall consist of two (2) hydraulic cylinders nitride piston rods and a minimum of 2-½ inch diameter and 10 inch stroke.  
· The hydraulic cylinder housing shall attach to the push frame and the hydraulic cylinder piston shall attach to the front table tube with 1 inch pins secured by ¼ inch roll pins.
· Hydraulic cylinders shall be positioned to unlatch the semicircle and angle the moldboard to the desired plowing position.  
· The latching mechanism shall operate automatically and monitor the moldboard in any of eleven (11) positions from 35 degrees right or left in 7 degree increments.
· High pressure hydraulic hose connections shall be made to each of the two (2) cylinders with long 90 degree JIC elbow female swivel crimp hose fittings and extend to the rear terminating in male and female brass quick disconnect couplings. This will allow the hoses shall be connected during storage. All couplings shall have lanyard attached rubber cap/plug covers. 
· During operation, the hoses shall connect to the corresponding connections on the Authority trucks.
MUSHROOM

The mushroom and its accessory parts shall be manufactured in accordance with the following drawings and specifications:

· Drawing SSP – 12 
· Drawing SSP - 18
· The skid shoe assemblies shall be of the hand adjustable type, enclosed and fully lubricated with replaceable chilled cast iron shoes “Mushroom” shaped of a minimum of 11 inch in diameter and 2-½ inch thick.    
· The design shall include an anti-flip top.
· The shoe housing shall be constructed of 3 inch square tubing x 12 inches long and the shoe post shall be constructed of 2-½ inch square tubing x 11 inches long
· The adjustment shall be accomplished by a threaded 1-¼ inch diameter screw operated by a hand crank with rotating knob, which shall be self- locking and shall operate without the use of any tools. The adjusting screw shall be fully enclosed.
LEVEL-LIFT ASSEMBLY:

The level-lift assembly and its accessory parts shall be manufactured in accordance with the following specifications:

· The level-lift assembly shall provide an automatic, mechanically activated mechanical control, which will hold a raised plow moldboard an equal distance from the ground to the bottom of the snow plow blade.
· The level-lift mechanism will hold an equal elevation regardless of height raised above the road surface and regardless of moldboard plowing angle.
· The moldboard plowing angle shall be able to be changed to any desired position, maintaining equal elevation without first lowering plow, changing plowing angle and then re-lifting.
PLOW MARKERS

The plow markers accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-01
· The snow plow shall be equipped with two (2) 36 inch orange reinforced markers constructed of ¾ inch polymer reinforced with a ⅜ inch galvanized cable.  
· Each plow marker shall be equipped with a crimped base 2-bolt mount installed at the upper outer most left and right corners of the moldboard and attached to a reinforced rib with bolts and nylock nuts.
RUBBER BAFFLE 

The rubber baffle and its accessory parts shall be manufactured in accordance with the following drawings and specifications: 

· Drawing SSP - 01 
· Drawing SSP - 02 
· Drawing SSP - 03
· The snow plow shall be equipped with a ½ inch thick x 12 inch wide x 11 foot long rubber belting baffle.  
· The baffle shall be bolted to top of moldboard with a ¼ inch x 2 inch x 11 foot steel keeper bar.
WELDING:

All welding shall meet the following requirements:

· All welds shall be continuous.
· All welding performed in the manufacturing of the snow plow shall be done by AWS certified welders.
· Proof of AWS certification shall be presented at time of delivery.
[bookmark: _Toc53748385][bookmark: _Toc54703927]NJTA Specific snow plow blade: Option A (Group 2, Price Line 12)

This section describes a snow plow blade that shall be included and installed with the Units specified in Section 3.4.8, 3.4.9, 3.4.10 and/or 3.4.11.

NOTE: Using Agencies will specify at time of order snow plow and snow plow blade combination/configuration. (i.e. Price Line 8 in combination with Price Line 12).

The snow plow blade and its accessory parts shall be manufactured in accordance with the following drawing and specifications:

· Drawing SSP-08
· The snow plow blade shall be fabricated from abrasion resistant steel with a Brinell Hardness of minimum 250 and maximum 325.      
· There shall be two (2) each of 1 inch thick x 8 inch wide x 66 inch long snow plow blades. 
· The snow plow blade shall be AASHTO standard punched, per Drawing: SSP-09
· All mounting hardware shall be Grade 8.
[bookmark: _Toc53748386][bookmark: _Toc54703928]NJTA Specific snow plow blade: OPTION B (Group 2, Price Line 13)

This section describes a snow plow blade that shall be included and installed with the Units specified in Section 3.4.8, 3.4.9, 3.4.10 and 3.4.11.

NOTE: Using Agencies will specify at time of order snow plow and snow plow blade combination/configuration. (i.e. Price Line  10  in combination with Price Line 13).

It is the intent of this specification to identify snow plow blades with carbide inserts within steel holders, encased in rubber between two plates of Hardox 400 steel. 

Approved Product: Kueper Model: Tuca SX.  No other makes and models will be considered.

The snow plow blade and its accessory parts shall be manufactured in accordance with the following drawing and specification:

· Drawing SSP-09
· There shall be two (2) each of 1 inch thick x 8 inch wide x 66 inch long snow plow blades installed as a manufactured system including curb bumpers, moldboard shoes and all mounting hardware. 
· The snow plow blades shall be AASHTO standard punched.
· All mounting hardware shall be minimum Grade 8
Curb Bumper  

Casting:	GX 300 cast iron

Hardness:	600 HB (Rc 57 approximate conversion from Brinell to Rockwell)

[bookmark: _Toc53748387][bookmark: _Toc54703929]NJTA Specific snow plow blade: OPTION C (Group 2, Price Line 14)

This section describes a snow plow blade that shall be included and installed with the Units specified in Section 3.4.8, 3.4.9, 3.4.10 and 3.4.11.

NOTE: Using Agencies will specify at time of order snow plow and snow plow blade combination/configuration. (I.e. Price Line 11 in combination with Price Line 14).

It is the intent of this specification is to identify rubber snow plow blades with ceramic inserts free floating in vulcanized rubber with the configuration of Steel-Rubber-Ceramic.

 Approved Product: Kueper Model: GK5.  No other makes and models will be considered.

The snow plow blade and its accessory parts shall be manufactured in accordance with the following drawing and specification:

· Drawing B SSP-10
· There shall be two (2) each of 1 inch thick x 8 inch wide x 66 inch long snow plow blades installed as a manufactured system including the moldboard shoes and all mounting hardware. 
· The snow plow blades shall be AASHTO standard punched.
· All mounting hardware shall be minimum Grade 8.
[bookmark: _Toc53748388][bookmark: _Toc54357880][bookmark: _Toc54703930]NJTA SPecific CERAMIC COMBINATION PLOW BLADES – Blades OnLY (Group 2, Price Line 15)

It is the intent of this specification to describe rubber snow plow blades with ceramic inserts free floating in vulcanized rubber with the configuration of Steel-Rubber-Ceramic. 

 Approved Product: Kueper Model: GK5.  No other makes and models will be considered.

The snow plow blade and its accessory parts shall be manufactured in accordance with the following drawing and specification:

· Drawing B SSP-10
· There shall be two (2) each of 1 inch thick x 8 inch wide x 66 inch long snow plow blades provided as a manufactured system including moldboard shoes and all mounting hardware. 
· The snow plow blades shall be AASHTO standard punched.
· All mounting hardware shall be minimum Grade 8.
[bookmark: _Toc54703931][bookmark: _Toc53748389][bookmark: _Toc54357881]NJTA SPECIFIc FLEXIBLE CARBIDE COMBINATION PLOW BLADes -  Blades Only (Group 2, Price Line 16)

It is the intent of this specifications to describe snow plow blades with carbide inserts within steel holders, encased in rubber between two plates of Hardox 400 steel. 

Approved Product: Kueper Model: Tuca SX.  No other makes and models will be considered.

The snow plow blade and its accessory parts shall be manufactured in accordance with the following drawing and specification:

· Drawing SSP-09
· There shall be two (2) each of 1 inch thick x 8 inch wide x 66 inch long snow plow blades provided as a manufactured system including curb bumpers, moldboard shoes and all mounting hardware. 
· The snow plow blades shall be AASHTO standard punched.
· All mounting hardware shall be minimum Grade 8
Curb Bumper  

Casting:	GX 300 cast iron

Hardness:	600 HB (Rc 57 approximate conversion from Brinell to Rockwell)

[bookmark: _Toc53748390][bookmark: _Toc54703932]HOURLY RATE FOR INSTALLATION, maintenance and repair of NJTA-SPECIFIC SNow Plow (Group 2, PRICE LINE 17)  

NJTA specific Units that require installation, maintenance and repair services for the Units specified in Sections 3.4.8, 3.4.9, 3.4.10, and 3.4.11 will utilize this price line item.

The Units shall be installed on various NJTA trucks. 

All interfacing structures, including framework and mounting hardware shall be the responsibility of the Vendor {Contractor}. All nuts, bolts, washers and other fasteners shall be corrosion-resistant American National Standard grade.  Note: When welding is being done, the truck battery terminals shall be disconnected to protect the truck’s Electronic Control Modules (ECM).

The Vendor {Contractor} should ensure that the manufacturer, whose product is supplied, has a servicing dealer or service location to provide installation, maintenance and repair work including, but not limited to drilling, welding and painting of trucks frames, located within a distance from Trenton, NJ, deemed to be reasonable by the State

Delivery of the trucks to the Vendor’s {Contractor’s} site shall be the responsibility of the Using Agency. Pick up from the site after installation and inspection by the Using Agency will also be made by Using Agency personnel. Pickup and delivery of vehicles shall be during regular work days and business hours.  Exceptions to these procedures are subject to the mutual agreement of the Vendor {Contractor} and the Using Agency.

[bookmark: _Toc53748391][bookmark: _Toc54703933]ONE ADDITIONAL SET OF PARTS, SERVICE AND O&M MANUALS (Group 2, Price line 18)

Optional Manuals: One set of parts, service and operation and maintenance manuals for each and every assembly system and/or component that makes up the Units specified in Sections 3.4.8, 3.4.9, 3.4.10, and 3.4.11 shall be provided as follows: 

1 - set of parts manuals (illustrations and text) bound or with binders, and on CD-ROM. 

1 - set of complete shop repair (factory service) manuals bound or with binders and on CD-ROM. 

1 - set of complete operation & routine maintenance manuals 

1 - set of electrical schematics 

1 - set of troubleshooting manuals

The manuals shall be delivered directly to the Using Agency upon delivery of the Unit. 

[bookmark: _Toc53748392][bookmark: _Toc54703934]TECHNICAL SUPPORT (HOURLY RATE) – OPERATORS AND MECHANICS TRAINING (Group 2, PRICE LINE 19)

Operator Training:

The Vendor {Contractor}, shall provide training for the Units specified in Sections 3.4.8, 3.4.9, 3.4.10, and 3.4.11 as described below.  

The Vendor {Contractor} shall coordinate with the Using Agency to provide an operator training session for a maximum of ten (10) personnel.

Complete instructions on the operation and maintenance of each Unit and a demonstration on the operation of the Unit shall be given by the Vendor {Contractor}. 

The training shall consist of, but is not limited to, operator training with instruction on proper operation of the Unit, safety, and basic preventive maintenance. 

This demonstration shall be a formal training session and shall be arranged with the Vendor {Contractor}. 

The training session shall be conducted at a specific location or a field location, within the State of New Jersey as agreed upon between the Vendor {Contractor} and the Using Agency.

Mechanics Training:

The Vendor {Contractor}, shall provide technical training for all components of the complete Unit specified in Sections 3.4.8, 3.4.9, 3.4.10, and 3.4.11.  

The Vendor {Contractor} shall coordinate with the Using Agency to provide a mechanics training session for a maximum of five (5) personnel.

Course content shall be tailored to meet the specific needs of the Using Agency mechanics, and shall not place emphasis on areas or components not specified in the Bid Solicitation. The course shall also include hands-on instruction and content to reinforce lecture content.

The training session shall be conducted at a specific location or a field location, within the State of New Jersey as agreed upon between the Vendor {Contractor} and the Using Agency.

[bookmark: _Toc53748393][bookmark: _Toc54703935]SPECIAL MONOTONE PAINT COLOR IN LIEU OF MANUFACTURER’S STANDARD PAINT COLOR (Group 2, PRice Line 20) 

The Unit’s steel components shall have the mill scale and oil removed by means of a high pressure chemical cleaner prior to painting. 

These surfaces shall be primed with a zinc rich, rust preventive primer. The finish paint shall be a high quality, high solid, polyurethane type enamel. 

For NJTA Units:

Paint color shall be DuPont Dulux Omaha Orange Enamel # 93-082. Paint shall be supplied in a two-step process. Orange base coat and additional polyurethane overcoat.

All other Using Agencies: Using Agency will specify special monotone paint color at the time of ordering. 

[bookmark: _Toc53748394][bookmark: _Toc54703936]SPECIAL two color PAINT IN LIEU OF MANUFACTURER’S STANDARD PAINT COLOR (GROUP 2, PRICE LINE 21)

The Unit’s steel components shall have the mill scale and oil removed by means of a high pressure chemical cleaner prior to painting.  

These surfaces shall be primed with a zinc rich, rust preventive primer. The finish paint shall be a high quality, high solid, polyurethane type enamel.

For NJTA Units:

Moldboard paint color shall be DuPont Dulux Omaha Orange Enamel # 93-082. Paint shall be supplied in a two-step process.

· Orange base coat and additional polyurethane overcoat.
The Units turntable assembly paint color shall be DuPont Dulux Black Enamel #93-005. Paint shall be supplied in a two-step process.

· Black base coat and additional polyurethane overcoat.
All other Using Agencies: Using Agency will specify special two-color paint at the time of ordering. 

[bookmark: _Toc53748395][bookmark: _Toc54703937]SJTA POWER REVERSIBLE SNOW PLOW (J STYLE), 11 FooT WIDE, 36 INCH HIGH (Group 3, Price Line 22)

It is the intent of these specifications to describe a 11 foot x 36 inch adjustable power reversible snow plow, built in accordance with the listed specifications
The plow shall be new and of the latest standard model and shall be of the high speed shallow “J” shaped moldboard type. 
General

The plow shall be designed to reverse under snow load while truck is plowing. The plow shall have a rolled J shaped moldboard and be designed so the moldboard, semicircle and push frame can be quickly attached and detached from the truck hitch. The push frame shall be designed to attach to the truck hitch on 21 inch centers by removing the hinge pins. The pins shall be drilled for ¼ inch cotter pins. The plow shall be equipped with an automatic safety blade trip, controlled by an automatic spring device to release blade when in contact with an obstruction. The plow shall return to the plowing position after the obstruction is passed
MOLDBOARD:

The moldboard and its accessory parts shall be manufactured in accordance with the following specifications:

· The moldboard shall be a shallow J shaped blade, reversible type rolled from a sheet of 10 gauge thick steel to give the snow a free rolling action. 

· The moldboard shall have an overall length of 11 feet. and overall height of 36 inches.
· The moldboard shall be reinforced vertically by eight (8) 3 inch x ½ inch ribs extending from the cutting edge reinforcement to the top channel. 
· There shall be double ribs at the center attaching point to the drive frame to allow four (4) variable adjustments for tilting of the moldboard. 
· The bottom edge of the plow shall be a full length 3 inch x 3 inch 5/8 inch angle iron with a minimum thirteen gussets for reinforcement. 
· The top brace shall be an integrally formed box rail full width. 
· Horizontal ribs 3/8 inch x 2-1/2 inches with drain holes shall be provided full width.
SNOW SHIELD:

The snow shield and its accessory parts shall be manufactured in accordance with the following specifications:

· A separate bolt-on snow shield shall be installed on each moldboard its length of moldboard), mating to holes.
· A ¼ inch x 2 inch steel backing plate (full length) shall be installed which will sandwich the snow shield to the moldboard.
CURB BUMPERS:

The curb bumper and its accessory parts shall be manufactured in accordance with the following drawings and specifications:
	
· Drawing 4-158 - Wrap Around - Right Side & Curb Bumper (Attachment A - NJDOT Specific Snow Plow Drawing)

· Drawing 4-159 - Wrap Around - Left Side (Attachment A - NJDOT Specific Snow Plow Drawings)

· The moldboards shall be equipped with two (2) bolt-on curb bumpers, one each side, conforming to NJDOT Drawing No. 4-158 or 4-159. 
The curb blocks shall be manufactured from square stock 2-½ inches x 3 feet x 10 inches long.
PLOWING:

The plowing width shall be the following for the plow angles shown, either right or left.
	Plow Angle:
	28 degrees
	35 degrees
	42 degrees

	Plow Width:
	9 feet 8 inches
	9 feet 0 inches
	8 feet 2 inches



snow plow blade:

The snow plow blade and its accessory parts shall be manufactured in accordance with the follow drawings and specifications:

· Drawing 4 -168 – Snow Plow Blades (Attachment A - NJDOT Specific Snow Plow Drawings)

· The snow plow blade shall be a replaceable ½ inch thick x 6 inches wide full-length high carbon steel type blade with a standard highway bolt pattern, conforming to Drawing No. 4-168.

SEMI-CIRCLE:

The semi-circe and its accessory parts shall be manufactured in accordance with the follow drawings and specifications:

· The semicircle shall be constructed of ½ inch x 3-½ inch x 3-½ inch angle. 
· The circle shall have a 24 inch radius angle terminating behind two (2) of the five (5) connecting hinge points.
· 3/8 inch x 3 inch bars shall be added to the semicircle for reinforcement.
· Reinforcing plates, ¼ inch thick, shall be welded to the radius and main angle to accommodate the housings for the adjustable caster wheels.
· A notched plate shall be welded to the circle's formed angle to receive the lock pin of the reversing mechanism.
· Pins connecting the moldboard to the semicircle shall be of hardened steel of ¾ inch diameter with a center swiveling block. 
· The semicircle shall have five hinge points with outside centers of 116 inches and seven plowing angles.
· The semicircle shall have a series of holes to accommodate three position adjustment for the trip springs.
ADJUSTABLE SWIVEL CASTER ASSEMBLIES:

The adjustable swivel caster assemblies and its accessory parts shall be manufactured in accordance with the following specifications:

· The semicircle shall be equipped with two heavy duty, full swiveling, spring loaded, adjustable self-locking caster assemblies having steel housings with grease fittings. 

· There shall be one (1) grease fitting for the adjusting bolt and one for the caster stem. 
· The wheel assemblies shall be mounted outside of the semicircle assembly.
TUNGSTEN CARBIDE SHOE:

The tungsten carbide shoe and its accessory parts shall be manufactured in accordance with the follow drawings and specifications:

· Drawing 4-205 – 6 inch Snow Plow Shoe with Extended Leg (Attachment A - NJDOT Specific Snow Plow Drawings)

· Each caster assembly shall have a tungsten carbide shoe conforming with NJDOT Drawing No. 4-205.
TRIP SPRING:

The trip spring and its accessory parts shall be manufactured in accordance with the following specifications:

· A fully automatic enclosed trip device shall be mounted on the semicircle assembly with heavy duty trunnion plates.

· The trunnion support sockets shall be equipped with grease fittings. 
· The trip device shall be 5/8 of an inch contained in a 6 inch O.D., 10 gauge tubular housing. The device shall be connected to the moldboard. 
· Recoil springs shall be provided on the spring rod to cushion the return action of the moldboard.
PUSH FRAME:

The push frame and its accessory parts shall be manufactured in accordance with the following specifications:

· The push frame side drive members shall be constructed of 3/8 inch formed steel channels and connected by means of an equalizer bar at the end.

· The drive barriers shall be 1 inch thick and 21 inches apart - on centers, with 1-¼ inch diameter drilled drive pin holes. 
· The drive pins shall be fabricated out of heat-treated hardened steel with rivet head, pointed end and ¼ inch cotter hole. 
· The pins shall have a diameter of 1 -1/4 inch and shaft of 6 inches long. 
· The pin locking mechanism shall be provided to hold the snowplow in a set position.
POWER REVERSING MECHANISM:

The power reversing mechanism and its accessory parts shall be manufactured in accordance with the following specifications:

· The push frame shall incorporate a hydraulic power reversing mechanism.
· The reversing mechanism shall consist of two (2) single acting cylinders with 2-½ inch diameter chrome plated rods and 10 inch strokes. 
· The mechanism shall be controlled by a joystick located in the truck cab.
· High pressure hydraulic hoses with swivel couplings at cylinders and quick disconnect couplers at the truck connections shall be provided.
· No hydraulic or mechanical load shall be carried by the reversing cylinders when the plow is locked into a plowing position.
· These shall be self-locking block that automatically removes from the lock positions and then after the pressure is released from cylinders automatically locks.
LIFT CHAIN

The lift chain and its accessory parts shall be manufactured in accordance with the following
· The lift chains shall be 7/16 inch zinc plated with adjustable cast steel chain block. 
· The chain shall be spring loaded at each end and have complete shackles.
Welding

· All welds shall be continuous; skip welding is not acceptable. All welding is shall be performed by a certified welder.
· All bolts shall be hardened Grade 8.
[bookmark: _Toc53748396][bookmark: _Toc54703938]SPECIAL MONOTONE PAINT COLOR IN LIEU OF MANUFACTURER’S STANDARD PAINT COLOR (Group 3, PRice Line 23) 

For SJTA Units:

The Unit and all its components shall be cleaned and painted with one (1) coat of DuPont #1858 primer and finished with two (2) coats of the color DuPont Centari #7744-A Lime Yellow. All paint shall be same shade. 

All other Using Agencies: Using Agency will specify special monotone paint color at the time of ordering. 

[bookmark: _Toc448401118][bookmark: _Toc467160952][bookmark: _Toc475717204][bookmark: _Toc493254943][bookmark: _Toc8647924][bookmark: _Toc19520371][bookmark: _Toc53748397]
[bookmark: _Toc54703939]BLANKET P.O. IMPLEMENTATION

[bookmark: _Toc475717205][bookmark: _Toc493254944][bookmark: _Toc8647925][bookmark: _Toc19520372][bookmark: _Toc53748398][bookmark: _Toc54703940]3.5.1 PLACING ORDERS FOR BLANKET P.O. UNITS

3.5.1.1. The Vendor {Contractor} shall not substitute any item (part, component, equipment, feature, accessory, material, performance, capacity, rating, design or control), which is a part of the Blanket P.O. Unit, without written authorization to do so from the Procurement Bureau.

3.5.1.2 During the Blanket P.O. period, no change is permitted in any terms or conditions unless the Vendor {Contractor} receives written approval from the Procurement Bureau.

3.5.1.3 An offer to sell a non-Blanket P.O. Unit against two or more purchase orders, one for the Blanket P.O. Unit and one or more for non-Blanket P.O. items, constitutes a serious violation of the Blanket P.O. and may be the basis for termination of the Blanket P.O. and may disqualify the Vendor {Contractor} from award of future State Blanket P.O.s.

[bookmark: _Toc475717206][bookmark: _Toc493254945][bookmark: _Toc8647926][bookmark: _Toc19520373][bookmark: _Toc53748399][bookmark: _Toc54703941]3.5.2 PRODUCT BROCHURE

3.5.2.1 The Vendor {Contractor} shall make sales literature and color charts available to Using Agencies and NJ State inspectors on an "as requested" basis.

3.5.2.2 The State reserves the right to communicate with the Vendor {Contractor} and request any information regarding Vendor {Contractors} obligations under the Blanket P.O., and require acknowledgement of such communication from the Vendor {Contractor} during the term of the Blanket P.O. and any extension(s) thereof. Failure to acknowledge and provide the required information within twenty-four (24) hours constitutes a Blanket P.O. violation which may result in Blanket P.O. cancellation.

[bookmark: _Toc475717207][bookmark: _Toc493254946][bookmark: _Toc8647927][bookmark: _Toc19520374][bookmark: _Toc53748400][bookmark: _Toc54703942]3.5.3 CONFIRMATION OF ORDERS

3.5.3.1 Purchase order confirmation shall be submitted to each Using Agency for each order accepted, to the attention of the contact person stated in the purchase order.

3.5.3.2 The Vendor {Contractor} must provide the order confirmation promptly following factory order entry.

3.5.3.3 Order confirmation shall mean that the Vendor {Contractor} has received the purchase order, has reviewed it for compatibility with the Unit currently on Blanket P.O., has resolved any non-compatibility problems with the Using Agency, has entered the order with the manufacturer and that the manufacturer has accepted the order and assigned an order number and anticipated build and delivery dates.

3.5.3.4 A Vendor {Contractor} shall not accept any purchase order on "will try" basis, unless instructed otherwise by the Using Agency in writing. If an order is not accepted for production by the manufacturer, the Vendor {Contractor} shall return the purchase order with "canceled" marked on the purchase order with authorized signature next to it, unless instructed to accept on "will try" basis by the Using Agency in writing. No exception shall be permitted.

[bookmark: _Toc475717208][bookmark: _Toc493254947][bookmark: _Toc8647928][bookmark: _Toc19520375][bookmark: _Toc53748401][bookmark: _Toc54703943]3.5.4 POST-ORDER PRE-PRODUCTION MEETING AND INSPECTION

3.5.4.1 Pre-production/pre-installation meeting and inspection: The Vendor {Contractor} shall coordinate and attend a post-order pre-production meeting, if required by the Using Agency, at a location convenient to the Using Agency, to provide all necessary information prior to building any prototype Unit or scheduling the production. Only after the post-order pre-production meeting, if required by the Using Agency, and subsequent approval from the Using Agency shall the Vendor {Contractor} begin the production. The Vendor {Contractor} shall coordinate with the Using Agency for a pre-paint inspection for each Unit ordered, if required by the Using Agency.

Vendor {Contractor} shall prepare and submit schematic drawings of all components as required by the Using Agency prior to the post order/pre-production meeting.

3.5.4.2 The State reserves the right to inspect the Vendor {Bidder} and/or aftermarket installer(s)' and/or Vendor {Contractor}’s facility. This provision applies during the Quote  evaluation period, the Blanket P.O. term and any extension(s) thereof. 

3.5.4.3 Pre-acceptance Inspections: The State Using Agency reserves the right to inspect the Unit at the Vendor’s {Contractor's} facility or require that the Vendor {Contractor} make the Unit available for inspection at the Using Agency site. If, during inspection at the agency site, it becomes apparent that corrections/alterations shall be made to the Unit to comply with the Blanket P.O. specifications which cannot be accomplished at the State Using Agency facility, the Unit will be rejected and the Vendor {Contractor} must transport the Unit to its facility at no expense to the agency. After the Vendor {Contractor} corrects the deficiencies, the Vendor {Contractor} must re-deliver the Unit to the State Using Agency for re-inspection at the expense of the Vendor {Contractor}. 

3.5.4.4 For all inspections performed at the Vendor’s {Contractor's} site, the Vendor {Contractor} must provide a bay in the repair shop to facilitate the inspection of the Unit.

3.5.4.5 The final inspection and acceptance of the Unit shall occur at the State Using Agency.

3.5.4.6 OEM Equipment/Parts: All of the standard and optional equipment/parts provided shall be original equipment manufacturers items when available.

3.5.4.7 The Vendor {Contractor} must make arrangements for the Using Agency’s inspection of each Unit prior to the delivery and acceptance of the Unit by the Using Agency. Prior to presentation for inspection, it shall be the Vendor’s {Contractor's} responsibility to pre-inspect each Unit. Each Unit presented for inspection shall be accompanied by an inspection package including, but not limited to, the following: purchase order, line set sheet (when available) - brief list of all features, items and accessories included in the Unit, pre-delivery inspection (PDI), and dealer's pre-inspection prep checklist. The checklist will list the responsible prep mechanic and acknowledge that the Unit conforms to pre-delivery specifications and that all added equipment and accessories have been properly installed.

3.5.4.8 The Vendor {Contractor} shall notify the State Using Agency by fax and e-mail that the Unit is ready for inspection.

3.5.4.9 Delivered Units will be inspected within ten (10) working days. If a Unit has been accepted, the warranty shall commence on the date of final acceptance, or if a Unit has been rejected, the Vendor {Contractor} will be notified. The notice will indicate the reason(s) for rejection. If rejected, the Vendor {Contractor} shall try to rectify the problem(s) at the State Using Agency site. If the problem cannot be corrected at the agency site, the rejected Unit shall be removed by the Vendor {Contractor} at its own expense. The Vendor {Contractor} shall present the corrected Unit for re-inspection within ten (10) working days. No additional freight or transportation charges are permitted.

3.5.4.10 Within five (5) working days of the Vendor’s {Contractor’s} notification, the State Using Agency will, if desired, send a team of qualified inspectors to the Vendor’s {Contractor's} facility to accomplish the inspection of the Unit(s) before delivery to the Using Agency. The Vendor {Contractor} must properly itemize, organize, and segregate all Units.  

3.5.4.11 Non-State Agencies authorized to purchase under this Blanket P.O. will make arrangements for Unit inspection directly with the Vendor {Contractor}. All Units shall be delivered to each Using Agency’s designated destination at no additional cost.

3.5.4.12 Inspected Units which do not comply with the Blanket P.O. requirements will be rejected. The Vendor {Contractor} must correct all rejected Units and the corrected Unit(s) shall be presented for re-inspection within ten (10) working days. The Using Agency may cancel the purchase order if the Vendor {Contractor} fails to correct any problem.

3.5.4.13 No additional freight or transportation charges are permitted under this Blanket P.O.  
 
[bookmark: MANUFACTURERSCERTIFCATEOFORIGIN][bookmark: NEWCARINSPECTIONSTICKER][bookmark: _Toc475717209][bookmark: _Toc493254948][bookmark: _Toc8647929][bookmark: _Toc19520376][bookmark: _Toc53748402][bookmark: _Toc54703944]3.5.5 DELIVERY AND FINAL ACCEPTANCE

3.5.5.1 Vendor {Contractor} deliveries for all items shall be made within the delivery timeframe noted on the price sheet and in strict accordance with the instructions from the Using Agency.  When there is a discrepancy between the delivery days listed in the General Tab in NJSTART and the Price Sheet, the Price Sheet delivery days shall govern.  Prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination.

3.5.5.2 All deliveries of Units shall be made upon approval and as instructed by the Using Agency, by prior arrangement only, during working hours, except on legal holidays.

Deliveries shall not be made on the following State observed holidays, which may be updated from time to time:


· New Year’s Day;
· Martin Luther King Jr. Day;
· Presidents Day;
· Good Friday;
· Memorial Day;
· Juneteenth
· Independence Day;
· Labor Day;
· Columbus Day;
· Election Day;
· Veterans Day;
· Thanksgiving Day; and
· Christmas Day.

For NJDOT deliveries Only: Deliveries will be accepted from Monday through Friday, excluding weekends and all State holidays, as noted above, from 8:00 am to 2:30 pm.  No deliveries will be accepted after 2:30 pm.  Twenty-four (24) hour advanced notice must be given prior to delivery.

For SJTA deliveries Only: Deliveries will be accepted from Monday through Friday, excluding all State holidays, as noted above, from 7:30 am - 3:00 pm.  Twenty-four (24) hour advanced notice must be given prior to delivery.

For All Other Using Agencies: Deliveries must be made in accordance with the delivery timeframe noted on the purchase order. 

3.5.5.3  No Unit will be accepted at the final delivery point without all supporting documentation and paperwork completed and delivered with the Unit, which include the warranty, any specified manuals, and invoice . No Unit will be considered accepted until it has undergone final inspection at the delivery point.

3.5.5.4 No more than ten (10) Units per day and fifty (50) Units per week (based on a 5-day work week) will be accepted at each delivery site. When necessary, and with the consent of both the agency and the Vendor {Contractor}, the number of Units delivered per day may be increased.

[bookmark: _3.5.6__WARRANTIES][bookmark: _Toc493254949][bookmark: _Toc8647930][bookmark: _Toc19520377][bookmark: _Toc53748403][bookmark: _Toc54703945]3.5.6 WARRANTIES

The manufacturer's standard warranty must be supplied with each Unit at the time of delivery and shall be in typed form. The warranty commences with the acceptance of the Unit at the delivery site, following the final inspection. 

The Vendor {Contractor} must guarantee that the Unit and all its component parts comply with the current, applicable safety standards, Federal Motor Vehicle Safety Standards (FMVSS) and New Jersey State Motor Vehicle Code Regulations, perform their functions adequately, and operate successfully without undue wear or failure.  The Vendor {Contractor} shall immediately replace and install free of charge any part that may fail by reason of defective material or workmanship.

[bookmark: _Toc475717211][bookmark: _Toc493254950][bookmark: _Toc8647931][bookmark: _Toc19520378][bookmark: _Toc53748404][bookmark: _Toc54703946]3.5.7 WARRANTY REQUIREMENTS

3.5.7.1 The Vendor {Contractor} shall ensure that the manufacturer whose product is supplied has a servicing dealer or service location to provide warranty and recall service and/or repair within twenty four (24) hours of notification by the Using Agency. 

3.5.7.2 The Vendor {Contractor} must perform any warranty service/repair/recall, which will be at Vendor’s {Contractor's} own expense. Events beyond Vendor’s {Contractor's} control, such as lack of parts due to strikes and unforeseen acts of God, shall constitute valid reasons for delay in making necessary repairs. However, the State will make such determination.

[bookmark: _Toc493254951][bookmark: _Toc8647932][bookmark: _Toc19520379][bookmark: _Toc53748405][bookmark: _Toc54703947]3.5.8 PAYMENT

3.5.8.1 Invoices will be processed for payment only after final acceptance of the Units by the Using Agency and the delivery ticket has been signed off by an authorized representative of the Using Agency. Partial payments may be made for Unit(s) accepted, if billed separately. Timely payment discounts will be taken if offered by the Vendor {Contractor}. The State reserves the right to make payments directly or through a third party.



[bookmark: _Toc475717213][bookmark: _Toc493254952][bookmark: _Toc8647933][bookmark: _Toc19520380][bookmark: _Toc53748406][bookmark: _Toc54703948]3.5.9 SUBSTITUTION OF DISCONTINUED PRODUCTS

The Vendor {Contractor} may offer a substitution for any product discontinued by the manufacturer in its Blanket P.O. The State may consider substituting the discontinued model with a new model provided that the unit offered meets or exceeds the Blanket P.O. specifications.  All substitutions must be approved by the State. 

The Vendor {Contractor} must notify the State immediately in writing to the Division’s assigned Procurement Specialist stating that an item has been discontinued by the manufacturer along with supporting documentation from that manufacturer that the item has been discontinued.  The Vendor {Contractor} must provide in its letter the discontinued model number, model number of the new product being offered, detailed literature for the new product being offered, the price of the discontinued item and the price of the product being offered as a replacement.  The State will not approve the substitution of a discontinued item without all of the above information.

The replacement product should be offered to the State at that same price as the discontinued product. 

[bookmark: _Toc54703949]REPLACEMENT OF UNSATISFACTORY PRODUCT

In the event the product delivered does not meet the specifications or is damaged prior to or at the time of delivery,  as determined by the Using Agency, the Vendor {Contractor} shall immediately remove and replace the unsatisfactory product, at no cost to the Using Agency. The timeframe for the replacement shall not exceed the delivery days ARO listed on the State-Supplied Price Sheet.  Failure to comply may result in the product being removed from the Blanket P.O. and similar product obtained from another Vendor {Contractor} with any additional costs assumed by the original Vendor {Contractor}.

[bookmark: _Toc51847202][bookmark: _Toc54703950]authorized dealers/distributors

The Vendor {Contractor} must provide a list of the Dealer(s)/Distributor(s) on company letterhead that will service the Blanket P.O.  The Vendor {Contractor} is required to submit the following forms for each Dealer/Distributor:

1. New Jersey Business Registration  (N.J.S.A. 52:32-44);
2. Ownership Disclosure  (N.J.S.A. 52:25-24.2);
3. Disclosure of Investment Activities in Iran (N.J.S.A. 52:32-55 et. seq.);
4. Executed MacBride Principles  (N.J.S.A. 52:34-12.2);
5. Completed Contractor Certification and Disclosure of Political Contributions (N.J.S.A. 19:44A-20:13 et. seq.);
6. Disclosure of Investigations and Actions Involving Bidder Form;
7. Vendor Certification (P.L. 2005, c.271);
8. Proof of insurance as specified herein;
9. Proof of compliance with New Jersey Affirmative Action requirements (N.J.A.C. 17:27-1.1 et. seq.):
a. New Jersey Form AA-302 Affirmative Action Employee Information Report; or 
b. New Jersey Affirmative Action Certificate; or 
c. Federal Affirmative Action Approval Letter.

A Vendor {Contractor} may submit a request to add or remove Dealers/Distributors at any time during the Blanket P.O. term, including any extension(s) thereof.  Any such request should be e-mailed to the Procurement Specialist assigned to this procurement.
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[bookmark: _Toc400531492][bookmark: _Toc428533963][bookmark: _Toc54703951]QUOTE PREPARATION AND SUBMISSION – REQUIREMENTS OF THE VENDOR {BIDDER}

Failure to submit information as indicated below may result in your Quote being deemed non-responsive.

[bookmark: _Toc400531493][bookmark: _Toc428533964][bookmark: _Toc54703952]General

A Vendor {Bidder} may submit additional terms as part of its Quote and Quotes including Vendor {Bidder} proposed terms and conditions may be accepted, but Vendor {Bidder} proposed terms or conditions that conflict with those contained in the Bid Solicitation, as defined in Section 2.0 of this Bid Solicitation, or that diminish the State’s rights under any Blanket P.O. resulting from the Bid Solicitation, may render a Quote non-responsive.  It is incumbent upon the Vendor {Bidder} to identify and remove its conflicting proposed terms and conditions prior to Quote submission. Where additional terms are submitted they may be accepted, rejected, or negotiated, in whole or in part, at the State’s sole discretion where the terms do not conflict with material terms of the Bid Solicitation or do not diminish the State’s rights under the Blanket P.O. resulting from the Bid Solicitation.

In the event that a Vendor {Bidder} intends to propose terms and conditions that conflict with the Bid Solicitation, those Vendor {Bidder} proposed terms and conditions shall only be considered if submitted and agreed to pursuant to the electronic question and answer procedure set forth in Section 1.3.1 of this Bid Solicitation.  Vendors {Bidders} shall not submit exceptions in the Quote or on the “Terms and Conditions” Tab through NJSTART. 

After award of the Blanket P.O., if a conflict arises between a Vendor’s {Bidder’s} additional terms included in the Quote and a term or condition of the Bid Solicitation, the term or condition of the Bid Solicitation will prevail.

Use of URLs in a Quote should be kept to a minimum and shall not be used to satisfy any material term of a Bid Solicitation. If a preprinted or other document included as part of the Quote contains a URL, a printed copy of the URL page shall be provided and will be considered as part of the Quote.

[bookmark: _Toc400531494]The forms discussed herein and required for submission of a Quote in response to this Bid Solicitation are available on the Division’s website unless noted otherwise.

[bookmark: _Toc428533965][bookmark: _Toc54703953]QUOTE Delivery and Identification

A Quote must arrive at the Division in accordance with this Bid Solicitation’s instructions within the time frames noted on the Bid Solicitation cover sheet and on the “Summary” page of the Bid Solicitation in NJSTART, or as indicated on the posted Bid Amendment if the Quote Opening Date has been changed.  Vendors {Bidders} submitting electronic Quotes via NJSTART are cautioned to allow adequate time to ensure timely uploads of all Quote documents to mitigate unforeseen delays or issues.  State regulation mandates that late Quotes are ineligible for consideration.  

[bookmark: _Toc428533966][bookmark: _Toc54703954]NJSTART electronic submission

[bookmark: _Toc428533967][bookmark: _Toc54703955]NJSTART SUBMISSION OF QUOTE

Vendors {Bidders} may refer to the “Vendor Registration” and “Submit a Quote” QRGs for additional instructions detailing how to enroll in NJSTART and submit a NJSTART electronic Quote.  QRGs are located on the NJSTART Vendor Support Page.  

When submitting a NJSTART Quote, do not use any symbols (i.e., #, @, $, &, *) in the filename.  
Uploaded files should be compatible with Microsoft Office and/or Adobe software applications.  
DO NOT UPLOAD files with extensions such as .zip, .numbers, or .pages.

The Vendor {Bidder} should select the “Confidential” option in NJSTART for attachments on the “Attachments” Tab to request that the documents not be displayed publicly through NJSTART. 

Note: Marking an attachment as "Confidential" in NJSTART shall not constitute the Vendor's {Bidder's} designation of the attachment as exempt from public disclosure under OPRA and/or the common law as outlined in Section 1.4.4.

[bookmark: _Toc400531497][bookmark: _Toc428533968][bookmark: _Toc54703956]RESERVED

[bookmark: _Toc400531498][bookmark: _Toc428533969][bookmark: _Toc54703957]QUOTE Content

The Quote should contain the State-Supplied Price Sheet and all forms/documents required by the Bid Solicitation.  The Vendor {Bidder} is cautioned to carefully read the Bid Solicitation to ensure that all required forms are completed, signed and submitted with the Vendor’s {Bidder’s} Quote.  NOTE:  Failure to submit required forms/documents may result in the Vendor’s {Bidder’s} Quote being deemed non-responsive.

A Vendor {Bidder} must complete the State-Supplied Price Sheet accompanying this Bid Solicitation and upload it as an attachment on the “Attachments” Tab (See Section 4.4.5 of this Bid Solicitation). 

The Vendor {Bidder} must enter a Unit Cost of $1.00 for each price line item on the “Items” Tab in NJSTART. The Vendor {Bidder} is instructed to do so only as a mechanism to comply with Bid Solicitation Section 6.8 and prevent all pricing from being publicly displayed in NJSTART. 

In the event that a Vendor {Bidder} using NJSTART to submit a Quote uploads a State-Supplied Price Sheet and completes the Items Tab in NJSTART (instead of entering a Unit Cost of $1.00 as instructed), the State-Supplied Price Sheet will govern. 

[bookmark: _Toc108508238][bookmark: _Toc54703958][bookmark: _Toc428533970]Forms, rEGISTRATIONS and CERTIFICATIONS required with QUOTE 

Vendors {Bidders} should refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

In the event that a Vendor {Bidder} fails to attach a required form, or the attached form is deemed deficient, the Division may access the Primary Form to be considered as part of the Quote.

Vendors {Bidders} are under a continuing obligation to report updates to the information contained in its required forms.

Unless otherwise specified, forms must contain an original, physical signature, or an electronic signature pursuant to Section 1.4.11 of this Bid Solicitation.

[bookmark: _4.4.1.1_Ownership_Disclosure][bookmark: _4.4.1.1_Signatory_page]OFFER AND ACCEPTANCE PAGE

[bookmark: OLE_LINK5][bookmark: OLE_LINK6]The Vendor {Bidder} shall complete and submit the Offer and Acceptance Page accompanying this Bid Solicitation prior to the initiation of negotiation.  The Vendor {Bidder} should submit the Offer and Acceptance Page with the Quote.  All information requested on the Offer and Acceptance Page must be submitted.   

If the Offer and Acceptance Page is not submitted with the Quote or is incomplete, the State will require the Vendor {Bidder} to submit the Offer and Acceptance Page.  If the Vendor {Bidder} fails to comply with the requirement within seven (7) business days of the demand, the State may deem the Quote non-responsive.

The Offer and Acceptance Page must be signed by an authorized representative of the Vendor {Bidder}.  If the Vendor {Bidder} is a limited partnership, the Offer and Acceptance Page must be signed by a general partner.  If the Vendor {Bidder} is a joint venture, the Offer and Acceptance Page must be signed by a principal of each party to the joint venture.  

MACBRIDE PRINCIPLES CERTIFICATION

The Vendor {Bidder} must certify pursuant to N.J.S.A. 52:34-12.2 that it is in compliance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of its compliance with those principles.  See Section 2.5 of the SSTC and N.J.S.A. 52:34-12.2 for additional information about the MacBride principles. 
 
By signing the Bid Solicitation Offer and Acceptance Page, the Vendor {Bidder} is automatically certifying that either:

A. The Vendor {Bidder} has no operations in Northern Ireland; or

B. The Vendor {Bidder} has business operations in Northern Ireland and is committed to compliance with the MacBride principles.

A Vendor {Bidder} electing not to certify to the MacBride Principles must nonetheless sign the Bid Solicitation Offer and Acceptance Page  AND must include, as part of its Quote, a statement indicating its refusal to comply with the provisions of this Act.

NON-COLLUSION

By submitting a Quote and signing the Bid Solicitation Offer and Acceptance Page, the Vendor {Bidder} certifies as follows:

A. The price(s) and amount of its Quote have been arrived at independently and without consultation, communication or agreement with any other Vendor {Contractor, Bidder} or any other party;

B. Neither the price(s) nor the amount of its Quote, and neither the approximate price(s) nor approximate amount of this Quote, have been disclosed to any other firm or person who is a Vendor {Bidder} or potential Vendor {Bidder}, and they will not be disclosed before the Quote submission;

C. No attempt has been made or will be made to induce any firm or person to refrain from bidding on this Blanket P.O., or to submit a Quote higher than this Quote, or to submit any intentionally high or noncompetitive Quote or other form of complementary Quote;

D. The Quote of the firm is made in good faith and not pursuant to any agreement or discussion with, or inducement from, any firm or person to submit a complementary or other noncompetitive Quote; and

E. The Vendor {Bidder}, its affiliates, subsidiaries, officers, directors, and employees are not, to Vendor’s {Bidder’s} knowledge, currently under investigation by any governmental agency for alleged conspiracy or collusion with respect to bidding on any Blanket P.O./public contract and have not in the last five (5) years been convicted or found liable for any act prohibited by state or federal law in any jurisdiction involving conspiracy or collusion with respect to bidding on any Blanket P.O./public contract.

NEW JERSEY BUSINESS ETHICS GUIDE CERTIFICATION

The Treasurer has established a business ethics guide to be followed by Vendors {Bidders/Contractors} in its dealings with the State.  The guide provides further information about compliance with Section 2.8 of the SSTC.  The guide can be found at: https://www.state.nj.us/treasury/purchase/ethics.shtml

By signing the Bid Solicitation Offer and Acceptance Page, the Vendor {Bidder} is automatically certifying that it has complied with all applicable laws and regulations governing the provision of State goods and services, including the Conflicts of Interest Law, N.J.S.A. 52:13D-12 to 28.  

nj standard BID SOLICITATION forms REQUIRED WITH THE QUOTE 
 
Vendor’s {Bidder’s} failure to complete, sign and submit the forms in Section 4.4.1.2 shall be cause to reject its Quote as non-responsive. 

Ownership Disclosure Form

Pursuant to N.J.S.A. 52:25-24.2, in the event the Vendor {Bidder} is a corporation, partnership or limited liability company, the Vendor {Bidder} must complete an Ownership Disclosure Form.  

A current completed Ownership Disclosure Form must be received prior to or accompany the submitted Quote.  A Vendor’s {Bidder’s} failure to submit the completed and signed form with its Quote will result in the rejection of the Quote as non-responsive and preclude the award of a Blanket P.O. to said Vendor {Bidder} unless the Division has on file a signed and accurate Ownership Disclosure Form dated and received no more than six (6) months prior to the Quote submission deadline for this procurement.  If any ownership change has occurred within the last six (6) months, a new Ownership Disclosure Form must be completed, signed and submitted with the Quote.

In the alternative, to comply with this section, a Vendor {Bidder} with any direct or indirect parent entity which is publicly traded may submit the name and address of each publicly traded entity and the name and address of each person that holds a 10 percent or greater beneficial interest in the publicly traded entity as of the last annual filing with the federal Securities and Exchange Commission or the foreign equivalent, and, if there is any person that holds a 10 percent or greater beneficial interest, also shall submit links to the websites containing the last annual filings with the federal Securities and Exchange Commission or the foreign equivalent and the relevant page numbers of the filings that contain the information on each person that holds a 10 percent or greater beneficial interest. N.J.S.A. 52:25-24.2.

Vendors {Bidders} using NJSTART to submit a Quote shall make the appropriate certification on the “Maintain Terms and Categories” Tab within its profile by checking the applicable box and, if required, completing and attaching the shortened Ownership Disclosure Form. Vendors {Bidders} not using NJSTART to submit a Quote must complete the full Ownership Disclosure Form located on the Division’s website.

Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

Vendors {Bidders} utilizing NJSTART should designate one version of the Ownership Disclosure Form as the Primary Form.  In the event that a Vendor {Bidder} fails to attach an Ownership Disclosure Form, or the attached Ownership Disclosure Form is deemed deficient, the Division may access the Primary Form and consider it as part of the Quote.  Note: The Primary Form must have a Date Created within six (6) months of the Quote submission deadline to be considered valid.
 
DISCLOSURE OF INVESTMENT ACTIVITIES IN IRAN form
 
Pursuant to N.J.S.A. 52:32-58, the Vendor {Bidder} must utilize this Disclosure of Investment Activities in Iran form to certify that neither the Vendor {Bidder}, nor one (1) of its parents, subsidiaries, and/or affiliates (as defined in N.J.S.A. 52:32-56(e)(3)), is listed on the Department of the Treasury’s List of Persons or Entities Engaging in Prohibited Investment Activities in Iran and that neither the Vendor {Bidder}, nor one (1) of its parents, subsidiaries, and/or affiliates, is involved in any of the investment activities set forth in N.J.S.A. 52:32-56(f).  If the Vendor {Bidder} is unable to so certify, the Vendor {Bidder} shall provide a detailed and precise description of such activities as directed on the form. A Vendor’s {Bidder’s} failure to submit the completed and signed form with its Quote will result in the rejection of the Quote as non-responsive and preclude the award of a Blanket P.O. to said Vendor {Bidder}.  

Vendors {Bidders} using NJSTART to submit a Quote shall make the appropriate certification on the “Maintain Terms and Categories” Tab within its profile by checking the applicable box and, if required, completing and attaching the shortened Disclosure of Investment Activities in Iran form. Vendors {Bidders} not using NJSTART to submit a Quote must complete the full Disclosure of Investment Activities in Iran form located on the Division’s website. 

Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

Vendors {Bidders} utilizing NJSTART should designate the most current version of the Disclosure of Investment Activities in Iran form as the Primary Form.  In the event that a Vendor {Bidder} fails to attach a Disclosure of Investment Activities in Iran form, or the attached Disclosure of Investment Activities in Iran form is deemed deficient, the Division may access the Primary Form, as designed in the Vendor {Bidder} profile, to be considered as part of the Quote.

subcontractor utilization plan

Please note that the State of New Jersey will not be utilizing the “Subcontractor” Tab in NJSTART. 

Vendors {Bidders} intending to use a Subcontractor shall submit a Subcontractor Utilization Plan form. The Subcontractor Utilization Plan form is located on the Division’s website. Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation through NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

NOTE: If the Blanket P.O. is a small business subcontracting set-aside, the Vendor {Bidder} certifies that in engaging Subcontractors, it shall make a good faith effort to achieve the subcontracting set-aside goals, and shall attach to the Subcontractor Utilization Plan documentation of such efforts in accordance with N.J.A.C. 17:13-4.1 et seq.

For a Quote that does NOT include the use of any Subcontractors, by signing the Bid Solicitation Offer and Acceptance Page, the Vendor {Bidder} is automatically certifying that in the event the award is granted to the Vendor’s {Bidder’s} firm and the Vendor {Bidder} later determines at any time during the term of the Blanket P.O. to engage Subcontractors to provide certain goods and/or services, pursuant to Section 5.8 of the SSTC, the Vendor {Bidder} shall submit a Subcontractor Utilization Plan form for approval to the Division in advance of any such engagement of Subcontractors. 

SMALL BUSINESS SET-ASIDE BLANKET P.O. 

Not applicable to this procurement.

DISABLED VETERANS’ BUSINESS SET-ASIDE BLANKET P.O. 

Not applicable to this procurement.

SMALL BUSINESS AND/OR DISABLED VETERANS’ BUSINESS SUBCONTRACTING SET-ASIDE BLANKET P.O. 

Not applicable to this procurement.

BID SECURITY

Not applicable to this procurement.

[bookmark: _Toc400531500][bookmark: _Toc428533971][bookmark: _Toc54703959]Forms, REGISTRATIONS AND CERTIFICATIONS REQUIRED before BLANKET P.O. award and THAT SHOULD BE SUBMITTED with the QUOTE

Unless otherwise specified, forms must contain an original, physical signature, or an electronic signature pursuant to Section 1.4.11 of this Bid Solicitation.

BUSINESS REGISTRATION

In accordance with N.J.S.A. 52:32-44(b), a Vendor {Bidder} and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Blanket P.O.  To facilitate the Quote evaluation and Blanket P.O. award process, the Vendor {Bidder} should submit a copy of its valid BRC and those of any named Subcontractors with its Quote.  See Section 2.1 of the SSTC.

Any Vendor {Bidder}, inclusive of any named Subcontractors, not having a valid business registration at the time of the Quote opening, or whose BRC was revoked prior to the submission of the Quote, should proceed immediately to register its business or seek reinstatement of a revoked BRC.  Vendors {Bidders} should verify its BRC status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} BRC, NJSTART provides a link to take corrective action. 

The Vendor {Bidder} is cautioned that it may require a significant amount of time to secure the reinstatement of a revoked BRC. The process can require actions by both the Division of Revenue and Enterprise Services and the Division of Taxation.  For this reason, a Vendor’s {Bidder’s} early attention to this requirement is highly recommended.  The Vendor {Bidder} and its named Subcontractors may register with the Division of Revenue and Enterprise Services, obtain a copy of an existing BRC or obtain information necessary to seek re-instatement of a revoked BRC online at http://www.state.nj.us/treasury/revenue/busregcert.shtml.

A Vendor {Bidder} otherwise identified by the Division as a responsive and responsible Vendor {Bidder}, inclusive of any named Subcontractors, but that was not business registered at the time of submission of its Quote must be so registered and in possession of a valid BRC by a deadline to be specified in writing by the Division.  A Vendor {Bidder} failing to comply with this requirement by the deadline specified by the Division will be deemed ineligible for Blanket P.O. award.  Under any circumstance, the Division will rely upon information available from computerized systems maintained by the State as a basis to verify independently compliance with the requirement for business registration.

A Vendor {Bidder} receiving a Blanket P.O. award as a result of this procurement and any Subcontractors named by that Vendor {Bidder} will be required to maintain a valid business registration with the Division of Revenue and Enterprise Services for the duration of the executed Blanket P.O., inclusive of any Blanket P.O. extensions.   

Disclosure of Investigations AND OTHER Actions Involving Bidder form
 
The Vendor {Bidder} should  submit the Disclosure of Investigations and Other Actions Involving Bidder Form,  with its Quote, to provide a detailed description of any investigation, litigation, including administrative complaints or other administrative proceedings, involving any public sector clients during the past five (5) years, including the nature and status of the investigation, and, for any litigation, the caption of the action, a brief description of the action, the date of inception, current status, and, if applicable, disposition.  If a Vendor {Bidder} does not submit the form with the Quote, the Vendor {Bidder} must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.

Vendors {Bidders} using NJSTART to submit a Quote shall make the appropriate certification on the “Maintain Terms and Categories” Tab within its profile by checking the applicable box and, if required, complete and attach the shortened NJSTART form. Vendors {Bidders} not using NJSTART to submit a Quote must complete the full version of the form located on the Division’s website. 

Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

Source Disclosure 

Not applicable to this procurement.

CONFIDENTIALITY/COMMITMENT TO DEFEND

Vendor {Bidder} should submit a completed and signed Confidentiality /Commitment to Defend form with the Quote.  In the event that Vendor {Bidder} does not submit the Confidentiality form with the Quote, the State reserves the right to request that the Vendor {Bidder} submit the form after Quote submission.

See Bid Solicitation Section 1.4.4 Contents of Quote for additional information.

AFFIDAVIT OF APPAREL FORM

Not applicable to this procurement.

[bookmark: _Toc449428257][bookmark: _Toc54703960]SUBmittals

Vendors {Bidders} may refer to the QRG “Submit a Quote” for instructions detailing how to submit a NJSTART electronic Quote. QRGs are located on the NJSTART Vendor Support Page.  

· Specification Conformance: 

· The Vendor {Bidder} shall submit with its Quote a Vendor’s {Bidder’s} certification in the form of the attachment titled “Specification Conformance Certification”, confirming that all items offered in response to this Bid Solicitation conform to the requirements set forth in Section 3.0 of this Bid Solicitation. Please see the attachment entitled “Specification Conformance Certification. 

Vendor {BIDDER} Experience

The Vendor {Bidder} should complete ALL the information requested on the Bidder Data Sheet attached to this Bid Solicitation so that the State is able to make a sound business judgment regarding the Vendor’s {Bidder’s} qualifications and capability to perform the Blanket P.O.  

The Contact Name, Contact Phone Number and Contact Email portions of the Bidder Data Sheet are for verification of the contract information provided on the Bidder Data Sheet only.  The persons identified will not be contacted for reference purposes.

COOPERATIVE PURCHASING PROGRAM

The Vendor {Bidder} should complete the Cooperative Purchasing Form indicating willingness or unwillingness to extend State Blanket P.O. pricing and terms to Cooperative Purchasing Program participants. The Cooperative Purchasing Form is located on the Division’s website.

specification Data Sheets

Not applicable to this procurement.

1.1.1.1 MANUFACTURER’S CERTIFICATION

The Vendor {Bidder} should submit a letter of certification from the manufacturer whose product is supplied, certifying that the Vendor {Bidder} is authorized by the manufacturer to supply the Unit specified. The State reserves the right to request such certification and to require that such certification be provided within five (5) business days from the time it is requested.  

1.1.1.2 MANUFACTURER’S PUBLISHED LIST OF OPTIONS AND ATTACHMENTS/PRICE LIST

Not applicable to this procurement.

DISCLOSURE OF PRODUCT COMPOSITION

Not applicable to this procurement.

SAMPLES/Sample Testing

Not applicable to this procurement.

[bookmark: _Toc54703961]Financial Capability of the Vendor {Bidder}

The Vendor {Bidder} should provide sufficient financial information to enable the State to assess the financial strength and creditworthiness of the Vendor {Bidder} and its ability to undertake and successfully complete the Blanket P.O.  In order to provide the State with the ability to evaluate the Vendor’s {Bidder’s} financial capacity and capability to undertake and successfully complete the Blanket P.O., the Vendor {Bidder} should submit the following:
 
A. For publicly traded companies the Vendor {Bidder} should provide copies or the electronic location of the annual reports filed for the two most recent years.
B. For privately held companies the Vendor {Bidder} should provide the certified financial statement (audited or reviewed) in accordance with applicable standards by an independent Certified Public Accountant which include a balance sheet, income statement, and statement of cash flow, and all applicable notes for the most recent calendar year or the Vendor’s {Bidder’s} most recent fiscal year. 
	
If the information is not supplied with the Quote, the State may still require the Vendor {Bidder} to submit it.  If the Vendor {Bidder} fails to comply with the request within seven (7) business days, the State may deem the Quote non-responsive.

A Vendor {Bidder} may designate specific financial information as not subject to disclosure when the Vendor {Bidder} has a good faith legal/factual basis for such assertion.  A Vendor {Bidder} may submit specific financial documents in a separate, sealed package clearly marked “Confidential-Financial Information” along with the Quote.

The State reserves the right to make the determination to accept the assertion and shall so advise the Vendor {Bidder}.
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The Vendor {Bidder} must submit its pricing using the State-Supplied Price Sheet accompanying this Bid Solicitation and located on the “Attachments” Tab. 

Vendors {Bidders} may refer to the QRG “Submit a Quote” for instructions detailing how to submit a NJSTART electronic Quote. QRGs are located on the NJSTART Vendor Support Page.  

In order for the State to make sound business judgments regarding products and prices offered in response to this Bid Solicitation, the Vendor {Bidder} must supply, with its Quote, the information requested on the Bid Solicitation’s pricing lines in sufficient detail as to allow the State to determine the firm, fixed Quote pricing and the precise product or service being offered, i.e., with no possible misinterpretation of the price or product/service being offered by the Vendor {Bidder}.  A Vendor’s {Bidder's} failure to provide, within its Quote, the information deemed by the State to be essential for product identification or price determination shall result in rejection of that Vendor’s {Bidder's} Quote.  Notwithstanding the aforementioned material obligation, in order to support the State's decision-making process, the State may require a Vendor {Bidder} to provide additional information or documentation that has been deemed not to be material to product identification or price determination, in which case, the Vendor {Bidder} shall, within the time limit set forth in the written request, comply with said request.  Each Vendor {Bidder} is required to hold its prices firm through issuance of Blanket P.O.

NJSTART pricing submission instructions

If the Vendor {Bidder} is submitting a NJSTART Quote, the Vendor {Bidder} must enter a Unit Cost of $1.00 for each price line item on the “Items” Tab in NJSTART. The Vendor {Bidder} is instructed to do so only as a mechanism to comply with Bid Solicitation Section 6.8 and prevent all pricing from being publicly displayed in NJSTART. 

STATE-SUPPLIED price sheet instructions

There are twenty-three (23) price lines, which are grouped and itemized as follows:

	Group Number
	Price Line Number
	Description

	Group 1
(Price lines 1 – 7)
	1
	NJDOT Specific Heavy-Duty Manual Reversible (Straight) Snow Plow, 11 Foot Wide, 36 Inches High (M.R. 11-36-MOD-J)

	
	2
	NJDOT Specific Heavy-Duty One-Way (Funnel), 12 Foot Wide (MODEL O.R.12.75 -53-1HD)

	
	3
	NJDOT Specific Heavy-Duty Power Reversible Snow Plow, 11 Foot Wide, 36 Inches High (Worm Gear Type)

	
	4
	N NJDOT Specific High Power Reversible Torsion Trip Edge Plow, 11 Foot Wide, 36 Inches High

	
	5
	One Additional Set Of Parts Service And O&M Manuals 

	
	6
	Technical Support (Hourly Rate) – Operators And Mechanics Training

	
	7
	Special Monotone Paint Color in Lieu of Manufacturer’s Standard Paint Color

	

	Group 2
(Price Lines 8 – 21)
	8
	NJTA Specific Manual Reversible One-Way Snow Plow, 11 Foot Long, 47 Inches High

	
	9
	NJTA Specific Manual Reversible Snow Plow, 11 Foot Long, 42 Inches High (J-STYLE)

	
	10
	NJTA Specific Power Reversible Expressway Snow Plow 11 Foot Long, 50 Inches High

	
	11
	NJTA Specific Power Reversible Snow Plow, 11 Foot Long, 42 Inches High,

	
	12
	NJTA Specific Snow Plow Blade: Option A

	
	13
	NJTA Specific Snow Plow Blade: Option B

	
	14
	NJTA Specific Snow Plow Blade: Option C

	
	15
	NJTA Specific Ceramic Combination Plow Blades - Blades Only

	
	16
	NJTA Specific Flexible Carbide Combination Plow Blades - Blades Only

	
	17
	Hourly Rate For Installation, Maintenance And Repair of   Snow Plow

	
	18
	One Additional Set Of Parts Service And O&M Manuals

	
	19
	Technical Support (Hourly Rate) – Operators And Mechanics Training

	
	20
	Special Monotone Paint Color in Lieu of Manufacturer’s Standard Paint Color 

	
	21
	Special Two Color Paint in Lieu of Manufacturer’s Standard Paint Color 

	

	Group 3
(Price Lines 22 and 23
	22
	SJTA Specific  Reversible Snow Plow (J STYLE), 11 Foot Wide, 36 Inches High

	
	23
	Special Monotone Paint Color in Lieu of Manufacturer’s Standard Paint Color

	



The State intends to make one award per group (Groups 1, Group 2, and Group 3), in accordance with Section 7.2 of this Bid Solicitation.  Vendors {Bidders} may bid on one, two Groups, or all Groups.

Price line items are grouped for Quote evaluation purposes only.  Upon Blanket P.O. award, Using Agencies will be able to order any price lines within the group individually.

For Group 1 Vendors {Bidders} must bid on all price lines (Price Lines 1 - 7) within the Group in order for its Quote to be considered for an award for the Group.  If a Vendor {Bidder} does not bid on all price lines within the Group its Quote will be considered non-responsive for the Group.

For Group 2 Vendors {Bidders} must bid on all price lines (Price Line 8 - 21) within the Group in order for its Quote to be considered for an award for the Group. If a Vendor {Bidder} does not bid on all price lines within the Group its Quote will be considered non-responsive for the Group.

For Group 3 Vendors {Bidders} must bid on all price lines (Price Lines 22 - 23) within the Group in order for its Quote to be considered for an award for the Group.  If a Vendor {Bidder} does not bid on all price lines within the Group its Quote will be considered non-responsive for the Group.

· Step1 - The Vendor {Bidder} should enter the Vendor’s {Bidder’s} name in the field titled “Vendor {Bidder} Name:” located at the top of the State-Supplied Price Sheet.
 
· Step 2 – For price lines 1 - 23 the Vendor {Bidder} shall insert a firm, fixed price in US dollars in the column titled “Unit Price” on the State-Supplied Price Sheet.  If a Vendor {Bidder} leaves the “Unit Price” column blank, it shall be considered that the Vendor {Bidder} provided
no Quote for that price line item.  

Any additional costs, including freight, must be included in the pricing offered on the State-Supplied Price Sheet.  

	For Price Lines 6, 17 and 19:

Vendors {Bidders} shall bid firm, fixed hourly rate in the “Unit Price” field, by entering the hourly rate bid in the “Unit Price” field on these specific price lines on the State-Supplied Price Sheet.  A Vendor’s {Bidder’s} entry in the “Unit Price” field for Price Lines 6, 17 and 19 shall be considered a firm price per hour.  For example, entry of “50” shall be considered “$50 per hour”.  Multiple or series or range of hourly rates or a fixed task price on any of these price lines shall not be accepted and will render the Quote non-responsive for that price line and the Group that price line item is part of.

Failure to bid on all price lines within a given Group will result in rejection of the Vendors {Bidders} Quote for the Group.  If a Vendor {Bidder} leaves the “Unit Price” field blank on any price line, it shall be considered that the Vendor {Bidder} provided no Quote for that price line item.  Multiple or series or range of prices will not be accepted.

The NJSTART system is able to accept Unit Prices containing up to two (2) decimal places to the right of the decimal point. Any price beyond 2 decimal points will be rounded to the second decimal place.  Unit Prices may be offered on the State-supplied Price Sheet up to two (2) decimal places to the right of the decimal point.  Price Sheet formatting will automatically round Unit Prices containing more than two (2) decimal places to the right of the decimal point so as not to exceed this limit.  The State will only consider pricing offered up to two (2) decimal places to the right of the decimal point and will not round any figures beyond two (2) decimal places to the right of the decimal point.  

· Step 3 - For price lines 1, 2, 3, 4, 8, 9, 10, 11 and 22, the Vendor {Bidder} shall enter the brand of the item being offered in the field titled “Brand” (e.g. Meyer) on the State-Supplied Price Sheet.

· Step 4 – For price lines 1, 2, 3, 4, 8, 9, 10, 11, 12, 13, 14, 15, 16,  and 22, the Vendor {Bidder} should enter the days required to make delivery upon receipt of an order into the field titled “Delivery Days ARO” on the State-Supplied Price Sheet.  If the “Delivery Days ARO” column is left blank, then the delivery days shall default to the delivery days set forth in Section 4.4.5.4.

· Step 5 – The Vendor {Bidder} should enter a cash discount, pursuant to Section 4.4.5.6, in the space provided on the State-Supplied Price Sheet.  If the Vendor {Bidder} leaves the “Cash Discount” field blank, it shall mean that the Vendor {Bidder} is not offering a cash discount. 

Use of “no bid” versus “no charge” on the State-Supplied Price Sheet

All price lines must be filled out in accordance with Section 4.4.5.2.  If the Vendor {Bidder} is not submitting a price for an item on a price line, the Vendor {Bidder} must indicate “No Bid” on the State-Supplied Price Sheet accompanying this Bid Solicitation. If the Vendor {Bidder} will supply an item on a price line free of charge, the Vendor {Bidder} must indicate “No Charge” on the State-Supplied Price Sheet accompanying this Bid Solicitation.  The use of any other identifier may result in the Vendor’s {Bidder’s} Quote being deemed non-responsive. 

DELIVERY TIME AND COSTS

Unless otherwise noted elsewhere in the Bid Solicitation, or price sheet all delivery times are  90 calendar days after receipt of order (ARO) and prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination (90 calendar days ARO/F.O.B.).  Quotes submitted other than 90 calendar days ARO/F.O.B. may be deemed non-responsive.  The Vendor {Contractor} shall assume all costs, liability and responsibility for the delivery of merchandise in good condition to the State's Using Agency or designated purchaser.  90 calendar days ARO/F.O.B. does not cover "spotting" but does include delivery on the receiving platform of the Using Agency at any destination in the State of New Jersey unless otherwise specified.

No additional charges will be allowed for any additional transportation costs resulting from partial shipments made at the Vendor’s {Contractor’s} convenience when a single shipment is ordered.

The weights and measures of the State's Using Agency receiving the shipment shall govern.

COLLECT ON DELIVERY (C.O.D.) TERMS

C.O.D. terms are not acceptable as part of a Quote and shall be deemed non-responsive.

CASH DISCOUNTS

The Vendor {Bidder} is encouraged to offer cash discounts based on expedited payment by the State.  The State will make efforts to take advantage of discounts, but discounts will not be considered in determining the price rankings of Quotes.

Should the Vendor {Bidder} choose to offer cash discounts the following shall apply:

A. Discount periods shall be calculated starting from the next business day after the Using Agency has accepted the goods or services, received a properly signed and executed invoice and, when required, a properly executed performance security, whichever is latest; and

B. The date on the check issued by the State in payment of that invoice shall be deemed the date of the State's response to that invoice.
[bookmark: _Toc449428261]
[bookmark: _4.4.1.9_eXECUTIVE_ORDER_129][bookmark: _4.4.1.10_eXECUTIVE_ORDER_129][bookmark: _4.4.1.8_Signatory_page][bookmark: _4.4.1.10_Bid_Bond][bookmark: _4.4.1.11_Bid_Bond][bookmark: _4.4.2.3__REFERENCE_DATA_SHEETS_-_SA][bookmark: _Attachment_"A][bookmark: _4.4.3.8_Subcontractor(s)]PRICE List and/or catalog pricing

Not applicable to this procurement. 



[bookmark: _Toc400531505][bookmark: _Toc428533976][bookmark: _Toc54703963]SPECIAL CONTRACTUAL TERMS AND CONDITIONS APPLICABLE TO THE BLANKET P.O.

[bookmark: _Toc400531506][bookmark: _Toc428533977][bookmark: _Toc54703964]PRECEDENCE OF SPECIAL CONTRACTUAL TERMS AND CONDITIONS

This Blanket P.O. awarded, and the entire agreement between the parties, as a result of this Bid Solicitation shall consist of this Bid Solicitation, including the SSTC, Bid Amendment to this Bid Solicitation, the Vendor’s {Contractor’s} Quote, any Best and Final Offer, and the Division's Notice of Award.

In the event of a conflict in the terms and conditions among the documents comprising this Blanket P.O., the order of precedence, for purposes of interpretation thereof, listed from highest ranking to lowest ranking, shall be:

A. Executed Offer and Acceptance Page;

B. Bid Solicitation Section 5, as may be amended by Bid Amendment;

C. The State of NJ Standard Terms and Conditions (SSTC) accompanying this Bid Solicitation;

D. All remaining sections of the Bid Solicitation, as may be amended by Bid Amendment; 

E. The Vendor’s {Contractor’s} final submitted Best and Final Offer; and

F. The Vendor’s {Contractor’s} Quote as accepted by the State.

Note: In the event of conflicting information between the Bid Solicitation and fields contained in NJSTART, the Bid Solicitation will govern and NJSTART will be updated via Bid Amendment or Change Order.
[bookmark: _Toc400531507][bookmark: _Toc428533978][bookmark: _Toc54703965]BLANKET P.O. Term and Extension Option

The base term of this Blanket P.O. shall be for a period of three (3) years.  The anticipated "Blanket P.O. Effective Date" is provided on the “Summary” page of the Bid Solicitation in NJSTART.  If delays in the procurement process result in a change to the anticipated Blanket P.O. Effective Date, the Vendor {Bidder} agrees to accept a Blanket P.O. for the full term of this Blanket P.O. 

This Blanket P.O. may be extended up to three (3) years with no single extension exceeding one (1) year, by the mutual written consent of the Vendor {Contractor} and the Director at the same terms, conditions, and pricing at the rates in effect in the last year of this Blanket P.O. or rates more favorable to the State or as per SSTC Section 6.1.

Purchase orders may be placed against the Blanket P.O. up to and including the end of business on the last day of the Blanket P.O., for delivery no more than forty-five (45) days after Blanket P.O. expiration.

[bookmark: _Toc474224535][bookmark: _Toc474939994][bookmark: _Toc54703966]PRODUCT ADDITION

Not applicable to this procurement.

[bookmark: _Toc400531508][bookmark: _Toc428533979][bookmark: _Toc54703967]BLANKET P.O. Transition

In the event that a new Blanket P.O. has not been awarded prior to this Blanket P.O. expiration date, including any extensions exercised, and the State exercises this Blanket P.O. transition, the Vendor {Contractor} shall continue this Blanket P.O. under the same terms, conditions and pricing until a new Blanket P.O. can be completely operational.  At no time shall this transition period extend more than 180 days beyond the expiration date of this Blanket P.O., including any extensions exercised.

[bookmark: _Toc54703968][bookmark: _Toc108508270][bookmark: _Toc428533980]CHANGE ORDER 

Any changes or modifications to the terms of this Blanket P.O. shall be valid only when they have been reduced to writing and signed by the Vendor {Contractor} and the Director.

[bookmark: _Toc400531510][bookmark: _Toc428533981][bookmark: _Toc54703969]Vendor {contractor} Responsibilities

The Vendor {Contractor} shall have sole responsibility for the complete effort specified in this Blanket P.O.  Payment will be made only to the Vendor {Contractor} or authorized dealers/distributors, if applicable.  The Vendor {Contractor} shall have sole responsibility for all payments due any Subcontractor.

The Vendor {Contractor} is responsible for the professional quality, technical accuracy and timely completion and submission of all deliverables, services or commodities required to be provided under this Blanket P.O.  The Vendor {Contractor} shall, without additional compensation, correct or revise any errors, omissions, or other deficiencies in its deliverables and other services.  The approval of deliverables furnished under this Blanket P.O. shall not in any way relieve the Vendor {Contractor} of responsibility for the technical adequacy of its work.  The review, approval, acceptance or payment for any of the services shall not be construed as a waiver of any rights that the State may have arising out of the Vendor’s {Contractor’s} performance of this Blanket P.O.

[bookmark: _Toc449428269][bookmark: _Toc54703970]Claims and Remedies

[bookmark: _Toc449428270][bookmark: _Toc54703971]Claims

All claims asserted against the State by the Vendor {Contractor} shall be subject to the New Jersey Tort Claims Act, N.J.S.A. 59:1-1, et seq., and/or the New Jersey Contractual Liability Act, N.J.S.A. 59:13-1, et seq.

[bookmark: _Toc449428271][bookmark: _Toc54703972]Remedies

Nothing in this Blanket P.O. shall be construed to be a waiver by the State of any warranty, expressed or implied, of any remedy at law or equity, except as specifically and expressly stated in a writing executed by the Director.

[bookmark: _Toc449428272][bookmark: _Toc54703973]Remedies for failure to comply with material Blanket P.O. requirements

In the event that the Vendor {Contractor} fails to comply with any material Blanket P.O. requirements, the Director may take steps to terminate this Blanket P.O. in accordance with the SSTC,  authorize the delivery of Blanket P.O. items by any available means, with the difference between the price paid and the defaulting Vendor’s {Contractor’s} price either being deducted from any monies due the defaulting Vendor {Contractor} or being an obligation owed the State by the defaulting Vendor {Contractor} as provided for in the State administrative code, or take any other action or seek any other remedies available at law or in equity.

[bookmark: _Toc449428273][bookmark: _Toc54703974]Items Ordered and Delivered

The Blanket P.O. involves items which are necessary for the continuation of ongoing critical State services.  Any delay in delivery of these items would disrupt State services and would force the State to immediately seek alternative sources of supply on an emergency basis.  Timely delivery is critical to meeting the State's ongoing needs.  Refer to Section 6.3(a) of the State of NJ Standard Terms and Conditions for additional information.

[bookmark: _Toc449428274][bookmark: _Toc54703975]MANUFACTURING/PACKAGING REQUIREMENTS

	All products must conform in every respect to the standards and regulations established by Federal and New Jersey State laws.

 	All products shall be manufactured and packaged under modern sanitary conditions in accordance with federal and state law and standard industry practice.

	All products are to be packaged in sizes as specified in this Bid Solicitation and shall be packaged in such a manner as to ensure delivery in first class condition and properly marked for identification.  All shipments must be comprised of original cartons associated with the commercial industry represented by the actual product contained within each carton.  Deliveries containing re-used, re-labeled, re-worked or alternate cartons are subject to rejection by the Using Agency at the Vendor’s {Contractor's} expense.

[bookmark: _Toc54703976]ELECTRONIC PAYMENTS	

With the award of this Blanket P.O., the successful Vendor(s) {Contractor(s)} will be required to receive its payment(s) electronically.  In order to receive your payments via automatic deposit from the State of New Jersey, you must complete the EFT information within your NJSTART Vendor Profile.  Please refer to Section 5.2 of the QRG entitled “Vendor Profile Management – Company Information and User Access” for instructions. QRGs are located on the NJSTART Vendor Support Page.  

[bookmark: _Toc400531512][bookmark: _Toc428533983][bookmark: _Toc54703977]Substitution or Addition of SubCONTRACTOR(s)

[bookmark: _Toc400531518][bookmark: _Toc428533989]This Section of the Bid Solicitation serves to supplement but not to supersede Sections 5.8 and 5.9 of the SSTC accompanying this Bid Solicitation.

The Vendor {Contractor} shall forward a written request to substitute or add a Subcontractor or to substitute its own staff for a Subcontractor to the Blanket P.O.’s assigned Procurement Specialist for consideration.  If the Procurement Specialist approves the request, the Procurement Specialist will forward the request to the Director for final approval.  No substituted or additional Subcontractors are authorized to begin work until the Vendor {Contractor} has received written approval from the Director.

If it becomes necessary for the Vendor {Contractor} to substitute a Subcontractor, add a Subcontractor, or substitute its own staff for a Subcontractor, the Vendor {Contractor} will identify the proposed new Subcontractor or staff member(s) and the work to be performed.  The Vendor {Contractor} must provide detailed justification documenting the necessity for the substitution or addition.

The Vendor {Contractor} must provide detailed information of its proposed replacement staff or of the proposed Subcontractor’s management, supervisory, and other key personnel that demonstrate knowledge, ability and experience relevant to that part of the work which the Subcontractor is to undertake.

The qualifications and experience of the replacement(s) must equal or exceed those of similar personnel proposed by the Vendor {Contractor} in its Quote.

[bookmark: _Toc400531538][bookmark: _Toc428534010][bookmark: _Toc54703978]BLANKET P.O. Activity Report

The Vendor {Contractor} must provide, on a biannual basis, a record of all purchases made under this Blanket P.O. resulting from this Bid Solicitation.  This reporting requirement includes sales to State Using Agencies, political sub-divisions thereof and, if permitted under the terms of this Blanket P.O., sales to counties, municipalities, school districts, volunteer fire departments, first aid squads and rescue squads, independent institutions of higher education, State and county colleges and quasi-State entities.  Quasi-State entities include any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member.

This information must be provided in Microsoft excel such that an analysis can be made to determine the following:

A. Vendor’s {Contractor’s} total sales volume, with line item detail, to each purchaser under this Blanket P.O.;

B. Subtotals by product, including, if applicable, catalog number and description, price list with appropriate page reference, and/or Blanket P.O. discount applied; and

C. Total dollars paid to Subcontractors.

Submission of purchase orders, confirmations, and/or invoices do not fulfill this Blanket P.O. requirement for information.  Failure to report this mandated information may be a factor in future award decisions.

The Vendor {Contractor} must submit the required information in Microsoft Excel format to NJSupplierReports@treas.nj.gov.

Reports are due:
		January 1st through June 30th – due by July 30th; and
		July1st through December 31st – due by January 30th.
	

[bookmark: _Toc400531540][bookmark: _Toc428534012][bookmark: _Toc54703979]PROGRAM EFFICIENCY ASSESSMENT FOR STATE USING AGENCIES

The Program Efficiency Assessment shall not be charged against the winning Vendor(s) {Contractor(s)} and therefore is not to be included in the Vendor’s {Bidder’s} pricing. The State Using Agencies shall be charged an assessment equal to one-quarter of one percent (0.25%) of the value of all transactions under this Blanket P.O.  This assessment is authorized by N.J.S.A. 52:27B-56 and N.J.A.C. 17:12-1.5, to maintain the State’s procurement system at a level to meet industry standards of efficiency.

For purposes of this section, “transaction” is defined as the payment or remuneration to the Vendor {Contractor} for services rendered or products provided to the State pursuant to the terms of this Blanket P.O., including but not limited to the following: purchase orders, invoices, hourly rates, firm fixed price, commission payments, progress payments and contingency payments.

[bookmark: _Toc54703980]  News Releases

The Vendor {Contractor} is not permitted to issue news releases pertaining to any aspect of the services being provided under this Blanket P.O. without the prior written consent of the Director.

[bookmark: _Toc400531519][bookmark: _Toc428533990][bookmark: _Toc54703981]  Advertising

The Vendor {Contractor} shall not use the State’s name, logos, images, or any data or results arising from this Blanket P.O. as a part of any commercial advertising without first obtaining the prior written consent of the Director.

[bookmark: _Toc332803059][bookmark: _Toc324415444][bookmark: _5.17_Retainage][bookmark: _5.21_Additional_Work][bookmark: _5.22_Additional_Work][bookmark: _5.9_Substitution_of][bookmark: _5.19_requirements_of_Executive_orde][bookmark: _5.20_requirements_of_Executive_orde][bookmark: _Toc400531541][bookmark: _Toc428534013][bookmark: _Toc54703982] QUOTE EVALUATION
[bookmark: _Toc118513836]
[bookmark: _Toc400531542][bookmark: _Toc428534014][bookmark: _Toc54703983]RIGHT TO WAIVE

[bookmark: _Toc400531543][bookmark: _Toc428534015]Pursuant to N.J.A.C. 17:12-2.7(d) the director may waive minor irregularities or omissions in a Quote.  The Director also reserves the right to waive a requirement provided that the requirement does not materially affect the procurement or the state's interests associated with the procurement.

[bookmark: _Toc54703984]director’s right of final quote acceptance

The Director reserves the right to reject any or all Quotes, or to award in whole or in part if deemed to be in the best interest of the State to do so. The Director shall have authority to award orders or Blanket P.O.s in accordance with N.J.S.A. 52:34-12. 

[bookmark: _Toc400531544][bookmark: _Toc428534016][bookmark: _Toc54703985]STATE'S RIGHT TO INSPECT VENDOR {BIDDER} FACILITIES

The State reserves the right to inspect the Vendor’s {Bidder’s} establishment before making an award, for the purposes of ascertaining whether the Vendor {Bidder} has the necessary facilities for performing the Blanket P.O.

The State may also consult with clients of the Vendor {Bidder} during the evaluation of Quotes. Such consultation is intended to assist the State in making a Blanket P.O. award that is most advantageous to the State.

[bookmark: _Toc400531545][bookmark: _Toc428534017][bookmark: _Toc54703986]Clarification of Quote / STATE'S RIGHT TO REQUEST FURTHER INFORMATION

After the submission of Quotes, unless requested by the State as noted below, Vendor {Bidder} contact with the State is not permitted. 

After the Quotes are reviewed, one (1), some or all of the Vendors {Bidders} may be asked to clarify certain aspects of its Quote.  A request for clarification may be made in order to resolve minor ambiguities, irregularities, informalities or clerical errors.  Clarifications cannot correct any deficiencies or material omissions, or revise or modify a Quote.

Further, the Director reserves the right to request a Vendor {Bidder} to explain, in detail, how the Quote price was determined.

[bookmark: _Toc54703987][bookmark: _Toc118513837][bookmark: _Toc400531547][bookmark: _Toc428534019]QUOTE EVALUATION COMMITTEE

Quotes may be evaluated by an Evaluation Committee composed of members of affected departments and agencies together with representative(s) from the Division.  Representatives from other governmental agencies may also serve on the Evaluation Committee.  On occasion, the Evaluation Committee may choose to make use of the expertise of outside consultant(s) in an advisory role.

[bookmark: _Toc54703988]Oral Presentation 

The Vendor {Bidder} may be required to give an oral presentation to the State concerning its Quote. 

A Vendor {Bidder} may not attend the oral presentations of its competitors.

It is within the State’s discretion whether to require the Vendor {Bidder} to give an oral presentation or require the Vendor {Bidder} to submit written responses to questions regarding its Quote.  Action by the State in this regard should not be construed to imply acceptance or rejection of a Quote. The Division will be the sole point of contact regarding any request for an oral presentation or clarification.

[bookmark: _Toc118513838][bookmark: _Toc400531548][bookmark: _Toc428534020][bookmark: _Toc54703989]Evaluation Criteria

The following criteria will be used to evaluate Quotes received in response to this Bid Solicitation.  The criteria are not necessarily listed in order of importance:

A. The Vendor’s {Bidder’s} demonstration in the Quote that the Vendor {Bidder} understands and is able to complete the requirements of the Scope of Work as sought; and

Group Price - Group 1 (sum of Price Lines 1 through 7), Group 2 (sum of Price Lines 8 through 21), and Group 3 (sum of Price Lines 22 and 23).

The State intends to make one (1) Statewide Blanket P.O. award per group (Group 1, Group 2, and Group 3).

[bookmark: _Toc118513841][bookmark: _Toc400531551][bookmark: _Toc428534023][bookmark: _Toc54703990]QUOTE discrepancies

In evaluating Quotes, discrepancies between words and figures will be resolved in favor of words.  Discrepancies between Unit Prices and totals of Unit Prices will be resolved in favor of Unit Prices.  Discrepancies in the multiplication of units of work and Unit Prices will be resolved in favor of the Unit Prices.  Discrepancies between the indicated total of multiplied Unit Prices and units of work and the actual total will be resolved in favor of the actual total.  Discrepancies between the indicated sum of any column of figures and the correct sum thereof will be resolved in favor of the correct sum of the column of figures.

In the event that a Vendor {Bidder} using NJSTART to submit a Quote uploads a State-Supplied Price Sheet and completes the “Items” Tab in NJSTART (instead of entering a Unit Cost of $1.00 as instructed), the State-Supplied Price Sheet will govern.

[bookmark: _Toc54703991][bookmark: _Toc400531552][bookmark: _Toc428534024][bookmark: _Toc503175937][bookmark: _Toc503176092][bookmark: _Toc503176755][bookmark: _Toc503176917]tIE-BREAKING CRITERIA

For the purposes of tie-breaking, any tie-break scenario shall be made utilizing the delivery schedule bid, followed by the criteria set forth in N.J.A.C. 17:12-2.10.  The delivery timeframe will be utilized in any tie-break scenario, and, in the case of a range of delivery days for the product bid, the highest day in the range will be used for the purposes of the tie-break.  For example, if a Vendor {Bidder} offers 10 - 20 days ARO for the product bid, the 20 days will be used for the basis of the tie-break.

[bookmark: _Toc54703992]Evaluation of the QUOTES

After the Evaluation Committee completes its evaluation, it recommends to the Director for award the responsible Vendor(s) {Bidder(s)} whose Quote, conforming to this Bid Solicitation, is most advantageous to the State, price and other factors considered. The Evaluation Committee considers and assesses price, technical criteria, and other factors during the evaluation process and makes a recommendation to the Director.  The Director may accept, reject or modify the recommendation of the Evaluation Committee. Whether or not there has been a negotiation process as outlined in Section 6.8 below, the Director reserves the right to negotiate price reductions with the selected Vendor(s) {Bidder(s)}.

[bookmark: _Toc118513842][bookmark: _Toc400531553][bookmark: _Toc428534025][bookmark: _Toc54703993]Negotiation and Best and Final Offer (BAFO) 
  
In accordance with N.J.S.A. 52:34-12(f) and N.J.A.C. 17:12-2-7, after evaluating Quotes, the Bureau may establish a competitive range and enter into negotiations with one (1) Vendor {Bidder} or multiple Vendors {Bidders} within this competitive range.  The primary purpose of negotiations is to maximize the State’s ability to obtain the best value based on the mandatory requirements, evaluation criteria, and cost.  Multiple rounds of negotiations may be conducted with one (1) Vendor {Bidder} or multiple Vendors {Bidders}.  Negotiations will be structured by the Bureau to safeguard information and ensure that all Vendors {Bidders} are treated fairly.

Similarly, the Bureau may invite one (1) Vendor {Bidder} or multiple Vendors {Bidders} to submit a Best and Final Offer (BAFO). Said invitation will establish the time and place for submission of the BAFO. Any BAFO that does not result in more advantageous pricing to the State will not be considered, and the State will evaluate the Vendor’s {Bidder’s} most advantageous previously submitted pricing.

If required, after review of the BAFO(s), clarification may be sought from the Vendor(s) {Bidder(s)}.  The Division may conduct more than one (1) round of negotiation and/or BAFO in order to attain the best value for the State. 

After evaluation of Quotes and as applicable, negotiation(s), and/or BAFO(s), the Bureau will recommend, to the Director, the responsible Vendor(s) {Bidder(s)} whose Quote(s), conforming to the Bid Solicitation, is/are most advantageous to the State, price, and other factors considered. The Director may accept, reject or modify the recommendation of the Bureau. The Director may initiate additional negotiation or BAFO procedures with the selected Vendor(s) {Bidder(s)}.

Negotiations will be conducted only in those circumstances where it is deemed by the Bureau or Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Vendor {Bidder} is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Blanket P.O. award based on the content of the initial submission, without further negotiation and/or BAFO with any Vendor {Bidder}.  

All contacts, records of initial evaluations, any correspondence with a Vendor {Bidder} related to any request for clarification, negotiation or BAFO, any revised technical and/or price Quotes, and related documents will remain confidential until a Notice of Intent to Award a Blanket P.O. is issued.

If the Bureau contemplates negotiation, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Vendor {Bidder} will be publicly announced at the Quote opening.

[bookmark: _Toc54703994]“REQUEST FOR REVISION” WITHIN NJSTART

The State may request a revision of the Vendor’s {Bidder’s} Quote within NJSTART. The Vendor {Bidder} shall respond to the “Request for Revision” (e.g., to reduce pricing if a BAFO is requested) only for the reason(s) identified by the State. Any changes made by a Vendor {Bidder} to the Quote other than as requested by the State shall be considered null and void. 

[bookmark: _Toc400531554][bookmark: _Toc428534026][bookmark: _Toc54703995]POOR PERFORMANCE

A Vendor {Bidder} with a history of performance problems may be bypassed for consideration of an award issued as a result of this Bid Solicitation.  The following materials may be reviewed to determine Vendor {Bidder} performance:  Blanket P.O. cancellations for cause pursuant to Section 5.7(B) of the SSTC; information contained in Vendor performance records; information obtained from audits or investigations conducted by a local, state or federal agency of the Vendor’s {Bidder’s} work experience; current licensure, registration, and/or certification status and relevant history thereof; or its status or rating with established business/financial reporting services, as applicable.  Vendors {Bidders} should note that this list is not exhaustive.
[bookmark: _Toc220920713][bookmark: _Toc400531555][bookmark: _Toc428534027][bookmark: _Toc54703996]
 BLANKET P.O. AWARD

[bookmark: _Toc220920714][bookmark: _Toc400531556][bookmark: _Toc428534028][bookmark: _Toc54703997]DOCUMENTS REQUIRED BEFORE BLANKET P.O. AWARD

[bookmark: _Toc220920715][bookmark: _Toc400531557][bookmark: _Toc428534029][bookmark: _Toc54703998]Requirements of Public Law 2005, CHAPTER 51, N.J.S.A. 19:44A-20.13 - N.J.S.A. 19:44A-20.25 (Formerly Executive Order NO. 134), EXECUTIVE ORDER No. 117 (2008) and N.J.A.C. 17:12-5 et seq.

A. The State shall not enter into a Blanket P.O. to procure services or any material, supplies or equipment, or to acquire, sell, or lease any land or building from any Business Entity, where the value of the transaction exceeds $17,500, if that Business Entity has solicited or made any contribution of money, or pledge of contribution, including in-kind contributions, to a candidate committee and/or election fund of any candidate for or holder of the public office of Governor or Lieutenant Governor, to any State, county, municipal political party committee, or to any legislative leadership committee during certain specified time periods; 

B. Prior to awarding any Blanket P.O. or agreement to any Business Entity, the Business Entity proposed as the intended Vendor {Contractor} of the Blanket P.O. shall submit the Two-Year Chapter 51/Executive Order 117 Vendor Certification and Disclosure of Political Contributions form, certifying that no contributions prohibited by either Chapter 51 or Executive Order No. 117 have been made by the Business Entity and reporting all qualifying contributions made by the Business Entity or any person or entity whose contributions are attributable to the Business Entity. The required form and instructions, available for review on the Division’s website at http://www.state.nj.us/treasury/purchase/forms/eo134/Chapter51.pdf, shall be provided to the intended Vendor {Contractor} for completion and submission to the Division with the Notice of Intent to Award. Upon receipt of a Notice of Intent to Award a Blanket P.O. {Contract}, the intended Vendor {Contractor} shall submit to the Division, in care of the Division Procurement Specialist, the Certification and Disclosure(s) within five (5) business days of the State’s request.  The Certification and Disclosure(s) may be executed electronically by typing the name of the authorized signatory in the “Signature” block as an alternative to downloading, physically signing the form, scanning the form, and uploading the form.  Failure to submit the required forms will preclude award of a Blanket P.O. under this Bid Solicitation, as well as future Blanket P.O. opportunities; and 

C. Further, the Vendor {Contractor} is required, on a continuing basis, to report any contributions it makes during the term of the Blanket P.O., and any extension(s) thereof, at the time any such contribution is made. The required form and instructions, available for review on the Division’s website at http://www.state.nj.us/treasury/purchase/forms/eo134/Chapter51.pdf, shall be provided to the intended Vendor {Contractor} with the Notice of Intent to Award. 

The Two-Year Chapter 51/Executive Order 117 Vendor Certification and Disclosure of Political Contributions form is located on the Division’s website.
Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation through NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

Vendors {Bidders} should verify its Chapter 51 Compliance status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Chapter 51 Compliance status, NJSTART provides a link to take corrective action.

[bookmark: _Toc400531558][bookmark: _Toc428534030][bookmark: _Toc54703999]SOURCE DISCLOSURE REQUIREMENTS

Not applicable to this procurement.

BREACH OF BLANKET P.O. 

Not applicable to this procurement.

[bookmark: _Toc400531559][bookmark: _Toc428534031][bookmark: _Toc54704000]AFFIRMATIVE Action 

The intended Vendor {Contractor} must submit a copy of a New Jersey Certificate of Employee Information Report, or a copy of Federal Letter of Approval verifying it is operating under a federally approved or sanctioned Affirmative Action program.  Intended Vendors {Contractors} not in possession of either a New Jersey Certificate of Employee Information Report or a Federal Letter of Approval  must complete the Affirmative Action Employee Information Report (AA-302) located on the web at http://www.nj.gov/treasury/purchase/forms/AA_%20Supplement.pdf.

Vendors {Bidders} should verify its Affirmative Action Compliance status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Affirmative Action Compliance status, NJSTART provides a link to take corrective action.

[bookmark: _Toc261501847][bookmark: _Toc400531560][bookmark: _Toc428534032][bookmark: _Toc54704001]BUSINESS REGISTRATION

In accordance with N.J.S.A. 52:32-44(b), a Vendor {Bidder} and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Blanket P.O.  See Section 4.4.2.1 of this Bid Solicitation for further information.

Vendors {Bidders} should verify its Business Registration Certification Active status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Business Registration Certification Active status, NJSTART provides a link to take corrective action. Vendors {Bidders} may refer to the QRG “Vendor Categories and Certifications” for instructions on completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

[bookmark: _Toc400531561][bookmark: _Toc428534033][bookmark: _Toc54704002]FINAL BLANKET P.O. AWARD

Blanket P.O. awards will be made with reasonable promptness by written notice to those responsible Vendors {Bidders}, whose Quotes, conforming to this Bid Solicitation, is are most advantageous to the State, price, and other factors considered.  Any or all Quotes may be rejected when the State Treasurer or the Director determines that it is in the public interest to do so.

The State intends to make one (1) Statewide Blanket P.O. award per group (Group 1, Group 2, and Group 3) in accordance with Bid Solicitation Section 6.7. 

[bookmark: _Toc400531562][bookmark: _Toc428534034][bookmark: _Toc54704003]INSURANCE CERTIFICATES

The Vendor {Contractor} shall provide the State with current certificates of insurance for all coverages required by the terms of this Blanket P.O., naming the State as an Additional Insured.   See Section 4.2 of the SSTC accompanying this Bid Solicitation.

Vendors {Bidders} should verify its Insurance Certification Compliance status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Insurance Certification Compliance status, contact the Division Procurement Specialist.

[bookmark: _Toc118513795][bookmark: _Toc400531563][bookmark: _Toc428534035][bookmark: _Toc54704004][bookmark: OLE_LINK3][bookmark: OLE_LINK4]Performance SECURITY

Not applicable to this procurement.
[bookmark: _Toc400531564][bookmark: _Toc428534036][bookmark: _Toc54704005]
 BLANKET P.O. ADMINISTRATION

[bookmark: _Toc400531565][bookmark: _Toc428534037][bookmark: _Toc54704006]STATE CONTRACT MANAGER

The State Contract Manager (SCM) is the State employee responsible for the overall management and administration of the Blanket P.O.  

The SCM for this project will be identified at the time of execution of Blanket P.O.  At that time, the Vendor {Contractor} will be provided with the State Contract Manager’s name, department, division, agency, address, telephone number, fax phone number, and email address.

[bookmark: _Toc400531566][bookmark: _Toc428534038][bookmark: _Toc54704007]state contract manager responsibilities

For an agency Blanket P.O. where only one (1) State office uses the Blanket P.O., the SCM will be responsible for engaging the Vendor {Contractor}, assuring that Purchase Orders are issued to the Vendor {Contractor}, directing the Vendor {Contractor} to perform the work of the Blanket P.O., approving the deliverables and approving payment vouchers.  The SCM is the person who the Vendor {Contractor} will contact after the Blanket P.O. is executed for answers to any questions and concerns about any aspect of the Blanket P.O.  The SCM is responsible for coordinating the use of the Blanket P.O. and resolving minor disputes between the Vendor {Contractor} and any component part of the SCM's Department.  The SCM is also responsible for notifying Office of Information Technology (OIT) and other appropriate parties of security and privacy violations or incidents.  The SCM cannot modify the Blanket P.O., direct or approve a Change Order.  

If the Blanket P.O. has multiple users, the SCM shall be the central coordinator of the use of the Blanket P.O. for all Using Agencies, while other State employees engage and pay the Vendor {Contractor}.  All persons and agencies using the Blanket P.O. must notify and coordinate the use of the Blanket P.O. with the SCM.  

[bookmark: _Toc400531567][bookmark: _Toc428534039][bookmark: _Toc54704008]Coordination with the State Contract manager

Any Blanket P.O. user that is unable to resolve disputes with a Vendor {Contractor} shall refer those disputes to the SCM for resolution.  Any questions related to performance of the work of the Blanket P.O. by Blanket P.O. users shall be directed to the SCM.  The Vendor {Contractor} may contact the SCM if the Vendor {Contractor} cannot resolve a dispute with Blanket P.O. users.



[bookmark: _Toc485041273][bookmark: _Toc54704009]9.0 STATE OF NEW JERSEY STANDARD TERMS AND CONDITIONS
(Rev: 10/21/19)

[bookmark: _Toc485039858][bookmark: _Toc485041274][bookmark: _Toc6227260][bookmark: _Toc6229388][bookmark: _Toc53996870][bookmark: _Toc54693101][bookmark: _Toc54704010]1. STANDARD TERMS AND CONDITIONS APPLICABLE TO THE CONTRACT
Unless the bidder/offeror is specifically instructed otherwise in the Request for Proposals (RFP), the following terms and conditions shall apply to all contracts or purchase agreements made with the State of New Jersey. These terms are in addition to the terms and conditions set forth in the RFP and should be read in conjunction with same unless the RFP specifically indicates otherwise. In the event that the bidder/offeror would like to present terms and conditions that are in conflict with either these terms and conditions or those set forth in the RFP, the bidder/offeror must present those conflicts during the Question and Answer period for the State to consider. Any conflicting terms and conditions that the State is willing to accept will be reflected in an addendum to the RFP. The State's terms and conditions shall prevail over any conflicts set forth in a bidder/offeror's Proposal that were not submitted through the question and answer process and approved by the State. Nothing in these terms and conditions shall prohibit the Director of the Division of Purchase and Property (Director) from amending a contract when the Director determines it is in the best interests of the State. 

[bookmark: _Toc485039859][bookmark: _Toc485041275][bookmark: _Toc6227261][bookmark: _Toc6229389][bookmark: _Toc53996871][bookmark: _Toc54693102][bookmark: _Toc54704011]1.1 contract terms CROSSWALK

	NJSTART Term
	Equivalent Statutory, Regulatory and/or Legacy Term

	Bid/Bid Solicitation 
	Request For Proposal (RFP)/Solicitation

	Bid Amendment 
	Addendum

	Change Order 
	Contract Amendment

	Master Blanket Purchase Order (Blanket P.O.) 
	Contract

	Offer and Acceptance Page
	Signatory Page

	Quote
	Proposal

	Vendor 
	Bidder/Contractor



[bookmark: _Toc469579742][bookmark: _Toc469932226][bookmark: _Toc476315911][bookmark: _Toc476644259][bookmark: _Toc485039860][bookmark: _Toc485041276][bookmark: _Toc6227262][bookmark: _Toc6229390][bookmark: _Toc53996872][bookmark: _Toc54693103][bookmark: _Toc54704012]2.	STATE LAW REQUIRING MANDATORY COMPLIANCE BY ALL CONTRACTORS
The statutes, laws or codes cited herein are available for review at the New Jersey State Library, 185 West State Street, Trenton, New Jersey 08625. 

[bookmark: _Toc469579743][bookmark: _Toc469932227][bookmark: _Toc476315912][bookmark: _Toc476644260][bookmark: _Toc485039861][bookmark: _Toc485041277][bookmark: _Toc6227263][bookmark: _Toc6229391][bookmark: _Toc53996873][bookmark: _Toc54693104][bookmark: _Toc54704013]2.1	BUSINESS REGISTRATION
Pursuant to N.J.S.A. 52:32-44, the State is prohibited from entering into a contract with an entity unless the bidder and each subcontractor named in the proposal have a valid Business Registration Certificate on file with the Division of Revenue and Enterprise Services.  A subcontractor named in a bid or other proposal shall provide a copy of its business registration to the bidder who shall provide it to the State.  

The contractor shall maintain and submit to the State a list of subcontractors and their addresses that may be updated from time to time with the prior written consent of the Director during the course of contract performance.  The contractor shall submit to the State a complete and accurate list of all subcontractors used and their addresses before final payment is made under the contract.

Pursuant to N.J.S.A. 54:49-4.1, a business organization that fails to provide a copy of a business registration, or that provides false business registration information, shall be liable for a penalty of $25 for each day of violation, not to exceed $50,000 for each business registration copy not properly provided under a contract with a contracting agency.

The contractor and any subcontractor providing goods or performing services under the contract, and each of their affiliates, shall, during the term of the contract, collect and remit to the Director of the Division of Taxation in the Department of the Treasury, the Use Tax due pursuant to the “Sales and Use Tax Act, P.L. 1966, c. 30 (N.J.S.A. 54:32B-1 et seq.) on all sales of tangible personal property delivered into the State. Any questions in this regard can be directed to the Division of Revenue at (609) 292-1730. Form NJ-REG can be filed online at http://www.state.nj.us/treasury/revenue/busregcert.shtml.

[bookmark: _Toc469579744][bookmark: _Toc469932228][bookmark: _Toc476315913][bookmark: _Toc476644261][bookmark: _Toc485039862][bookmark: _Toc485041278][bookmark: _Toc6227264][bookmark: _Toc6229392][bookmark: _Toc53996874][bookmark: _Toc54693105][bookmark: _Toc54704014]2.2	ANTI-DISCRIMINATION
All parties to any contract with the State agree not to discriminate in employment and agree to abide by all anti-discrimination laws including those contained within N.J.S.A. 10:2-1 through N.J.S.A. 10:2-4, N.J.S.A. 10:5-1 et seq. and N.J.S.A. 10:5-31 through 10:5-38, and all rules and regulations issued thereunder are hereby incorporated by reference. The agreement to abide by the provisions of N.J.S.A. 10:5-31 through 10:5-38 include those provisions indicated for Goods, Professional Service and General Service Contracts (Exhibit A, attached) and Constructions Contracts (Exhibit B and Executive Order 151, August 28, 2009, attached) as appropriate.

The contractor or subcontractor, where applicable, agrees to comply with any regulations promulgated by the Treasurer pursuant to N.J.S.A. 10:5-31 et seq., as amended and supplemented from time to time.

[bookmark: _Toc469579745][bookmark: _Toc469932229][bookmark: _Toc476315914][bookmark: _Toc476644262][bookmark: _Toc485039863][bookmark: _Toc485041279][bookmark: _Toc6227265][bookmark: _Toc6229393][bookmark: _Toc53996875][bookmark: _Toc54693106][bookmark: _Toc54704015]2.3	PREVAILING WAGE ACT
The New Jersey Prevailing Wage Act, N.J.S.A. 34: 11-56.25 et seq. is hereby made part of every contract entered into on behalf of the State of New Jersey through the Division of Purchase and Property, except those contracts which are not within the contemplation of the Act. The bidder's signature on [this proposal] is his/her guarantee that neither he/she nor any subcontractors he/she might employ to perform the work covered by [this proposal] has been suspended or debarred by the Commissioner, Department of Labor and Workforce Development for violation of the provisions of the Prevailing Wage Act and/or the Public Works Contractor Registration Acts; the bidder’s signature on the proposal is also his/her guarantee that he/she and any subcontractors he/she might employ to perform the work covered by [this proposal] shall comply with the provisions of the Prevailing Wage and Public Works Contractor Registration Acts, where required. 

2.4	AMERICANS WITH DISABILITIES ACT
The contractor must comply with all provisions of the Americans with Disabilities Act (ADA), P.L 101-336, in accordance with 42 U.S.C. 12101, et seq. 

[bookmark: _Toc469579746][bookmark: _Toc469932230][bookmark: _Toc476315915][bookmark: _Toc476644263][bookmark: _Toc485039864][bookmark: _Toc485041280][bookmark: _Toc6227266][bookmark: _Toc6229394][bookmark: _Toc53996876][bookmark: _Toc54693107][bookmark: _Toc54704016]2.5	MACBRIDE PRINCIPLES
The bidder must certify pursuant to N.J.S.A. 52:34-12.2 that it either has no ongoing business activities in Northern Ireland and does not maintain a physical presence therein or that it will take lawful steps in good faith to conduct any business operations it has in Northern Ireland in accordance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of their compliance with those principles. 

[bookmark: _Toc469579747][bookmark: _Toc469932231][bookmark: _Toc476315916][bookmark: _Toc476644264][bookmark: _Toc485039865][bookmark: _Toc485041281][bookmark: _Toc6227267][bookmark: _Toc6229395][bookmark: _Toc53996877][bookmark: _Toc54693108][bookmark: _Toc54704017]2.6	PAY TO PLAY PROHIBITIONS
Pursuant to N.J.S.A. 19:44A-20.13 et seq. (P.L. 2005, c. 51), and specifically, N.J.S.A. 19:44A-20.21, it shall be a breach of the terms of the contract for the business entity to: 

A. Make or solicit a contribution in violation of the statute; 
B. Knowingly conceal or misrepresent a contribution given or received; 
C. Make or solicit contributions through intermediaries for the purpose of concealing or misrepresenting the source of the contribution; 
D. Make or solicit any contribution on the condition or with the agreement that it will be contributed to a campaign committee or any candidate of holder of the public office of Governor or Lieutenant Governor, or to any State or county party committee; 
E. Engage or employ a lobbyist or consultant with the intent or understanding that such lobbyist or consultant would make or solicit any contribution, which if made or solicited by the business entity itself, would subject that entity to the restrictions of the Legislation; 
F. Fund contributions made by third parties, including consultants, attorneys, family members, and employees; 
G. Engage in any exchange of contributions to circumvent the intent of the Legislation; or 
H. Directly or indirectly through or by any other person or means, do any act which would subject that entity to the restrictions of the Legislation. 

[bookmark: _Toc469579748][bookmark: _Toc469932232][bookmark: _Toc476315917][bookmark: _Toc476644265][bookmark: _Toc485039866][bookmark: _Toc485041282][bookmark: _Toc6227268][bookmark: _Toc6229396][bookmark: _Toc53996878][bookmark: _Toc54693109][bookmark: _Toc54704018]2.7	POLITICAL CONTRIBUTION DISCLOSURE
The contractor is advised of its responsibility to file an annual disclosure statement on political contributions with the New Jersey Election Law Enforcement Commission (ELEC), pursuant to N.J.S.A. 19:44A-20.27 (P.L. 2005, c. 271, §3 as amended) if in a calendar year the contractor receives one (1) or more contracts valued at $50,000.00 or more. It is the contractor’s responsibility to determine if filing is necessary. Failure to file can result in the imposition of penalties by ELEC. Additional information about this requirement is available from ELEC by calling 1(888)313-3532 or on the internet at http://www.elec.state.nj.us/.

[bookmark: _Toc469579749][bookmark: _Toc469932233][bookmark: _Toc476315918][bookmark: _Toc476644266][bookmark: _Toc485039867][bookmark: _Toc485041283][bookmark: _Toc6227269][bookmark: _Toc6229397][bookmark: _Toc53996879][bookmark: _Toc54693110][bookmark: _Toc54704019]2.8	STANDARDS PROHIBITING CONFLICTS OF INTEREST
The following prohibitions on contractor activities shall apply to all contracts or purchase agreements made with the State of New Jersey, pursuant to Executive Order No. 189 (1988). 

No vendor shall pay, offer to pay, or agree to pay, either directly or indirectly, any fee, commission, compensation, gift, gratuity, or other thing of value of any kind to any State officer or employee or special State officer or employee, as defined by N.J.S.A. 52:13D-13b. and e., in the Department of the Treasury or any other agency with which such vendor transacts or offers or proposes to transact business, or to any member of the immediate family, as defined by N.J.S.A. 52:13D-13i., of any such officer or employee, or partnership, firm or corporation with which they are employed or associated, or in which such officer or employee has an interest within the meaning of N.J.S.A. 52: 13D-13g;
 
The solicitation of any fee, commission, compensation, gift, gratuity or other thing of value by any State officer or employee or special State officer or employee from any State vendor shall be reported in writing forthwith by the vendor to the New Jersey Office of the Attorney General and the Executive Commission on Ethical Standards, now known as the State Ethics Commission;

No vendor may, directly or indirectly, undertake any private business, commercial or entrepreneurial relationship with, whether or not pursuant to employment, contract or other agreement, express or implied, or sell any interest in such vendor to, any State officer or employee or special State officer or employee having any duties or responsibilities in connection with the purchase, acquisition or sale of any property or services by or to any State agency or any instrumentality thereof, or with any person, firm or entity with which he/she is employed or associated or in which he/she has an interest within the meaning of N.J.S.A. 52:13D-13g. Any relationships subject to this provision shall be reported in writing forthwith to the Executive Commission on Ethical Standards, now known as the State Ethics Commission, which may grant a waiver of this restriction upon application of the State officer or employee or special State officer or employee upon a finding that the present or proposed relationship does not present the potential, actuality or appearance of a conflict of interest;

No vendor shall influence, or attempt to influence or cause to be influenced, any State officer or employee or special State officer or employee in his/her official capacity in any manner which might tend to impair the objectivity or independence of judgment of said officer or employee;

No vendor shall cause or influence, or attempt to cause or influence, any State officer or employee or special State officer or employee to use, or attempt to use, his/her official position to secure unwarranted privileges or advantages for the vendor or any other person; and
 
The provisions cited above in paragraphs 2.8a through 2.8e shall not be construed to prohibit a State officer or employee or Special State officer or employee from receiving gifts from or contracting with vendors under the same terms and conditions as are offered or made available to members of the general public subject to any guidelines the Executive Commission on Ethical Standards, now known as the State Ethics Commission may promulgate under paragraph 3c of Executive Order No. 189. 

[bookmark: _Toc469579750][bookmark: _Toc469932234][bookmark: _Toc476315919][bookmark: _Toc476644267][bookmark: _Toc485039868][bookmark: _Toc485041284][bookmark: _Toc6227270][bookmark: _Toc6229398][bookmark: _Toc53996880][bookmark: _Toc54693111][bookmark: _Toc54704020]2.9	NOTICE TO ALL CONTRACTORS SET-OFF FOR STATE TAX NOTICE
Pursuant to N.J.S.A. 54:49-19, effective January 1, 1996, and notwithstanding any provision of the law to the contrary, whenever any taxpayer, partnership or S corporation under contract to provide goods or services or construction projects to the State of New Jersey or its agencies or instrumentalities, including the legislative and judicial branches of State government, is entitled to payment for those goods or services at the same time a taxpayer, partner or shareholder of that entity is indebted for any State tax, the Director of the Division of Taxation shall seek to set off that taxpayer’s or shareholder’s share of the payment due the taxpayer, partnership, or S corporation. The amount set off shall not allow for the deduction of any expenses or other deductions which might be attributable to the taxpayer, partner or shareholder subject to set-off under this act. 
The Director of the Division of Taxation shall give notice to the set-off to the taxpayer and provide an opportunity for a hearing within 30 days of such notice under the procedures for protests established under R.S. 54:49-18. No requests for conference, protest, or subsequent appeal to the Tax Court from any protest under this section shall stay the collection of the indebtedness. Interest that may be payable by the State, pursuant to P.L. 1987, c.184 (c.52:32-32 et seq.), to the taxpayer shall be stayed. 

[bookmark: _Toc469579751][bookmark: _Toc469932235][bookmark: _Toc476315920][bookmark: _Toc476644268][bookmark: _Toc485039869][bookmark: _Toc485041285][bookmark: _Toc6227271][bookmark: _Toc6229399][bookmark: _Toc53996881][bookmark: _Toc54693112][bookmark: _Toc54704021]2.10	COMPLIANCE - LAWS
The contractor must comply with all local, State and Federal laws, rules and regulations applicable to this contract and to the goods delivered and/or services performed hereunder. 

[bookmark: _Toc469579752][bookmark: _Toc469932236][bookmark: _Toc476315921][bookmark: _Toc476644269][bookmark: _Toc485039870][bookmark: _Toc485041286][bookmark: _Toc6227272][bookmark: _Toc6229400][bookmark: _Toc53996882][bookmark: _Toc54693113][bookmark: _Toc54704022]2.11	COMPLIANCE - STATE LAWS
It is agreed and understood that any contracts and/or orders placed as a result of [this proposal] shall be governed and construed and the rights and obligations of the parties hereto shall be determined in accordance with the laws of the State of New Jersey.

[bookmark: _Toc485039871][bookmark: _Toc485041287][bookmark: _Toc6227273][bookmark: _Toc6229401][bookmark: _Toc53996883][bookmark: _Toc54693114][bookmark: _Toc54704023]2.12	Warranty of no solicitation on commission or contingent fee basis
The contractor warrants that no person or selling agency has been employed or retained to solicit or secure the contract upon an agreement or understanding for a commission, percentage, brokerage or contingent fee, except bona fide employees or bona fide established commercial or selling agencies maintained by the contractor for the purpose of securing business.  If a breach or violation of this section occurs, the State shall have the right to terminate the contract without liability or in its discretion to deduct from the contract price or consideration the full amount of such commission, percentage, brokerage or contingent fee.

[bookmark: _Toc485039872][bookmark: _Toc485041288][bookmark: _Toc6227274][bookmark: _Toc6229402][bookmark: _Toc53996884][bookmark: _Toc54693115][bookmark: _Toc54704024]3.	STATE LAW REQUIRING MANDATORY COMPLIANCE BY CONTRACTORS UNDER CIRCUMSTANCES SET FORTH IN LAW OR BASED ON THE TYPE OF CONTRACT 

[bookmark: _Toc485039873][bookmark: _Toc485041289][bookmark: _Toc6227275][bookmark: _Toc6229403][bookmark: _Toc53996885][bookmark: _Toc54693116][bookmark: _Toc54704025]3.1	COMPLIANCE - CODES
The contractor must comply with NJUCC and the latest NEC70, B.O.C.A. Basic Building code, OSHA and all applicable codes for this requirement. The contractor shall be responsible for securing and paying all necessary permits, where applicable. 

[bookmark: _Toc485039874][bookmark: _Toc485041290][bookmark: _Toc6227276][bookmark: _Toc6229404][bookmark: _Toc53996886][bookmark: _Toc54693117][bookmark: _Toc54704026]3.2	PUBLIC WORKS CONTRACTOR REGISTRATION ACT
The New Jersey Public Works Contractor Registration Act requires all contractors, subcontractors and lower tier subcontractor(s) who engage in any contract for public work as defined in N.J.S.A. 34:11-56.26 be first registered with the New Jersey Department of Labor and Workforce Development pursuant to N.J.S.A. 34:11-56.51. Any questions regarding the registration process should be directed to the Division of Wage and Hour Compliance at (609) 292-9464. 

[bookmark: _Toc485039875][bookmark: _Toc485041291][bookmark: _Toc6227277][bookmark: _Toc6229405][bookmark: _Toc53996887][bookmark: _Toc54693118][bookmark: _Toc54704027]3.3	PUBLIC WORKS CONTRACT - ADDITIONAL AFFIRMATIVE ACTION REQUIREMENTS
N.J.S.A. 10:2-1 requires that during the performance of this contract, the contractor must agree as follows: 

A. In the hiring of persons for the performance of work under this contract or any subcontract hereunder, or for the procurement, manufacture, assembling or furnishing of any such materials, equipment, supplies or services to be acquired under this contract, no contractor, nor any person acting on behalf of such contractor or subcontractor, shall, by reason of race, creed, color, national origin, ancestry, marital status, gender identity or expression, affectional or sexual orientation or sex, discriminate against any person who is qualified and available to perform the work to which the employment relates;

B. No contractor, subcontractor, nor any person on his/her behalf shall, in any manner, discriminate against or intimidate any employee engaged in the performance of work under this contract or any subcontract hereunder, or engaged in the procurement, manufacture, assembling or furnishing of any such materials, equipment, supplies or services to be acquired under such contract, on account of race, creed, color, national origin, ancestry, marital status, gender identity or expression, affectional or sexual orientation or sex;

C. There may be deducted from the amount payable to the contractor by the contracting public agency, under this contract, a penalty of $50.00 for each person for each calendar day during which such person is discriminated against or intimidated in violation of the provisions of the contract; and

D. This contract may be canceled or terminated by the contracting public agency, and all money due or to become due hereunder may be forfeited, for any violation of this section of the contract occurring after notice to the contractor from the contracting public agency of any prior violation of this section of the contract.

N.J.S.A. 10:5-33 and N.J.A.C. 17:27-3.5 require that during the performance of this contract, the contractor must agree as follows: 

A. The contractor or subcontractor, where applicable, will not discriminate against any employee or applicant for employment because of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Except with respect to affectional or sexual orientation and gender identity or expression, the contractor will take affirmative action to ensure that such applicants are recruited and employed, and that employees are treated during employment, without regard to their age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Such action shall include, but not be limited to the following: employment, upgrading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship. The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided by the contracting officer setting forth the provisions of this nondiscrimination clause; 

B. The contractor or subcontractor, where applicable will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex; 

C. The contractor or subcontractor where applicable, will send to each labor union or representative of workers with which it has a collective bargaining agreement or other contract or understanding, a notice, to be provided by the agency contracting officer, advising the labor union or workers' representative of the contractor's commitments under this act and shall post copies of the notice in conspicuous places available to employees and applicants for employment, N.J.A.C. 17:27-3.7 requires all contractors and subcontractors, if any, to further agree as follows: 

1. The contractor or subcontractor agrees to make good faith efforts to meet targeted county employment goals established in accordance with N.J.A.C. 17:27-5.2;

2. The contractor or subcontractor agrees to inform in writing its appropriate recruitment agencies including, but not limited to, employment agencies, placement bureaus, colleges, universities, and labor unions, that it does not discriminate on the basis of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, and that it will discontinue the use of any recruitment agency which engages in direct or indirect discriminatory practices;

3. The contractor or subcontractor agrees to revise any of its testing procedures, if necessary, to assure that all personnel testing conforms with the principles of job-related testing, as established by the statutes and court decisions of the State of New Jersey and as established by applicable Federal law and applicable Federal court decisions; and
 
4. In conforming with the targeted employment goals, the contractor or subcontractor agrees to review all procedures relating to transfer, upgrading, downgrading and layoff to ensure that all such actions are taken without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, consistent with the statutes and court decisions of the State of New Jersey, and applicable Federal law and applicable Federal court decisions. 
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Pursuant to N.J.S.A. 34:11-56.58 et seq., in any contract for building services, as defined in N.J.S.A. 34:11-56.59, the employees of the contractor or subcontractors shall be paid prevailing wage for building services rates, as defined in N.J.S.A. 34:11.56.59. The prevailing wage shall be adjusted annually during the term of the contract. 
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The provisions of N.J.S.A. 34:5A-1 et seq. which require the labeling of all containers of hazardous substances are applicable to this contract. Therefore, all goods offered for purchase to the State must be labeled by the contractor in compliance with the provisions of the statute. 
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Under N.J.S.A. 52:34-13.2, all contracts primarily for services awarded by the Director shall be performed within the United States, except when the Director certifies in writing a finding that a required service cannot be provided by a contractor or subcontractor within the United States and the certification is approved by the State Treasurer. 
A shift to performance of services outside the United States during the term of the contract shall be deemed a breach of contract. If, during the term of the contract, the contractor or subcontractor, proceeds to shift the performance of any of the services outside the United States, the contractor shall be deemed to be in breach of its contract, which contract shall be subject to termination for cause pursuant to Section 5.7(b) (1) of the Standard Terms and Conditions, unless previously approved by the Director and the Treasurer. 
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Pursuant to N.J.S.A. 52:32-1, if manufactured items or farm products will be provided under this contract to be used in a public work, they shall be manufactured or produced in the United States and the contractor shall be required to so certify. 

3.8	DIANE B. ALLEN EQUAL PAY ACT
Pursuant to N.J.S.A. 34:11-56.14, a contractor performing “qualifying services” or “public work” to the State or any agency or instrumentality of the State shall provide the Commissioner of Labor and Workforce Development a report regarding the compensation and hours worked by employees categorized by gender, race, ethnicity, and job category.  For more information and report templates see https://nj.gov/labor/equalpay/equalpay.html.  
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The contractor’s liability to the State and its employees in third party suits shall be as follows: 

A. Indemnification for Third Party Claims - The contractor shall assume all risk of and responsibility for, and agrees to indemnify, defend, and save harmless the State of New Jersey and its employees from and against any and all claims, demands, suits, actions, recoveries, judgments and costs and expenses in connection therewith which shall arise from or result directly or indirectly from the work and/or materials supplied under this contract, including liability of any nature or kind for or on account of the use of any copyrighted or uncopyrighted composition, secret process, patented or unpatented invention, article or appliance furnished or used in the performance of this contract;

B. The contractor’s indemnification and liability under subsection (a) is not limited by, but is in addition to the insurance obligations contained in Section 4.2 of these Terms and Conditions; and

C. In the event of a patent and copyright claim or suit, the contractor, at its option, may: (1) procure for the State of New Jersey the legal right to continue the use of the product; (2) replace or modify the product to provide a non-infringing product that is the functional equivalent; or (3) refund the purchase price less a reasonable allowance for use that is agreed to by both parties.

[bookmark: _Toc485039882][bookmark: _Toc485041298][bookmark: _Toc6227284][bookmark: _Toc6229412][bookmark: _Toc53996894][bookmark: _Toc54693125][bookmark: _Toc54704034]4.2	INSURANCE
The contractor shall secure and maintain in force for the term of the contract insurance as provided herein. All required insurance shall be provided by insurance companies with an A-VIII or better rating by A.M. Best & Company. All policies must be endorsed to provide 30 days’ written notice of cancellation or material change to the State of New Jersey at the address shown below. If the contractor’s insurer cannot provide 30 days written notice, then it will become the obligation of the contractor to provide the same.  The contractor shall provide the State with current certificates of insurance for all coverages and renewals thereof. Renewal certificates shall be provided within 30 days of the expiration of the insurance. The contractor shall not begin to provide services or goods to the State until evidence of the required insurance is provided. The certificates of insurance shall indicate the contract number or purchase order number and title of the contract in the Description of Operations box and shall list the State of New Jersey, Department of the Treasury, Division of Purchase & Property, Contract Compliance & Audit Unit, P.O. Box 236, Trenton, New Jersey 08625 in the Certificate Holder box. The certificates and any notice of cancelation shall be emailed to the State at: 
ccau.certificate@treas.nj.gov

The insurance to be provided by the contractor shall be as follows: 

A. Occurrence Form Commercial General Liability Insurance or its equivalent: The minimum limit of liability shall be $1,000,000 per occurrence as a combined single limit for bodily injury and property damage. The above required Commercial General Liability Insurance policy or its equivalent shall name the State, its officers, and employees as “Additional Insureds” and include the blanket additional insured endorsement or its equivalent. The coverage to be provided under these policies shall be at least as broad as that provided by the standard basic Commercial General Liability Insurance occurrence coverage forms or its equivalent currently in use in the State of New Jersey, which shall not be circumscribed by any endorsement limiting the breadth of coverage; 

B. Automobile Liability Insurance which shall be written to cover any automobile used by the insured. Limits of liability for bodily injury and property damage shall not be less than $1,000,000 per occurrence as a combined single limit. The State must be named as an “Additional Insured” and a blanket additional insured endorsement or its equivalent must be provided when the services being procured involve vehicle use on the State’s behalf or on State controlled property;

C. Worker’s Compensation Insurance applicable to the laws of the State of New Jersey and Employers Liability Insurance with limits not less than: 

1. $1,000,000 BODILY INJURY, EACH OCCURRENCE; 
2. $1,000,000 DISEASE EACH EMPLOYEE; and 
3. $1,000,000 DISEASE AGGREGATE LIMIT. 

A. This $1,000,000 amount may have been raised by the RFP when deemed necessary by the Director; and

B. In the case of a contract entered into pursuant to N.J.S.A. 52:32-17 et seq., (small business set asides) the minimum amount of insurance coverage in subsections a., b., and c. above may have been lowered in the RFP for certain commodities when deemed in the best interests of the State by the Director. 
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The contractor's status shall be that of any independent contractor and not as an employee of the State. 
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The estimated amount of the contract(s), when stated on the RFP form, shall not be construed as either the maximum or minimum amount which the State shall be obliged to order as the result of the RFP or any contract entered into as a result of the RFP. 
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If, in the opinion of the Director, it is in the best interest of the State to extend a contract, the contractor shall be so notified of the Director’s Intent at least 30 days prior to the expiration date of the existing contract. The contractor shall have 15 calendar days to respond to the Director's request to extend the term and period of performance of the contract. If the contractor agrees to the extension, all terms and conditions of the original contract shall apply unless more favorable terms for the State have been negotiated. 
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The State has the option, in its sole discretion, to reduce the scope of work for any deliverable, task or subtask called for under this contract. In such an event, the Director shall provide to the contractor advance written notice of the change in scope of work and what the Director believes should be the corresponding adjusted contract price. Within five (5) business days of receipt of such written notice, if either is applicable: 

A. If the contractor does not agree with the Director’s proposed adjusted contract price, the contractor shall submit to the Director any additional information that the contractor believes impacts the adjusted contract price with a request that the Director reconsider the proposed adjusted contract price. The parties shall negotiate the adjusted contract price. If the parties are unable to agree on an adjusted contract price, the Director shall make a prompt decision taking all such information into account, and shall notify the contractor of the final adjusted contract price; and

B. If the contractor has undertaken any work effort toward a deliverable, task or subtask that is being changed or eliminated such that it would not be compensated under the adjusted contract, the contractor shall be compensated for such work effort according to the applicable portions of its price schedule and the contractor shall submit to the Director an itemization of the work effort already completed by deliverable, task or subtask within the scope of work, and any additional information the Director may request. The Director shall make a prompt decision taking all such information into account, and shall notify the contractor of the compensation to be paid for such work effort. 
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If, after award, a change in applicable law or regulation occurs which affects the Contract, the parties may amend the Contract, including pricing, in order to provide equitable relief for the party disadvantaged by the change in law.  The parties shall negotiate in good faith, however if agreement is not possible after reasonable efforts, the Director shall make a prompt decision as to an equitable adjustment, taking all relevant information into account, and shall notify the Vendor {Contractor} of the final adjusted contract price.  
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The State may, for valid reason, issue a stop order directing the contractor to suspend work under the contract for a specific time. The contractor shall be paid for goods ordered, goods delivered, or services requested and performed until the effective date of the stop order. The contractor shall resume work upon the date specified in the stop order, or upon such other date as the State Contract Manager may thereafter direct in writing. The period of suspension shall be deemed added to the contractor's approved schedule of performance. The Director shall make an equitable adjustment, if any is required, to the contract price. The contractor shall provide whatever information that Director may require related to the equitable adjustment. 
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A. For Convenience: 
Notwithstanding any provision or language in this contract to the contrary, the Director may terminate this contract at any time, in whole or in part, for the convenience of the State, upon no less than 30 days written notice to the contractor;

B. For Cause:
1. Where a contractor fails to perform or comply with a contract or a portion thereof, and/or fails to comply with the complaints procedure in N.J.A.C. 17:12-4.2 et seq., the Director may terminate the contract, in whole or in part, upon ten (10) days’ notice to the contractor with an opportunity to respond; and
 
2. Where in the reasonable opinion of the Director, a contractor continues to perform a contract poorly as demonstrated by e.g., formal complaints, late delivery, poor performance of service, short-shipping, so that the Director is required to use the complaints procedure in N.J.A.C. 17:12-4.2 et seq., and there has been a failure on the part of the contractor to make progress towards ameliorating the issue(s) or problem(s) set forth in the complaint, the Director may terminate the contract, in whole or in part, upon ten (10) days’ notice to the contractor with an opportunity to respond.
 
C. In cases of emergency the Director may shorten the time periods of notification and may dispense with an opportunity to respond; and

D. In the event of termination under this section, the contractor shall be compensated for work performed in accordance with the contract, up to the date of termination. Such compensation may be subject to adjustments. 
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A. Subcontracting: The contractor may not subcontract other than as identified in the contractor’s proposal without the prior written consent of the Director. Such consent, if granted in part, shall not relieve the contractor of any of his/her responsibilities under the contract, nor shall it create privity of contract between the State and any subcontractor. If the contractor uses a subcontractor to fulfill any of its obligations, the contractor shall be responsible for the subcontractor’s: (a) performance; (b) compliance with all of the terms and conditions of the contract; and (c) compliance with the requirements of all applicable laws; and 

B. Assignment: The contractor may not assign its responsibilities under the contract, in whole or in part, without the prior written consent of the Director. 
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Nothing contained in any of the contract documents, including the RFP and vendor’s bid or proposal shall be construed as creating any contractual relationship between any subcontractor and the State. 
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If, during the term of this contract, the contractor shall merge with or be acquired by another firm, the contractor shall give notice to the Director as soon as practicable and in no event longer than 30 days after said merger or acquisition. The contractor shall provide such documents as may be requested by the Director, which may include but need not be limited to the following: corporate resolutions prepared by the awarded contractor and new entity ratifying acceptance of the original contract, terms, conditions and prices; updated information including ownership disclosure and Federal Employer Identification Number. The documents must be submitted within 30 days of the request. Failure to do so may result in termination of the contract for cause. 

If, at any time during the term of the contract, the contractor's partnership, limited liability company, limited liability partnership, professional corporation, or corporation shall dissolve, the Director must be so notified. All responsible parties of the dissolved business entity must submit to the Director in writing, the names of the parties proposed to perform the contract, and the names of the parties to whom payment should be made. No payment shall be made until all parties to the dissolved business entity submit the required documents to the Director. 
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The contractor hereby certifies that: 
A. The equipment offered is standard new equipment, and is the manufacturer's latest model in production, with parts regularly used for the type of equipment offered; that such parts are all in production and not likely to be discontinued; and that no attachment or part has been substituted or applied contrary to manufacturer's recommendations and standard practice;

B. All equipment supplied to the State and operated by electrical current is UL listed where applicable;

C. All new machines are to be guaranteed as fully operational for the period stated in the contract from time of written acceptance by the State. The contractor shall render prompt service without charge, regardless of geographic location;

D. Sufficient quantities of parts necessary for proper service to equipment shall be maintained at distribution points and service headquarters;

E. Trained mechanics are regularly employed to make necessary repairs to equipment in the territory from which the service request might emanate within a 48-hour period or within the time accepted as industry practice; 

F. During the warranty period the contractor shall replace immediately any material which is rejected for failure to meet the requirements of the contract; and

G. All services rendered to the State shall be performed in strict and full accordance with the specifications stated in the contract. The contract shall not be considered complete until final approval by the State's using agency is rendered. 
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A. Deliveries shall be made at such time and in such quantities as ordered in strict accordance with conditions contained in the contract;

B. The contractor shall be responsible for the delivery of material in first class condition to the State's using agency or the purchaser under this contract and in accordance with good commercial practice;
 
C. Items delivered must be strictly in accordance with the contract; and

D. In the event delivery of goods or services is not made within the number of days stipulated or under the schedule defined in the contract, the using agency shall be authorized to obtain the material or service from any available source, the difference in price, if any, to be paid by the contractor. 
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This contract and any and all litigation arising therefrom or related thereto shall be governed by the applicable laws, regulations and rules of evidence of the State of New Jersey without reference to conflict of laws principles and shall be filed in the appropriate Division of the New Jersey Superior Court. 
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Except as provided herein, the contract may only be amended by written agreement of the State and the contractor. 
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The contractor shall maintain records for products and/or services delivered against the contract for a period of five (5) years from the date of final payment unless a longer period is required by law. Such records shall be made available to the State, including the Comptroller, for audit and review.

[bookmark: _Toc485039899][bookmark: _Toc485041315][bookmark: _Toc6227301][bookmark: _Toc6229429][bookmark: _Toc53996911][bookmark: _Toc54693142][bookmark: _Toc54704051]5.16	ASSIGNMENT OF ANTITRUST CLAIM(S)
The contractor recognizes that in actual economic practice, overcharges resulting from antitrust violations are in fact usually borne by the ultimate purchaser. Therefore, and as consideration for executing this contract, the contractor, acting herein by and through its duly authorized agent, hereby conveys, sells, assigns, and transfers to the State of New Jersey, for itself and on behalf of its political subdivisions and public agencies, all right, title and interest to all claims and causes of action it may now or hereafter acquire under the antitrust laws of the United States or the State of New Jersey, relating to the particular goods and services purchased or acquired by the State of New Jersey or any of its political subdivisions or public agencies pursuant to this contract. 
In connection with this assignment, the following are the express obligations of the contractor: 

A. It shall take no action that will in any way diminish the value of the rights conveyed or assigned hereunder; 
B. It shall advise the Attorney General of New Jersey: 
1. In advance of its intention to commence any action on its own behalf regarding any such claim or cause(s) of action; and
2. Immediately upon becoming aware of the fact that an action has been commenced on its behalf by some other person(s) of the pendency of such action. 
C. It shall notify the defendants in any antitrust suit of the within assignment at the earliest practicable opportunity after the contractor has initiated an action on its own behalf or becomes aware that such an action has been filed on its behalf by another person. A copy of such notice shall be sent to the Attorney General of New Jersey; and 
D. It is understood and agreed that in the event any payment under any such claim or cause of action is made to the contractor, it shall promptly pay over to the State of New Jersey the allotted share thereof, if any, assigned to the State hereunder. 
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Unless otherwise agreed to in writing by the State, all prices quoted shall be firm through issuance of contract or purchase order and shall not be subject to increase during the period of the contract. 
In the event of a manufacturer's or contractor's price decrease during the contract period, the State shall receive the full benefit of such price reduction on any undelivered purchase order and on any subsequent order placed during the contract period. The Director must be notified, in writing, of any price reduction within five (5) days of the effective date. 

Failure to report price reductions may result in cancellation of contract for cause, pursuant to provision 5.7(b)1. 

In an exceptional situation the State may consider a price adjustment. Requests for price adjustments must include justification and documentation.
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The State of New Jersey is exempt from State sales or use taxes and Federal excise taxes. Therefore, price quotations must not include such taxes. The State's Federal Excise Tax Exemption number is 22-75-0050K. 
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A. The using agency(ies) is (are) authorized to order and the contractor is authorized to ship only those items covered by the contract resulting from the RFP. If a review of orders placed by the using agency(ies) reveals that goods and/or services other than that covered by the contract have been ordered and delivered, such delivery shall be a violation of the terms of the contract and may be considered by the Director as a basis to terminate the contract and/or not award the contractor a subsequent contract. The Director may take such steps as are necessary to have the items returned by the agency, regardless of the time between the date of delivery and discovery of the violation. In such event, the contractor shall reimburse the State the full purchase price; 

B. The contractor must submit invoices to the using agency with supporting documentation evidencing that work or goods for which payment is sought has been satisfactorily completed or delivered. For commodity contracts, the invoice, together with the original Bill of Lading, express receipt and other related papers must be sent to the State Contract Manager or using agency on the date of each delivery. For contracts featuring services, invoices must reference the tasks or subtasks detailed in the Scope of Work section of the RFP and must be in strict accordance with the firm, fixed prices submitted for each task or subtask on the RFP pricing sheets. When applicable, invoices should reference the appropriate RFP price sheet line number from the contractor’s bid proposal. All invoices must be approved by the State Contract Manager or using agency before payment will be authorized; 

C. In all time and materials contracts, the State Contract Manager or designee shall monitor and approve the hours of work and the work accomplished by contractor and shall document both the work and the approval. Payment shall not be made without such documentation. A form of timekeeping record that should be adapted as appropriate for the Scope of Work being performed can be found at www.nj.gov/treasury/purchase/forms/Vendor_Timesheet.xls; and

D. The contractor shall provide, on a monthly and cumulative basis, a breakdown in accordance with the budget submitted, of all monies paid to any small business, minority or woman-owned subcontractor(s). This breakdown shall be sent to the Chief of Operations, Division of Revenue, P.O. Box 628, Trenton, NJ 08646. 

[bookmark: _Toc485039904][bookmark: _Toc485041320][bookmark: _Toc6227306][bookmark: _Toc6229434][bookmark: _Toc53996916][bookmark: _Toc54693147][bookmark: _Toc54704056]6.4	OPTIONAL PAYMENT METHOD: P-CARD
The State offers contractors the opportunity to be paid through the MasterCard procurement card (p-card). A contractor’s acceptance and a State agency’s use of the p-card are optional. P-card transactions do not require the submission of a contractor invoice; purchasing transactions using the p-card will usually result in payment to a contractor in three (3) days. A contractor should take note that there will be a transaction-processing fee for each p-card transaction. To participate, a contractor must be capable of accepting the MasterCard. Additional information can be obtained from banks or merchant service companies. 
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The New Jersey Prompt Payment Act, N.J.S.A. 52:32-32 et seq., requires state agencies to pay for goods and services within 60 days of the agency's receipt of a properly executed State Payment Voucher or within 60 days of receipt and acceptance of goods and services, whichever is later. Properly executed performance security, when required, must be received by the State prior to processing any payments for goods and services accepted by state agencies. Interest will be paid on delinquent accounts at a rate established by the State Treasurer. Interest shall not be paid until it exceeds $5.00 per properly executed invoice. 

Cash discounts and other payment terms included as part of the original agreement are not affected by the Prompt Payment Act. 
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The State’s obligation to make payment under this contract is contingent upon the availability of appropriated funds and receipt of revenues from which payment for contract purposes can be made. No legal liability on the part of the State for payment of any money shall arise unless and until funds are appropriated each fiscal year to the using agency by the State Legislature and made available through receipt of revenue.

[bookmark: _Toc485039907][bookmark: _Toc485041323][bookmark: _Toc6227309][bookmark: _Toc6229437][bookmark: _Toc53996919][bookmark: _Toc54693150][bookmark: _Toc54704059]7.	TERMS RELATING TO ALL CONTRACTS FUNDED, IN WHOLE OR IN PART, BY FEDERAL FUNDS 
The provisions set forth in this Section 7 of the Standard Terms and Conditions apply to all contracts funded, in whole or in part, by Federal funds as required by 2 CFR 200.317.  
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To the extent that the scope of work or specifications in the contract requires the contractor to provide any of the following items, this Section 7.1 of the Standard Terms and Conditions modifies the terms of the scope of work or specification.

Pursuant to 2 CFR 200.322, the contractor must comply with section 6002 of the Solid Waste Disposal Act, as amended by the Resource Conservation and Recovery Act, 42 U.S.C. § 6962. The requirements of Section 6002 include procuring only items designated in guidelines of the Environmental Protection Agency (EPA) at 40 CFR Part 247 that contain the highest percentage of recovered materials practicable, consistent with maintaining a satisfactory level of competition, where the purchase price of the item exceeds $ 10,000 or the value of the quantity acquired during the preceding fiscal year exceeded $ 10,000; procuring solid waste management services in a manner that maximizes energy and resource recovery; and establishing an affirmative procurement program for procurement of recovered materials identified in the EPA guidelines.  

A. Designated items are those set forth in 40 CFR 247 subpart B, as may be amended from time to time, including:
1. Paper and paper products listed in 40 C.F.R. 247.10;
2. Certain vehicular products as listed in 40 CFR 247.11;
3. Certain construction products listed in 40 C.F.R. 247.12;
4. Certain transportation products listed in 40 C.F.R. 247.13;
5. Certain park and recreation products, 40 C.F.R. 247.14;
6. Certain landscaping products listed in 40 C.F.R. 247.15; 
7. Certain non-paper office products listed in 40 C.F.R. 247.16; and 
8. Other miscellaneous products listed in 40 C.F.R. 247.17.

B. As defined in 40 CFR 247.3, “recovered material” means:
1. waste materials and byproducts which have been recovered or diverted from solid waste, but such term does not include those materials and byproducts generated from, and commonly reused within, an original manufacturing process; and
2. for purposes of purchasing paper and paper products, means waste material and byproducts that have been recovered or diverted from solid waste, but such term does not include those materials and byproducts generated from, and commonly reused within, an original manufacturing process. In the case of paper and paper products, the term recovered materials includes:
a. Postconsumer materials such as --
i. Paper, paperboard, and fibrous wastes from retail stores, office buildings, homes, and so forth, after they have passed through their end-usage as a consumer item, including: used corrugated boxes; old newspapers; old magazines; mixed waste paper; tabulating cards; and used cordage; and
ii. All paper, paperboard, and fibrous wastes that enter and are collected from municipal solid waste, and
b. Manufacturing, forest residues, and other wastes such as --
i. Dry paper and paperboard waste generated after completion of the papermaking process (that is, those manufacturing operations up to and including the cutting and trimming of the paper machine reel in smaller rolls of rough sheets) including: envelope cuttings, bindery trimmings, and other paper and paperboard waste, resulting from printing, cutting, forming, and other converting operations; bag, box, and carton manufacturing wastes; and butt rolls, mill wrappers, and rejected unused stock; and
ii. Finished paper and paperboard from obsolete inventories of paper and paperboard manufacturers, merchants, wholesalers, dealers, printers, converters, or others;
iii. Fibrous byproducts of harvesting, manufacturing, extractive, or wood-cutting processes, flax, straw, linters, bagasse, slash, and other forest residues;
iv. Wastes generated by the conversion of goods made from fibrous material (that is, waste rope from cordage manufacture, textile mill waste, and cuttings); and
v. Fibers recovered from waste water which otherwise would enter the waste stream.

C. For contracts in an amount greater than $ 100,000, at the beginning of each contract year, contractor shall provide the State estimates of the total percentage of recovered material utilized in the performance of its contract for each of the categories listed is subsection (A). For all contracts subject to this Section 7.1 of the Standard Terms and Conditions, at the conclusion of each contract year, contractor shall certify to the State the minimum recovered material content actually utilized in the prior contract year. 

[bookmark: _Toc485039909][bookmark: _Toc485041325][bookmark: _Toc6227311][bookmark: _Toc6229439][bookmark: _Toc53996921][bookmark: _Toc54693152][bookmark: _Toc54704061]7.2	EQUAL EMPLOYMENT OPPORTUNITY
Except as otherwise provided under 41 CFR Part 60, all contracts that meet the definition of "federally assisted construction contract" in 41 CFR Part 60-1.3 must include the equal opportunity clause provided under 41 CFR 60-1.4(b), in accordance with Executive Order 11246, "Equal Employment Opportunity" (30 FR 12319, 12935, 3 CFR Part, 1964-1965 Comp., p. 339), as amended by Executive Order 11375, "Amending Executive Order 11246 Relating to Equal Employment Opportunity," and implementing regulations at 41 CFR part 60, "Office of Federal Contract Compliance Programs, Equal Employment Opportunity, Department of Labor."

During the performance of this contract, the contractor agrees as follows:
(1) The contractor will not discriminate against any employee or applicant for employment because of race, color, religion, sex, sexual orientation, gender identity, or national origin. The contractor will take affirmative action to ensure that applicants are employed, and that employees are treated during employment without regard to their race, color, religion, sex, sexual orientation, gender identity, or national origin. Such action shall include, but not be limited to the following:
Employment, upgrading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship. The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided setting forth the provisions of this nondiscrimination clause.
(2) The contractor will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to race, color, religion, sex, sexual orientation, gender identity, or national origin.
(3) The contractor will not discharge or in any other manner discriminate against any employee or applicant for employment because such employee or applicant has inquired about, discussed, or disclosed the compensation of the employee or applicant or another employee or applicant. This provision shall not apply to instances in which an employee who has access to the compensation information of other employees or applicants as a part of such employee's essential job functions discloses the compensation of such other employees or applicants to individuals who do not otherwise have access to such information, unless such disclosure is in response to a formal complaint or charge, in furtherance of an investigation, proceeding, hearing, or action, including an investigation conducted by the employer, or is consistent with the contractor's legal duty to furnish information.
(4) The contractor will send to each labor union or representative of workers with which he/she has a collective bargaining agreement or other contract or understanding, a notice to be provided advising the said labor union or workers' representatives of the contractor's commitments under this section, and shall post copies of the notice in conspicuous places available to employees and applicants for employment.
(5) The contractor will comply with all provisions of Executive Order 11246 of September 24, 1965, and of the rules, regulations, and relevant orders of the Secretary of Labor.
(6) The contractor will furnish all information and reports required by Executive Order 11246 of September 24, 1965, and by rules, regulations, and orders of the Secretary of Labor, or pursuant thereto, and will permit access to his/her books, records, and accounts by the administering agency and the Secretary of Labor for purposes of investigation to ascertain compliance with such rules, regulations, and orders.
(7) In the event of the contractor's noncompliance with the nondiscrimination clauses of this contract or with any of the said rules, regulations, or orders, this contract may be canceled, terminated, or suspended in whole or in part and the contractor may be declared ineligible for further Government contracts or federally assisted construction contracts in accordance with procedures authorized in Executive Order 11246 of September 24, 1965, and such other sanctions may be imposed and remedies invoked as provided in Executive Order 11246 of September 24, 1965, or by rule, regulation, or order of the Secretary of Labor, or as otherwise provided by law.
(8) The contractor will include the portion of the sentence immediately preceding paragraph (1) and the provisions of paragraphs (1) through (8) in every subcontract or purchase order unless exempted by rules, regulations, or orders of the Secretary of Labor issued pursuant to section 204 of Executive Order 11246 of September 24, 1965, so that such provisions will be binding upon each subcontractor or vendor. The contractor will take such action with respect to any subcontract or purchase order as the administering agency may direct as a means of enforcing such provisions, including sanctions for noncompliance:
Provided, however, that in the event a contractor becomes involved in, or is threatened with, litigation with a subcontractor or vendor as a result of such direction by the administering agency, the contractor may request the United States to enter into such litigation to protect the interests of the United States.
The applicant further agrees that it will be bound by the above equal opportunity clause with respect to its own employment practices when it participates in federally assisted construction work: Provided, That if the applicant so participating is a State or local government, the above equal opportunity clause is not applicable to any agency, instrumentality or subdivision of such government which does not participate in work on or under the contract.
The applicant agrees that it will assist and cooperate actively with the administering agency and the Secretary of Labor in obtaining the compliance of contractors and subcontractors with the equal opportunity clause and the rules, regulations, and relevant orders of the Secretary of Labor, that it will furnish the administering agency and the Secretary of Labor such information as they may require for the supervision of such compliance, and that it will otherwise assist the administering agency in the discharge of the agency's primary responsibility for securing compliance.
The applicant further agrees that it will refrain from entering into any contract or contract modification subject to Executive Order 11246 of September 24, 1965, with a contractor debarred from, or who has not demonstrated eligibility for, Government contracts and federally assisted construction contracts pursuant to the Executive Order and will carry out such sanctions and penalties for violation of the equal opportunity clause as may be imposed upon contractors and subcontractors by the administering agency or the Secretary of Labor pursuant to Part II, Subpart D of the Executive Order. In addition, the applicant agrees that if it fails or refuses to comply with these undertakings, the administering agency may take any or all of the following actions: Cancel, terminate, or suspend in whole or in part this grant (contract, loan, insurance, guarantee); refrain from extending any further assistance to the applicant under the program with respect to which the failure or refund occurred until satisfactory assurance of future compliance has been received from such applicant; and refer the case to the Department of Justice for appropriate legal proceedings.

[bookmark: _Toc485039910][bookmark: _Toc485041326][bookmark: _Toc6227312][bookmark: _Toc6229440][bookmark: _Toc53996922][bookmark: _Toc54693153][bookmark: _Toc54704062]7.3	DAVIS-BACON ACT, 40 U.S.C. 3141-3148, AS AMENDED
When required by Federal program legislation, all prime construction contracts in excess of $ 2,000 awarded by non-Federal entities must include a provision for compliance with the Davis-Bacon Act (40 U.S.C. 3141-3144, and 3146-3148) as supplemented by Department of Labor regulations (29 CFR Part 5, "Labor Standards Provisions Applicable to Contracts Covering Federally Financed and Assisted Construction"). In accordance with the statute, contractors must be required to pay wages to laborers and mechanics at a rate not less than the prevailing wages specified in a wage determination made by the Secretary of Labor. In addition, contractors must be required to pay wages not less than once a week. The non-Federal entity must place a copy of the current prevailing wage determination issued by the Department of Labor in each solicitation. The decision to award a contract or subcontract must be conditioned upon the acceptance of the wage determination. The non-Federal entity must report all suspected or reported violations to the Federal awarding agency. The contracts must also include a provision for compliance with the Copeland "Anti-Kickback" Act (40 U.S.C. 3145), as supplemented by Department of Labor regulations (29 CFR Part 3, "Contractors and Subcontractors on Public Building or Public Work Financed in Whole or in Part by Loans or Grants from the United States"). The Act provides that each contractor or subrecipient must be prohibited from inducing, by any means, any person employed in the construction, completion, or repair of public work, to give up any part of the compensation to which he or she is otherwise entitled. The non-Federal entity must report all suspected or reported violations to the Federal awarding agency.

[bookmark: _Toc485039911][bookmark: _Toc485041327][bookmark: _Toc6227313][bookmark: _Toc6229441][bookmark: _Toc53996923][bookmark: _Toc54693154][bookmark: _Toc54704063]7.4	CONTRACT WORK HOURS AND SAFETY STANDARDS ACT, 40 U.S.C. 3701-3708
Where applicable, all contracts awarded by the non-Federal entity in excess of $ 100,000 that involve the employment of mechanics or laborers must include a provision for compliance with 40 U.S.C. 3702 and 3704, as supplemented by Department of Labor regulations (29 CFR Part 5). Under 40 U.S.C. 3702 of the Act, each contractor must be required to compute the wages of every mechanic and laborer on the basis of a standard work week of 40 hours. Work in excess of the standard work week is permissible provided that the worker is compensated at a rate of not less than one and a half times the basic rate of pay for all hours worked in excess of 40 hours in the work week. The requirements of 40 U.S.C. 3704 are applicable to construction work and provide that no laborer or mechanic must be required to work in surroundings or under working conditions which are unsanitary, hazardous or dangerous. These requirements do not apply to the purchases of supplies or materials or articles ordinarily available on the open market, or contracts for transportation or transmission of intelligence.

[bookmark: _Toc485039912][bookmark: _Toc485041328][bookmark: _Toc6227314][bookmark: _Toc6229442][bookmark: _Toc53996924][bookmark: _Toc54693155][bookmark: _Toc54704064]7.5	RIGHTS TO INVENTIONS MADE UNDER A CONTRACT OR AGREEMENT
If the Federal award meets the definition of "funding agreement" under 37 CFR § 401.2 (a) and the recipient or subrecipient wishes to enter into a contract with a small business firm or nonprofit organization regarding the substitution of parties, assignment or performance of experimental, developmental, or research work under that "funding agreement," the recipient or subrecipient must comply with the requirements of 37 CFR Part 401, "Rights to Inventions Made by Nonprofit Organizations and Small Business Firms Under Government Grants, Contracts and Cooperative Agreements," and any implementing regulations issued by the awarding agency.

[bookmark: _Toc485039913][bookmark: _Toc485041329][bookmark: _Toc6227315][bookmark: _Toc6229443][bookmark: _Toc53996925][bookmark: _Toc54693156][bookmark: _Toc54704065]7.6	CLEAN AIR ACT, 42 U.S.C. 7401-7671Q, AND THE FEDERAL WATER POLLUTION CONTROL ACT, 33 U.S.C. 1251-1387, AS AMENDED 
Contracts and subgrants of amounts in excess of $ 150,000 must contain a provision that requires the non-Federal award to agree to comply with all applicable standards, orders or regulations issued pursuant to the Clean Air Act (42 U.S.C. 7401-7671q) and the Federal Water Pollution Control Act as amended (33 U.S.C. 1251-1387). Violations must be reported to the Federal awarding agency and the Regional Office of the Environmental Protection Agency (EPA).

[bookmark: _Toc485039914][bookmark: _Toc485041330][bookmark: _Toc6227316][bookmark: _Toc6229444][bookmark: _Toc53996926][bookmark: _Toc54693157][bookmark: _Toc54704066]7.7	DEBARMENT AND SUSPENSION (EXECUTIVE ORDERS 12549 AND 12689) 
A contract award (see 2 CFR 180.220) must not be made to parties listed on the government wide exclusions in the System for Award Management (SAM), in accordance with the OMB guidelines at 2 CFR 180 that implement Executive Orders 12549 (3 CFR part 1986 Comp., p. 189) and 12689 (3 CFR part 1989 Comp., p. 235), "Debarment and Suspension." SAM Exclusions contains the names of parties debarred, suspended, or otherwise excluded by agencies, as well as parties declared ineligible under statutory or regulatory authority other than Executive Order 12549.

[bookmark: _Toc485039915][bookmark: _Toc485041331][bookmark: _Toc6227317][bookmark: _Toc6229445][bookmark: _Toc53996927][bookmark: _Toc54693158][bookmark: _Toc54704067]7.8	BYRD ANTI-LOBBYING AMENDMENT, 31 U.S.C. 1352 
Contractors that apply or bid for an award exceeding $ 100,000 must file the required certification. Each tier certifies to the tier above that it will not and has not used Federal appropriated funds to pay any person or organization for influencing or attempting to influence an officer or employee of any agency, a member of Congress, officer or employee of Congress, or an employee of a member of Congress in connection with obtaining any Federal contract, grant or any other award covered by 31 U.S.C. 1352. Each tier must also disclose any lobbying with non-Federal funds that takes place in connection with obtaining any Federal award. Such disclosures are forwarded from tier to tier up to the non-Federal award.


EXHIBIT A

MANDATORY EQUAL EMPLOYMENT OPPORTUNITY LANGUAGE
N.J.S.A. 10:5-31 et seq. (P.L. 1975, c. 127)
N.J.A.C. 17:27 et seq.

GOODS, GENERAL SERVICE AND PROFESSIONAL SERVICES CONTRACTS

During the performance of this contract, the contractor agrees as follows:

The contractor or subcontractor, where applicable, will not discriminate against any employee or applicant for employment because of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Except with respect to affectional or sexual orientation and gender identity or expression, the contractor will ensure that equal employment opportunity is afforded to such applicants in recruitment and employment, and that employees are treated during employment, without regard to their age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex.  Such equal employment opportunity shall include, but not be limited to the following: employment, upgrading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship.  The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided by the Public Agency Compliance Officer setting forth provisions of this nondiscrimination clause.

The contractor or subcontractor, where applicable will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex.

The contractor or subcontractor will send to each labor union, with which it has a collective bargaining agreement, a notice, to be provided by the agency contracting officer, advising the labor union of the contractor's commitments under this chapter and shall post copies of the notice in conspicuous places available to employees and applicants for employment.

The contractor or subcontractor, where applicable, agrees to comply with any regulations promulgated by the Treasurer pursuant to N.J.S.A. 10:5-31 et seq., as amended and supplemented from time to time and the Americans with Disabilities Act.

The contractor or subcontractor agrees to make good faith efforts to meet targeted county employment goals established in accordance with N.J.A.C. 17:27-5.2.

The contractor or subcontractor agrees to inform in writing its appropriate recruitment agencies including, but not limited to, employment agencies, placement bureaus, colleges, universities, and labor unions, that it does not discriminate on the basis of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, and that it will discontinue the use of any recruitment agency which engages in direct or indirect discriminatory practices.

The contractor or subcontractor agrees to revise any of its testing procedures, if necessary, to assure that all personnel testing conforms with the principles of job related testing, as established by the statutes and court decisions of the State of New Jersey and as established by applicable Federal law and applicable Federal court decisions.

In conforming with the targeted employment goals, the contractor or subcontractor agrees to review all procedures relating to transfer, upgrading, downgrading and layoff to ensure that all such actions are taken without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, consistent with the statutes and court decisions of the State of New Jersey, and applicable Federal law and applicable Federal court decisions.

The contractor shall submit to the public agency, after notification of award but prior to execution of a goods and services contract, one of the following three documents:

Letter of Federal Affirmative Action Plan Approval;

	Certificate of Employee Information Report; or

Employee Information Report Form AA302 (electronically provided by the Division and distributed to the public agency through the Division’s website at http://www.state.nj.us/treasury/contract_compliance).

The contractor and its subcontractors shall furnish such reports or other documents to the Division of Purchase an Property, CCAU, EEO Monitoring Program as may be requested by the office from time to time in order to carry out the purposes of these regulations, and public agencies shall furnish such information as may be requested by the Division of Purchase an Property, CCAU, EEO Monitoring Program for conducting a compliance investigation pursuant to N.J.A.C. 17:27-1 et seq.


EXHIBIT B

MANDATORY EQUAL EMPLOYMENT OPPORTUNITY LANGUAGE
N.J.S.A. 10:5-31 et seq. (P.L. 1975, c. 127)
N.J.S.A. 10:5-39 et. seq. (P.L. 1983, c. 197)
N.J.A.C. 17:27-1.1 et seq.

CONSTRUCTION CONTRACTS

During the performance of this contract, the contractor agrees as follows:

The contractor or subcontractor, where applicable, will not 	discriminate against any employee or applicant for employment because of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Except with respect to affectional or sexual orientation and gender identity or expression, the contractor will ensure that equal employment opportunity is afforded to such applicants in recruitment and employment, and that employees are treated during employment, without regard to their age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Such equal employment opportunity shall include, but not be limited to the following: employment, up grading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship. The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided by the Public Agency Compliance Officer setting forth provisions of this nondiscrimination clause.

The contractor or subcontractor, where applicable will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex.

N.J.S.A. 10:5-39 et seq. requires contractors, subcontractors, and permitted assignees performing construction, alteration, or repair of any building or public work in excess of $250,000 to guarantee equal employment opportunity to veterans.

The contractor or subcontractor will send to each labor union, with which it has a collective bargaining agreement, a notice, to be provided by the agency contracting officer, advising the labor union or workers' representative of the contractor's commitments under this act and shall post copies of the notice in conspicuous places available to employees and applicants for employment.

The contractor or subcontractor, where applicable, agrees to comply with any regulations promulgated by the Treasurer, pursuant to N.J.S.A. 10:5-31 et seq., as amended and supplemented from time to time and the Americans with Disabilities Act.

When hiring or scheduling workers in each construction trade, the contractor or subcontractor agrees to make good faith efforts to employ 	minority and women workers in each construction trade consistent with the targeted employment goal prescribed by N.J.A.C. 17:27-7.2; provided, however, that the Dept. of LWD, Construction EEO Monitoring Program may, in its discretion, exempt a contractor or subcontractor from compliance with the good faith procedures prescribed by the following provisions, A, B and C, as long as the Dept. of LWD, Construction EEO Monitoring Program is satisfied that the contractor or subcontractor is employing workers provided by a union which provides evidence, in accordance with standards prescribed by the Dept. of LWD, Construction EEO Monitoring Program, that its percentage of active "card carrying" members who are minority and women workers is equal to or greater than the targeted employment goal established in accordance with N.J.A.C. 17:27-7.2.  The contractor or subcontractor agrees that a good faith effort shall include compliance with the following procedures:

(A)	If the contractor or subcontractor has a referral agreement or arrangement with a union for a construction trade, the contractor or subcontractor shall, within three business days of the contract award, seek assurances from the union that it will cooperate with the contractor or subcontractor as it fulfills its affirmative action obligations under this contract and in accordance with the rules promulgated by the Treasurer pursuant to N.J.S.A. 10:5-31 et. seq., as supplemented and amended from time to time and the Americans with Disabilities Act.  If the contractor or subcontractor is unable to obtain said assurances from the construction trade union at least five business days prior to the commencement of construction work, the contractor or subcontractor agrees to afford equal employment opportunities minority and women workers directly, consistent with this chapter.  If the contractor's or subcontractor's prior experience with a construction trade union, regardless of whether the union has provided said assurances, indicates a significant possibility that the trade union will not refer sufficient minority and women workers consistent with affording equal employment opportunities as specified in this chapter, the contractor or subcontractor agrees to be prepared to provide such opportunities to minority and women workers directly, consistent with this chapter, by complying with the hiring or scheduling procedures prescribed under (B) below; and the contractor or subcontractor further agrees to take said action immediately if it determines that the union is not referring minority and women workers consistent with the equal employment opportunity goals set forth in this chapter.

(B)	If good faith efforts to meet targeted employment goals have not or cannot be met for each construction trade by adhering to the procedures of (A) above, or if the contractor does not have a referral agreement or arrangement with a union for a construction trade, the contractor or subcontractor agrees to take the following actions:

(1) To notify the public agency compliance officer, the Dept. of LWD, Construction EEO Monitoring Program, and minority and women referral organizations listed by the Division pursuant to N.J.A.C. 17:27-5.3, of its workforce needs, and request referral of minority and women workers;
		
(2) To notify any minority and women workers who have been listed with it as awaiting available vacancies;

(3) Prior to commencement of work, to request that the local construction trade union refer minority and women workers to fill job openings, provided the contractor or subcontractor has a referral agreement or arrangement with a union for the construction trade;

(4) To leave standing requests for additional referral to minority and women workers with the local construction trade union, provided the contractor or subcontractor has a referral agreement or arrangement with a union for the construction trade, the State Training and Employment Service and other approved referral sources in the area;

(5) If it is necessary to lay off some of the workers in a given trade on the construction site, layoffs shall be conducted in compliance with the equal employment opportunity and non-discrimination standards set forth in this regulation, as well as with applicable Federal and State court decisions;

(6) To adhere to the following procedure when minority and women workers apply or are referred to the contractor or subcontractor:

(i) The contactor or subcontractor shall interview the referred minority or women worker.

(ii) If said individuals have never previously received any document or certification signifying a level of qualification lower than that required in order to perform the work of the construction trade, the contractor or subcontractor shall in good faith determine the qualifications of such individuals. The contractor or subcontractor shall hire or schedule those individuals who satisfy appropriate qualification standards in conformity with the equal employment opportunity and non-discrimination principles set forth in this chapter. However, a contractor or subcontractor shall determine that the individual at least possesses the requisite skills, and experience recognized by a union, apprentice program or a referral agency, provided the referral agency is acceptable to the Dept. of LWD, Construction EEO Monitoring Program. If necessary, the contractor or subcontractor shall hire or schedule minority and women workers who qualify as trainees pursuant to these rules. All of the requirements, however, are limited by the provisions of (C) below.

(iii) The name of any interested women or minority individual shall be maintained on a waiting list, and shall be considered for employment as described in (i) above, whenever vacancies occur. At the request of the Dept. of LWD, Construction EEO Monitoring Program, the contractor or subcontractor shall provide evidence of its good faith efforts to employ women and minorities from the list to fill vacancies.

(iv) If, for any reason, said contractor or subcontractor determines that a minority individual or a woman is not qualified or if the individual qualifies as an advanced trainee or apprentice, the contractor or subcontractor shall inform the individual in writing of the reasons for the determination, maintain a copy of the determination in its files, and send a copy to the public agency compliance officer and to the Dept. of LWD, Construction EEO Monitoring Program.

(7) To keep a complete and accurate record of all requests made for the referral of workers in any trade covered by the contract, on forms made available by the Dept. of LWD, Construction EEO Monitoring Program and submitted promptly to the Dept. of LWD, Construction EEO Monitoring Program upon request.

(C)	The contractor or subcontractor agrees that nothing contained in (B) above shall preclude the contractor or subcontractor from complying with the union hiring hall or apprenticeship policies in any applicable collective bargaining agreement or union hiring hall arrangement, and, where required by custom or agreement, it shall send journeymen and trainees to the union for referral, or to the apprenticeship program for admission, pursuant to such agreement or arrangement. However, where the practices of a union or apprenticeship program will result in the exclusion of minorities and women or the failure to refer minorities and women consistent with the targeted county employment goal, the contractor or subcontractor shall consider for employment persons referred pursuant to (B) above without regard to such agreement or arrangement; provided further, however, that the contractor or subcontractor shall not be required to employ women and minority advanced trainees and trainees in numbers which result in the employment of advanced trainees and trainees as a percentage of the total workforce for the construction trade, which percentage significantly exceeds the apprentice to journey worker ratio specified in the applicable collective bargaining agreement, or in the absence of a collective bargaining agreement, exceeds the ratio established by practice in the area for said construction trade.  Also, the contractor or subcontractor agrees that, in implementing the procedures of (B) above, it shall, where applicable, employ minority and women workers residing within the geographical jurisdiction of the union.

After notification of award, but prior to signing a construction contract, the contractor shall submit to the public agency compliance officer and the Dept. of LWD, Construction EEO Monitoring Program an initial project workforce report (Form AA-201) electronically provided to the public agency by the Dept. of LWD, Construction EEO Monitoring Program, through its website, for distribution to and completion by the contractor, in accordance with N.J.A.C. 17:27-7. 

The contractor also agrees to submit a copy of the Monthly Project Workforce Report once a month thereafter for the duration of this contract to the Dept. of LWD, Construction EEO Monitoring Program and to the public agency compliance officer.

The contractor agrees to cooperate with the public agency in the payment of budgeted funds, as is necessary, for on the job and/or off the job programs for outreach and training of minorities and women.

(D)	The contractor and its subcontractors shall furnish such reports or other documents to the  Dept. of LWD, Construction EEO Monitoring Program as may be requested by the Dept. of LWD, Construction EEO Monitoring Program from time to time in order to carry out the purposes of these regulations, and public agencies shall furnish such information as may be requested by the Dept. of LWD, Construction EEO Monitoring Program for conducting a compliance investigation pursuant to N.J.A.C. 17:27-1.1 et seq.


EXECUTIVE ORDER NO. 151 REQUIREMENTS

It is the policy of the Division of Purchase and Property that its contracts should create a workforce that reflects the diversity of the State of New Jersey. Therefore, contractors engaged by the Division of Purchase and Property to perform under a construction contract shall put forth a good faith effort to engage in recruitment and employment practices that further the goal of fostering equal opportunities to minorities and women. 

The contractor must demonstrate to the Division of Purchase and Property’s satisfaction that a good faith effort was made to ensure that minorities and women have been afforded equal opportunity to gain employment under the Division of Purchase and Property’s contract with the contractor. Payment may be withheld from a contractor’s contract for failure to comply with these provisions. 

Evidence of a “good faith effort” includes, but is not limited to:

1. The Contractor shall recruit prospective employees through the State Job bank website, managed by the Department of Labor and Workforce Development, available online at http://NJ.gov/http://NJ.gov/JobCentralNJ; 
2. The Contractor shall keep specific records of its efforts, including records of all individuals interviewed and hired, including the specific numbers of minorities and women;
3. The Contractor shall actively solicit and shall provide the Division of Purchase and Property with proof of solicitations for employment, including but not limited to advertisements in general circulation media, professional service publications and electronic media; and 
4. The Contractor shall provide evidence of efforts described at 2 above to the Division of Purchase and Property no less frequently than once every 12 months. 
5. The Contractor shall comply with the requirements set forth at N.J.A.C. 17:27. 

This language is in addition to and does not replace good faith efforts requirements for construction contracts required by N.J.A.C. 17:27-3.6, 3.7 and 3.8, also known as Exhibit B.
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