Exhibit B: Specification

PENNDOT is asking vendors to provide a quote on the below single wall brine storage tanks.
All tanks must meet the below specifications:
· All tanks must be single walled construction
· All tanks must have adequate UV protection
· All Tanks are being bid as F.O.B destination to the below ship to points
· No installation service will be required.
· Tanks must be new and have a minimum Manufacturer’s Warranty period of 3 years or more.
· Minimum of 2” port 
· Number of tanks and capacities needed are listed below:

Eight (8) 5,000-gallon Brine Storage Tanks
2- 5000 Gal tanks Delivered to PennDOT Engineering District 2-0
70 PennDOT Drive, Clearfield PA 16830
 6- 5000 Gal tanks Delivered to (EPTF) Eastern PA Training Facility (EPTF)
Rt 443 Box 7042 Grantville PA 17028

Seven (7) 10,000-gallon Brine Storage Tanks
7- 10,000 Gal tank Delivered to Eastern PA Training Facility (EPTF)
Rt 443 Box 7042 Grantville PA 17028


(2)  6,100-gallon Brine Storage Tanks
 2- 6100 Gal tanks Delivered to (EPTF) Eastern PA Training Facility (EPTF)
Rt 443 Box 7042 Grantville PA 17028


All brine tanks shall be delivered to the below locations within 60 days of receipt of the Purchase Order.

[bookmark: _Hlk228274251]Eastern PA Training Facility (EPTF)
Rt 443 Box 7042 Grantville PA 17028

[bookmark: _Hlk228273923]PennDOT Engineering District 2-0
70 PennDOT Drive, Clearfield PA 16830


