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March 30, 2017


To: All Interested Vendors {Bidders} 


Re:  Bid Solicitation {RFP} # 17DPP00105
        T-3063 Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Optional Hook 
        Lift System, Various Bodies, Salt Spreader, Snow Plow & Accessories

[bookmark: _GoBack]     Original Quote {Proposal} Submission Due Date: March 30, 2017 (2:00 p.m. ET)
     Revised Quote {Proposal} Submission Due Date: April 12, 2017 (2:00 p.m. ET)

Bid Amendment {Addendum} # 2


The following constitutes Bid Amendment {Addendum} # 2 to the above referenced Bid Solicitation {RFP}:
  
· This Bid Amendment {Addendum} includes answers to questions and revisions.  
· Please note that for all additions, deletions, clarifications and modifications to the Bid Solicitation {RFP} # 17DPP00105, please refer to the Revised Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”. 

It is the sole responsibility of the Vendor {Bidder} to be knowledgeable of all of the additions, deletions, clarifications, and modifications to the Bid Solicitation {RFP} and/or the New Jersey Standard Terms and Conditions relative to this Bid Solicitation {RFP} as set forth in all Bid Amendments {Addenda}. 

All other instructions, terms, and conditions of the Bid Solicitation {RFP} shall remain the same.



T-3063 Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Optional Hook Lift   
        System, Various Bodies, Salt Spreader, Snow Plow & Accessories

Bid Solicitation {RFP} Number: 17DPP00105

Answers to Questions

Note: Some of the questions have been paraphrased in the interest of readability and clarity.  Each question is referenced by the appropriate Bid Solicitation {RFP} page number(s) and section where applicable.  

	#
	Page #
	Bid Solicitation {RFP} Section Reference
	Question
	Answer

	1
	18
	3.1
and
3.1.2
	Do to extend discounts from the various manufactures for multiple unit orders and the freight cost, how many trucks and various bodies is the NJ DOT considering ordering?
	Please refer to Section 3.1 and 3.1.2 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”. 


	2
	25
	3.4.1.16
	What size ball on the combo hitch does the NJDOT use?
	The paragraph has been changed to read as follows: 

“A combination ball/pintle hook Buyers Product model #10040 or comparable with pintle hook mounting plate must be provided. Combination ball/pintle hook with 2 5/16 inch ball shall be mounted 18” from ground. A heavy duty 2 inch receiver tube with pin must be provided on a ½ inch thick steel hitch plate. The pintle hook assembly may require an elbow to meet 18 inch height. Two (2) lunettes must be securely fastened to the hitch plate.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	3
	25
	3.4.1.18
	Safety Features and Equipment: Does the NJDOT have a minimum spec requirement and mounting location for this listed items ?« 5 lb. fire extinguisher and mount ?« Mechanical jack ?« Triangle kit ?« First aid kit
	The Safety Features and  Equipment section has been changed to read as follows:
Each unit shall include the following:

5 lb. class ABC fire extinguisher and mount. 
Mechanical jack rated to lift vehicle GVWR.

Triangle kit with one set of three triangles in a case, that meets FMVSS 125 standards.

First aid kit that meets ANSI Z308.1 standards.

Mounting locations for all of the above to be determined at pre-production meeting.

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.


	4
	   25
	3.4.1.19
	Would a ECCO brand light with the same functions be an acceptable alternative to the Whelen Edge Freedom IV ?
	Please refer to Section 3.3.8 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	5
	28
	3.4.3
	Would a crossmemberless stainless steel {ss}dump body with a 3/16 ss floor in lue of a 10ga be an acceptable alternative ?
	The specification will not be revised.

	6
	28
	3.4.10.1
	Would a crossmemberless Domax rust resistant steel dump body with a 3/16 Hard Ox floor in lue of a 10ga be an acceptable alternative ?
	The specification will not be revised.

	7
	36
and 20
	3.4.12
and
3.3.8
	Douglas Dynamics is the parent company to Fisher, Western, & Snow Ex snow plows. All 3 brand use the same basic electrical, hydraulic and mounting technology with some minor change to each plow line. Would a Snow Ex. brand plow with the same size and functions be an acceptable alternative to the brands listed the RFP?
	Please refer to Section 3.3.8 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	8
	21
	
	What year is the truck please?
	Please refer to section 3.4.1 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	9
	
	
	What year is the truck please?
	Please see question 8.

	10
	34
	3.4.11
	Item: 3.4.11, Salt Spreader price line:11 Is it the intention of the State to require 304 stainless steel construction of the salt spreader?
	201 or 304 stainless steel construction will be acceptable.

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	11
	25
	3.4.1.15
	This section asks for two (2) Cole Hersee or comparable female trailer connectors at rear. Is this a typo?
	The specification has been modified to read as follows:

“Truck must have one (1) A.T.A. and S.A.E. approved, 7-wire trailer connector (female type), Cole Hersee 12080 or comparable. Connector must be mounted on the rear bumper with cover provided.  Wiring must conform to A.T.A. color code.  All wiring must be protected from salt and corrosion.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	12
	28
	3.4.3.1
	States: Cabshield shall be 1/4 inch stainless steel. I believe this should say "Quarter (1/4) style" which is approximately 12'15" typical extension?
	The specification has been modified to read as follows: 

“Cab shield shall be ¼ style, stainless steel.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	13
	35
	3.4.11.2
	Lever action feedgate requested would be standard equipment on conveyor style spreaders of this size and type. Due to limited size of auger opening feedgates are not required with these models. Speed of auger will be regulate material flow. Is this method acceptable?
	The specification has been modified and the following paragraph has been removed:

“A lever action style stainless steel feed gate shall be provided in the rear wall of the hopper. The feed gate shall have a maximum opening of 70 square inches, and a clamp to allow for a positive gate setting.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	14
	28
	3.4.3
	Is there a specific stainless steel required?
	304 stainless steel is required.

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	15
	28
	3.4.3
	Are there any specifications or requirements on the tailgate latch mechanism available?
	The specification has been modified to read as follows:

“Tailgate control lever shall be located at the front end of the body at the driver’s side. Lever shall be vertical in latched position and offset as required.”
  
Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	16
	28



	3.4.3.1
	The hook lift longitudinal shall be 6 inches x 24 inches x 1/4 inch thick steel, primed and painted black. Could you please confirm the dimensions of the hook life longitudinal? What attributes does each dimension describe (length,height, width)?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	17
	28
	3.4.3.1
	The dump body and tailgate shall be stainless steel. Dump body shall be of standard single wall construction. The top sides of the body shall have 24 inch x 8 inch hardwood boards and have two intermediate vertical side braces, plus 6 inch front and rear board pocket extension pockets.Could you please confirm the dimensions of the hardwood boards? 24 inch appears to be an error.
	The specification has been modified to read as follows:

“The top sides of the body shall have 2 inch x 8 inch hardwood boards and have two intermediate vertical side braces, plus 6 inch front and rear board pocket extension pockets. “

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	18
	28
	3.4.3.1
	Cab shield shall be 1/4 inch stainless steel. What is the Cab shield height to the Chassis? Does the entire Cab Shield require 1/4 inch steel?
	The specification has been modified to read as follows:

“Cab shield shall be at a height that does not interfere with equipment movement or the cab safety lighting.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	19
	28
	3.4.3.1
	The floor shall be 10-gauge thick. Is the 10-gauge floor steel or stainless steel?
	The specification has been modified to read as follows:

“The floor shall be 10-gauge thick stainless steel.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	20
	28
	3.4.3.1
	The cross members shall be 3 inch structural steel channel spaced on 12 inch centers and full width rear bolster.What is the paint specifications for the floor and cross members?
	The correct Bid Solicitation {RFP} Section Reference is 3.4.3.1

The specification has been modified to read as follows: 

“Cross members shall be painted with corrosion resistant paint.”

Section 3.3.5.1 has been modified to read as follows: 

“Unless otherwise indicated in the specification the Cab, chassis and bodies shall be finished as indicated below. All stainless steel components shall remain unpainted.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	21
	28
	3.4.3.1
	A two-way gate shall be provided with heavy duty cast stainless steel hardware, one (1) set of banjo eyes and chains with abrasion resistant covers.Can heavy duty, fabricated (from stainless plate) be used in lieu of heavy duty cast stainless?
	The specification has been modified to read as follows:

“A two-way gate shall be provided with heavy duty cast or fabricated stainless steel hardware, one (1) set of banjo eyes and chains with abrasion resistant covers”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	22
	  26
	3.4.2.1
	Will you require a shipping weight not to exceed 1500# to maximize payload?
	The specification will not be revised.

	23
	  26
	3.4.2.2
	Will you require the hook close and latch when hook is in transport position for safety?
	The specification was modified in Section 3.4.2.2 to read as follows:

“A positive locking system must be supplied to prevent the body from moving rearward in the event that a hydraulic line fails.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	24
	27
	3.4.2.3
	Will you require a whisker switch to verify position of load that would work better than lines painted on and may not be visible on framerails?
	Please refer to Section 3.4.2.2 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	25
	27
	3.4.3
	Will you require the dump body be manufactured from 304 stainless for maximum resistance to corrosion and staining?
	Please refer to question number 14.

	26
	28
	3.4.3.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	27
	29
	3.4.4.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	28
	29
	3.4.5.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	29
	30
	3.4.6.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	30
	31
	3.4.7.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	31
	31

	3.4.8.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	32
	32
	3.4.1.8
	What "metal" material shall the tank cradle be? Aluminum or steel?
	The correct Bid Solicitation {RFP} section reference is 3.4.8.2.

The specification has been modified to read as follows:

“Metal cradle shall be fabricated from steel or aluminum.” 

“If steel fabricated cradle is offered it shall be powder coated or painted with corrosion resistant paint.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	33
	32
	3.4.8.3
	Does the NJDOT require an electronic, multiprocessor based spray control system?
	Section 3.4.13 has been modified to answer this question as follows:

“The in-cab controller shall be compatible with and ensure full functionality of herbicide sprayer and applicable components.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	34
	31
	3.4.8.1
	Is the correct Longitudinal 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	35
	32
	3.4.1.8
	What "metal" material shall the tank cradle be? Aluminum or steel?
	Please refer to the answer to question 32.

	36
	32
	3.4.8.3
	Does the NJDOT require an electronic, multiprocessor based spray control system?
	Please refer to the answer to question 33.

	37
	32
	3.4.8.3
	What does the NJDOT require for Range of spray width in feet?
	Please refer to Section 3.4.8.2  of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	38
	32
	3.4.8.3
	What does the NJDOT require for Range of speed in MPH that spraying is desired?
	Less than 20 MPH.

	39
	32
	3.4.8.3
	What does the NJDOT require for Range of flow rate requires in Gallons per Acre or Per lane mile for each head?
	The correct Bid Solicitation {RFP} Section is 3.4.8.2

The specification has been changed to read as follow:

 “A gasoline powered engine, pump and sprayer shall be properly sized to meet the spray volume of 5 to 125 gallons per acre or more on swath widths of 5 to 40 feet with accuracy.”

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	40
	32
	3.4.8.3
	Do both spray heads need to operate and be controlled simultaneously?  

	No.

	41
	-
	3.4.8.3
	Does the NJDOT require GPS mapping?
	No.

	42
	-
	3.4.8.3
	Does the NJDOT require the inclusion of accessories for adding chemical injection pumps?
	No.

	43
	33
	3.4.9.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	44
	34
	3.4.10.1
	Is the correct Longitudinal dimension 5.5 x 2 x 1/4" thick cut to length?
	The specification has been modified to read as follows:

“The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black.” 

Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	45
	35
	3.4.11.1
	Remove Meyers Brand and Model number from bid as prejudicial. Chassis dealer, unsure of alternatives, seldom consider "or equal" as equal?  
	Please refer to Section 1.4.2 and Section 3.3.8 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	46
	34
	3.4.11.1
	Length of spreader hopper is inconsistent with the hooklift frame length. 8' as specified it would need to sit far rearwards to get spinner out over rear roller and bumper. Would the NJDOT modify the request to require a 10' hopper to allow more of salt load to be forward of axle?
	The specification has been modified to read as follows:

“It is the intent of this section to describe the specifications for a 108 inch- 120 inch, medium duty, 4.0 cubic yard V-box electric salt spreader with single auger, Meyers MDV-A 944 Electric 9’ SS, Part # 64539 or comparable. The salt spreader must be capable of hauling and spreading free flowing granular materials. The salt spreader and hook lift frame assembly must be compatible with the hook lift system specified in Section 3.4.2.”
 
Please see revisions to and utilize the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	47
	35
	3.4.11.2
	Does the NJDOT intend to require 304 stainless steel construction for the spreader?
	See answer to question 10.

	48
	35
	3.4.11.4
	Does the flip up spinner need to flip backwards?  
	Yes. 

	49
	18
	3.1.1
	What is the term of this Blanket P.O and Contract?
	Please refer to Section 5.2 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	50
	18
	3.1.1
	Is there an opportunity for pricing adjustments for increase commodity costs through the term?
	Please refer to Section 5.2.1 of the Bid Solicitation {RFP} titled “Revised 17DPP00105 Universal Truck RFP 3.22.17”.

	51
	25
	3.4.1.19
	Would the NJDOT specify and require an LED spotlight?
	No. The light bar, as specified in Section 3.4.1.19, is configured with rear facing spot lights.
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