ROOF INSTALLATION AND SHINGLE SPECKS:
BID TO TEAR OFF ALL LAYERS OF OLD SHINGLES, REPLACE ANY BAD DECKING, REPLACE WITH HERITAGE OR BETTER DIMENSIONAL SHINGLES, INSTALL NEW FELT, (SQUARE D DRIP EDGE 1 ½” X 3” WITH 1” PROJECTION FROM FASCIA EDGE), VALLEY METAL, ROOF JACKS, RIDGE VENTS. HAUL OFF ALL OLD MATERIAL. INSTALL ALL VENT PIPES BACK LEVEL AND CONNECTED TO DEVICE CORRECTLY. 
