Questions and answers:



1) what location will this be set at? WWTP- 1100 Fall-Line FWY - Please see attached map for unit placement.
2) Is the area staked off to be able to determine elevations? The unit will be placed in front of existing building.
3) what utilities are there and will connection to these be required in the price? The Utility connections will be provided by the city.
4) are there specs as to the gauge of the metal or profile used? The metal for the roof will need to be 14 gauge in thickness and the side walls can be 16-18 gauge 

5) should the power to the unit be a plug in for temporary use, or should it be wired for permanent power? if temporary, what type 240v, 50amp? 240v, 30amp. If permanent should there be a panel box installed with an exterior disconnect? The unit needs to be wired for permanent use. The power panel 125-amp 120/240- volt single phase

6) the rendering shows a bathroom, are there any specific info as to fixture types or brands? The bathroom fixtures need to be of good quality.  
7) Does the trailer have to be left with tongue, axles, wheels, and tires or can those be removed before underpinning? The wheels, axles and tongue will need left with the unit for future use
8) the rendering seems to show coffee/snack area, is this a requirement? If so, what are the dimensions? There will be no breakroom area as shown in the drawings.
