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	Bid Solicitation #
	24DPP01013

	T0896 - Asphaltic Oil and Aggregate Surface Treatment - Statewide



	
	Date
	Time

	Due Date For Electronic Questions
Refer to Bid Solicitation Section 2.1 for more information.
	                   7/9/2024
	2:00 PM

	Optional Pre-Quote Submission Conference 
Refer to Bid Solicitation Section 2.5 for more information.
	6/27/2024
	11:00 AM

	Mandatory/Optional Site Visit
Refer to Bid Solicitation Section 2.4 for more information.
	
N/A
	
N/A

	Quote Opening Date
Refer to Bid Solicitation Section 3 for more information.
	8/28/2024
	2:00 PM



Dates are subject to change.  All times contained in the Bid Solicitation refer to Eastern Time. 
All changes will be reflected in Bid Amendments to the Bid Solicitation posted on www.njstart.gov.

	SET-ASIDES

	     Small Business Set-Aside
For Goods and Services:
☒  I          ☒  II          ☒  III
For Construction:
☐  IV          ☐  V          ☐  VI
	☐  Not Applicable
☐  Entire Contract 
☒  Partial Contract 
☐  Subcontracting Only
☐  Preference

	     Disabled Veteran-Owned Business Set-Aside
	☒  Not Applicable
☐  Entire Contract 
☐  Partial Contract 
☐  Subcontracting Only
☐  Preference



	Bid Solicitation Issued By:
State of New Jersey
Department of the Treasury
Division of Purchase and Property
Trenton, New Jersey 08625‑0230
	On Behalf of:
State of New Jersey
Department of Environmental Protection
Cooperative Purchasing Participants



Date:  6/13/2024
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[bookmark: _Toc169179867]INTRODUCTION AND SUMMARY OF THE BID SOLICITATION
This Bid Solicitation is issued by the Department of the Treasury, Division of Purchase and Property (Division), Procurement Bureau, on behalf of Department of Environmental Protection. Quotes submitted in response to this Bid Solicitation shall be through the State of New Jersey’s eProcurement system, NJSTART.  Bidders are advised to thoroughly read all sections of this Bid Solicitation and follow all instructions.  

Bidders are strongly encouraged to visit the NJSTART Vendor Support Page, which contains Quick Reference Guides (QRGs), supporting videos, a glossary of NJSTART terms, and helpdesk contact information.  Bidders should utilize the QRGs before attempting to submit a Quote through NJSTART.   It is the Bidder’s responsibility to ensure that the Quote and attachments have been properly submitted.  Inquiries concerning the use of NJSTART may be directed to njstart@treas.nj.gov. The Division will not respond to substantive questions related to the Bid Solicitation or any other Contract via this email address.

[bookmark: _Toc400531467][bookmark: _Toc428533937][bookmark: _Toc32310614][bookmark: _Toc169179868]PURPOSE AND INTENT
The purpose of this Bid Solicitation is to solicit Quotes for Asphaltic Oil and Aggregate Surface Treatment for paving pathways and other small confined spaces.

It is the intent of the State to award Contracts to those responsible Bidders whose Quotes, conforming to this Bid Solicitation are most advantageous to the State of New Jersey (State), price and other factors considered.  The State may award any or all price lines.  The State, however, reserves the right to separately procure individual requirements that are the subject of the Contract during the Contract term, when deemed by the Director of the Division (Director) to be in the State’s best interest.

There are eight (8) price lines, which are divided by four (4) regions and itemized as follows:

	Region Number
	Price Line Number
	Item Description

	Region 1
(Price Lines 1-2)



	1

	Asphaltic Oil and Aggregate Surface Treatment: Region 1 Consists of Burlington, Camden, Gloucester, Salem, Cumberland, Atlantic, and Cape May Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	2
	Asphaltic Oil and Aggregate Surface Treatment: Region 1 Consists of Burlington, Camden, Gloucester, Salem, Cumberland, Atlantic, and Cape May Counties.
This Price Line Item is for Method 2 – Single Coat Application.

	
	
	

	Region 2
(Price Lines 3-4)
	3
	Asphaltic Oil and Aggregate Surface Treatment: Region 2 Consists of Essex, Union, Mercer, Hunterdon, Somerset, and Warren Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	4

	Asphaltic Oil and Aggregate Surface Treatment: Region 2 Consists of Essex, Union, Mercer, Hunterdon, Somerset, and Warren Counties.
This Price Line Item is for Method 2 – Single Coat Application.

	
	
	

	Region 3
(Price Lines 5-6)
	5

	Asphaltic Oil and Aggregate Surface Treatment: Region 3 Consists of Sussex, Bergen, Warren, Morris, and Passaic Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	6
	Asphaltic Oil and Aggregate Surface Treatment: Region 3 Consists of Sussex, Bergen, Warren, Morris, and Passaic Counties.
This Price Line Item is for Method 2 – Single Coat Application.

	
	
	

	Region 4
(Price Lines 7-8)
	7
	Asphaltic Oil and Aggregate Surface Treatment: Region 4 Consists of Monmouth, Middlesex, Hudson, and Ocean Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	8

	Asphaltic Oil and Aggregate Surface Treatment: Region 4 Consists of Monmouth, Middlesex, Hudson, and Ocean Counties.
This Price Line Item is for Method 2 – Single Coat Application.



The State intends to make one (1) award per Region (Region 1, Region 2, Region 3, and Region 4), and each Region shall be awarded separately or any combination thereof. For each Region bid, the Bidder must be capable of providing services to any location as listed in Section 1.2.1 of this Bid Solicitation.

Bidders must bid on all price lines contained within a Region (example: Region 1 priclines 1 – 2) in order to be considered responsive for that region. If a Bidder does not bid on all price lines within a region, its Quote will be considered non-responsive for that region only.

Bidders may submit a Quote for one, multiple, or all regions.

The State of New Jersey Standard Terms and Conditions (SSTCs) included with this Bid Solicitation will apply to all Contracts made with the State.  These terms are in addition to the terms and conditions set forth in this Bid Solicitation and should be read in conjunction with them unless the Bid Solicitation specifically indicates otherwise.  

[bookmark: _Toc400531468][bookmark: _Toc428533938][bookmark: _Toc32310615][bookmark: _Toc169179869]BACKGROUND 
This is a reprocurement of the services under Asphaltic Oil and Aggregate Surface Treatment.  Bidders interested in reviewing the current Contract specifications and pricing information may do so by following the instruction below.  Bidders should not rely upon or use data or information from the contract when preparing a response to this Bid Solicitation as this Bid Solicitation addresses the State’s current requirements. 
· Go to: www.njstart.gov 
· Select “Active Blankets”
· In the search bar, select “Blankets” from the drop down menu
· Enter the T0896 and click “[image: ]”
· The current Contract list will appear under “Results”.

[bookmark: _Toc160454742][bookmark: _Toc169179870]GEOGRAPHICAL REGIONS
For the purpose of this Bid Solicitation, the State shall be divided into four (4) separate regions. Each region shall be referred to as the following:
· Region one (1);
· Region two (2);
· Region three (3); and
· Region four (4).
Each region contains anywhere between four (4) to seven (7) counties.
[bookmark: _Toc531776170][bookmark: _Toc160454743][bookmark: _Toc169179871]FOUR (4) REGIONS:  RESPECTIVE COUNTIES AND LOCATIONS:

	Counties Within Region

	Region One (1)
	Region Two (2)
	Region Three (3)
	Region Four (4)

	Burlington 
	Essex 
	Sussex 
	Monmouth 

	Camden 
	Union 
	Bergen 
	Middlesex 

	Gloucester 
	Mercer 
	Warren
	Hudson

	Salem 
	Warren 
	Morris 
	Ocean 

	Cumberland
	Hunterdon 
	Passaic 

	Atlantic 
	Somerset 

	Cape May 




	Locations Within Region

	Region One (1)
	Region Two (2)
	Region Three (3)
	Region Four (4)

	Atsion (Wharton State Forest)
	Allamuchy Mountain Park
	Edison State Park
	Allaire State Park

	Bass River State Forest
	Bull's Island State Park
	Hacklebarney State Park 
	Barnegat Lighthouse State Park

	Belle Plain State Forest
	Delaware Raritan State Park
	High Point State Park
	Cheesequake State Park

	Cape May Point Park
	Princeton Battleground State Park 
	Hermitage House historic site
	Double Trouble State Park

	Corson's Inlet State Park
	Round Valley State Park
	Hopatcong State Park
	

	Fort Mott State Park 
	Spruce Run State Park 
	Jenny Jump State Forest
	Forked River State Marina

	Hancock House 
	Voorhees State Park 
	Ramapo Mountain Forest
	Island Beach State Park

	Indian King Tavern 
	Washington Crossing State Park 
	Ringwood State Park
	Leonardo State Marina

	Lebanon State Forest 
	Rockingham Washington Headquarters 
	Stokes State Forest
	Liberty State Park

	Parvin State Park 
	Morven House historic site 
	Swartswood State Park
	Monmouth Battlefield State Park

	Penn State Forest 
	Clark House historic site 
	Wawayanda State Park
	Spring Meadow Golf Course

	Rancocas 35 State Park 
	Old Dutch Parsonage historic site 
	Worthington State Forest
	Washington Rock State Park

	Walt Whitman House 
	Wallace House historic site 
	Baron von Steuben historic site
	Boxwood Hall historic site

	Wharton State Forest 
	Drumwacket-Governers residence 
	
	Craig House Historic site

	Somer's Mansion historic site 
	Grover Cleveland Historic site 
	
	Twinlights historic site



[bookmark: _Toc169179872]CONTRACT AMOUNT
The estimated amount of the Contract, if stated, shall not be construed as either the maximum or minimum amount which the State shall be obliged to order.

[bookmark: _Toc400531506][bookmark: _Toc428533977][bookmark: _Toc32310702][bookmark: _Toc169179873]ORDER OF PRECEDENCE OF CONTRACTUAL TERMS
The Contract awarded, and the entire agreement between the parties, as a result of this Bid Solicitation shall consist of:  (1) the final Bid Solicitation, (2) the State of New Jersey Standard Terms and Conditions, (3) the Quote, and if applicable (4) any Bidder responses to clarifications; (5) a Bidder’s Best and Final Offer, (6) other negotiated document, and/or (7) third party document.  In the event of a conflict in the terms and conditions among the documents comprising this Contract, the order of precedence, for purposes of interpretation thereof, listed from highest ranking to lowest ranking as noted above. 

Any other terms or conditions, not included with the Bidder’s Quote and accepted by the State, shall not be incorporated into the Contract awarded.  Any references to external documentation, including those documents referenced by a URL, including without limitation, technical reference manuals, technical support policies, copyright notices, additional license terms, etc., are subject to the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Conditions.  In the event of any conflict between the terms of a document incorporated by reference, the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Conditions shall prevail.

[bookmark: _Toc169179874]INTRASTATE COOPERATIVE PURCHASING
The State intends to extend the Contracts awarded to the State's Intrastate Cooperative Purchasing Participants.  Although the State is making the use of any Contract resulting from this Bid Solicitation available to Intrastate Cooperative Purchasing Participants, The State makes no representation as to the acceptability of the Bid Solicitation’s terms and conditions to any Intrastate Cooperative Purchasing Participants.

[bookmark: _Toc169179875]PRE-QUOTE SUBMISSION INFORMATION
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote and for reviewing the Quote submission requirements and the Scope of Work requirements.  

[bookmark: _Toc428533940][bookmark: _Toc32310617][bookmark: _Toc169179876]ELECTRONIC QUESTION AND ANSWER PERIOD
The Division will electronically accept questions and inquiries from all potential Bidders via the “Q&A” Tab of the Bid Solicitation in NJSTART.  Questions should be directly tied to a Bid Solicitation Section, the State-Supplied Price Sheet, Form or Attachment; and should reference the specific Bid Solicitation Section or document to which it relates.

The cut-off date for electronic questions and inquiries relating to this Bid Solicitation is indicated on the Bid Solicitation cover page.  In the event that questions are posed by Bidders, answers to such questions will be issued by Bid Amendment.  
[bookmark: _1.3.3__Mandatory_Pre-Bid_Conference][bookmark: _1.3.5__SUBMISSION_OF_BID_PROPOSAL][bookmark: _1.3.2_SUBMISSION_OF_BID_PROPOSAL]
A Bidder shall not contact the Using Agency and/or the Procurement Specialist directly, in person, by telephone or by e-mail, concerning this Bid Solicitation, prior to Contract award.

[bookmark: _Toc169179877]EXCEPTIONS TO THE STATE OF NJ STANDARD TERMS AND CONDITIONS (SSTC)
Questions regarding the State of New Jersey Standard Terms and Conditions and exceptions to mandatory requirements MUST be posed during the Electronic Question and Answer period and shall contain the Bidder’s suggested changes and the reason(s) for the suggested change(s).

[bookmark: _Toc169179878]BID AMENDMENTS
In the event that it becomes necessary to clarify or revise this Bid Solicitation, such clarification or revision will be by Bid Amendment.  Any Bid Amendment will become part of this Bid Solicitation and part of any Contract awarded. Bid Amendments will be posted as a file attachment on the “Summary” page of the Bid Solicitation in NJSTART after the cut-off date.  

There are no designated dates for release of Bid Amendments.  Those Bidders who are on the bid holder list either through commodity code registration in NJSTART or by acknowledging the bid in NJSTART should receive notification of any Bid Amendment(s). If a Bidder is not on the bid holder list, Bid Amendments are still viewable on the “Summary” page of the Bid Solicitation in NJSTART.

It is the sole responsibility of the Bidder to be knowledgeable of all Bid Amendments related to this procurement. An interested Bidder should check the NJSTART “Open Bids” Tab on a daily basis to ensure review of the most updated information.

[bookmark: _1.3.4_MANDATORY/OPTIONAL_SITE][bookmark: _1.3.45_MANDATORY/OPTIONAL_SITE][bookmark: _Toc224543885][bookmark: _Toc238623352][bookmark: _Toc400531474][bookmark: _Toc428533944][bookmark: _Toc32310620][bookmark: _Toc169179879]MANDATORY/OPTIONAL SITE VISIT
Not applicable to this procurement.

[bookmark: _1.3.5__MANDATORY/OPTIONAL][bookmark: _1.3.6__MANDATORY/OPTIONAL][bookmark: _OPTIONAL_PRE-QUOTE_CONFERENCE][bookmark: _Toc224543888][bookmark: _Toc238623354][bookmark: _Toc428533945][bookmark: _Toc32310621][bookmark: _Toc169179880]OPTIONAL PRE-QUOTE CONFERENCE
The date and time of the Optional Pre-Quote Conference is indicated on the Bid Solicitation cover sheet. Attendees may attend the Optional Pre-Quote Conference with the following call-in details:
Join the meeting now
Meeting ID: 254 124 916 235
Passcode: Qmis6o
To call in, audio only, to the optional Pre-Quote Conference:
                                                                                               United State: +1-856-338-7074
Access Code: 848 644 92#
The Optional Pre-Quote Conference may be recorded.
The purpose of the Optional Pre-Quote Conference is to address procedural questions regarding the Bid Solicitation and Bidder Quote Submission Requirements only. No substantive questions regarding the Bid Solicitation Scope of Work will be accepted or answered during the pre-Quote conference. All questions are to be submitted during the Electronic Question and Answer Period.

[bookmark: _Toc95619434][bookmark: _Toc109701220][bookmark: _Toc225321579][bookmark: _Toc400531476][bookmark: _Toc428533946][bookmark: _Toc32310622][bookmark: _Toc94946029][bookmark: _Toc72744593][bookmark: _Toc169179881]PRE-QUOTE DOCUMENT REVIEW 
Not applicable to this procurement.

[bookmark: _Toc169179882]QUOTE SUBMISSION REQUIREMENTS

[bookmark: _Toc169179883]QUOTE SUBMISSION 
In order to be considered for award, the Quote must be received electronically by the Division’s Proposal Review Unit, through NJSTART, by the required date and time. 

The date and time of the Quote opening are indicated on the Bid Solicitation cover sheet and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  If the Quote opening deadline has been revised, the new Quote opening deadline will be shown on the posted Bid Amendment and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  Quotes not received prior to the Quote opening deadline shall be rejected.

Quotes will be publicly opened and announced by telephone conference on the date and time of the quote opening. 
(Dial-in phone number: 888-204-5984 / Access code: 2602305)

When submitting a Quote through NJSTART, do not use any symbols (i.e., #, @, $, &, *) in the filename as this may prevent the Quote from being properly uploaded.  Uploaded files must be compatible with Microsoft Office and/or Adobe software applications. DO NOT UPLOAD files with extensions such as .zip, .numbers, or .pages.

When uploading the documents to NJSTART, the Bidder should select the “Confidential” option in NJSTART for attachments on the “Attachments” Tab to request that the documents not be displayed publicly through NJSTART. Marking an attachment as "Confidential" in NJSTART shall not constitute the Bidder's designation of the attachment as exempt from public disclosure under the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know.

[bookmark: _Toc169179884]BIDDER RESPONSIBILITY
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote in response to this Bid Solicitation.  No special consideration will be given after Quotes are opened because of a Bidder’s failure to be knowledgeable as to all of the requirements of this Bid Solicitation.  The State assumes no responsibility and bears no liability for costs incurred by a Bidder in the preparation and submittal of a Quote in response to this Bid Solicitation or any pre-contract award costs incurred.

[bookmark: _Toc169179885]ANNOUNCEMENT OF QUOTE INFORMATION
On the date and time Quotes are due under the Bid Solicitation, all information concerning the Quotes submitted may be publicly announced and shall be available for inspection and copying except otherwise noted:  
A. Information appropriately designated as proprietary and/or confidential in a Bidder’s Quote shall not be available for inspection and copying; and
B. Where negotiation is contemplated, only the names and addresses of the Bidders submitting Quotes will be announced, and the contents of the Quotes shall not be available for inspection and copying until the Notice of Intent to Award is issued by the Director. 

[bookmark: _Toc169179886]QUOTE ERRORS
In accordance with N.J.A.C. 17:12-2.11 “Proposal errors,” a Bidder may withdraw its Quote as described below.

[bookmark: _Toc169179887]QUOTE WITHDRAWAL PRIOR TO QUOTE OPENING
A Bidder may withdraw its Quote submission in NJSTART prior to the Quote opening; however, Bidders should note that while withdrawn NJSTART Quotes remain viewable by the Bidder on its Vendor Profile Homepage, they are removed from the Division’s view and cannot be considered for Contract award. The Bidder may submit a revised Quote as long as the Quote is received prior to the announced date and time for Quote submission. Bidders may refer to the QRG “Submit a Quote” for additional instructions.

[bookmark: _Toc169179888]QUOTE WITHDRAWAL AFTER QUOTE OPENING, BUT PRIOR TO CONTRACT AWARD
If, after the Quote opening, but before Contract award, a Bidder discovers an error in its Quote, the Bidder may make a written request to the Procurement Bureau to withdraw its Quote, or a portion thereof, from consideration for award.  If the Bidder’s request to withdraw is made in good faith, and the State will not be significantly prejudiced by granting the withdrawal of the Quote beyond the loss of the benefit of the bargain to the State of the withdrawing Bidder’s offer, the request shall be granted.  Evidence of the Bidder’s good faith in making this request can be demonstrated by one (1) or more of the following factors: A mistake is so significant that to enforce the Contract resulting from the Quote would be unconscionable; that the mistake relates to a material feature or term of the Contract; and that the mistake occurred notwithstanding the Bidder’s exercise of reasonable care.  After Quote opening, while pursuant to the provisions of this section a Bidder may request to withdraw its Quote and the Director may in his/her discretion allow said Bidder to withdraw it, the Division also may take notice of repeated or unusual requests to withdraw by a Bidder and take those prior requests to withdraw into consideration when evaluating the Bidder’s future Quotes.

The Quote withdrawal request must include the Bid Solicitation Number, Bid Solicitation Title, and the Quote submission date and should be sent to Procurement.Bureau@treas.nj.gov.

If, during a Quote evaluation process, an obvious pricing error made by a potential Contract awardee is found, the Director or his/her designee shall issue written notice to the Bidder.  The Bidder will have up to five (5) business days after receipt of the notice to confirm its pricing.  If the Bidder fails to respond, its Quote shall be considered withdrawn, and no further consideration shall be given to it.

[bookmark: _Toc169179889]JOINT VENTURE
If a Joint Venture is submitting a Quote, the agreement between the parties relating to such Joint Venture should be submitted with the Joint Venture’s Quote.  Authorized signatories from each party comprising the Joint Venture must sign the Offer and Acceptance Page.  Each party to the Joint Venture must individually complete and comply with all the forms and certification requirements in Bid Solicitation Section 3 – Quote Submission Requirements. 

[bookmark: _Toc169179890]SMALL BUSINESS SET-ASIDE CONTRACTS
Pursuant to the provisions of N.J.S.A. 52:32-17 et seq. and N.J.A.C. 17:13 et seq. this is a full Set-Aside Contract for Category IV, V or VI for Small Businesses.  

This Bid Solicitation includes an evaluation preference for those Bidders who are registered as a Small Business Enterprise (SBE) with the Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit as of the Quote Opening Date.   

The Bidder must be registered as a qualified small business with the Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit, by the date the Quote is received and opened.   

A Bidder should verify its Small, Minority, Veteran, and Women Owned Business Certification status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Bidder’s Small, Minority, Veteran, and Women Owned Business Certification status, NJSTART provides a link to take corrective action.

If the Bidder has previously registered or been certified as a Small Business Enterprise, the Bidder should ensure it is currently registered and that its registration is active with the Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit, prior to the quote opening date, to be eligible for award.  The Bidder should ensure that it has completed the annual verification, if required.

Information, registration requirements and application are available at https://www.nj.gov/treasury/revenue/ucs.shtml.

[bookmark: _Toc169179891]DISABLED VETERANS’ BUSINESS SET-ASIDE CONTRACT 
Not applicable to this procurement.

[bookmark: _Toc169179892]BID SECURITY
Not applicable to this procurement.

[bookmark: _Toc169179893]BIDDER ADDITIONAL TERMS SUBMITTED WITH THE QUOTE
A Bidder may submit additional terms as part of its Quote.  Additional terms are Bidder-proposed terms or conditions that do not conflict with the scope of work required in this Bid Solicitation, the terms and conditions of this Bid Solicitation, or the State of New Jersey Standard Terms and Conditions.  Bidder proposed terms or conditions that conflict with those contained in the State of New Jersey Standard Terms and Conditions will render a Quote non-responsive.  It is incumbent upon the Bidder to identify and remove its conflicting proposed terms and conditions prior to Quote submission.  

Quotes including Bidder proposed additional terms may be accepted, rejected, or negotiated, in whole or in part, at the State’s sole discretion. 

If Bidder intends to propose terms and conditions that conflict with the State of New Jersey Standard Terms and Conditions, those Bidder proposed terms and conditions shall only be considered if submitted and agreed to pursuant to the electronic question and answer procedure.  Bidders shall not submit exceptions or modifications as part of the Quote or on the “Terms and Conditions” Tab through NJSTART. 

[bookmark: _Toc169179894]QUOTE CONTENT
The Quote should be submitted with the attachments organized in the following manner:
· Forms
· Technical Quote
· State-Supplied Price Sheet

A Bidder should not password protect any submitted documents. Use of URLs in a Quote should be kept to a minimum and shall not be used to satisfy any material term of a Bid Solicitation. If a preprinted or other document included as part of the Quote contains a URL, a printed copy of the information should be provided and will be considered as part of the Quote. 

[bookmark: _Toc169179895]FORMS, REGISTRATIONS AND CERTIFICATIONS TO BE SUBMITTED WITH QUOTE 
A Bidder is required to complete and submit the following forms.  As an alternative to uploading certain forms with the submitted Quote, a Bidder may complete several certifications electronically in NJSTART on the “Terms and Categories” Tab within the Vendor Profile.  Those forms that may be completed on the NJSTART “Terms and Categories” Tab are noted below. Additionally, a Bidder may attach completed forms to the Vendor Profile.  Refer to QRGs “Vendor Forms” and “Attaching Files” for additional instructions.  VENDOR QUICK REFERENCE GUIDES

OFFER AND ACCEPTANCE PAGE 
The Bidder should complete and submit the Offer and Acceptance Page with the Quote.  The Offer and Acceptance Page must be signed by an authorized representative of the Bidder.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.    

OWNERSHIP DISCLOSURE FORM 
Pursuant to N.J.S.A. 52:25-24.2, in the event the Bidder is a corporation, partnership or limited liability company, the Bidder must disclose all 10% or greater owners by (a) completing and submitting the Ownership Disclosure Form with the Quote; (b) if the Bidder has submitted a signed and accurate Ownership Disclosure Form dated and received no more than six (6) months prior to the Quote submission deadline for this procurement, the Division may rely upon that form; however, if there has been a change in ownership within the last six (6) months, a new Ownership Disclosure Form must be completed, signed and submitted with the Quote; or, (c) a Bidder with any direct or indirect parent entity which is publicly traded may submit the name and address of each publicly traded entity and the name and address of each person that holds a 10 percent or greater beneficial interest in the publicly traded entity as of the last annual filing with the federal Securities and Exchange Commission or the foreign equivalent, and, if there is any person that holds a 10 percent or greater beneficial interest, also shall submit links to the websites containing the last annual filings with the federal Securities and Exchange Commission or the foreign equivalent and the relevant page numbers of the filings that contain the information on each person that holds a 10 percent or greater beneficial interest. N.J.S.A. 52:25-24.2.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this form online in NJSTART on the “Terms and Categories” Tab.  

A Bidder’s failure to submit the information required by N.J.S.A. 52:25-24.2 will result in the rejection of the Quote as non-responsive and preclude the award of a Contract to said Bidder.

  DISCLOSURE OF INVESTMENT ACTIVITIES IN IRAN FORM
The Bidder should  submit Disclosure of Investment Activities in Iran form to certify that, pursuant to N.J.S.A. 52:32-58, neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates (as defined in N.J.S.A. 52:32-56(e)(3)), is listed on the Department of the Treasury’s List of Persons or Entities Engaging in Prohibited Investment Activities in Iran and that neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates, is involved in any of the investment activities set forth in N.J.S.A. 52:32-56(f).  If the Bidder is unable to so certify, the Bidder shall provide a detailed and precise description of such activities as directed on the form.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  

DISCLOSURE OF INVESTIGATIONS AND OTHER ACTIONS INVOLVING BIDDER FORM
The Bidder should submit the Disclosure of Investigations and Other Actions Involving Bidder Form,  with its Quote, to provide a detailed description of any investigation, litigation, including administrative complaints or other administrative proceedings, involving any public sector clients during the past five (5) years, including the nature and status of the investigation, and, for any litigation, the caption of the action, a brief description of the action, the date of inception, current status, and, if applicable, disposition.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  

MACBRIDE PRINCIPLES FORM
The Bidder should submit the MacBride Principles Form.  Pursuant to N.J.S.A. 52:34-12.2, a Bidder is required to certify  that it either has no ongoing business activities in Northern Ireland and does not maintain a physical presence therein or that it will take lawful steps in good faith to conduct any business operations it has in Northern Ireland in accordance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of their compliance with those principles.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  

SERVICE PERFORMANCE WITHIN THE UNITED STATES
The Bidder should submit a completed Source Disclosure Form. Pursuant to N.J.S.A. 52:34-13.2, all Contracts primarily for services shall be performed within the United States. If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive. 

CONFIDENTIALITY/COMMITMENT TO DEFEND
Pursuant to the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know, Quotes can be released to the public in accordance with N.J.A.C. 17:12-1.2(b) and (c).  

The Bidder should submit a completed and signed Confidentiality/Commitment to Defend Form with the Quote.  In the event that the Bidder does not submit the Confidentiality form with the Quote, the State reserves the right to request that the Bidder submit the form after Quote submission.

After the opening of sealed Quotes, all information submitted by a Bidder in response to a Bid Solicitation is considered public information notwithstanding any disclaimers to the contrary submitted by a Bidder.  Proprietary, financial, security and confidential information may be exempt from public disclosure by OPRA and/or the common law when the Bidder has a good faith, legal/factual basis for such assertion. 

When the Bid Solicitation contains a negotiation component, the Quote will not be subject to public disclosure until a notice of intent to award a Contract is announced. 

As part of its Quote, a Bidder may request that portions of the Quote be exempt from public disclosure under OPRA and/or the common law. The Bidder must provide a detailed statement clearly identifying those sections of the Quote that it claims are exempt from production, and the legal and factual basis that supports said exemption(s) as a matter of law.  The State will not honor any attempts by a Bidder to designate its price sheet, price list/catalog, and/or the entire Quote as proprietary and/or confidential, and/or to claim copyright protection for its entire Quote.  If the State does not agree with a Bidder’s designation of proprietary and/or confidential information, the State will use commercially reasonable efforts to advise the Bidder. Copyright law does not prohibit access to a record which is otherwise available under OPRA.

The State reserves the right to make the determination as to what to disclose in response to an OPRA request.  Any information that the State determines to be exempt from disclosure under OPRA will be redacted.  

In the event of any challenge to the Bidder’s assertion of confidentiality that is contrary to the State’s determination of confidentiality, the Bidder shall be solely responsible for defending its designation, but in doing so, all costs and expenses associated therewith shall be the responsibility of the Bidder. The State assumes no such responsibility or liability.  

In order not to delay consideration of the Quote or the State’s response to a request for documents, the State requires that Bidder respond to any request regarding confidentiality markings within the timeframe designated in the State’s correspondence regarding confidentiality.  If no response is received by the designated date and time, the State will be permitted to release a copy of the Quote with the State making the determination regarding what may be proprietary or confidential.

SUBCONTRACTOR UTILIZATION PLAN
Bidders intending to use Subcontractor(s) shall list all subcontractors on the Subcontractor Utilization Plan form or may list the Subcontractor(s) on the “Subcontractor” Tab in NJSTART. 

For a Quote that does NOT include the use of any Subcontractors, the Bidder is automatically certifying that, if selected for an award, the Bidder will be performing all work required by the Contract. 

If it becomes necessary for the Contractor to substitute a Subcontractor, add a Subcontractor, or substitute its own staff for a Subcontractor, the Contractor will identify the proposed new Subcontractor or staff member(s) and the work to be performed.  The Contractor shall forward a written request to substitute or add a Subcontractor or to substitute its own staff for a Subcontractor to the State Contract Manager for consideration.    The Contractor must provide a completed Subcontractor Utilization Plan, a detailed justification documenting the necessity for the substitution or addition, and resumes of its proposed replacement staff or of the proposed Subcontractor’s management, supervisory, and other key personnel that demonstrate knowledge, ability and experience relevant to that part of the work which the Subcontractor is to undertake. The qualifications and experience of the replacement(s) must equal or exceed those of similar personnel proposed by the Contractor in its Quote.  The State Contract Manager will forward the request to the Director for approval.  

NOTE: No substituted or additional Subcontractors are authorized to begin work until the Contractor has received written approval from the Director.

SMALL BUSINESS AND/OR DISABLED VETERANS’ BUSINESS SUBCONTRACTING SET-ASIDE CONTRACT 
Not applicable to this procurement.

[bookmark: _Toc169179904]RESERVED
Not applicable to this procurement.

AFFIRMATIVE ACTION
The intended Contractor and its named Subcontractor(s) must submit a copy of a New Jersey Certificate of Employee Information Report, or a copy of Federal Letter of Approval verifying it is operating under a federally approved or sanctioned Affirmative Action program.  If the Contractor and/or its named Subcontractor(s) are not in possession of either a New Jersey Certificate of Employee Information Report or a Federal Letter of Approval, it/they must complete and submit the Affirmative Action Employee Information Report (AA-302).  Information, instruction and the application are available at https://www.state.nj.us/treasury/contract_compliance/index.shtml.

[bookmark: _Toc169179906]RESERVEd
Not applicable to this procurement.
[bookmark: _Toc169179907]STATE OF NEW JERSEY SECURITY DUE DILIGENCE THIRD-PARTY INFORMATION SECURITY QUESTIONNAIRE 
Not applicable to this procurement.

BUSINESS REGISTRATION
[bookmark: OLE_LINK1]In accordance with N.J.S.A. 52:32-44(b), a Bidder and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Contract.  A Bidder should verify its Business Registration Certification Active status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Bidder’s Business Registration Certification Active status, NJSTART provides a link to take corrective action. 

[bookmark: _Toc99544656][bookmark: _Toc169179909]3.13.14	Certification of Non-Involvement in Prohibited Activities in Russia or Belarus Pursuant to P.L.2022, c.3
The Bidder should submit the Certification of Non-Involvement in Prohibited Activities in Russia or Belarus Form.  Pursuant to P.L.2022, c.3, a person or entity seeking to enter into or renew a contract for the provision of goods or services shall certify that it is not Engaging in Prohibited Activities in Russia or Belarus as defined by P.L.2002, c.3, sec. 1(e).  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
[bookmark: _Toc169179910]TECHNICAL QUOTE 
The Bidder shall describe its approach and plans for accomplishing the work outlined in the Scope of Work.  The Bidder must set forth its understanding of the requirements of this Bid Solicitation and its approach to successfully complete the Contract. The Bidder should include the level of detail it determines necessary to assist the Evaluation Committee in its review of the Bidder’s Quote.

[bookmark: _Toc169179911]BIDDER QUOTE OVERVIEW FORM
The Bidder should submit the Bidder Quote Overview Form with its Quote. The Bidder should complete all of the information requested on the form, so that the State is able to evaluate the Bidder’s ability to complete the Scope of Work.  The Bidder’s responses to the questions on the form should demonstrate to the State that the Bidder’s plans and approach to complete the Scope of Work are realistic, attainable, appropriate, and that the Bidder’s Quote will lead to the successful completion of the tasks required.

[bookmark: _Toc169179912]BIDDER DATA SHEET/FORM
The Bidder should submit the Bidder Data Sheet with its Quote.  The Bidder Data Sheet will be used to evaluate the Bidder’s ability to complete the Scope of Work.  

The Bidder should provide in its response to Part I of the Bidder Data Sheet all relevant information regarding its experience in successfully completing contracts of a similar size and scope to the work required by this Bid Solicitation.  

The Bidder must provide, in Part II of the Bidder Data Sheet, details of any negative actions taken by other contracting entities against it in the course of performing these projects including, but not limited to, receipt of letters of potential default, default, cure notices, termination of services for cause, or other similar notifications/processes.  Additionally, the Bidder should provide details, including any negative audits, reports, or findings by any governmental agency for which the Bidder is/was the contractor on any contracts of similar scope.  In the event a Bidder neglects to include this information in its Quote, the Bidder’s omission of necessary disclosure information may be cause for rejection of the Bidder’s Quote by the State.

If proposing to use a Subcontractor, the Bidder should provide as an attachment to the Bidder Data Sheet documented experience to demonstrate that each Subcontractor has successfully performed work on contracts of a similar size and scope to the work that the Subcontractor is designated to perform in the Bidder’s Quote.  The Bidder must provide a detailed description of services to be provided by each Subcontractor.  

[bookmark: _Toc169179913]MANAGEMENT OVERVIEW
The Bidder shall set forth its overall technical approach and plans to meet the requirements of the Bid Solicitation in a narrative format.  This narrative should demonstrate to the Evaluation Committee that the Bidder understands the objectives that the Contract is intended to meet, the nature of the required work, and the level of effort necessary to successfully complete the Contract.  The narrative should demonstrate that the Bidder’s approach and plans to undertake and complete the Contract are appropriate to the tasks and subtasks involved. 

Mere reiterations of Bid Solicitation tasks and subtasks are strongly discouraged, as they do not provide insight into the Bidder’s approach to complete the Contract. The Bidder’s response to this section should demonstrate to the Evaluation Committee that the Bidder’s detailed plans and approach proposed to complete the Scope of Work are realistic, attainable and appropriate, and that the Bidder’s Quote will lead to successful Contract completion.

[bookmark: _Toc169179914]CONTRACT MANAGEMENT
The Bidder should describe its specific plans to manage, control and supervise the Contract to ensure satisfactory Contract completion according to the required schedule.  The plan should include the Bidder’s approach to communicate with the State Contract Manager including, but not limited to, status meetings, status reports, etc.

[bookmark: _Toc169179915]CONTRACT SCHEDULE
The Bidder shall include a draft Contract schedule.  If key dates are a part of this Bid Solicitation, the Bidder’s schedule should incorporate such key dates and should identify the completion date for each task and sub-task required by the Scope of Work.  Such schedule should also identify the associated deliverable item(s) to be submitted as evidence of completion of each task and/or subtask.

The Bidder should identify the Contract scheduling and control methodology to be used and should provide the rationale for choosing such methodology.  

[bookmark: _Toc169179916]MOBILIZATION PLAN
Not applicable to this procurement.
[bookmark: _Toc169179917]ADDITIONAL PLAN(S)
Not applicable to this procurement.

[bookmark: _Toc169179918]ORGANIZATIONAL EXPERIENCE
The Bidder should include information relating to its organization, personnel, and experience, including, but not limited to, references, together with contact names and telephone numbers, evidencing the Bidder’s qualifications, and capabilities to perform the services required by this Bid Solicitation.  The Bidder should include the level of detail it determines necessary to assist the Evaluation Committee in its review of Bidder’s Quote.

[bookmark: _Toc169179919]LOCATION
The Bidder should include the address of where responsibility for managing the Contract will take place.  The Bidder should include the telephone number and name of the individual to contact.

[bookmark: _Toc169179920]ORGANIZATION CHARTS
The Bidder should include an organization chart, with names showing management, supervisory and other key personnel (including Subcontractor management, supervisory, or other key personnel) to be assigned to the Contract.  The chart should include the labor category and title of each such individual.

[bookmark: _Toc169179921]RESUMES
Detailed resumes should be submitted for all management, supervisory, and key personnel to be assigned to the Contract. Resumes should emphasize relevant qualifications and experience of these individuals in successfully completing Contracts of a similar size and scope to those required by this Bid Solicitation.  Resumes should include the following:
A. The individual's previous experience in completing each similar Contract;
B. Beginning and ending dates for each similar Contract;
C. A description of the Contract demonstrating how the individual's work on the completed Contract relates to the individual's ability to contribute to successfully providing the services required by this Bid Solicitation; and
D. With respect to each similar Contract, the name and address of each reference together with a person to contact for a reference check and a telephone number.

The Bidder should provide detailed resumes for each Subcontractor’s management, supervisory, and other key personnel that demonstrate knowledge, ability, and experience relevant to that part of the work which the Subcontractor is designated to perform.  

[bookmark: _Toc169179922]EXPERIENCE WITH CONTRACTS OF SIMILAR SIZE AND SCOPE
The Bidder should provide a comprehensive listing of contracts of similar size and scope that it has successfully completed, as evidence of the Bidder’s ability to successfully complete services similar to those required by this Bid Solicitation.  Emphasis should be placed on contracts that are similar in size and scope to the work required by this Bid Solicitation.  A description of all such contracts should be included and should show how such contracts relate to the ability of the firm to complete the services required by this Bid Solicitation.  For each such contract listed, the Bidder should provide two (2) names and telephone numbers of individuals for contracting party. Beginning and ending dates should also be given for each contract.

The Bidder must provide details of any negative actions taken by other contracting entities against them in the course of performing these projects including, but not limited to, receipt of letters of potential default, default, cure notices, termination of services for cause, or other similar notifications/processes.  Additionally, the Bidder should provide details, including any negative audits, reports, or findings by any governmental agency for which the Bidder is/was the contractor on any contracts of similar scope.  In the event a Bidder neglects to include this information in its Quote, the Bidder’s omission of this necessary disclosure information may be cause for rejection of the Bidder’s Quote by the State.

The Bidder should provide documented experience to demonstrate that each Subcontractor has successfully performed work on contracts of a similar size and scope to the work that the Subcontractor is designated to perform in the Bidder’s Quote.  The Bidder must provide a detailed description of services to be provided by each Subcontractor.

[bookmark: _Toc169179923]FINANCIAL CAPABILITY OF THE BIDDER
The Bidder should provide sufficient financial information to enable the State to assess the financial strength and creditworthiness of the Bidder and its ability to undertake and successfully complete the Contract.  In order to provide the State with the ability to evaluate the Bidder’s financial capacity and capability to undertake and successfully complete the Contract, the Bidder should submit the following:
A. For publicly traded companies the Bidder should provide copies or the electronic location of the annual reports filed for the two most recent years; or
B. For privately held companies the Bidder should provide the certified financial statement (audited or reviewed) in accordance with applicable standards by an independent Certified Public Accountant, including a balance sheet, income statement, and statement of cash flow, and all applicable notes for the most recent calendar year or the Bidder’s most recent fiscal year. 

If the information is not supplied with the Quote, the State may still require the Bidder to submit it.  If the Bidder fails to comply with the request within seven (7) business days, the State may deem the Quote non-responsive.

A Bidder may designate specific financial information as not subject to disclosure when the Bidder has a good faith legal/factual basis for such assertion.  The State reserves the right to make the determination to accept the assertion and will so advise the Bidder.

[bookmark: _Toc169179924]STATE-SUPPLIED PRICE SHEET INSTRUCTIONS
The Bidder must submit its pricing using the State-Supplied Price Sheet accompanying this Bid Solicitation and located on the “Attachments” Tab. 

 There are eight (8) price lines, which are divided by regions and are itemized as follows:

	Region Number
	Price Line Number
	Item Description

	Region 1
(Price Lines 1-2)



	1

	Asphaltic Oil and Aggregate Surface Treatment: Region 1 Consists of Burlington, Camden, Gloucester, Salem, Cumberland, Atlantic, and Cape May Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	2
	Asphaltic Oil and Aggregate Surface Treatment: Region 1 Consists of Burlington, Camden, Gloucester, Salem, Cumberland, Atlantic, and Cape May Counties.
This Price Line Item is for Method 2 – Single Coat Application.

	
	
	

	Region 2
(Price Lines 3-4)
	3
	Asphaltic Oil and Aggregate Surface Treatment: Region 2 Consists of Essex, Union, Mercer, Hunterdon, Somerset, and Warren Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	4

	Asphaltic Oil and Aggregate Surface Treatment: Region 2 Consists of Essex, Union, Mercer, Hunterdon, Somerset, and Warren Counties.
This Price Line Item is for Method 2 – Single Coat Application.

	
	
	

	Region 3
(Price Lines 5-6)
	5

	Asphaltic Oil and Aggregate Surface Treatment: Region 3 Consists of Sussex, Bergen, Warren, Morris, and Passaic Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	6
	[bookmark: _GoBack]Asphaltic Oil and Aggregate Surface Treatment: Region 3 Consists of Sussex, Bergen, Warren, Morris, and Passaic Counties.
This Price Line Item is for Method 2 – Single Coat Application.

	
	
	

	Region 4
(Price Lines 7-8)
	7
	Asphaltic Oil and Aggregate Surface Treatment: Region 4 Consists of Monmouth, Middlesex, Hudson, and Ocean Counties.
This Price Line Item is for Method 1 – Double Coat Application.

	
	8

	Asphaltic Oil and Aggregate Surface Treatment: Region 4 Consists of Monmouth, Middlesex, Hudson, and Ocean Counties.
This Price Line Item is for Method 2 – Single Coat Application.



The State intends to make one (1) award per Region (Region1, Region 2, Region 3, and Region 4), and each Region shall be awarded separately or any combination thereof. For each Region bid, the Bidder must be capable of providing services to any location as listed in Section 1.2.1 of this Bid Solicitation.
 
Bidders may submit a Quote for one, several or all Regions.

· Step 1 - The Bidder should enter the Bidder’s name in the field titled “Bidder Name:” located at the top of the State-Supplied Price Sheet.

· Step 2 – For Region 1, Price Lines 1 - 2, the Bidder shall insert a firm, fixed price in US dollars for Year 1, Year 2, and Year 3 in the corresponding columns titled “Unit Pricing –Year 1”, “Unit Pricing –Year 2”, and “Unit Pricing –Year 3) on the State-Supplied Price Sheet.  If a Bidder leaves the unit price column blank, it shall be considered that the Bidder provided no Quote for that price line item. 

· Step 3 - For Region 2, Price Lines 3 – 4, the Bidder shall insert a firm, fixed price in US dollars for Year 1, Year 2, and Year 3 in the corresponding columns titled “Unit Pricing –Year 1”, “Unit Pricing –Year 2”, and “Unit Pricing –Year 3) on the State-Supplied Price Sheet.  If a Bidder leaves the unit price column blank, it shall be considered that the Bidder provided no Quote for that price line item.

· Step 4 -For Region 3, Price Lines 5 – 6, the Bidder shall insert a firm, fixed price in US dollars for Year 1, Year 2, and Year 3 in the corresponding columns titled “Unit Pricing –Year 1”, “Unit Pricing –Year 2”, and “Unit Pricing –Year 3) on the State-Supplied Price Sheet.  If a Bidder leaves the unit price column blank, it shall be considered that the Bidder provided no Quote for that price line item.

· Step 5 -For Region 4, Price Lines 7 – 8, the Bidder shall insert a firm, fixed price in US dollars for Year 1, Year 2, and Year 3 in the corresponding columns titled “Unit Pricing –Year 1”, “Unit Pricing –Year 2”, and “Unit Pricing –Year 3) on the State-Supplied Price Sheet.  If a Bidder leaves the unit price column blank, it shall be considered that the Bidder provided no Quote for that price line item.

· Step 6 - The Bidder may submit pricing for all four (4) regions, one (1) region, or any combination thereof. For each region bid, the Bidder must be capable of providing services to any location as listed in Section 1.2.1 of this Bid Solicitation, in addition to any location throughout the State...

To be considered responsive, Bidders must follow the instruction on the State-Supplied Price Sheet. Failure to do so may result in rejection of its Quote. Bidders must provide firm fixed pricing for the materials and/or services listed on the State-Supplied Price Sheet. Firm fixed pricing is all-inclusive of direct cost and indirect costs, including, but not limited to, direct labor costs, overhead, fee or profit, clerical support, equipment, materials, supplies, managerial (administrative) support, all documents, reports, forms, travel, reproduction and any other costs.

Bidders must bid on all price lines contained within a group in order to be considered responsive for that group. If a Bidder does not bid on all price lines within a group, its Quote will be considered non-responsive for that group only. A blank price line will be interpreted as a “No Bid” for that price line, and not as “No Charge”.

If a bid on a price line within a region is deemed non-responsive, the entire region that price line item is part of will be deemed non-responsive, as these price lines were grouped to create a single award, with the intent that all price lines in the group will be awarded. 

Price line items are grouped for Quote evaluation purposes only.  Upon Contract award, Using Agencies will be able to order any price lines within the group individually.

Any price changes including hand written revisions or “white-outs” must be initialed.  Failure to initial price changes shall preclude a Contract award from being made to the Bidder pursuant to N.J.A.C. 17:12-2.2(a) (8).

Where the State-Supplied Price Sheet includes an estimated quantity column, Bidders are advised that estimated quantities may vary throughout the Contract term resulting from this Bid Solicitation.  There is no guaranteed minimum or maximum volume for these price lines. 

[bookmark: _Toc169179925]DELIVERY TIME AND COSTS
Unless otherwise noted elsewhere in the Bid Solicitation or State-Supplied Price sheet, all delivery times are as noted in Bid Solicitation Section 5.6 Delivery Time and Costs.  Bidder may submit alternate delivery days on the State-Supplied Price Sheet.  Alternate delivery times shall not exceed the delivery days noted in Bid Solicitation Section 5.6 Delivery Requirements, as applicable.  Quotes that exceed the delivery days of Bid Solicitation Section 4.2 Delivery Requirements may be deemed non-responsive. 

When there is a discrepancy between the delivery days listed in the General Tab in the Quote in NJSTART and the State-Supplied Price Sheet, the State-Supplied Price Sheet delivery days shall govern.  

[bookmark: _Toc169179926]CASH DISCOUNTS
The Bidder is encouraged to offer cash discounts based on expedited payment by the State.  The State will make efforts to take advantage of discounts, but discounts will not be considered in determining the price rankings of Quotes.  Should the Bidder choose to offer cash discounts, the following shall apply:
A. Discount periods shall be calculated starting from the next business day after the Using Agency has accepted the goods or services, received a properly signed and executed invoice and, when required, a properly executed performance security, whichever is latest; and
B. The date on the check issued by the State in payment of that invoice shall be deemed the date of the State's response to that invoice.

[bookmark: _Toc169179927]VOLUME DISCOUNTS
Not applicable to this procurement.

[bookmark: _Toc169179928]USE OF “NO BID” VERSUS “NO CHARGE” ON THE STATE-SUPPLIED PRICE SHEET
All price lines must be filled out in accordance with the instructions above.  If the Bidder is not submitting a price for an item on a price line, the Bidder must indicate “No Bid” on the State-Supplied Price Sheet accompanying this Bid Solicitation. If the Bidder will supply an item on a price line free of charge, the Bidder must indicate “No Charge” on the State-Supplied Price Sheet accompanying this Bid Solicitation.  A blank price line will be interpreted as a “No Bid” for that price line, and not as “No Charge”.  The use of any other identifier may result in the Bidder’s Quote being deemed non-responsive.

[bookmark: _Toc169179929]ORAL PRESENTATIONS
Not applicable to this procurement.


[bookmark: _Toc169179930]SCOPE OF WORK
[bookmark: _Toc400531507][bookmark: _Toc428533978][bookmark: _Toc32310703][bookmark: _Toc169179931]GENERAL
This Contract is for the surface paving of recreational areas with “chip and oil” type paving in constricted spaces. The Contractor must have specialized equipment that will allow for tight access in small areas like campsites and pathways. The Contractor may be required to furnish more than one crew at a time, at the discretion of the Using Agency.

1.1 [bookmark: _Toc531776196][bookmark: _Toc92529]USING AGENCY RESPONSIBILITIES
The Using Agency shall notify the Contractor by telephone with the following information:
 
· Project location;

· Required response time; and

· Approximate estimate of quantities.

1.2 [bookmark: _Toc531776197][bookmark: _Toc92530][bookmark: _Toc160454811][bookmark: _Toc169179932]CONTRACTOR RESPONSIBILITIES
[bookmark: _Toc531776198][bookmark: _Toc160454812]The Contractor must comply with the following:

· Provide all work required for the layout and construction of each project;

· Not begin work until the location and extent of the work has been verified and approved by the Using Agency; 

· Begin the project within ten (10) working days after receipt of written notification to proceed from the Using Agency;

· Advise the Using Agency at least 48 hours prior to the commencement of work; and

· Coordinate the maintenance and protection of vehicular and pedestrian traffic for all work under this Contract. All safety set-up shall conform to the “Manual On Uniform Traffic Control Devices" (MUTCD) and in conjunction with traffic control detail sheets contained in the MUTCD per http://mutcd.fhwa.dot.gov/.

· To ensure that the project remains clean, the Contractor shall: 

· Be responsible for cleaning, sweeping, and/or clearing all rubble and other foreign or loose matter immediately prior to the first application of bituminous material;  

· Be responsible for sweeping up all loose or dislodged debris generated from cleaning the area prior to the application of the asphaltic oil;  

· Dispose of any debris or matter at sites outside of the Using Agency locale;

· Acquire written permission from the property owner on whose property the material or debris is to be placed, prior to placement;

· Obtain copies of the notices of agreement from property owners who have allowed the disposal of debris on their land, which are to be shown to the Using Agency; and

· Be responsible for maintaining areas occupied by the Contractor equipment.

[bookmark: _Toc169179933]HOURS OF OPERATION
Normal hours of operation shall be from 8:00 a.m. to 3:30 p.m. The Using Agency, in its use of this Contract, reserves the right to adjust these hours due to varying conditions or scheduled events.
[bookmark: _Toc531776199][bookmark: _Toc92531][bookmark: _Toc160454813][bookmark: _Toc169179934]WORK DELAYS
The Using Agency reserves the right to postpone a project in its entirety, or halt operations already in progress, due to hazardous road and weather conditions, or public inconvenience. Work shall not be permitted to continue until conditions are deemed acceptable by the Using Agency. Acceptable working conditions include non-freezing temperatures and no rain the day of treatment.

1.3 [bookmark: _Toc531776200][bookmark: _Toc92532][bookmark: _Toc160454814][bookmark: _Toc169179935]PUBLIC CONVENIENCE AND SAFETY
· The Contractor shall, at all times, conduct its work as to result in the least possible obstruction to vehicular and pedestrian traffic. The safety and convenience of the general public and the protection of persons and property shall be directed by and in cooperation with the Using Agency;

· Precautions shall be exercised at all times for the protection of persons and property. The safety provisions of applicable laws, Occupational Safety and Health Administration (OSHA) regulations, building and construction codes, and the rules and regulations of the State’s Department of Labor and Workforce Development shall be observed; and

· The Contractor shall not occupy with its equipment, materials, or personnel, any space open to vehicular and pedestrian traffic, adjacent to the site. Only when necessary during working hours, and with approval from the Using Agency shall this be allowed.
· If approved by the Using Agency, the Contractor shall use State property adjacent to roadway or parking areas for storage of equipment and materials, provided the equipment and materials are placed behind State barriers or fences, or equipment and materials are stored at a distance away from active traffic.

1.4 [bookmark: _Toc531776201][bookmark: _Toc92533][bookmark: _Toc160454815][bookmark: _Toc169179936]EMPLOYEES, METHODS, AND EQUIPMENT
 The Contractor shall provide the following:

· Workers with sufficient skills and experience to satisfactorily perform the work assigned to them;

· Employ sufficient labor and equipment to complete all projects as per the terms of this Contract;

· At any time if any person employed by the Contractor who does not perform the work in a proper and skillful manner, or is intemperate or disorderly shall, at the written request of the Using Agency, be removed and replaced by another employee;

· All equipment which is proposed to be used on the work shall be of sufficient size and in such a mechanical condition as to meet requirements of the work and to produce a satisfactory quality of work. Equipment used on any portion of the project shall be such that no injury to adjacent property, passing vehicles, or persons results from its use; and

· Equipment shall include a self-propelled power broom apparatus for heating bituminous material, a pressure distributor, rollers, and aggregate spreading apparatus that can be adjusted to spread at the specified rate. Other equipment and small tools maybe required.

1.5 [bookmark: _Toc531776202][bookmark: _Toc92534][bookmark: _Toc160454816][bookmark: _Toc169179937]COMPACTION EQUIPMENT SHALL CONFORM TO ONE OR MORE OF THE FOLLOWING TYPES:
If a Pneumatic-tire Roller is utilized for compaction, it must be the following: 

· A self-propelled type consisting of two (2) axles equipped with pneumatic tires mounted so as to completely cover the area to be compacted in a single pass;  

· The wheels shall be capable of producing a uniform ground-contact pressure on a level, unyielding surface through a range of 60 to 95 pounds per square inch on all wheels;

· The pneumatic tire roller shall be provided with a device for wetting and cleaning the tires;

· Charts and tabulations shall be furnished showing the contact areas and contact pressures for the full range of loadings for the tires used; and

· Wobble-wheel rollers shall NOT be permitted.  

If a Dynamic Compactor is utilized for compaction it shall meet the following: 

· A vibrating compactor capable of operating at the optimum frequency of vibration required for the aggregate size and type of aggregate being compacted; 

· A calibrated vibrating reed tachometer shall be provided with each roller to permit a mechanical check of the roller vibration control system; 

· Vibratory rollers shall be of the self-propelled type and shall have at least two (2) smooth steel drums;

· Vibratory rollers shall have a static weight of no less than six and a half (6 ½) tons and shall be capable of maintaining the frequency of vibration and the amplitude specified by the manufacturer; 

· A mechanical override system shall be provided in the event of temporary failure of the automatic system which shuts off the vibration when the roller is in a stationary position; 

· Rollers shall be equipped with adjustable scrapers to keep the wheels clean and with a means of keeping the wheels moist to prevent bituminous material from sticking to the wheels;  

· Wheels shall also be free of flat areas, openings, or projections which will mar the surface; and  

· Rollers shall be capable of reversing without backlash.

If a Three-wheel 10-ton roller is utilized for compaction it shall be the following: 

· Smooth-faced power rollers, weighing no less than ten (10) tons and having a load of no-less than 330 pounds per inch of width of roller surface when all wheels are in contact with a level surface;  

· Rollers shall be equipped with adjustable scrapers to keep the wheels clean and moist to prevent bituminous material from sticking to the wheels; and  

· Wheels shall also be free of flat areas, openings, or projections which will mar the surface.

1.6 [bookmark: _Toc531776203][bookmark: _Toc92535][bookmark: _Toc160454817][bookmark: _Toc169179938]BITUMINUOUS DISTRIBUTOR
The bituminous distributor equipment shall be designed, equipped, maintained, and operated so that bituminous material at a consistent temperature may be applied uniformly on variable widths of surfaces up to 15 feet within the specified range. Distributor equipment shall include a tachometer, pressure gauges, a calibrated tank, and a thermometer for measuring temperature of tank contents. Accurate thermometers shall be placed and installed in the truck body to indicate the temperature of the bituminous material contained.
 
· The bituminous distributor equipment shall be equipped with a separate power unit for the pump, and full circulation spray bars that adjust laterally and vertically;

· The following must be furnished with each distributor:
· A gauging sheet which shows the number of the truck body, the capacity, and an outage table in increments of not over half (1/2) an inch. This gauging steel must be certified by the State’s Division of Consumer Affairs, Office of Weights and Measures.

· All tanks used for bulk storage, distribution, or delivery of bituminous materials must be equipped and sampling valves and devices shall be provided. Safe and convenient access must be provided for all sampling valves; and 

· Distribution tanks and delivery vehicle tanks shall be provided with either a submerged valve mounted in the lower half of a bulkhead, or with a valve inserted in the distributor line. The valves must be labeled "sampling valve."
[bookmark: _Toc531776204][bookmark: _Toc92536][bookmark: _Toc160454818]
1.7 [bookmark: _Toc169179939]CONSTRUCTION
· A test strip shall be completed by the Contractor with the material distribution equipment, aggregate spreading equipment, and compaction equipment prior to the commencement of operations. Operations shall only begin after it is determined that the specified material placement and compaction requirements can be obtained. The Using Agency, shall make this determination;

· Only the bituminous material shall be applied under the minimum following conditions: 
· When the surface that the material being applied to is dry, firm, and cured; 

· Between the dates of April first (1st) and November first (1st); and 

· When the temperature is above 50 degrees Fahrenheit (F). 

· The existing surface shall be cleaned of all dirt, foreign, and loose matter prior to the first application of bituminous material. This matter shall be disposed of in accordance with Section 4.3 of this Bid Solicitation. Where dirt remains that cannot be removed by the use of power brooms and/or power blowers, then at the option of the Using Agency, the surface shall be flushed with water and allowed to dry. All holes and surface deficiencies shall be repaired in advance of the treatment. 
· An estimated time for cleaning the existing surface debris, prior to first application of bituminous material, shall be provided in conjunction with the Using Agency and the Contractor. This estimation of time for cleaning the existing surface of debris shall be used as measurement for Contractor performance. The Using Agency, shall have final determination regarding ANY discrepancies in the estimation of time for the removal of such debris.
[bookmark: _Toc531776205][bookmark: _Toc92537][bookmark: _Toc160454819]
1.8 [bookmark: _Toc169179940]  BITUMINOUS TREATED SURFACES
Bituminous treated surfaces shall be prepared for surface treatment as follows: 

· Where there are indications of unstable foundation or base failure, excavation shall be made to the depth required, and the unstable material shall be removed and replaced with patch material; 

· The surface shall be patched with plant mixed bituminous mixture by cutting out the present pavement, so as to form square openings with vertical sides;  

· The openings shall be cleaned out and painted with a bituminous tack coat material, then filled with patch material which shall be compacted; and  

· The tack coat material shall be composed of emulsified asphalts conforming to section 4.10.1 of this Bid Solicitation.

[bookmark: _Toc531776206][bookmark: _Toc160454820][bookmark: _Toc169179941]EMULSIFIED ASPHALTS
Emulsified asphalts of the rapid setting (RS), medium setting (MS), and slow setting (SS) types shall conform to the American Association of State Highway and Transportation Officials (AASHTO) M 140. Please see the following link for information regarding the AASHTO: https://ihsmarkit.com/products/aashto-standards.html. 

Also, see the following link for Emulsified Asphalts: https://pavementinteractive.org/reference-desk/materials/asphalt/emulsified-asphalt/.
 Cationic Emulsified asphalts of the rapid setting (CRS), medium setting (CMS), and slow setting (CSS) types shall conform to AASHTO M 208.

[bookmark: _Toc531776207][bookmark: _Toc160454821][bookmark: _Toc169179942]CERTIFICATION OF COMPLIANCE 
· The Using Agency reserves the right to request the submission of Certifications of Compliance for any or all materials. Materials as specified will be accepted on the basis of Certificates of Compliance stating that such materials fully comply with the requirements of this Bid Solicitation. If requested, the Certificates of Compliance form shall be provided and subject to approval by the Using Agency; and  

· Materials provided on the basis of Certification of Compliance are subjected to sampling and testing at any time. If the materials do not conform with the requirements herein the Bid Solicitation, then they are subject to rejection. Upon the delivery of materials, provided by the Supplier, the Contractor shall supply two (2) copies of the originally signed Certificates of Compliance to the Using Agency, if requested. 

1.8.1.1 REQUIREMENT FOR CERTIFICATES OF COMPLIANCE 
· Project to which the material is consigned;

· Name of Contractor to which material is supplied;

· Type of material supplied;

· Quantity of material supplied;

· Means of identifying the consignment, such as label marking, seal number, etc;

· Date and method of shipment;

· Statement that the material has been tested and found in conformity with the pertinent Contract requirements stated in the certificate;

· Signature of a person having legal authority to bind the supplier must accompany the Certification of Compliance;

· The Certification of Compliance must be notarized; 

· Payments related to materials shall not be made until the Using Agency has in their possession an acceptable Certificate of Compliance;

· The State reserves the right to test any materials used on the project in a State owned laboratory to verify material compliance; and

· The State reserves the right to reject materials and any payments due for non-complying material or failure to submit Certificates of Compliance. 

1.9 [bookmark: _Toc531776208][bookmark: _Toc92538][bookmark: _Toc160454822][bookmark: _Toc169179943]BITUMINOUS MATERIALS
Bituminous materials shall either be cut-back asphalts, emulsified asphalts, or inverted emulsified asphalts. This is determined by both the Contractor and the Using Agency in conjunction, based on the condition of the subsurface that is being recoated. The grades for these types of Asphalts can be found below in Sections 4.11.1, 4.11.2, and 4.11.3. 

[bookmark: _Toc531776209][bookmark: _Toc160454823][bookmark: _Toc169179944]Cut-back asphalts Grades
Cut-back asphalts shall be grades RC-250, RC-800, RC-3000, MC-250, MC-800, and MC3000, and shall conform to Section 4.10.1 of this Bid Solicitation.

[bookmark: _Toc531776210][bookmark: _Toc160454824][bookmark: _Toc169179945]emulsified asphalts grades
Emulsified asphalts shall be grades RS-1, RS-2, CRS-1, and CRS-2, and shall conform to Section 4.10.1 of this Bid Solicitation.

[bookmark: _Toc531776211][bookmark: _Toc160454825][bookmark: _Toc169179946]inverted emulsified asphalts grades
Inverted emulsified asphalts shall be grades IEMC-250 and IEMC-800, and shall conform to Section 4.14.1.1 of this Bid Solicitation.

1.10 [bookmark: _Toc531776212][bookmark: _Toc92539][bookmark: _Toc160454826][bookmark: _Toc169179947]REQUIREMENT FOR BITUMINOUS MATERIAL AND AGGREGATE  APPLICATION  

[bookmark: _Toc531776213][bookmark: _Toc160454827][bookmark: _Toc169179948]METHOD 1 - DOUBLE COAT APPLICATION
· The first application of bituminous material shall be applied by pressure distributors at a uniform rate of 0.4 a gallon per square yard. Each application of spread shall be no less than half of the surface to be treated. Areas which are inaccessible to the distributor shall be treated either with hand sprays or pouring pots. If an area being treated requires more than one (1) pass, then the Contractor shall have a six (6) inch overlap between passes; and 
    
· Immediately after each application of bituminous material has been made, it shall be covered uniformly with size No. 6 or 67 aggregate. The aggregate shall be free of surface moisture except when asphalt emulsion is used as the bituminous material. The aggregate shall be spread from trucks equipped with mechanical spreaders or self-propelled mechanical spreaders, at a rate of 25 pounds per square yard. The second application of bituminous material shall be applied in the same manner as the first application at a uniform rate of 0.5 a gallon per square yard. Aggregate size No. 8 shall then be spread in the same manner as the first application at a rate of 25 pounds per square yard. Immediately after each application of cover aggregate, uniform coverage shall be achieved by hand-brooming. Additional aggregate shall be placed by hand on thin or bare areas.

[bookmark: _Toc531776214][bookmark: _Toc160454828][bookmark: _Toc169179949]METHOD 2 – SINGLE COAT APPLICATION
· This method shall be used when only one (1) single coat application is required and shall be applied following all the procedures described in Method #1 with bituminous material being applied at a uniform rate of 0.45 a gallon per square yard & covered with No.8 aggregate at a rate of 25 lbs. per square yard; and 

· Immediately after spreading the cover aggregate and hand-brooming where required, the entire surface shall be rolled, beginning at the edges and progressing to the center. Initial rolling shall be done with steel wheel rollers or by pneumatic tire rollers followed by a minimum of three (3) complete coverages with a pneumatic tire roller. The first application of bituminous material and aggregate shall be allowed to cure for the required length of time, before the second application. The same rolling and curing procedures required in making the first application of bituminous material and cover aggregate shall be repeated in making the second application.

[bookmark: _Toc531776215][bookmark: _Toc160454829][bookmark: _Toc169179950]Clean up procedures 
· Cleanup shall include sweeping up all quantities of loose or dislodged cover aggregate from the completed surface and along the edges of the completed surface. Disposing of the material shall be in accordance with Section 4.3 of this Bid Solicitation; and 

· At the discretion of the Using Agency, slow and controlled vehicular traffic may be permitted to use areas after the bituminous material has been covered with aggregate and cured. 

[bookmark: _Toc531776216][bookmark: _Toc160454830][bookmark: _Toc169179951]Addtional information for applying bituminous material
· [bookmark: _Toc531776217][bookmark: _Toc160454831]Both methods for applying bituminous material shall require the same tools and materials for completing the job; and 

· [bookmark: _Toc531776218][bookmark: _Toc160454832]Before any work commences, the Using Agency and the Contractor in conjunction, shall determine which method for applying bituminous material shall be used. The Using Agency shall have the final determination on the matter. 

1.11 [bookmark: _Toc531776219][bookmark: _Toc92540][bookmark: _Toc160454833][bookmark: _Toc169179952]MATERIALS
Aggregates for bituminous surface treatment shall be in conformance with the following:

· Coarse aggregate for cover material for bituminous surface treatment shall be broken stone, washed gravel, blast furnace slag, and boiler slag conforming to Sections 4.13.1, 4.13.2, and 4.13.3 of this Bid Solicitation. Gradation of the aggregates shall meet the requirements shown in “Table for Standard Sizes of Course Aggregate” as referenced in Section 4.14.4 of this Bid Solicitation; and 

· Fine aggregate for cover material for bituminous surface treatment shall be composed of natural, and hard durable pebbles, crushed stone or stone sand, to be mixed in such proportions that the material will conform to the grading requirements specified below:

	Sieve Size
	Percent

	1".
	100

	No. 8.
	65 - 100

	No 50.
	10 - 30

	No. 200
	0 - 7



[bookmark: _Toc531776220][bookmark: _Toc160454834][bookmark: _Toc169179953]broken stone and types of rocks 
Broken stone shall be uniform in texture and quality, and shall conform to section 4.18 of this Bid Solicitation and to the following quality requirements:

	Graph 1
	Maximum Percent

	Weathered and decomposed stone 
	5%

	Broken stone other than classification approved for use
	5%

	Flat or elongated pieces for graded material no. 57 & larger (Length greater than 4 times maximum thickness or width)
	7%

	Absorption in cold water 
	

	No. 8 and larger
	1.7%

	Nos. 89 and 9
	1.8%

	Sodium sulfate soundness, loss 
	

	Ledge rock
	10%

	Graded sizes
	10%

	Adherent fines in coarse aggregates
	

	Bituminous concrete
	1.5%

	Portland cement concrete
	1.0%



The percent of wear (Los Angeles test) shall be as follows for various uses:

	Graph 2
	Maximum Percent

	Bituminous concrete surface course, top layer
	40%

	Bituminous concrete surface course, bottom layer
	45%

	Bituminous-stabilized base course
	45%

	Concrete surface course and bridge decks
	40%

	Concrete, other
	50%



Types of rocks permissible for use in white concrete shall be free from dirt and discoloring matter. The geologic classifications are as follows:

· Argillite: Shall mean a thoroughly indurated and cohesive rock composed predominantly of silt size or smaller particles of clay, quartz and feldspar, or the fine grained thermal recrystallization products of this assemblage (hornfels). It shall be bedded thickly enough so as to break into thin pieces at plane stratification;

· Carbonate rock: Shall mean a thoroughly indurated and cohesive rock composed predominantly of calcite and dolomite, bedded thickly enough so as not to break into thin pieces at planes of stratification. Minerals insoluble in hot hydrochloric acid shall be discrete grains of quartz, clay, and mica;

· Gneiss: Shall mean a metamorphic rock consisting principally of quartz and feldspar. It shall have a dense structure and shall not break into thin pieces at lines of stratification and shall have a uniform distribution of minerals;

· Granite: Shall mean as equigranular or porphyritic igneous rock consisting principally of quartz and feldspar. It shall be of medium or fine grain texture;

· Quartzite: Shall mean a metamorphic rock composed principally of quartz. It shall be quarried so that only the nonarkosic, uniformly compacted quartzites are included in the graded products, and shall not be schistose in structure; and

· Trap rock: Shall mean either basalt or diabase. It shall have a distribution of constituent   minerals.

[bookmark: _Toc531776221][bookmark: _Toc160454835][bookmark: _Toc169179954]Washed Gravel 
Washed gravel shall either be crushed or uncrushed as specified.

· The gravel shall conform to Section 4.18 of this Bid Solicitation and to the following quality requirements:

	Graph 3
	Maximum Percent

	Sodium sulfate soundness, loss
	10%

	Soft particles as determined by scratch hardness test
	5%

	Absorption in cold water
	

	No. 8 size and larger
	1.7%

	Nos. 89 and 9
	1.8%

	Clay lumps, organic material, coal, and other foreign or deleterious matter
	

	(Percent by weight or volume whichever is greater)
	0.5%

	Sea salt
	

	Crushed gravel material with at least one fractured face
	0.2%

	(Nickel gravel will not be considered crushed)
	60% minimum

	Adherent fines in coarse aggregates
	

	Bituminous concrete
	1.5%

	Portland cement concrete
	1.0%



· The percent of wear determined in accordance with the Los Angeles test shall be specified for the various uses, except that the percent maximum loss for quartz gravel shall be 50 percent. Quartz gravel shall mean a material composed of natural pebbles of which the overwhelming majorities are coarsely crystalline quartz. The individual crystals within each pebble shall be inter-grown into a tenacious, nonporous, interlocking texture which fractures as a single unit.

Please note: When the sodium sulfate soundness and scratch hardness tests total 10 percent or more, a petrographic analysis shall be performed to determine the amount of unsound and weathered material. Unsound and weathered materials shall be no more than ten (10) percent by weight.

[bookmark: _Toc531776222][bookmark: _Toc160454836][bookmark: _Toc169179955]Blast Furnace and boiler Slag 
· Blast furnace slag shall be the air-cooled residue resulting from the production of pig iron and shall consist of tough, durable angular fragments uniform in density, absorption, quality, and shall be free from flux stone, dirt or other objectionable material. The slag shall conform to Section 4.18 of this Bid Solicitation and to the following quality requirements:

	Weight per cubic foot (loose measure), lbs.
	60lbs min.

	Percent of wear (Los Angeles test)
	50% max.

	Sulfur, percentage by weight
	1% max.



· Blast furnace slag used as dense graded aggregate material, the gradation, and percentage of wear shall be as specified for that item; and

· Boiler slag shall be fused water-cooled residue from the combustion of pulverized or powdered coal used in generating plants or from refuse incinerating plants. The color of which shall be black or nearly black. The gradation of boiler slag shall conform to size No. 10. The boiler slag shall conform to Section 4.18 of this Bid Solicitation and the following quality requirements:

	Weight per cubic foot (loose measure), lbs
	85lbs min.

	Specific gravity (bulk)
	2.80 min.

	Absorption in cold water, percent
	1.2% max.

	Percent of wear (Los Angeles test)
	50% max.




[bookmark: _Toc169179956]TABLES FOR STANDARD SIZES OF COARSE AGGREGATE

	SIZE
NUMBER
	NOMINAL SIZE
SQUARE
OPENINGS
	AMOUNTS FINER THAN EACH LABORATORY SIEVE (SQUARE OPENINGS),
PERCENTAGE BY WEIGHT

	
	(1)
	4”
	3-1/2”
	3”
	2 ½”
	2”
	1 ½”
	1”
	¾”
	½”

	1
	3-½ to 1-1/2
	100
	90-100
	
	25 -60
	
	0 -15
		
	0 - 5
	

	2
	2 ½ to 1-1/2
	
	
	100
	90-100
	35–70
	0 -15
	
	0– 5
	

	
	
	
	
	
	
	
	
	
	
	

	
	(1)
	
	
	
	
	
	
	
	
	

	24
	2-1/2 to ¾
	
	
	100
	90-100
	
	25-60
	
	0-10
	0-5

	3
	2  TO 1
	
	
	
	100
	90-100
	35-70
	0-15
	
	0. 



· In inches, except where otherwise indicated. Numbered sieves are those of the United States Sieve Series. The following link contains the regulated numbered sieves, https://www.azom.com/article.aspx?ArticleID=1417.

	SIZE
NUMBER
	NOMINAL
SIZE SQUARE OPENINGS
	AMOUNTS FINER THAN EACH LABORATORY SIEVE (SQUARE OPENING)
PERCENTAGE BY WEIGHT

	
	(1)
	2 ½”
	2”
	1 ½”
	1”
	¾”
	½”
	3/8”
	No.4

	357
	2 to No. 4
	100
	95-100
	
	35-70
	
	10-30
	
	0-5

	4
	1-1/2 to No. ¾
	
	100
	90-100
	20-55
	0-15
	
	0-5
	

	67
	1-1/2 to No. 4
	
	100
	95-100
	
	35-70
	
	10-30
	0-5

	5
	1 to ½
	
	
	100
	90-100
	20-55
	0-10
	0-5
	

	56
	1 to 3/8
	
	
	100
	90-100
	40-75
	15-35
	0-15
	0-5

	SIZE
NUMBER
	NOMINAL
SIZE SQUARE OPENINGS
	AMOUNTS FINER THAN EACH LABORATORY SIEVE (SQUARE OPENING)
PERCENTAGE BY WEIGHT

	
	(1)
	1 ½”
	1”
	¾”
	½”
	3/8”
	No.4
	No. 8
	No. 16

	57
	1 to No.4
	100
	95-100
	
	25-60
	
	0-10
	0-5
	

	6
	¾ to 3/8
	
	100
	90-100
	20-55
	0-15
	0-5
	
	

	67
	¾ to No. 4
	
	100
	90-100
	
	20-55
	0-10
	0-5
	

	68
	¾ to No. 8
	
	100
	90-100
	
	30-65
	5-25
	0-10
	0. 



· In inches, except where otherwise indicated. Numbered sieves are those of the United States Sieve Series. The following link contains the regulated numbered sieves, https://www.azom.com/article.aspx?ArticleID=1417.


	SIZE
NUMBER
	NOMINAL
SIZE SQUARE
OPENINGS
	E
	AMOUNTS FINER THAN EACH LABORATORY SIEVE (SQUARE OPENING)
PERCENTAGE BY WEIGHT

	
	(1)
	¾”
	½”
	3/8”
	No. 4
	No. 8
	No. 16
	No. 50
	No. 100

	7
	½ to No. 4
	100
	90-100
	40-70
	0-15
	0-5
	
	
	

	78
	½ to No. 8
	100
	90-100
	40-75
	5-25
	0-10
	0-5
	
	

	8
	3/8 to No. 8
	
	100
	85-100
	10-30
	0-10
	0-5
	
	

	89
	3/8 to No. 16
	
	100
	90-100
	20-55
	5-30
	0-10
	0-5
	

	9
	No. 4 to No. 16
	
	
	100
	85-100
	10-40
	0-10
	0-5
	

	10
	No. 4 to 0
(2)
	
	
	100
	85-100
	
	
	
	10-30



·  In inches, except where otherwise indicated. Numbered sieves are those of the United States Sieve Series. The following link contains the regulated numbered sieves, https://www.azom.com/article.aspx?ArticleID=1417.

[bookmark: _Toc92541]Please note: All additives for the aggregate mixtures shall be determined in conjunction with the Using Agency and Contractor at the site. However, the Using Agency shall have final say in the determination. 

1.12 [bookmark: _Toc531776223][bookmark: _Toc160454837][bookmark: _Toc169179957]BITUMINOUS CONCRETE FOR PATCH  
Bituminous concrete for patch may be used either as a hot mixture direct from a mixing plant or cold from a stockpile at temperatures as low as 15 degrees Fahrenheit (F). The Contractor and the Using Agency shall make this determination on site, in conjunction. In addition, all mixtures shall be sufficiently workable to allow spreading and raking for a period of at least six (6) months when stockpiled, and shall be sufficiently stable after compaction to carry traffic without undue marking or displacement.

[bookmark: _Toc531776224][bookmark: _Toc160454838][bookmark: _Toc169179958]MATERIALS FOR BITUMINOUS CONCRETE PATCH 
· Coarse aggregate for top layer of bituminous concrete surface course (total retained on No. 8 sieve) shall be broken stone or crushed gravel;

· Broken stone shall conform to section 4.13.3 of this Bid Solicitation except that carbonate rock shall not be used; 

· Carbonate rock may be used for the top layer in areas other than the traveled way; 

· Coarse aggregate for bottom layer of bituminous concrete surface course: (total retained on No. 8 sieve) shall be broken stone or crushed gravel conforming to sections 4.13.3  of this Bid Solicitation respectively, except that the gravel need not be washed; and

· Crushed stone shall conform to Section 4.13.2 of this Bid Solicitation except that it need not be washed and it shall contain no more than 50 percent of total carbonates.

· Reclaimed asphalt pavement (RAP): shall pass a two and a half (2 ½) inch sieve. The bituminous material contained in the RAP shall be asphalt contaminating substances;

· The coarse aggregate contained in the RAP shall conform to the standard percentage of recycled bituminous requirements for coarse aggregates in the bituminous mixture being produced; and

· The fine aggregate contained in the RAP shall conform to the quality requirements in graph 4 below.

· Fine aggregate for top and bottom layers of bituminous concrete surface course shall be stone sand or natural sand;  

· Stone sand shall be argillite, gneiss, granite, quartzite, or trap rock conforming to the quality requirements in Section 4.13.3 of this Bid Solicitation. However, no more than 15 percent based on oven dry weight shall pass the No. 200 sieve. When the percent passing the No. 200 sieve exceeds 15 percent, use of the stone sand will be permitted if blended with natural sand so that the combination contains no more than 15 percent passing the No. 200 sieve based on stockpile samples, oven dried and theoretically combined;  

· Each sand source used shall be fed into the plant through a separate cold feed hopper; and

· Natural sand shall consist of material composed of predominantly angular particles of quartz or other hard durable minerals conforming to the following quality and gradation requirements. 

	Graph 4
	Maximum Percent

	MICA
	2%

	Absorption, Cold Water
	2%

	Sodium Sulfate Soundness, loss 
	5%

	Clay and Clay lumps as determined by AASHTO T 88
	5%



	SIEVE SIZE
	Percent

	3/8
	100%

	No. 4
	95-100%

	No. 8
	80-100%



Please note: Natural fine aggregates for the top layer of the surface course shall be washed and graded products. After washing, no more than a total of five (5) percent, based on oven dry weight shall pass the No. 200 sieve. In lieu of the above requirements for gradation and washing, the appropriate provisions of ASTM C 33 may be substituted, except that no more than a total of five (5) percent based on oven dry weight shall pass the No. 200 sieve. 
(Please see the following link for information regarding the American Society for Testing Materials [ASTM]: https://ihsmarkit.com/products/aashto-standards.html.)

· Mineral filler for bituminous concrete shall be carbonate rock, trap rock, fly ash, or other inert mineral matter, free from lumps and foreign materials, and shall conform to the following:

· Fly ash: shall conform to ASTM C 593 except that the loss on ignition shall be no more than ten (10) percent and the combined content of silica and aluminum oxide shall be no less than 50 percent; and 

· Mineral filler: shall be of such quality that a bituminous mixture containing the filler shall retain 70 percent of its initial strength after an immersion cycle of 14 days when prepared in accordance with AASHTO T 165. The mineral filler shall conform to the following grading requirements:

	SIEVE SIZE
	Percent

	No. 50
	95-100%

	No. 200
	70-100%



1.12.1.1 CUT-BACK AND INVERTED EMULSIFIED ASPHALTS
· Cut-back asphalts shall conform to section 4.11.1 of this Bid Solicitation. The grades shall be MC 250 OR MC 800 and shall contain an anti-stripping additive; and

· Inverted emulsified asphalt of the medium curing (IEMC) type shall be prepared using a suitable grade of medium curing cut-back asphalt conforming to Section 4.11.1 of this Bid Solicitation, with the necessary water and emulsifier required for the mixture of the bituminous. The asphalt emulsions shall be homogenous and shall conform to the following:

	Graph 5
	IEMC-250
	IEMC-800

	Miscibility
	Not Miscible
	Not Miscible

	Settlement, % Max.
	1
	1

	Freezing (all grades)
	Shall remain
	Homogeneous



	Kinematic viscosity
	IEMC-250
	IEMC-800

	140 deg F Centistrokes
	250 - 500
	800 - 1600



	Distillation
	IEMC-250
	IEMC-800

	Asphalt content, % Min
	67%
	74%

	Water, %
	3-10%
	3-10%

	Solvent (by difference)  % Min.
	15%
	8%




	Residue from distillation
	IEMC-250
	IEMC-800

	Specific gravity at 60 Deg F/60 Deg F Min
	1
	1

	Penetration at 77 Deg F
	120 – 250
	120 - 250

	Ductility at 77 Deg F,  CM Min
	100
	100

	Solubility in CCL 4,% Min
	98
	98

	Ash, % Max
	1
	1



1.12.1.2 BITUMINOUS CONCRETE PATCH MIXTURE 
Composition of the bituminous concrete patch mixture shall be composed of aggregates and bituminous materials combined with such proportions that the resulting composite blend shall meet the following:

	SIEVE SIZE
	Total Percent

	½”
	100%

	3/8”
	80 – 100%

	No. 4
	55 – 75%

	No. 8
	30 – 60%

	No. 50
	10 – 30%

	No. 200
	4 – 10%

	Residual Bitumen Content %
	5.5 – 7.5%



In calculating the percentages of aggregates of the various sizes, the bituminous material is excluded.

Please note: Material passing the No. 200 sieve may consist of fine particles of the aggregate or mineral filler, or both. Material passing the No. 40 sieve shall be non-plastic when tested in accordance with AASHTO T90.

1.12.1.3 TEMPERATURE OF BITUMINOUS CONCRETE PATCH MIXTURE 
The aggregate shall be surface dry at the time of mixing, however, its temperature shall not exceed 250 Degrees F. The temperature of the bituminous material shall not exceed 170 Degrees F. The temperature of the components at the mixing time shall be such that a minimum of 90 percent of the aggregate is coated when tested.

1.13 [bookmark: _Toc531776225][bookmark: _Toc160454839][bookmark: _Toc92542][bookmark: _Toc169179959]THE RANGE OF APPLICATION TEMPERATURES 

	Range of Application Temperatures

	Grade
	Temperature range
	Grade
	Temperature range

	RC - 250
	170 – 200 Deg
	RS 1
	70 – 140 Deg

	RC - 800
	205 – 235 Deg
	RS 2
	125 – 185 Deg

	RC - 3000
	235 – 265 Deg
	CRS- 1
	70 – 140 Deg

	MC - 250
	170 – 200 Deg
	CRS- 2
	125 – 185 Deg

	MC - 800
	205 – 235 Deg
	IEMC- 250
	125 – 175 Deg

	MC - 3000
	235 – 265 Deg
	IEMC- 800
	150 – 185 Deg



The purpose of the foregoing chart is to indicate temperature ranges necessary to provide proper viscosity for spraying and mixing applications for the grades shown. It must be recognized, that the temperature ranges indicated by this chart generally are above the minimum flash point for RC and MC cut-back asphalts. Some of these cut-back asphalts will flash at temperatures below these indicated ranges.
[bookmark: _Toc531776227][bookmark: _Toc160454841][bookmark: _Toc92543]
1.14 [bookmark: _Toc169179960]SAFETY PRECAUTIONS 
Safety precautions shall be followed at all times when handling these cut-back asphalts. These safety precautions shall include, but not be limited to the following:

· Do not permit open flames or sparks of any kind close to materials, except in heating kettles, mixers, distributors, or other equipment designed for handling and applying them;

· Do not use an open flame to inspect or examine containers in which these materials have been stored;

· Vent and ground vehicles transporting materials;

· Permit only experienced personnel to supervise the handling of materials; and

· Comply with all applicable local, State, and federal laws and regulations.

1.15 [bookmark: _Toc531776228][bookmark: _Toc92544][bookmark: _Toc160454842][bookmark: _Toc169179961]DELIVERY SLIPS
Duplicate delivery slips shall accompany each load of bituminous material and shall contain the following: 

· Name of the producer and the supplier; 

· Type and grade of material;

· The loading temperature of material; and 

· The lot number and date of approval of the material from which delivery is made.

1.16 [bookmark: _Toc531776229][bookmark: _Toc92545][bookmark: _Toc160454843][bookmark: _Toc169179962]AGGREGATE MATERIAL
Only aggregate from a single source shall be used in any one construction item. Aggregates from different sources may be permitted if they are of the same: 

· Geologic classification; 

· Have similar specific gravities; and 

· Share the same color.

[bookmark: _Toc531776230][bookmark: _Toc160454844][bookmark: _Toc169179963]AGGregate Material Stockpile
The area for each stockpile shall be of adequate size, reasonably uniform in cross section, well drained, and cleared of foreign materials. The aggregate stockpiles shall be placed on a firm, hard surface such as a compacted aggregate or stabilized base, bituminous or concrete surface, and shall be constructed by placing the aggregates in layers no more than three (3) feet thick.

[bookmark: _Toc531776231][bookmark: _Toc160454845][bookmark: _Toc169179964]CONTRACTOR insturctions for handling stockpiles of aggregate material 
The Contractor must comply with the following: 

· Aggregates from haul way areas shall not be used;  

· The piles shall be located so that there is no contamination by foreign material and no intermingling of aggregates from adjacent piles;  

· Aggregates from different sources and of different gradings shall not be stockpiled near each other unless a bulkhead is placed between the different materials;  

· Aggregates of different gradings and from different sources for use in blends shall be blended by proportion through the weigh hoppers;  

· Aggregates found segregated or contaminated shall be rejected for use; 

· A rejected stockpile may be removed from stockpiles in a manner such as to prevent segregation;

· Aggregates which require washing shall not be used sooner than 24 hours after washing or until the surplus water has drained out and the material has uniform moisture content; and

· Coarse aggregate shall be broken stone, washed gravel, blast furnace slag, and boiler slag conforming to sections 4.13.1, 4.13.2, and 4.13.3 of this Bid Solicitation and shall be graded to comply with the “Table for Standard Sizes of Coarse Aggregate” referenced in this Bid Solicitation.
[bookmark: _Toc531776232][bookmark: _Toc92546][bookmark: _Toc160454846]
1.17 [bookmark: _Toc169179965]PUBLIC WORKS CONTRACTOR REGISTRATION ACT
The New Jersey Public Works Contractor Registration Act requires all contractors, subcontractors and lower tier subcontractor(s) who engage in any contract for public work as defined in N.J.S.A. 34:11-56.26 be first registered with the New Jersey Department of Labor and Workforce Development pursuant to N.J.S.A. 34:11-56.51. Any questions regarding the registration process should be directed to the Division of Wage and Hour Compliance at (609) 292-9464. 

[bookmark: _Toc531776233][bookmark: _Toc160454847][bookmark: _Toc169179966]PUBLIC WORKS CONTRACT - ADDITIONAL AFFIRMATIVE ACTION REQUIREMENTS

N.J.S.A. 10:2-1 requires that during the performance of this contract, the contractor must agree as follows: 

· In the hiring of persons for the performance of work under this contract or any subcontract hereunder, or for the procurement, manufacture, assembling or furnishing of any such materials, equipment, supplies or services to be acquired under this contract, no contractor, nor any person acting on behalf of such contractor or subcontractor, shall, by reason of race, creed, color, national origin, ancestry, marital status, gender identity or expression, affectional or sexual orientation or sex, discriminate against any person who is qualified and available to perform the work to which the employment relates;

· No contractor, subcontractor, nor any person on his/her behalf shall, in any manner, discriminate against or intimidate any employee engaged in the performance of work under this contract or any subcontract hereunder, or engaged in the procurement, manufacture, assembling or furnishing of any such materials, equipment, supplies or services to be acquired under such contract, on account of race, creed, color, national origin, ancestry, marital status, gender identity or expression, affectional or sexual orientation or sex;

· There may be deducted from the amount payable to the contractor by the contracting public agency, under this contract, a penalty of $50.00 for each person for each calendar day during which such person is discriminated against or intimidated in violation of the provisions of the contract; and

· This contract may be canceled or terminated by the contracting public agency, and all money due or to become due hereunder may be forfeited, for any violation of this section of the contract occurring after notice to the contractor from the contracting public agency of any prior violation of this section of the contract.

N.J.S.A. 10:5-33 and N.J.A.C. 17:27-3.5 require that during the performance of this contract, the contractor must agree as follows: 

· The contractor or subcontractor, where applicable, will not discriminate against any employee or applicant for employment because of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Except with respect to affectional or sexual orientation and gender identity or expression, the contractor will take affirmative action to ensure that such applicants are recruited and employed, and that employees are treated during employment, without regard to their age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Such action shall include, but not be limited to the following: employment, upgrading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship. The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided by the contracting officer setting forth the provisions of this nondiscrimination clause; 

· The contractor or subcontractor, where applicable will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex; 

· The contractor or subcontractor where applicable, will send to each labor union or representative of workers with which it has a collective bargaining agreement or other contract or understanding, a notice, to be provided by the agency contracting officer, advising the labor union or workers' representative of the contractor's commitments under this act and shall post copies of the notice in conspicuous places available to employees and applicants for employment, N.J.A.C. 17:27-3.7 requires all contractors and subcontractors, if any, to further agree as follows: 

· The contractor or subcontractor agrees to make good faith efforts to meet targeted county employment goals established in accordance with N.J.A.C. 17:27-5.2;

· The contractor or subcontractor agrees to inform in writing its appropriate recruitment agencies including, but not limited to, employment agencies, placement bureaus, colleges, universities, and labor unions, that it does not discriminate on the basis of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, and that it will discontinue the use of any recruitment agency which engages in direct or indirect discriminatory practices;

· The contractor or subcontractor agrees to revise any of its testing procedures, if necessary, to assure that all personnel testing conforms with the principles of job-related testing, as established by the statutes and court decisions of the State of New Jersey and as established by applicable Federal law and applicable Federal court decisions; and

· In conforming with the targeted employment goals, the contractor or subcontractor agrees to review all procedures relating to transfer, upgrading, downgrading and layoff to ensure that all such actions are taken without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, consistent with the statutes and court decisions of the State of New Jersey, and applicable Federal law and applicable Federal court decisions. 

1.18 [bookmark: _Toc531776234][bookmark: _Toc92547][bookmark: _Toc160454848][bookmark: _Toc169179967]QUANTITY AND PAYMENT
· The quantity of asphaltic oil and aggregate surface treatment shall be decided by the Using Agency;

· Payment for the asphaltic oil and aggregate surface treatment will be made for the quantity, as above determined, measured by the square yard. Payment will be made at the Contract unit price for the respective region, and the all-inclusive unit price shall include the cost of completing the test strip, removal, cleanup and disposal of dirt, foreign matter or loose or dislodged cover aggregate, mobilization, maintenance and protection of traffic, travel costs, all labor, equipment, and all else necessary therefore and incidental thereto; and

· The number of gallons of bituminous material and the tonnage of aggregates shall not exceed the quantities as determined by the application rates as established by the Using Agency in accordance with Section 4.8 of this Bid Solicitation.

[bookmark: _Toc531776235][bookmark: _Toc160454849][bookmark: _Toc169179968]Minimim Call-out and payment 
The minimum call-out and payment for any asphaltic oil and aggregate surface treatment will be for 500 square yards, and this will be the minimum paid for any specific location. A location shall be construed to mean any Using Agency defined locations (for example a complete State Park). This section shall not be construed to mean that the State will be required to pay the Contractor a minimum of 500 square yards of asphaltic oil and aggregate surface treatment per day.

1.19 [bookmark: _Toc531776237][bookmark: _Toc92548][bookmark: _Toc160454851][bookmark: _Toc169179969][bookmark: _Toc531776238][bookmark: _Toc160454852]TEMPERATURE-VOLUME CORRECTION FACTORS FOR ASPHALT

	[bookmark: _Toc169179970]ASPHALT CEMENTS (ALL GRADES); CUT-BACK ASPHALT (GRADES RC-800, RC-3000, MC-800 AND MC-3000); INVERTED EMULSIFIED ASPHALT (GRADE IEMC-800)


	Temperature
	Factor
	Temperature
	Factor
	Temperature
	Factor
	Temperature
	Factor

	40
	1.0070
	85
	0.9913
	130
	0.9758
	175
	0.9604

	41
	1.0067
	86
	0.9909
	131
	0.9754
	176
	0.9601

	42
	1.0063
	87
	0.9906
	132
	0.9751
	177
	0.9597

	43
	1.0060
	88
	0.9902
	133
	0.9747
	178
	0.9594

	44
	1.0056
	89 
	0.9899
	134
	0.9744
	179
	0.9590

	45
	1.0053
	90
	0.9896
	135
	0.9740
	180
	0.9587

	46
	1.0049
	91
	0.9892
	136
	0.9737
	181
	0.9584

	47
	1.0046
	92
	0.9889
	137
	0.9734
	182
	0.9580

	48
	1.0042
	93
	0.9885
	138
	0.9730
	183
	0.9577

	49
	1.0038
	94
	0.9882
	139
	0.9727
	184
	0.9574

	50
	1.0035
	95
	0.9878
	140
	0.9723
	185
	0.9570

	51
	1.0031
	96
	0.9875
	141
	0.9720
	186
	0.9567

	52
	1.0028
	97
	0.9871
	142
	0.9716
	187
	0.9563

	53
	1.0024
	98
	0.9868
	143
	0.9713
	188
	0.9560

	54
	1.0021
	99
	0.9864
	144
	0.9710
	189
	0.9557

	55
	1.0017
	100
	0.9861
	145
	0.9706
	190
	0.9553

	56
	1.0014
	101
	0.9857
	146
	0.9703
	191
	0.9550

	57
	1.0010
	102
	0.9854
	147
	0.9699
	192
	0.9547

	58
	1.0007
	103
	0.9851
	148
	0.9696
	193
	0.9543

	59
	1.0003
	104
	0.9847
	149
	0.9693
	194
	0.9540

	60
	1.0000
	105
	0.9844
	150
	0.9689
	195
	0.9536

	61
	0.9997
	106
	0.9840
	151
	0.9686
	196
	0.9533

	62
	0.9993
	107
	0.9837
	152
	0.9682
	197
	0.9530

	63
	0.9990
	108
	0.9833
	153
	0.9679
	198
	0.9526

	64
	0.9986
	109
	0.9830
	154
	0.9675
	199
	0.9523

	65
	0.9983
	110
	0.9826
	155
	0.9672
	200
	0.9520

	66
	0.9979
	111
	0.9823
	156
	0.9669
	201
	0.9516

	67
	0.9976
	112
	0.9819
	157
	0.9665
	202
	0.9513

	68
	0.9972
	113
	0.9816
	158
	0.9662
	203
	0.9509

	69
	0.9969
	114
	0.9813
	159
	0.9658
	204
	0.9506

	70
	0.9965
	115
	0.9609
	160
	0.9655
	205
	0.9503

	71
	0.9962
	116
	0.9806
	161
	0.9652
	206
	0.9499

	72
	0.9958
	117
	0.9802
	162
	0.9648
	207
	0.9496

	73
	0.9955
	118
	0.9799
	163
	0.9645
	208
	0.9493

	74
	0.9951
	119
	0.9795
	164
	0.9641
	209
	0.9489

	75
	0.9948
	120
	0.9792
	165
	0.9638
	210
	0.9486

	76
	0.9944
	121
	0.9788
	166
	0.9635
	211
	0.9483

	77
	0.9941
	122
	0.9785
	167
	0.9631
	212
	0.9479

	78
	0.9937
	123
	0.9782
	168
	0.9628
	213
	0.9476

	79
	0.9934
	124
	0.9778
	169
	0.9624
	214
	0.9472

	80
	0.9930
	125
	0.9775
	170
	0.9621
	215
	0.9469

	81
	0.9927
	126
	0.9771
	171
	0.9618
	216
	0.9466

	82
	0.9923
	127
	0.9768
	172
	0.9614
	217
	0.9416

	83
	0.9920
	128
	0.9764
	173
	0.9611
	218
	0.9459

	84
	0.9916
	129
	0.9761
	174
	0.9607
	219
	0.9456





	220
	0.9452
	265
	0.9302
	310
	0.9154
	355
	0.9008

	221
	0.9449
	266
	0.9299
	311
	0.9151
	356
	0.9005

	222
	0.9449
	267
	0.9296
	312
	0.9148
	357
	0.9002

	223
	0.9442
	268
	0.9293
	313
	0.9145
	358
	0.8998

	224
	0.9439
	269
	0.9289
	314
	0.9141
	359
	0.8995

	225
	0.9436
	270
	0.9286
	315
	0.9138
	360
	0.8992

	226
	0.9432
	271
	0.9283
	316
	0.9135
	361
	0.8989

	227
	0.9429
	272
	0.9279
	317
	0.9132
	362
	0.8986

	228
	0.9426
	273
	0.9276
	318
	0.9128
	363
	0.8982

	229
	0.9422
	274
	0.9273
	319
	0.9125
	364
	0.8979

	230
	0.9419
	275
	0.9269
	320
	0.9122
	365
	0.8976

	231
	0.9416
	276
	0.9266
	321
	0.9118
	366
	0.8973

	232
	0.9412
	277
	0.9263
	322
	0.9115
	367
	0.8969

	233
	0.9409
	278
	0.9259
	323
	0.9112
	368
	0.8966

	234
	0.9405
	279
	0.9256
	324
	0.9109
	369
	0.8963

	235
	0.9402
	280
	0.9253
	325
	0.9105
	370
	0.896

	236
	0.9399
	281
	0.925
	326
	0.9102
	371
	0.8957

	237
	0.9395
	282
	0.9246
	327
	0.9099
	372
	0.8953

	238
	0.9392
	283
	0.9243
	328
	0.9096
	373
	0.895

	239
	0.9389
	284
	0.924
	329
	0.9092
	374
	0.8947

	240
	0.9385
	285
	0.9236
	330
	0.9089
	375
	0.8944

	241
	0.9382
	286
	0.9233
	331
	0.9086
	376
	0.8941

	242
	0.9379
	287
	0.923
	332
	0.9083
	377
	0.8937

	243
	0.9375
	288
	0.9227
	333
	0.9079
	378
	0.8934

	244
	0.9372
	289
	0.9223
	334
	0.9076
	379
	0.8931

	245
	0.9369
	290
	0.922
	335
	0.9073
	380
	0.8928

	246
	0.9365
	291
	0.9217
	336
	0.907
	381
	0.8924

	247
	0.9362
	292
	0.9213
	337
	0.9066
	382
	0.8921

	248
	0.9359
	293
	0.921
	338
	0.9063
	383
	0.8918

	249
	0.9356
	294
	0.9207
	339
	0.906
	384
	0.8915

	250
	0.9352
	295
	0.9204
	340
	0.9057
	385
	0.8912

	251
	0.9349
	296
	0.92
	341
	0.9053
	386
	0.8908

	252
	0.9346
	297
	0.9197
	342
	0.905
	387
	0.8905

	253
	0.9342
	298
	0.9194
	343
	0.9047
	388
	0.8902

	254
	0.9339
	299
	0.919
	344
	0.9044
	389
	0.8899

	255
	0.9336
	300
	0.9187
	345
	0.904
	390
	0.8896

	256
	0.9332
	301
	0.9184
	346
	0.9037
	391
	0.8892

	257
	0.9329
	302
	0.9181
	347
	0.9034
	392
	0.8889

	258
	0.9326
	303
	0.9177
	348
	0.9031
	393
	0.8886

	259
	0.9322
	304
	0.9174
	349
	0.9028
	394
	0.8883

	260
	0.9319
	305
	0.9171
	350
	0.9024
	395
	0.888

	261
	0.9316
	306
	0.9167
	351
	0.9021
	396
	0.8876

	262
	0.9312
	307
	0.9164
	352
	0.9018
	397
	0.8873

	263
	0.9309
	308
	0.9161
	353
	0.9015
	398
	0.887

	264
	0.9306
	309
	0.9158
	354
	0.9011
	399
	0.8867

	
	
	
	
	
	
	400
	0.8864



	
	[bookmark: _Toc531776239][bookmark: _Toc160454853]Cut-back Asphalt, (Grades RC-T, RC-70, RC-250, MC-30, MC-70, MC-250); Inverted Emulsified asphalt, (Grade IEMC-250)

	Temperature
	Factor
	Temperature
	Factor
	Temperature
	Factor
	Temperature
	Factor

	40
	1.0080
	85
	0.9901
	130
	0.9725
	175
	0.9551

	41
	1.0076
	86
	0.9897
	131
	0.9721
	176
	0.9547

	42
	1.0072
	87
	0.9893
	132
	0.9717
	177
	0.9543

	43
	1.0068
	88
	0.9889
	133
	0.9713
	178
	0.9539

	44
	1.0064
	89
	0.9885
	134
	0.9709
	179
	0.9536

	45
	1.0060
	90
	0.9881
	135
	0.9705
	180
	0.9532

	46
	1.0056
	91
	0.9877
	136
	0.9701
	181
	0.9528

	47
	1.0052
	92
	0.9873
	137
	0.9697
	182
	0.9524

	48
	1.0048
	93
	0.9869
	138
	0.9693
	183
	0.9520

	49
	1.0044
	94
	0.9865
	139
	0.9690
	184
	0.9517

	50
	1.0040
	95
	0.9861
	140
	0.9686
	185
	0.9513

	51
	1.0036
	96
	0.9857
	141
	0.9682
	186
	0.9509

	52
	1.0032
	97
	0.9854
	142
	0.9678
	187
	0.9505

	53
	1.0028
	98
	0.9850
	143
	0.9674
	188
	0.9501

	54
	1.0024
	99
	0.9846
	144
	0.9670
	189
	0.9498

	55
	1.0020
	100
	0.9842
	145
	0.9666
	190
	0.9494

	56
	1.0016
	101
	0.9838
	146
	0.9662
	191
	0.9490

	57
	1.0012
	102
	0.9834
	147
	0.9659
	192
	0.9486

	58
	1.0008
	103
	0.9830
	148
	0.9655
	193
	0.9482

	59
	1.0004
	104
	0.9826
	149
	0.9651
	194
	0.9478

	60
	1.0000
	105
	0.9822
	150
	0.9647
	195
	0.9475

	61
	0.9996
	106
	0.9818
	151
	0.9643
	196
	0.9471

	62
	0.9992
	107
	0.9814
	152
	0.9639
	197
	0.9467

	63
	0.9988
	108
	0.9810
	153
	0.9635
	198
	0.9463

	64
	0.9984
	109
	0.9806
	154
	0.9632
	199
	0.9460

	65
	0.9980
	110
	0.9803
	155
	0.9628
	200
	0.9456

	66
	0.9976
	111
	0.9799
	156
	0.9624
	201
	0.9452

	67
	0.9972
	112
	0.9795
	157
	0.9620
	202
	0.9448

	68
	0.9968
	113
	0.9791
	158
	0.9616
	203
	0.9444

	69
	0.9964
	114
	0.9787
	159
	0.9612
	204
	0.9441

	70
	0.9960
	115
	0.9783
	160
	0.9609
	205
	0.9437

	71
	0.9956
	116
	0.9779
	161
	0.9605
	206
	0.9433

	72
	0.9952
	117
	0.9775
	162
	0.9601
	207
	0.9429

	73
	0.9948
	118
	0.9771
	163
	0.9597
	208
	0.9425

	74
	0.9944
	119
	0.9767
	164
	0.9593
	209
	0.9422

	75
	0.9940
	120
	0.9763
	165
	0.9589
	210
	0.9418

	76
	0.9936
	121
	0.9760
	166
	0.9585
	211
	0.9414

	77
	0.9932
	122
	0.9756
	167
	0.9582
	212
	0.9410

	78
	0.9929
	123
	0.9752
	168
	0.9578
	213
	0.9407

	79
	0.9925
	124
	0.9748
	169
	0.9574
	214
	0.9403

	80
	0.9921
	125
	0.9744
	170
	0.9570
	215
	0.9399

	81
	0.9917
	126
	0.9740
	171
	0.9566
	216
	0.9395

	82
	0.9913
	127
	0.9736
	172
	0.9562
	217
	0.9391

	83
	0.9909
	128
	0.9732
	173
	0.9559
	218
	0.9388

	84
	0.9905
	129
	0.9728
	174
	0.9555
	219
	0.9384

	


	
	
	
	
	
	
	





	220
	0.9380
	265
	0.9212
	310
	0.9047
	355
	0.8884

	221
	0.9376
	266
	0.9208
	311
	0.9043
	356
	0.8881

	222
	0.9373
	267
	0.9205
	312
	0.9039
	357
	0.8877

	223
	0.9369
	268
	0.9201
	313
	0.9036
	358
	0.8873

	224
	0.9365
	269
	0.9197
	314
	0.9032
	359
	0.8870

	225
	0.9361
	270
	0.9194
	315
	0.9029
	360
	0.8866

	226
	0.9358
	271
	0.9190
	316
	0.9025
	361
	0.8863

	227
	0.9354
	272
	0.9186
	317
	0.9021
	362
	0.8859

	228
	0.9350
	273
	0.9182
	318
	0.9018
	363
	0.8856

	229
	0.9346
	274
	0.9179
	319
	0.9014
	364
	0.8852

	230
	0.9343
	275
	0.9175
	320
	0.9010
	365
	0.8848

	231
	0.9339
	276
	0.9171
	321
	0.9007
	366
	0.8345

	232
	0.9335
	277
	0.9168
	322
	0.9003
	367
	0.8841

	233
	0.9331
	278
	0.9164
	323
	0.9000
	368
	0.8338

	234
	0.9328
	279
	0.9160
	324
	0.8996
	369
	0.8834

	235
	0.9324
	280
	0.9157
	325
	0.8992
	370
	0.8831

	236
	0.9320
	281
	0.9153
	326
	0.8989
	371
	0.8827

	237
	0.9316
	282
	0.9149
	327
	0.8985
	372
	0.8823

	238
	0.9313
	283
	0.9146
	328
	0.8981
	373
	0.8820

	239
	0.9309
	284
	0.9142
	329
	0.8978
	374
	0.8816

	240
	0.9305
	285
	0.9138
	330
	0.8974
	375
	0.8813

	241
	0.9301
	286
	0.9135
	331
	0.8971
	376
	0.8809

	242
	0.9298
	287
	0.9131
	332
	0.8967
	377
	0.8806

	243
	0.9294
	288
	0.9127
	333
	0.8963
	378
	0.8802

	244
	0.9290
	289
	0.9124
	334
	0.8960
	379
	0.8799

	245
	0.9286
	290
	0.9120
	335
	0.8956
	380
	0.8795

	246
	0.9283
	291
	0.9116
	336
	0.8952
	381
	0.8792

	247
	0.9279
	292
	0.9113
	337
	0.8949
	382
	0.8788

	248
	0.9275
	293
	0.9109
	338
	0.8945
	383
	0.8784

	249
	0.9272
	294
	0.9105
	339
	0.8942
	384
	0.8781

	250
	0.9268
	295
	0.9102
	340
	0.8938
	385
	0.8777

	251
	0.9264
	296
	0.9098
	341
	0.8934
	386
	0.8774

	252
	0.9260
	297
	0.9094
	342
	0.8931
	387
	0.8770

	253
	0.9257
	298
	0.9091
	343
	0.8927
	388
	0.8967

	254
	0.9253
	299
	0.9087
	344
	0.8924
	389
	0.8763

	255
	0.9249
	300
	0.9083
	345
	0.8920
	390
	0.8760

	256
	0.9245
	301
	0.9080
	346
	0.8916
	391
	0.8756

	257
	0.9242
	302
	0.9076
	347
	0.8913
	392
	0.8753

	258
	0.9238
	303
	0.9072
	348
	0.8909
	393
	0.8749

	259
	0.9234
	304
	0.9069
	349
	0.8906
	394
	0.8746

	260
	0.9231
	305
	0.9065
	350
	0.8902
	395
	0.8742

	261
	0.9227
	306
	0.9061
	351
	0.8899
	396
	0.8738

	262
	0.9223
	307
	0.9058
	352
	0.8895
	397
	0.8735

	263
	0.9219
	308
	0.9054
	353
	0.8891
	398
	0.8731

	264
	0.9216
	309
	0.9050
	354
	0.8888
	399
	0.8728

	
	
	
	
	
	
	400
	0.8724






[bookmark: _Toc169179971]GENERAL CONTRACT TERMS
The Contractor shall have sole responsibility for the complete effort specified in this Contract.  Payment will be made only to the Contractor or to the authorized dealers/distributors, if applicable.  The Contractor is responsible for the professional quality, technical accuracy and timely completion and submission of all deliverables, services or commodities required to be provided under this Contract.  The Contractor shall, without additional compensation, correct or revise any errors, omissions, or other deficiencies in its deliverables and other services.  The approval of deliverables furnished under this Contract shall not in any way relieve the Contractor of responsibility for the technical adequacy of its work.  The review, approval, acceptance or payment for any of the deliverables, goods or services, shall not be construed as a waiver of any rights that the State may have arising out of the Contractor’s performance of this Contract.

[bookmark: _Toc169179972]CONTRACT TERM AND EXTENSION OPTION
The base term of this Contract shall be for a period of three (3) years.  The anticipated Contract effective date is provided on the “Summary” page of the Bid Solicitation in NJSTART.  If delays in the procurement process result in a change to the anticipated Contract effective date, the Contractor agrees to accept a Contract for the full term of this Contract. 

This Contract may be extended up to two (2) years with no single extension exceeding one (1) year, by the mutual written consent of the Contractor and the Director at the same terms, conditions, and pricing at the rates in effect in the last year of this Contract or rates more favorable to the State.  

[bookmark: _Toc400531508][bookmark: _Toc428533979][bookmark: _Toc32310704][bookmark: _Toc169179973]CONTRACT TRANSITION
In the event that a new Contract has not been awarded prior to the expiration date for this Contract, including any extensions exercised, and the State exercises this Contract transition, the Contractor shall continue this Contract under the same terms, conditions, and pricing until a new Contract can be completely operational.  At no time shall this transition period extend more than 180 calendar days beyond the expiration date of this Contract, including any extensions exercised.

[bookmark: _Toc118513795][bookmark: _Toc400531563][bookmark: _Toc428534035][bookmark: _Toc32310758][bookmark: OLE_LINK3][bookmark: OLE_LINK4][bookmark: _Toc169179974]PERFORMANCE SECURITY
Not applicable to this procurement.

[bookmark: _Toc400531513][bookmark: _Toc428533984][bookmark: _Toc32310709][bookmark: _Toc169179975]OWNERSHIP OF MATERIAL
A. State Data – The State owns State Data. Contractor shall not obtain any right, title, or interest in any State Data, or information derived from or based on State Data.  State Data provided to Contractor shall be delivered or returned to the State of New Jersey upon thirty (30) days’ notice by the State or thirty (30) days after the expiration or termination of the Contract.  Except as specifically required by the requirements of the Bid Solicitation, State Data shall not be disclosed, sold, assigned, leased or otherwise disposed of to any person or entity other than the State unless specifically directed to do so in writing by the State Contract Manager.
B. Work Product; Services – The State owns all Deliverables developed for the State in the course of providing Services under the Contract, including but not limited to, all data, technical information, materials gathered, originated, developed, prepared, used or obtained in the performance of the Contract, including but not limited to all reports, surveys, plans, charts, literature, brochures, mailings, recordings (video and/or audio), pictures, drawings, analyses, graphic representations, print-outs, notes and memoranda, written procedures and documents, regardless of the state of completion, which are prepared for or are a result of the Services required under the Contract. 
C. Contractor Intellectual Property; Commercial off the Shelf Software (COTS) and Customized Software – Contractor retains ownership of all Contractor Intellectual Property, and any modifications thereto and derivatives thereof, that the  Contractor supplies to the State pursuant to the Contract, and grants the State a non-exclusive, royalty-free license to use Contractor Intellectual Property delivered to the State for the purposes contemplated by the Contract for the duration of the Contract including all extensions.  In the event Contractor provides its standard license agreement terms with its Quote, such terms and conditions must comply with Bid Solicitation Section 1.4 – Order of Precedence of Contractual Terms.
D. Third Party Intellectual Property – Unless otherwise specified in the Bid Solicitation that the State, on its own, will acquire and obtain a license to Third Party Intellectual Property, Contractor shall secure on the State’s behalf, in the name of the State and subject to the State’s approval, a license to Third Party Intellectual Property sufficient to fulfill the business objectives, requirements and specifications identified in the Contract at no additional cost to the State beyond that in the Quote price.  In the event Contractor is obligated to flow-down commercially standard third party terms and conditions customarily provided to the public associated with Third Party Intellectual Property and such terms and conditions conflict with Bid Solicitation requirements, including the SSTC, the State will accept such terms and conditions with the exception of the following:  indemnification, limitation of liability, choice of law, governing law, jurisdiction, and confidentiality.  The Bid Solicitation including the SSTC shall prevail with respect to such conflicting terms and conditions.  In addition, the State will not accept any provision requiring the State to indemnify a third party or to submit to arbitration.  Such terms are considered void and of no effect.  Third party terms and conditions should be submitted with the Quote. If Contractor uses Third Party Intellectual Property, Contractor must indemnify the State for infringement claims with respect to the Third Party Intellectual Property.   Contractor agrees that its use of Third Party Intellectual Property shall be consistent with the license for the Third Party Intellectual Property, whether supplied by the Contractor, secured by the State as required by the Bid Solicitation, or otherwise supplied by the State. 
E. Work Product; Custom Software – The State owns all Custom Software which shall be considered “work made for hire”, i.e., the State, not the Contractor, subcontractor, or third party, shall have full and complete ownership of all such Custom Software.  To the extent that any Custom Software may not, by operation of the law, be a “work made for hire” in accordance with the terms of the Contract, Contractor, subcontractor, or third party hereby assigns to the State, or Contractor shall cause to be assigned to the State, all right, title and interest in and to any such Custom Software and any copyright thereof, and the State shall have the right to obtain and hold in its own name any copyrights, registrations and any other proprietary rights that may be available. 
F. State Intellectual Property – The State owns all State Intellectual Property provided to Contractor pursuant to the Contract.  State Intellectual Property shall be delivered or returned to the State of New Jersey upon thirty (30) days’ notice by the State or thirty (30) days after the expiration or termination of the Contract.  The State grants Contractor a non-exclusive, royalty-free, license to use State Intellectual Property for the purposes contemplated by the Contract.  Except as specifically required by the requirements of the Bid Solicitation, State Intellectual Property shall not  be disclosed, sold, assigned, leased or otherwise disposed of to any person or entity other than the State unless specifically directed to do so in writing by the State Contract Manager. The State’s license to Contractor is limited by the term of the Contract and the confidentiality obligations set forth in Bid Solicitation Section 6 – Data Security Requirements – Contractor Responsibility.
G. No Rights – Except as expressly set forth in the Contract, nothing in the Contract shall be construed as granting to or conferring upon Contractor any right, title, or interest in State Intellectual Property or any intellectual property that is now owned or licensed to or subsequently owned by or licensed by the State.  Except as expressly set forth in the Contract, nothing in the Contract shall be construed as granting to or conferring upon the State any right, title, or interest in any Contractor Intellectual Property that is now owned or subsequently owned by Contractor.  Except as expressly set forth in the Contract, nothing in the Contract shall be construed as granting to or conferring upon the State any right, title, or interest in any Third Party Intellectual Property that is now owned or subsequently owned by a third party.

[bookmark: _Toc169179976]SUBSTITUTION OF STAFF
If a Contractor needs to substitute any management, supervisory or key personnel, the Contractor shall identify the substitute personnel and the work to be performed.  The Contractor must provide detailed justification documenting the necessity for the substitution.  Resumes must be submitted for the individual(s) proposed as substitute(s) who must have qualifications and experience equal to or better than the individual(s) originally proposed or currently assigned.

The Contractor shall forward a request to substitute staff to the State Contract Manager for consideration and approval.  No substitute personnel are authorized to begin work until the Contractor has received written approval to proceed from the State Contract Manager.

[bookmark: _Toc169179977]DELIVERY TIME AND COSTS
Unless otherwise noted in this Bid Solicitation or on the State-Supplied Price Sheet, all delivery times are thirty (30) calendar days after receipt of order (ARO) and prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination (30 calendar days ARO/F.O.B.).  The Contractor shall assume all costs, liability and responsibility for the delivery of merchandise in good condition to the State's Using Agency or designated purchaser.  Thirty calendar days ARO/F.O.B. does not cover "spotting" but does include delivery on the receiving platform of the Using Agency at any destination in the State of New Jersey unless otherwise specified.  No additional charges will be allowed for any additional transportation costs resulting from partial shipments made at the Contractor’s convenience when a single shipment is ordered.  The weights and measures of the State's Using Agency receiving the shipment shall govern.  Collect on Delivery (C.O.D.) Terms are not permitted.

[bookmark: _Toc400531525][bookmark: _Toc428533996][bookmark: _Toc32310718][bookmark: _Toc169179978]LIQUIDATED DAMAGES
Not applicable to this procurement.

[bookmark: _Toc400531531][bookmark: _Toc428534002][bookmark: _Toc32310724][bookmark: _Toc169179979]RETAINAGE
Not applicable to this procurement.

[bookmark: _Toc169179980]ELECTRONIC PAYMENTS
With the award of this Contract, the successful Contractor(s) will be required to receive its payment(s) electronically.  In order to receive payments via automatic deposit from the State of New Jersey, the Contractor must complete the EFT information within its NJSTART Vendor Profile.  Please refer to the QRG entitled “Vendor Profile Management – Company Information and User Access” for instructions. 

[bookmark: _Toc169179981]PROCUREMENT EFFICIENCY PROGRAM
A. Quarterly Sales Reporting - The Contractor shall submit a Sales Report documenting all sales made under the Contract.  The Sales Report shall be submitted directly to Periscope no later than thirty (30) calendar days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31. The Sales Report must contain the following information:  
· Complete and accurate details of all sales, credits, returns, refunds, and the like for the reporting quarter;
· Purchasing entity;
· Total of Procurement Efficiency Program Fee amount due for the reporting quarter;
· Such other information as the State may reasonably request;
· If no sales were made against this Contract during the reporting quarter, then a report shall be submitted showing zero sales and zero Procurement Efficiency Program Fee due; and
· Quarterly Sales Reporting and remittance of the Procurement Efficiency Program Fee shall begin on the first calendar quarter starting after the effective date of the Contract.
B. Procurement Efficiency Program Fee - For all purchases made under this Contract, that have been invoiced, the Contractor shall remit the Procurement Efficiency Program Fee in the amount of one percent (1%) of all Purchases to Periscope acting on behalf of the State of New Jersey. 
C. Remittance of the Procurement Efficiency Program Fee - On a quarterly basis, the Contractor shall remit the Procurement Efficiency Program Fee directly to Periscope no later than thirty (30) days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31.  Failure to remit the Procurement Efficiency Program Fee timely and accurately may result in Contract termination as outlined in the “Termination of Contract” clause of the State of New Jersey Standard Terms and Conditions. 
D. NJSTART Marketplace Catalog Enablement - Contractor shall cooperate with State and/or Periscope as requested to upload catalog items and pricing consistent with this Contract. Contractor shall upload catalog within (thirty) 30 calendar days of the date of execution of this Contract. Failure to cooperate will result in the Contractor’s good and/or services not being represented in the NJSTART Marketplace. The Contractor shall ensure that the catalog complies with the scope, and terms and conditions of this Contract. Any identified deviation from the Contract must be corrected immediately. Any catalog that does not comply with the scope and terms and conditions of this Contract can lead to a breach of contract and will be escalated to the Division of Purchase and Property’s Contract Compliance and Audit Unit for review and possible action.  
E. Retention and Inspection of Records and Audit - The Contractor shall keep records of all sales made to all Using Agencies in sufficient detail to enable the State to determine the Procurement Efficiency Program Fee payable by the Contractor. The State and/or Periscope may examine and audit, at its own expense, Contractor’s sales records and Sales Reports for completeness and accuracy. If such examination reveals underpayment of the Procurement Efficiency Program Fee, the Contractor shall immediately pay to Periscope the amount of deficiency. If the examination reveals an underpayment of 5% or more, then the Contractor shall reimburse the State and/or Periscope for the cost of the audit. 

[bookmark: _Toc169179982]DATA SECURITY REQUIREMENTS – CONTRACTOR RESPONSIBILITY 
Not applicable to this procurement.



[bookmark: _4.4.1.1_Ownership_Disclosure][bookmark: _4.4.1.1_Signatory_page][bookmark: _4.4.2.3_Contract_Schedule][bookmark: _4.4.2.4_mobilization_and][bookmark: _Toc169179983]MODIFICATIONS TO THE STATE OF NEW JERSEY STANDARD TERMS AND CONDITIONS

[bookmark: _Toc169179984]INDEMNIFICATION
Section 4.1 of the SSTC is deleted in its entirety and replaced with the following:

4.1 INDEMNIFICATION
The Contractor’s liability to the State and its employees in third party suits shall be as follows:
A. The Contractor shall assume all risk of and responsibility for, and agrees to indemnify, defend, and save harmless the State and its officers, agents, servants and employees, from and against any and all third party claims, demands, suits, actions, recoveries, judgments and costs and expenses in connection therewith:
1. For or on account of the loss of life, property or injury or damage to the person, body or property of any person or persons whatsoever, which shall arise from or result directly or indirectly from the work and/or products supplied under this Contract or the order; and
2. For or on account of the use of any patent, copyright, trademark, trade secret or other proprietary right of any copyrighted or uncopyrighted composition, secret process, patented or unpatented invention, article or appliance (“Intellectual Property Rights”) furnished or used in the performance of this Contract; and
3. The Contractor’s indemnification and liability under subsection (A) is not limited by, but is in addition to the insurance obligations.  
B. In the event of a claim or suit involving third-party Intellectual Property Rights, the Contractor, at its option, may: 
1. procure for the State the legal right to continue the use of the product; 
2. replace or modify the product to provide a non-infringing product that is the functional equivalent; or 
3. in the event that the Contractor cannot do (1) or (2) refund the purchase price less a reasonable allowance for use that is agreed to by both parties.  
C. The State will:
1. promptly notify Contractor in writing of the claim or suit; 
2. give Contractor control of the defense and settlement of any claim that is subject to Section 4.1(a); provided; however, that the State must approve any settlement of the alleged claim, which approval shall not be unreasonably withheld. The State may observe the proceedings relating to the alleged claim and confer with the Contractor at its expense. 
D. Notwithstanding the foregoing, Contractor has no obligation or liability for any claim or suit concerning third-party Intellectual Property Rights arising from: 
1. the State’s unauthorized combination, operation, or use of a product supplied under this Contract with any product, device, or Software not supplied by Contractor; 
2. the State’s unauthorized alteration or modification of any product supplied under this Contract; 
3. the Contractor’s compliance with the State’s designs, specifications, requests, or instructions, provided that if the State provides Contractor with such designs, specifications, requests, or instructions, Contractor reviews same and advises that such designs, specifications, requests or instructions present potential issues of patent or copyright infringement and the State nonetheless directs the Contractor to proceed with one (1) or more designs, specifications, requests or instructions that present potential issues of patent or copyright infringement; or 
4. the State’s failure to promptly implement a required update or modification to the product provided by Contractor. 
E. Contractor will be relieved of its responsibilities under Subsection 4.1(a)(i) and (ii) for any claims made by an unaffiliated third party that arise solely from the actions or omissions of the State, its officers, employees or agents.  
F. Subject to the New Jersey Tort Claims Act (N.J.S.A. 59:1-1 et seq.), the New Jersey Contractual Liability Act (N.J.S.A. 59:13-1 et seq.) and the appropriation and availability of funds, the State will be responsible for any cost or damage arising out of actions or inactions of the State, its employees or agents under Subsection 4.1(a)(i) and (ii) which results in an unaffiliated third party claim.  This is the Contractor’s exclusive remedy for these claims;

G. This section states the entire obligation of Contractor and its suppliers, and the exclusive remedy of the State, in respect of any infringement or alleged infringement of any Intellectual Property Rights.  This indemnity obligation and remedy are given to the State solely for its benefit and in lieu of, and Contractor disclaims, all warranties, conditions and other terms of non-infringement or title with respect to any product; and
H. Furthermore, neither Contractor nor any attorney engaged by Contractor shall defend the claim in the name of the State of New Jersey or any Authorized Purchaser, nor purport to act as legal representative of the State of New Jersey or any Authorized Purchaser, without having provided notice to the Director of the Division of Law in the Department of Law and Public Safety and to the Director of the Division of Purchase and Property.  The State of New Jersey may, at its election and expense, assume its own defense and settlement; and
I. The State of New Jersey will not indemnify, defend, pay or reimburse for claims or take similar actions on behalf of the Contractor.
[bookmark: _Toc169179985]INSURANCE

[bookmark: _Toc400531536][bookmark: _Toc428534007][bookmark: _Toc32310729][bookmark: _Toc169179986]PROFESSIONAL LIABILITY INSURANCE
Section 4.2 of the SSTC is supplemented with the following:  

Professional Liability Insurance:  The Contractor shall carry Errors and Omissions, Professional Liability Insurance, and/or Professional Liability Malpractice Insurance sufficient to protect the Contractor from any liability arising out of the professional obligations performed pursuant to the requirements of this Contract.  The insurance shall be in the amount of not less than $1,000,000 or higher if appropriate per each occurrence, and in such policy forms as shall be approved by the State.  If the Contractor has claims-made coverage and subsequently changes carriers during the term of this Contract, it shall obtain from its new Errors and Omissions, Professional Liability Insurance, and/or Professional Malpractice Insurance carrier an endorsement for retroactive coverage.















































[bookmark: _Toc169179987]QUOTE EVALUATION AND AWARD

[bookmark: _Toc400531542][bookmark: _Toc428534014][bookmark: _Toc32310736][bookmark: _Toc169179988]RIGHT TO WAIVE
Pursuant to N.J.A.C. 17:12-2.7(d) the Director may waive minor irregularities or omissions in a Quote.  The Director reserves the right to waive a requirement provided that the requirement does not materially affect the procurement or the State's interests associated with the procurement.
[bookmark: _Toc400531543][bookmark: _Toc428534015][bookmark: _Toc32310737]
[bookmark: _Toc169179989]DIRECTOR’S RIGHT TO ACCEPT OR REJECT A QUOTE
The Director reserves the right to reject any or all Quotes, or to award in whole or in part if deemed to be in the best interest of the State to do so. The Director shall have authority to award Contracts in accordance with N.J.S.A. 52:34-12. 

[bookmark: _Toc169179990]RECIPROCITY FOR JURISDICTIONAL BIDDER PREFERENCE
In accordance with N.J.S.A. 52:32-1.4 and N.J.A.C. 17:12-2.13, the State of New Jersey will invoke reciprocal action against an out-of-State Bidder whose state or locality maintains a preference practice for its in-state Bidders.  The State of New Jersey will use the annual surveys compiled by the Council of State Governments, National Association of State Procurement Officials, or the National Institute of Governmental Purchasing or a State’s statutes and regulations to identify States having preference laws, regulations, or practices and to invoke reciprocal actions. The State of New Jersey may obtain additional information as it deems appropriate to supplement the stated survey information.

A Bidder may submit information related to preference practices enacted for a State or Local entity outside the State of New Jersey. This information may be submitted in writing as part of the Quote response, including name of the locality having the preference practice, as well as identification of the county and state, and should include a copy of the appropriate documentation, i.e., resolution, regulation, law, notice to Bidder, etc.  It is the responsibility of the Bidder to provide documentation with the Quote or submit it to the Director within five (5) business days after the deadline for Quote submission.  Written evidence for a specific procurement that is not provided to the Director within five (5) business days of the public Quote submission date may not be considered in the evaluation of that procurement, but may be retained and considered in the evaluation of subsequent procurements.

[bookmark: _Toc400531545][bookmark: _Toc428534017][bookmark: _Toc32310739][bookmark: _Toc169179991]CLARIFICATION OF QUOTE
After the Quote Opening Date, unless requested by the State as noted below, Bidder contact with the Procurement Bureau regarding this Bid Solicitation and the submitted Quote is not permitted. 

After the Quotes are reviewed, one (1), some or all of the Bidders may be asked to clarify certain aspects of its Quote.  A request for clarification may be made in order to resolve minor ambiguities, irregularities, informalities or clerical errors.  Clarifications cannot correct any deficiencies, material omissions, or used to revise or modify a Quote.

The Director reserves the right to request that a Bidder to explain, in detail, how the Quote price was determined.

[bookmark: _Toc32310741][bookmark: _Toc118513837][bookmark: _Toc400531547][bookmark: _Toc428534019][bookmark: _Toc169179992]ORAL PRESENTATION 
Not applicable to this procurement.

[bookmark: _Toc169179993]TIE QUOTES
Tie Quotes will be awarded by the Director in accordance with N.J.A.C. 17:12-2.10. 

[bookmark: _Toc169179994]STATE'S RIGHT TO INSPECT BIDDER’S FACILITIES
The State reserves the right to inspect the Bidder’s establishment before making an award, for the purposes of ascertaining whether the Bidder has the necessary facilities for performing the Contract.

[bookmark: _Toc169179995]STATE'S RIGHT TO CHECK REFERENCES
The State may also consult with clients of the Bidder during the evaluation of Quotes. Such consultation is intended to assist the State in making a Contract award that is most advantageous to the State.

[bookmark: _Toc169179996]EVALUATION CRITERIA
The following evaluation criteria categories, not necessarily listed in order of significance, will be used to evaluate Quotes received in response to this Bid Solicitation.  The evaluation criteria categories may be used to develop more detailed evaluation criteria to be used in the evaluation process.

[bookmark: _Toc118513839][bookmark: _Toc400531549][bookmark: _Toc428534021][bookmark: _Toc32310743][bookmark: _Toc169179997]TECHNICAL EVALUATION CRITERIA
The following criteria will be used to evaluate and score Quotes received in response to this Bid Solicitation.  Each criterion will be scored, and each score multiplied by a predetermined weight to develop the Technical Evaluation Score:
A. Personnel:  The qualifications and experience of the Bidder’s management, supervisory, and key personnel assigned to the Contract, including the candidates recommended for each of the positions/roles required;
B. Experience of firm:  The Bidder’s documented experience in successfully completing Contract of a similar size and scope in relation to the work required by this Bid Solicitation; and
C. Ability of firm to complete the Scope of Work based on its Technical Quote:  The Bidder’s demonstration in the Quote that the Bidder understands the requirements of the Scope of Work and presents an approach that would permit successful performance of the technical requirements of the Contract.

[bookmark: _Toc118513840][bookmark: _Toc400531550][bookmark: _Toc428534022][bookmark: _Toc32310744][bookmark: _Toc169179998]PRICE EVALUATION
The Procurement Bureau will utilize a weighted consumption/market basket model to evaluate pricing.  The pricing model will be date-stamped and entered into the record before Quote opening.  

[bookmark: _Toc118513841][bookmark: _Toc400531551][bookmark: _Toc428534023][bookmark: _Toc32310745][bookmark: _Toc169179999]QUOTE DISCREPANCIES
In evaluating Quotes, discrepancies between words and figures will be resolved in favor of words.  Discrepancies between Unit Prices and totals of Unit Prices will be resolved in favor of Unit Prices.  Discrepancies in the multiplication of units of work and Unit Prices will be resolved in favor of the Unit Prices.  Discrepancies between the indicated total of multiplied Unit Prices and units of work and the actual total will be resolved in favor of the actual total.  Discrepancies between the indicated sum of any column of figures and the correct sum thereof will be resolved in favor of the correct sum of the column of figures.

[bookmark: _Toc118513842][bookmark: _Toc400531553][bookmark: _Toc428534025][bookmark: _Toc32310747][bookmark: _Toc169180000]NEGOTIATION
In accordance with N.J.S.A. 52:34-12(f) and N.J.A.C. 17:12-2-7, after evaluating Quotes, the Procurement Bureau may establish a competitive range and enter into negotiations with one (1) Bidder or multiple Bidders within this competitive range.  The primary purpose of negotiations is to maximize the State’s ability to obtain the best value based on the mandatory requirements, evaluation criteria, and cost.  Multiple rounds of negotiations may be conducted with one (1) Bidder or multiple Bidders.  Negotiations will be structured by the Procurement Bureau to safeguard information and ensure that all Bidders are treated fairly.

Negotiations will be conducted only in those circumstances where it is deemed by the Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Bidder is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Contract award based on the content of the initial submission.  

If the Procurement Bureau contemplates negotiation, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Bidder will be publicly announced at the Quote opening.

[bookmark: _Toc169180001]BEST AND FINAL OFFER (BAFO) 
The Procurement Bureau may invite one (1) Bidder or multiple Bidders to submit a Best and Final Offer (BAFO). Said invitation will establish the time and place for submission of the BAFO. Any BAFO that does not result in more advantageous pricing to the State will not be considered, and the State will evaluate the Bidder’s most advantageous previously submitted pricing.

The Division may conduct more than one (1) round of BAFO in order to attain the best value for the State. 

BAFOs will be conducted only in those circumstances where it is deemed by the Procurement Bureau or Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Bidder is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Contract award based on the content of the initial submission 

If the Procurement Bureau contemplates BAFOs, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Bidder will be publicly announced at the Quote opening.

[bookmark: _Toc32310748][bookmark: _Toc169180002]“REQUEST FOR REVISION” WITHIN NJSTART
The State may request a revision of the Bidder’s Quote within NJSTART. The Bidder shall respond to the “Request for Revision” only for the reason(s) identified by the State. Any changes made by a Bidder to the Quote other than as requested by the State shall be considered null and void. 

[bookmark: _Toc400531554][bookmark: _Toc428534026][bookmark: _Toc32310749][bookmark: _Toc169180003]POOR PERFORMANCE
A Bidder with a history of performance problems may be bypassed for consideration of an award issued as a result of this Bid Solicitation. The following materials may be reviewed to determine Bidder performance:  
A. Contract cancellations for cause pursuant to State of New Jersey Standard Terms and Conditions Section 5.7(B); 
B. Information contained in Contractor performance records; 
C. Information obtained from audits or investigations conducted by a local, state or federal agency of the Bidder’s work experience; 
D. Current licensure, registration, and/or certification status and relevant history thereof; or 
E. Bidder’s status or rating with established business/financial reporting services, as applicable.  

Bidders should note that this list is not exhaustive.

[bookmark: _Toc169180004]RECOMMENDATION FOR AWARD 
After the evaluation of the submitted Quotes is complete, the Procurement Bureau will recommend to the Director for award, the responsible Bidder(s) whose Quote, conforming to this Bid Solicitation, is most advantageous to the State, price and other factors considered.  The Director may accept, reject or modify the recommendation of the Procurement Bureau.

[bookmark: _Toc400531561][bookmark: _Toc428534033][bookmark: _Toc32310756][bookmark: _Toc169180005]CONTRACT AWARD
Contract award(s) will be made with reasonable promptness by written notice to those responsible Bidder(s), whose Quote(s), conforming to this Bid Solicitation, is(are) most advantageous to the State, price, and other factors considered.  Any or all Quotes may be rejected when the State Treasurer or the Director determines that it is in the public interest to do so.  Contract awards will be publicly posted under the relevant contract number and available on NJSTART.

The State intends to make one (1) award per Region (Region1, Region 2, Region 3, and Region 4), and each Region shall be awarded separately or any combination thereof. For each Region bid, the Bidder must be capable of providing services to any location as listed in Section 1.2.1 of this Bid Solicitation.
.



[bookmark: _Toc169180006]GLOSSARY

[bookmark: _Toc169180007]CROSSWALK

	Current DPP Template Term
	Equivalent Statutory, Regulatory NJSTART and/or Legacy Term

	Bid Solicitation 
	Request For Proposal (RFP)/Solicitation

	Bid Amendment 
	Addendum

	Contract 
	Master Blanket Purchase Order (Blanket/Blanket P.O.)

	Contract Amendment 
	Change Order

	Administrative Change Order
	Change Order

	Quote
	Proposal/Bid

	Contractor
	Vendor/Contractor

	Bidder
	Bidder/Contractor



[bookmark: _Toc169180008]DEFINITIONS
Unless otherwise specified in the Bid Solicitation, the following definitions will be part of any Contract awarded, or order placed, as a result of this Bid Solicitation.  Note that not all definitions included here apply to all Bid Solicitations.
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Acceptance – The written confirmation by the Using Agency that Contractor has completed a Deliverable according to the specified requirements.

Administrative Change Order – A unilateral administrative modification to the Contract in the NJSTART system by the Division. Administrative Change Orders are not to be considered formal Contract Amendments.
All-Inclusive Hourly Rate – An hourly rate comprised of all direct and indirect costs including, but not limited to: labor costs, overhead, fee or profit, clerical support, travel expenses, per diem, safety equipment, materials, supplies, managerial support and all documents, forms, and reproductions thereof.  This rate also includes portal-to-portal expenses as well as per diem expenses such as food.

Apparel – means any clothing, headwear, linens or fabric.  

Apparel Contracts – include all purchases, rentals or other acquisition of apparel products by the State of New Jersey, including authorizations by the State of New Jersey for contractors to sell apparel products through cash allowances or vouchers issued by the State of New Jersey, and license agreements with a public body.

Apparel Production – includes the cutting and manufacturing of apparel products performed by the contractor or by any subcontractors, but not including the production of supplies or sundries such as buttons, zippers, and thread.

Approved Products – Those products that have been identified in Bid Solicitation as meeting Using Agency needs and confirmed as meeting product specifications.

Best and Final Offer or BAFO – Pricing timely submitted by a Bidder upon invitation by the Procurement Bureau after Quote opening, with or without prior discussion or negotiation.

Bid or Bid Solicitation – The documents which establish the bidding and Contract requirements and solicits Quotes to meet the needs of the Using Agencies as identified herein, and includes the Bid Solicitation, State of New Jersey Standard Terms and Conditions (SSTC), State-Supplied Price Sheet, Attachments, and Bid Amendments.

Bid Amendment – Written clarification or revision to this Bid Solicitation issued by the Division. Bid Amendments, if any, will be issued prior to Quote opening.

Bid Opening Date – The date Quotes will be opened for evaluation and closed to further Quote submissions.
Bid Security - means a guarantee, in a form acceptable to the Division, that the bidder, if selected, will accept the contract as bid; otherwise, the bidder or, as applicable, its guarantor will be liable for the amount of the loss suffered by the State, which loss may be partially or completely recovered by the State in exercising its rights against the instrument of bid security.

Bidder – An entity offering a Quote in response to the Division’s Bid Solicitation.

Breach of Security – as defined by N.J.S.A. 56:8-161, means unauthorized access to electronic files, media, or data containing Personal Data that compromises the security, confidentiality, or integrity of Personal Data when access to the Personal Data has not been secured by encryption or by any other method or technology that renders the Personal Data unreadable or unusable.  Good faith acquisition of Personal Data by an employee or agent of the Provider for a legitimate business purpose is not a Breach of Security, provided that the Personal Data is not used for a purposes unrelated to the business or subject to further unauthorized disclosure.  

Business Day – Any weekday, excluding Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Calendar Day – Any day, including Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Commercial off the Shelf Software or COTS – Software provided by Provider that is commercially available and that can be used with little or no modification.

Customized Software – COTS that is adapted or configured by Provider to meet specific requirements of the Authorized Purchaser that differ from the standard requirements of the base product. For the avoidance of doubt, “Customized Software” is not permitted to be sold to the State under the scope of this Contract.

Contract – The Contract consists of the State of NJ Standard Terms and Conditions (SSTC), the Bid Solicitation, the responsive Quote submitted by a responsible Bidder as accepted by the State, the notice of award, any Best and Final Offer, any subsequent written document memorializing the agreement, any modifications to any of these documents approved by the State and any attachments, Bid Amendment or other supporting documents, or post-award documents including Contract Amendments agreed to by the State and the Contractor, in writing.

Contract Amendment – An amendment, alteration, or modification of the terms of a Contract between the State and the Contractor(s). A Contract Amendment is not effective until it is signed and approved in writing by the person with the appropriate signing authority.  Contract Amendments are tracked using Change Orders in NJSTART. Please note that Administrative Change Orders (see definition above) are not considered Contract Amendments.  

Contractor – The Bidder awarded a Contract resulting from this Bid Solicitation.

Contractor Intellectual Property – Any intellectual property that is owned by Contractor and contained in or necessary for the use of the Deliverables or which the Contractor makes available for the State to use as part of the work under the Contract.  Contractor Intellectual Property includes COTS or Customized Software owned by Contractor, Contractor’s technical documentation, and derivative works and compilations of any Contractor Intellectual Property.

Cooperative Purchasing Program – The Division’s intrastate program that provides procurement-related assistance to New Jersey local governmental entities and boards of education, State and county colleges and other public entities having statutory authority to utilize select State Contract s issued by the Division, pursuant to the provisions of N.J.S.A. 52:25-16.1 et seq.
Cooperative Purchasing Participants – These participants include quasi-State entities, counties, municipalities, school districts, volunteer fire departments, first aid squads, independent institutions of higher learning, County colleges, and State colleges.

Days After Receipt of Order (ARO) – The number of calendar days ‘After Receipt of Order’ in which the Using Agency will receive the ordered materials and/or services.

Dealer/Distributor – A Company authorized by a Bidder or Contractor as having the contractual ability to accept and fulfill orders and receive payments directly on behalf of the Contractor that is awarded a Contract.  Any authorized Dealer/Distributor must agree to all terms and conditions contained within the Bid Solicitation and must agree to provide all products and services in accordance with the Contract specifications, terms, conditions and pricing.  

Deliverable – Goods, products, Services and Work Product that Contractor is required to deliver to the State under the Contract.
Director – Director, Division of Purchase and Property, Department of the Treasury, who by statutory authority is the Chief Contracting Officer for the State of New Jersey; or the Director’s designee.

Disabled Veterans’ Business - means a business which has its principal place of business in the State, is independently owned and operated and at least 51% of which is owned and controlled by persons who are disabled veterans or a business which has its principal place of business in this State and has been officially verified by the United States Department of Veterans Affairs as a service disabled veteran-owned business for the purposes of department contracts pursuant to federal law.  N.J.S.A. 52:32-31.2.

Disabled Veterans’ Business Set-Aside Contract – means a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from disabled veterans’ businesses, or a portion of a Contract when that portion has been so designated.  N.J.S.A. 52:32-31.2.

Discount – The standard price reduction applied by the Bidder to all items.

Division – The Division of Purchase and Property.

Equivalent Products – Products offered other than those identified as an Approved Product in this Bid Solicitation that meet the specifications herein. Equivalent Products will be evaluated to ensure that they meet all technical, nutritional, and packaging specifications herein as part of the Quote evaluation process.

Evaluation Committee – A group of individuals or a Division staff member assigned by the Director to review and evaluate Quotes submitted in response to this Bid Solicitation and recommend a Contract award to the Director.

Firm Fixed Price – A price that is all-inclusive of direct cost and indirect costs, including, but not limited to, direct labor costs, overhead, fee or profit, clerical support, equipment, materials, supplies, managerial (administrative) support, all documents, reports, forms, travel, reproduction and any other costs.

Hardware – Includes computer equipment and any Software provided with the Hardware that is necessary for the Hardware to operate.

Internet of Things (IoT) – the network of physical devices, vehicles, home appliances and other items embedded with electronics, software, sensors, actuators, and network connectivity which enables these objects to connect and exchange data.

Intrastate cooperative purchasing participants – refers to political subdivisions, volunteer fire departments and first aid squads, and independent institutions of higher education and school districts pursuant to N.J.S.A. 52:25-16.1 et seq., State and county colleges pursuant to N.J.S.A. 18A:64-60 and 18A:64A-25.9, quasi-State agencies and independent authorities pursuant to N.J.S.A. 52:27B-56.1, and other New Jersey public entities having statutory authority to utilize select State contracts issued by the Division.

Joint Venture – A business undertaking by two (2) or more entities to share risk and responsibility for a specific project.

Life cycle assessment – The comprehensive examination of a product’s environmental and economic aspects and potential impacts throughout its lifetime, including raw material extraction, transportation, manufacturing, use and disposal.

Life cycle cost – The amortized total cost of a product, including capital costs, installation costs, operating costs, maintenance costs, and disposal costs discounted over the lifetime of the product.

Master Blanket Purchase Order (Blanket/Blanket P.O.) – A Term Contract that allows repeated purchases from an awarded contract.

Materials in Solid Waste – Material found in the various components of the solid waste stream. General, solid waste has several components, such as municipal solid waste (MSW), construction and demolition debris (C&D), and nonhazardous industrial waste.  Under RCRA Section 6002, EPA considers materials recovered from any component of the solid waste stream when designating items containing Recovered Materials.

May – Denotes that which is permissible or recommended, not mandatory.

Mobile Device – means any device used by Provider that can move or transmit data, including but not limited to laptops, hard drives, and flash drives.

Must – Denotes that which is a mandatory requirement.  

Net Purchases – means the total gross purchases, less credits, taxes, regulatory fees and separately stated shipping charges not included in unit prices, made by Intrastate Cooperative Purchasing Participants, regardless of whether or not NJSTART is used as part of the purchase process.

No Bid – The Bidder is not submitting a price Quote for an item on a price line.

No Charge – The Bidder will supply an item on a price line free of charge.

Non-Public Data – means data, other than Personal Data, that is not subject to distribution to the public as public information. Non-Public Data is data that is identified by the State as non-public information or otherwise deemed to be sensitive and confidential by the State because it contains information that is exempt by statute, ordinance or administrative rule from access by the general public as public information.

Percentage Discount or Markup – The percentage bid applied as a Markup or a Discount to a firm, fixed price contained within a price list/catalog. 

Performance Security – means a guarantee, executed subsequent to award, in a form acceptable to the Division, that the successful bidder will complete the contract as agreed and that the State will be protected from loss in the event the contractor fails to complete the contract as agreed.

Personal Data means – 
“Personal Information” as defined in N.J.S.A. 56:8-161, means an individual’s first name or first initial and last name linked with any one or more of the following data elements: (1) Social Security number, (2) driver’s license number or State identification card number or (3) account number or credit or debit card number, in combination with any required security code, access code, or password that would permit access to an individual’s financial account.  Dissociated data that, if linked would constitute Personal Information is Personal Information if the means to link the dissociated were accessed in connection with access to the dissociated data.  Personal Information shall not include publicly available information that is lawfully made available to the general public from federal, state or local government records, or widely distributed media; and/or 

Data, either alone or in combination with other data, that includes information relating to an individual that identifies the person or entity by name, identifying number, mark or description that can be readily associated with a particular individual and which is not a public record, including but not limited to, Personally Identifiable Information (PII); government-issued identification numbers (e.g., Social Security, driver’s license, passport); Protected Health Information (PHI) as that term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and defined below; and Education Records, as that term is defined in the Family Educational Rights and Privacy Act (FERPA), 20 U.S.C. § 1232g.

Personally Identifiable Information or PII - as defined by the U.S. Department of Commerce, National Institute of Standards and Technology, means any information about an individual maintained by an agency, including (1) any information that can be used to distinguish or trace an individual’s identity, such as name, social security number, date and place of birth, mother’s maiden name, or biometric records; and (2) any other information that is linked or linkable to an individual, such as medical, educational, financial, and employment information.

Post-Consumer Material – Material or finished product that has served its intended use and has been diverted or recovered from waste destined for disposal, having completed its life as a consumer item.  Post-Consumer Materials are part of the broader category of Recovered Materials.

Pre-Consumer Material – Materials generated in manufacturing and converting processes, such as manufacturing scrap and trimmings/cuttings.

Price List/Catalog – A document published by a manufacturer, resellers, Dealers, or Distributors that typically contains product descriptions, a list of products with fixed prices to which a Bidder’s percentage discount or markup bid is applied. 

Procurement Bureau (Bureau) – The Division unit responsible for the preparation, advertisement, and issuance of Bid Solicitations, for the tabulation of Quotes and for recommending award(s) of Contract(s) to the Director and the Deputy Director.

Project – The undertakings or services that are the subject of this Bid Solicitation.

Protected Health Information or PHI – has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 means Individually Identifiable Health Information (as defined below) transmitted by electronic media, maintained in electronic media, or transmitted or maintained in any other form or medium. PHI excludes education records covered by the Family Educational Rights and Privacy Act (FERPA), as amended, 20 U.S.C. 1232g, records described at 20 U.S.C. 1232g(a)(4)(B)(iv) and employment records held by a covered entity in its role as employer. The term “Individually Identifiable Health Information” has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and means information that is a subset of Protected Health Information, including demographic information collected from an individual, and (1) is created or received by a health care provider, health plan, employer or health care clearinghouse; and (2) relates to the past, present or future physical or mental health or condition of an individual; the provision of health care to an individual; or the past, present or future payment for the provision of health care to an individual; and (a) that identifies the individual; or (b) with respect to which there is a reasonable basis to believe the information can be used to identify the individual.

Purchases - means the total gross purchases, less credits, taxes, regulatory fees and separately stated shipping charges not included in unit prices, made regardless of whether or not NJSTART is used as part of the purchase process.

Quasi-State Agency – is any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member, as defined in N.J.S.A. 52:27B-56.1, provided that any sale to any such bi-state governmental entity is for use solely within the State of New Jersey.

Quick Reference Guides (QRGs) – Informational documents which provide Vendors with step-by-step instructions to navigate the NJSTART eProcurement System. QRGs are available on the NJSTART Vendor Support Page.

Quote – Bidder’s timely response to the Bid Solicitation including, but not limited to, technical Quote, price Quote including Best and Final Offer, any licenses, forms, certifications, clarifications, negotiated documents, and/or other documentation required by the Bid Solicitation.

Quote Opening Date – The date Quotes will be opened for evaluation and closed to further Quote submissions.

Recovered Material – Waste material and byproduct that have been recovered or diverted from solid waste, but does not include materials and byproducts generated from, and commonly reused within, an original manufacturing process.

Recycling – The series of activities, including collection, separation, and processing, by which products or other materials are recovered from the solid waste stream for use in the form of raw materials in the manufacture of new products other than fuel for producing heat or power by combustion.
Recyclability – The ability of a product or material to be recovered from, or otherwise diverted from, the solid waste stream for the purpose of recycling.
Retainage – The amount withheld from the Contractor payment that is retained and subsequently released upon satisfactory completion of performance milestones by the Contractor.

Revision – A response to a BAFO request or a requested clarification of the Bidder’s Quote. 

RMAN – Recovered Materials Advisory Notices provide purchasing guidance and recommendations for Recovered and Post-Consumer Material content levels for designated items. 

Security Incident – means the potential access by non-authorized person(s) to Personal Data or Non-Public Data that the Provider believes could reasonably result in the use, disclosure, or access or theft of State’s unencrypted Personal Data or Non-Public Data within the possession or control of the Provider. A Security Incident may or may not turn into a Breach of Security.

Services – Includes, without limitation (i) Information Technology (IT) professional services, (ii) Software and Hardware-related services, including without limitation, installation, configuration, and training, and (iii) Software and Hardware maintenance and support and/or Software and Hardware technical support services. 

Shall – Denotes that which is a mandatory requirement.  

Should – Denotes that which is permissible or recommended, not mandatory.

Small Business – Pursuant to N.J.S.A. 52:32-19, N.J.A.C. 17:13-1.2, and N.J.A.C. 17:13-2.1, “small business” means a business that meets the requirements and definitions of “small business” and has applied for and been approved by the New Jersey Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit as (i) independently owned and operated, (ii) incorporated or registered in and has its principal place of business in the State of New Jersey; (iii)  has 100 or fewer full-time employees; and has gross revenues falling in one (1) of the six (6) following categories:  
For goods and services - (A) 0 to $500,000 (Category I); (B) $500,001 to $5,000,000 (Category II); and (C) $5,000,001 to $12,000,000, or the applicable federal revenue standards established at 13 CFR 121.201, whichever is higher (Category III). 
For construction services: (A) 0 to $3,000,000 (Category IV); (B) gross revenues that do not exceed 50 percent of the applicable annual revenue standards established at 13 CFR 121.201 (Category V); and (C) gross revenues that do not exceed the applicable annual revenue standards established at CFR 121.201, (Category VI).

Small Business Set-Aside Contract – means (1) a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from small businesses, or (2) a portion of a Contract when that portion has been so designated.”  N.J.S.A. 52:32-19.

Software – means, without limitation, computer programs, source codes, routines, or subroutines supplied by Provider, including operating software, programming aids, application programs, application programming interfaces and software products, and includes COTS, unless the context indicates otherwise.  

Software as a Service or SaaS – means the capability provided to a purchaser to use the Provider’s applications running on a cloud infrastructure. The applications are accessible from various client devices through a thin client interface such as a Web browser (e.g., Web-based email) or a program interface. The purchaser does not manage or control the underlying cloud infrastructure, including network, servers, operating systems, storage or even individual application capabilities, with the possible exception of limited user-specific application configuration settings.

State – The State of New Jersey.

State Confidential Information – shall consist of State Data and State Intellectual Property  supplied by the State, any information or data gathered by the Contractor in fulfillment of the Contract and any analysis thereof (whether in fulfillment of the Contract or not).

State Contract Manager or SCM – The individual, responsible for the approval of all deliverables, i.e., tasks, sub-tasks or other work elements in the Scope of Work.  The SCM cannot direct or approve a Contract Amendment.

State Data – means all data and metadata created or in any way originating with the State, and all data that is the output of computer processing of or other electronic manipulation of any data that was created by or in any way originated with the State, whether such data or output is stored on the State’s hardware, the Provider’s hardware or exists in any system owned, maintained or otherwise controlled by the State or by the Provider.  State Data includes Personal Data and Non-Public Data.

State Intellectual Property – Any intellectual property that is owned by the State.  State Intellectual Property includes any derivative works and compilations of any State Intellectual Property.

State Price Sheet or State-Supplied Price Sheet – the bidding document created by the State and attached to this Bid Solicitation on which the Bidder submits its Quote pricing as is referenced and described in the Bid Solicitation.   

Subtasks – Detailed activities that comprise the actual performance of a task.
Subcontractor – An entity having an arrangement with a Contractor, whereby the Contractor uses the products and/or services of that entity to fulfill some of its obligations under its State Contract, while retaining full responsibility for the performance of all  Contractor's obligations under the Contract, including payment to the Subcontractor.  The Subcontractor has no legal relationship with the State, only with the Contractor.
Task – A discrete unit of work to be performed.

Third Party Intellectual Property – Any intellectual property owned by parties other than the State or Contractor and contained in or necessary for the use of the Deliverables.  Third Party Intellectual Property includes COTS owned by Third Parties, and derivative works and compilations of any Third Party Intellectual Property. 
Unit Cost or Unit Price – All-inclusive, firm fixed price charged by the Bidder for a single unit identified on a price line.

US CERT – United States Computer Emergency Readiness Team.

USEPA – United States Environmental Protection Agency.

Using Agency[ies] – A State department or agency, a quasi-State governmental entity, or an Intrastate Cooperative Purchasing participant, authorized to purchase products and/or services under a Contract procured by the Division. 

Vendor – Either the Bidder or the Contractor.

Work Product – Every invention, modification, discovery, design, development, customization, configuration, improvement, process, Software program, work of authorship, documentation, formula, datum, technique, know how, secret, or intellectual property right whatsoever or any interest therein (whether patentable or not patentable or registerable under copyright or similar statutes or subject to analogous protection) that is specifically made, conceived, discovered, or reduced to practice by Contractor or Contractor’s subcontractors or a third party engaged by Contractor or its subcontractor pursuant to the Contract Notwithstanding anything to the contrary in the preceding sentence, Work Product does not include State Intellectual Property, Contractor Intellectual Property or Third Party Intellectual Property. 
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AASHTO – American Association of State Highway and Transportation Officials. A Standard for the materials being used for the type of work herein this Bid Solicitation. 
Aggregate - A whole formed by combining several (typically disparate) elements.
ASTM – American Society for Testing Materials. A Standard for sizing of the materials being used for the type of work herein this Bid Solicitation. 
Bituminous Distributor - A truck equipped with a tank body and with a system for pumping hot tar, road oil, or other bituminous material through a perforated spray bar at the rear; used to lay down a surface coating of the bituminous material.

Cationic Emulsified Asphalts - The first designation is based on electrical charge. Cationic (positively charged) emulsions are identified with a “C.” If the C is not included, the emulsion is normally anionic, negatively charged.     

Certification of Compliance - A document certified by a competent authority that the supplied good or service meets the required specifications.

Chip and Oil – A generic term and synonym for Asphaltic Oil and Aggregate Surface treatment. 

Cut-back asphalts - A combination of asphalt cement and petroleum solvent. Like emulsions, cutbacks are used because they reduce asphalt viscosity for lower temperature uses (tack coats, fog seals, slurry seals, stabilization material). Similar to emulsified asphalts, after a cutback asphalt is applied, the petroleum solvent evaporates leaving behind asphalt cement residue on the surface to which it was applied. A cutback asphalt is said to “cure” as the petroleum solvent evaporates away.

Dynamic Compactor - A method that is used to increase the density of the soil when certain subsurface constraints make other methods inappropriate. It is a method that is used to increase the density of soil deposits. The process involves dropping a heavy weight repeatedly on the ground at regularly spaced intervals. The weight and the height determine the amount of compaction that would occur. The weight that is used depends on the degree of compaction desired and is between 8 tonne to 36 tonne. The height varies from 1m to 30m.

Emulsified Asphalts - A suspension of small asphalt cement globules in water, which is assisted by an emulsifying agent (such as soap). The emulsifying agent assists by imparting an electrical charge to the surface of the asphalt cement globules so that they do not coalesce (Roberts et al., 1996[1]).
Flash Point - When the item will combust. 

Fly Ash - A coal combustion product that is composed of the particulates (fine particles of burned fuel) that are driven out of coal-fired boilers together with the flue gases. Ash that falls to the bottom of the boiler is called bottom ash. In modern coal-fired power plants, fly ash is generally captured by electrostatic precipitators or other particle filtration equipment before the flue gases reach the chimneys. Together with bottom ash removed from the bottom of the boiler, it is known as coal ash. Depending upon the source and composition of the coal being burned, the components of fly ash vary considerably, but all fly ash includes substantial amounts of silicon dioxide (SiO2) (both amorphous and crystalline), aluminum oxide (Al2O3) and calcium oxide (CaO), the main mineral compounds in coal-bearing rock strata.

Gallon - A unit of volume for liquid measure equal to four (4) quarts, in particular.

Inverted Emulsified Asphalts - Simply a suspension of small asphalt cement globules in water, which is assisted by an emulsifying agent (such as soap). The emulsifying agent assists by imparting an electrical charge to the surface of the asphalt cement globules so that they do not coalesce (Roberts et al., 1996[1]). Emulsions are used because they effectively reduce asphalt viscosity for lower temperature uses (tack coats, fog seals, slurry seals, bituminous surface treatments (BST), stabilization material). Emulsions are typically either anionic (asphalt droplets are negatively charged) or cationic (asphalt particles are positively charged). 
Los Angeles test - A common test used to indicate aggregate toughness and abrasion characteristics. 
MC – Medium Curing. 

No. 6, 67, and 8 - The sizes of the stone to be used to cover the tar. 

OSHA – The Occupational Safety and Health Administration (OSHA): This organization regulates worker safety in the United States and its territories. Health and safety standards are contained in Title 29 of the Code of Federal Regulations (29 CFR), and are available online.
Pneumatic-tire Roller - A large roller that has rubber rear tires. 

Reclaimed asphalt pavement (RAP) - The term given to remove and/or reprocessed pavement materials containing asphalt and aggregates. These materials are generated when asphalt pavements are removed for reconstruction, resurfacing, or to obtain access to buried utilities. When properly crushed and screened, RAP consists of high-quality, well-graded aggregates coated by asphalt cement.
Self-Propelled Power Broom - This piece of equipment is a rotary broom mounted to either a bucket loader or is a walk behind unit, which sweeps up any loose debris on the road.
Three wheel 10-ton roller - Smooth wheeled rollers that consists of one large steel drum in front and two steel drums on the rear. The gross weight of these rollers is in the range of 8-10 tonnes (18000 to 22000 lbs). 

United States Sieve Series – One of two scales used to classify particle sizes. The other scale is the Tyler Equivalent, which is also referred to as the Tyler Mesh Size or Tyler Standard Sieve Series. United States Sieve sizes differ from Tyler Screen sizes in that they are arbitrary numbers. For the sake of this Blanket P.O., only the United States Sieve Series shall be utilized.  
Vibratory Rollers - A compactor type engineering vehicle used to compact soil, gravel, concrete, or asphalt in the construction of roads and foundations. Similar rollers are used also at landfills or in agriculture.

Wobble – Wheel Rollers – A skip body mounted on nine or more oscillating, smooth, rubber-tired wheels for compaction and fine rolling of soil. For the sake of this Bid Solicitation, this piece of equipment shall not be used. 
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