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	Bid Solicitation #
	24DPP00976

	T3063 Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Optional Hook Lift System, Various Bodies, Salt Spreader, Snow Plow & Accessories



	
	Date
	Time

	Due Date For Electronic Questions
Refer to Bid Solicitation Section 2.1 for more information.
	March 8, 2024
	2:00 PM

	Mandatory/Optional Pre-Quote Conference 
Refer to Bid Solicitation Section 2.5 for more information.
	Not Applicable to this Procurement.

	Mandatory/Optional Site Visit
Refer to Bid Solicitation Section 2.4 for more information.
	
Not Applicable to this Procurement.

	Quote Opening Date
Refer to Bid Solicitation Section 3 for more information.
	March 22, 2024
	2:00 PM



Dates are subject to change.  All times contained in the Bid Solicitation refer to Eastern Time. 
All changes will be reflected in Bid Amendments to the Bid Solicitation posted on www.njstart.gov.

	SET-ASIDES

	     Small Business Set-Aside
For Goods and Services:
☐  I          ☐  II          ☐  III
For Construction:
☐  IV          ☐  V          ☐  VI
	☒  Not Applicable
☐  Entire Contract 
☐  Partial Contract 
☐  Subcontracting Only
☐  Preference

	     Disabled Veteran-Owned Business Set-Aside
	☒  Not Applicable
☐  Entire Contract 
☐  Partial Contract 
☐  Subcontracting Only
☐  Preference



	Bid Solicitation Issued By:
State of New Jersey
Department of the Treasury
Division of Purchase and Property
Trenton, New Jersey 08625‑0230
	On Behalf of:
State of New Jersey
Using Agency/Agencies
Cooperative Purchasing Participants



Date:  3/14/2024
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[bookmark: _Toc161300742]INTRODUCTION AND SUMMARY OF THE BID SOLICITATION
This Bid Solicitation is issued by the Department of the Treasury, Division of Purchase and Property (Division), Procurement Bureau, on behalf of the New Jersey Department of Transportation (DOT), other State Using Agencies and the Cooperative Purchasing Program Participants. Quotes submitted in response to this Bid Solicitation shall be through the State of New Jersey’s eProcurement system, NJSTART.  Bidders are advised to thoroughly read all sections of this Bid Solicitation and follow all instructions.  

Bidders are strongly encouraged to visit the NJSTART Vendor Support Page, which contains Quick Reference Guides (QRGs), supporting videos, a glossary of NJSTART terms, and helpdesk contact information.  Bidders should utilize the QRGs before attempting to submit a Quote through NJSTART.   It is the Bidder’s responsibility to ensure that the Quote and attachments have been properly submitted.  Inquiries concerning the use of NJSTART may be directed to njstart@treas.nj.gov. The Division will not respond to substantive questions related to the Bid Solicitation or any other Contract via this email address.

[bookmark: _Toc400531467][bookmark: _Toc428533937][bookmark: _Toc32310614][bookmark: _Toc161300743]PURPOSE AND INTENT
The purpose of this Bid Solicitation is to solicit Quotes for Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Optional Hook Lift System, Various Bodies, Salt Spreader, Snow Plow & Accessories.

It is the intent of the State to award a Contract to that responsible Bidder whose Quote, conforming to this Bid Solicitation is most advantageous to the State of New Jersey (State), price and other factors considered.  The State may award any or all price lines.  The State, however, reserves the right to separately procure individual requirements that are the subject of the Contract during the Contract term, when deemed by the Director of the Division (Director) to be in the State’s best interest.

There are sixteen (16) price lines, which are itemized as follows:

	Price Line Number
	Description

	1 
	19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD

	1A
	Vehicle Manufacturer’s Published Options 

	2
	Hook Lift System

	3
	Stainless Steel Dump Body with Tilt/Dump Interlock

	4
	Stake Body

	5
	Landscape Box Body

	6
	Chipper Body

	7
	Enclosed Steel Storage Body

	8
	Platform Body with 300 -Gallon, Gasoline Powered Herbicide Sprayer 

	9
	Platform Body with Toolboxes

	10 
	Dump Body with Multi-Function Tailgate 

	11
	Salt Spreader

	12
	Snow Plow

	13
	In-Cab Controller for Herbicide Sprayer

	14
	In-Cab Controller for Salt Spreader

	15
	One Set of Parts, Service and Operation and Maintenance Manuals

	16
	Technical Support



Price lines 1 through 16 are grouped to create a single award.  Bidders must bid on all price line items in the group (price lines 1 through 16) to be eligible for a Contract award. 
The State intends to make one (1) Statewide Contract award.
This Bid Solicitation has not been designated as a full or partial Small Business set aside or a Disabled Veteran-Owned Business set aside. 

The State of New Jersey Standard Terms and Conditions (SSTCs) included with this Bid Solicitation will apply to all Contracts made with the State.  These terms are in addition to the terms and conditions set forth in this Bid Solicitation and should be read in conjunction with them unless the Bid Solicitation specifically indicates otherwise.  

[bookmark: _Toc400531468][bookmark: _Toc428533938][bookmark: _Toc32310615][bookmark: _Toc161300744]BACKGROUND 
This is a reprocurement of the products/services under T3063 Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Various Bodies.  Bidders interested in reviewing the current Contract specifications and pricing information may do so by following the instruction below.  Bidders should not rely upon or use data or information from the contract when preparing a response to this Bid Solicitation as this Bid Solicitation addresses the State’s current requirements. 
· Go to: www.njstart.gov 
· Select “Active Blankets”
· In the search bar, select “Blankets” from the drop down menu
· Enter the T3063 and click “[image: ]”
· The current Contract list will appear under “Results”

[bookmark: _Toc161300745]CONTRACT AMOUNT
The estimated amount of the Contract, if stated, shall not be construed as either the maximum or minimum amount which the State shall be obliged to order.

[bookmark: _Toc400531506][bookmark: _Toc428533977][bookmark: _Toc32310702][bookmark: _Toc161300746]ORDER OF PRECEDENCE OF CONTRACTUAL TERMS
The Contract awarded, and the entire agreement between the parties, as a result of this Bid Solicitation shall consist of:  (1) the final Bid Solicitation, (2) the State of New Jersey Standard Terms and Conditions, (3) the Quote, and if applicable (4) any Bidder responses to clarifications; (5) a Bidder’s Best and Final Offer, (6) other negotiated document, and/or (7) third party document.  In the event of a conflict in the terms and conditions among the documents comprising this Contract, the order of precedence, for purposes of interpretation thereof, listed from highest ranking to lowest ranking as noted above. 

Any other terms or conditions, not included with the Bidder’s Quote and accepted by the State, shall not be incorporated into the Contract awarded.  Any references to external documentation, including those documents referenced by a URL, including without limitation, technical reference manuals, technical support policies, copyright notices, additional license terms, etc., are subject to the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Conditions.  In the event of any conflict between the terms of a document incorporated by reference, the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Conditions shall prevail.

[bookmark: _Toc161300747]INTRASTATE COOPERATIVE PURCHASING
The State intends to extend the Contract awarded to the State's Intrastate Cooperative Purchasing Participants.  Although the State is making the use of any Contract resulting from this Bid Solicitation available to Intrastate Cooperative Purchasing Participants, the State makes no representation as to the acceptability of the Bid Solicitation’s terms and conditions to any Intrastate Cooperative Purchasing Participants.



[bookmark: _Toc161300748]PRE-QUOTE SUBMISSION INFORMATION
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote and for reviewing the Quote submission requirements and the Scope of Work requirements.  

[bookmark: _ELECTRONIC_QUESTION_AND][bookmark: _Toc428533940][bookmark: _Toc32310617][bookmark: _Toc161300749]ELECTRONIC QUESTION AND ANSWER PERIOD
The Division will electronically accept questions and inquiries from all potential Bidders via the “Q&A” Tab of the Bid Solicitation in NJSTART.  Questions should be directly tied to a Bid Solicitation Section, the Price Sheet, Form or Attachment; and should reference the specific Bid Solicitation Section or document to which it relates.

The cut-off date for electronic questions and inquiries relating to this Bid Solicitation is indicated on the Bid Solicitation cover page.  In the event that questions are posed by Bidders, answers to such questions will be issued by Bid Amendment.  
[bookmark: _1.3.3__Mandatory_Pre-Bid_Conference][bookmark: _1.3.5__SUBMISSION_OF_BID_PROPOSAL][bookmark: _1.3.2_SUBMISSION_OF_BID_PROPOSAL]
A Bidder shall not contact the Using Agency and/or the Procurement Specialist directly, in person, by telephone or by e-mail, concerning this Bid Solicitation, prior to Contract award.

[bookmark: _Toc161300750]EXCEPTIONS TO THE STATE OF NJ STANDARD TERMS AND CONDITIONS (SSTC)
Questions regarding the State of New Jersey Standard Terms and Conditions and exceptions to mandatory requirements MUST be posed during the Electronic Question and Answer period and shall contain the Bidder’s suggested changes and the reason(s) for the suggested change(s).

[bookmark: _Toc161300751]BID AMENDMENTS
In the event that it becomes necessary to clarify or revise this Bid Solicitation, such clarification or revision will be by Bid Amendment.  Any Bid Amendment will become part of this Bid Solicitation and part of any Contract awarded. Bid Amendments will be posted as a file attachment on the “Summary” page of the Bid Solicitation in NJSTART after the cut-off date.  

There are no designated dates for release of Bid Amendments.  Those Bidders who are on the bid holder list either through commodity code registration in NJSTART or by acknowledging the bid in NJSTART should receive notification of any Bid Amendment(s). If a Bidder is not on the bid holder list, Bid Amendments are still viewable on the “Summary” page of the Bid Solicitation in NJSTART.

It is the sole responsibility of the Bidder to be knowledgeable of all Bid Amendments related to this procurement. An interested Bidder should check the NJSTART “Open Bids” Tab on a daily basis to ensure review of the most updated information.

[bookmark: _1.3.4_MANDATORY/OPTIONAL_SITE][bookmark: _1.3.45_MANDATORY/OPTIONAL_SITE][bookmark: _MANDATORY/OPTIONAL_SITE_VISIT][bookmark: _Toc224543885][bookmark: _Toc238623352][bookmark: _Toc400531474][bookmark: _Toc428533944][bookmark: _Toc32310620][bookmark: _Toc161300752]MANDATORY/OPTIONAL SITE VISIT
Not applicable to this procurement.

[bookmark: _1.3.5__MANDATORY/OPTIONAL][bookmark: _1.3.6__MANDATORY/OPTIONAL][bookmark: _MANDATORY/OPTIONAL_PRE-QUOTE_CONFER][bookmark: _Toc224543888][bookmark: _Toc238623354][bookmark: _Toc428533945][bookmark: _Toc32310621][bookmark: _Toc161300753]MANDATORY/OPTIONAL PRE-QUOTE CONFERENCE
Not applicable to this procurement.

[bookmark: _QUOTE_SUBMISSION_REQUIREMENTS][bookmark: _Toc161300754]QUOTE SUBMISSION REQUIREMENTS

[bookmark: _Toc161300755]QUOTE SUBMISSION 
In order to be considered for award, the Quote must be received electronically by the Division’s Proposal Review Unit, through NJSTART, by the required date and time. 

The date and time of the Quote opening are indicated on the Bid Solicitation cover sheet and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  If the Quote opening deadline has been revised, the new Quote opening deadline will be shown on the posted Bid Amendment and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  Quotes not received prior to the Quote opening deadline shall be rejected.

Quotes will be publicly opened and announced by telephone conference on the date and time of the quote opening. 
(Dial-in phone number: 888-204-5984 / Access code: 2602305)

When submitting a Quote through NJSTART, do not use any symbols (i.e., #, @, $, &, *) in the filename as this may prevent the Quote from being properly uploaded.  Uploaded files must be compatible with Microsoft Office and/or Adobe software applications. DO NOT UPLOAD files with extensions such as .zip, .numbers, or .pages.

When uploading the documents to NJSTART, the Bidder should select the “Confidential” option in NJSTART for attachments on the “Attachments” Tab to request that the documents not be displayed publicly through NJSTART. Marking an attachment as "Confidential" in NJSTART shall not constitute the Bidder's designation of the attachment as exempt from public disclosure under the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know.

[bookmark: _Toc161300756]BIDDER RESPONSIBILITY
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote in response to this Bid Solicitation.  No special consideration will be given after Quotes are opened because of a Bidder’s failure to be knowledgeable as to all of the requirements of this Bid Solicitation.  The State assumes no responsibility and bears no liability for costs incurred by a Bidder in the preparation and submittal of a Quote in response to this Bid Solicitation or any pre-contract award costs incurred.

[bookmark: _Toc161300757]ANNOUNCEMENT OF QUOTE INFORMATION
On the date and time Quotes are due under the Bid Solicitation, all information concerning the Quotes submitted may be publicly announced and shall be available for inspection and copying except otherwise noted:  
A. Information appropriately designated as proprietary and/or confidential in a Bidder’s Quote shall not be available for inspection and copying; and
B. Where negotiation is contemplated, only the names and addresses of the Bidders submitting Quotes will be announced, and the contents of the Quotes shall not be available for inspection and copying until the Notice of Intent to Award is issued by the Director. 

[bookmark: _Toc161300758]QUOTE ERRORS
In accordance with N.J.A.C. 17:12-2.11 “Proposal errors,” a Bidder may withdraw its Quote as described below.

[bookmark: _Toc161300759]QUOTE WITHDRAWAL PRIOR TO QUOTE OPENING
A Bidder may withdraw its Quote submission in NJSTART prior to the Quote opening; however, Bidders should note that while withdrawn NJSTART Quotes remain viewable by the Bidder on its Vendor Profile Homepage, they are removed from the Division’s view and cannot be considered for Contract award. The Bidder may submit a revised Quote as long as the Quote is received prior to the announced date and time for Quote submission. Bidders may refer to the QRG “Submit a Quote” for additional instructions.

[bookmark: _Toc161300760]QUOTE WITHDRAWAL AFTER QUOTE OPENING, BUT PRIOR TO CONTRACT AWARD
If, after the Quote opening, but before Contract award, a Bidder discovers an error in its Quote, the Bidder may make a written request to the Procurement Bureau to withdraw its Quote from consideration for award.  If the Bidder’s request to withdraw is made in good faith, and the State will not be significantly prejudiced by granting the withdrawal of the Quote beyond the loss of the benefit of the bargain to the State of the withdrawing Bidder’s offer, the request shall be granted.  Evidence of the Bidder’s good faith in making this request can be demonstrated by one (1) or more of the following factors: A mistake is so significant that to enforce the Contract resulting from the Quote would be unconscionable; that the mistake relates to a material feature or term of the Contract; and that the mistake occurred notwithstanding the Bidder’s exercise of reasonable care.  After Quote opening, while pursuant to the provisions of this section a Bidder may request to withdraw its Quote and the Director may in his/her discretion allow said Bidder to withdraw it, the Division also may take notice of repeated or unusual requests to withdraw by a Bidder and take those prior requests to withdraw into consideration when evaluating the Bidder’s future Quotes.

The Quote withdrawal request must include the Bid Solicitation Number, Bid Solicitation Title, and the Quote submission date and should be sent to Procurement.Bureau@treas.nj.gov.

If, during a Quote evaluation process, an obvious pricing error made by a potential Contract awardee is found, the Director or his/her designee shall issue written notice to the Bidder.  The Bidder will have up to five (5) business days after receipt of the notice to confirm its pricing.  If the Bidder fails to respond, its Quote shall be considered withdrawn, and no further consideration shall be given to it.

[bookmark: _Toc161300761]JOINT VENTURE
If a Joint Venture is submitting a Quote, the agreement between the parties relating to such Joint Venture should be submitted with the Joint Venture’s Quote.  Authorized signatories from each party comprising the Joint Venture must sign the Offer and Acceptance Page.  Each party to the Joint Venture must individually complete and comply with all the forms and certification requirements in Bid Solicitation Section 3 – Quote Submission Requirements. 

[bookmark: _Toc161300762]SMALL BUSINESS SET-ASIDE CONTRACTS
Not applicable to this procurement.

[bookmark: _Toc161300763]DISABLED VETERANS’ BUSINESS SET-ASIDE CONTRACT 
Not applicable to this procurement.

[bookmark: _Toc161300764]BID SECURITY
Not applicable to this procurement.

[bookmark: _Toc161300765]BIDDER ADDITIONAL TERMS SUBMITTED WITH THE QUOTE
A Bidder may submit additional terms as part of its Quote.  Additional terms are Bidder-proposed terms or conditions that do not conflict with the scope of work required in this Bid Solicitation, the terms and conditions of this Bid Solicitation, or the State of New Jersey Standard Terms and Conditions.  Bidder proposed terms or conditions that conflict with those contained in the State of New Jersey Standard Terms and Conditions will render a Quote non-responsive.  It is incumbent upon the Bidder to identify and remove its conflicting proposed terms and conditions prior to Quote submission.  

Quotes including Bidder proposed additional terms may be accepted, rejected, or negotiated, in whole or in part, at the State’s sole discretion. 

If Bidder intends to propose terms and conditions that conflict with the State of New Jersey Standard Terms and Conditions, those Bidder proposed terms and conditions shall only be considered if submitted and agreed to pursuant to the electronic question and answer procedure.  Bidders shall not submit exceptions or modifications as part of the Quote or on the “Terms and Conditions” Tab through NJSTART. 

[bookmark: _Toc161300766]QUOTE CONTENT
The Quote should be submitted with the attachments organized in the following manner:
· Forms
· State-Supplied Price Sheet

A Bidder should not password protect any submitted documents. Use of URLs in a Quote should be kept to a minimum and shall not be used to satisfy any material term of a Bid Solicitation. If a preprinted or other document included as part of the Quote contains a URL, a printed copy of the information should be provided and will be considered as part of the Quote. 

[bookmark: _Toc161300767]FORMS, REGISTRATIONS AND CERTIFICATIONS TO BE SUBMITTED WITH QUOTE 
A Bidder is required to complete and submit the following forms.  As an alternative to uploading certain forms with the submitted Quote, a Bidder may complete several certifications electronically in NJSTART on the “Terms and Categories” Tab within the Vendor Profile.  Those forms that may be completed on the NJSTART “Terms and Categories” Tab are noted below. Additionally, a Bidder may attach completed forms to the Vendor Profile.  Refer to QRGs “Vendor Forms” and “Attaching Files” for additional instructions.  VENDOR QUICK REFERENCE GUIDES

OFFER AND ACCEPTANCE PAGE 
The Bidder should complete and submit the Offer and Acceptance Page with the Quote.  The Offer and Acceptance Page must be signed by an authorized representative of the Bidder.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.    

OWNERSHIP DISCLOSURE FORM 
Pursuant to N.J.S.A. 52:25-24.2, in the event the Bidder is a corporation, partnership or limited liability company, the Bidder must disclose all 10% or greater owners by (a) completing and submitting the Ownership Disclosure Form with the Quote; (b) if the Bidder has submitted a signed and accurate Ownership Disclosure Form dated and received no more than six (6) months prior to the Quote submission deadline for this procurement, the Division may rely upon that form; however, if there has been a change in ownership within the last six (6) months, a new Ownership Disclosure Form must be completed, signed and submitted with the Quote; or, (c) a Bidder with any direct or indirect parent entity which is publicly traded may submit the name and address of each publicly traded entity and the name and address of each person that holds a 10 percent or greater beneficial interest in the publicly traded entity as of the last annual filing with the federal Securities and Exchange Commission or the foreign equivalent, and, if there is any person that holds a 10 percent or greater beneficial interest, also shall submit links to the websites containing the last annual filings with the federal Securities and Exchange Commission or the foreign equivalent and the relevant page numbers of the filings that contain the information on each person that holds a 10 percent or greater beneficial interest. N.J.S.A. 52:25-24.2.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this form online in NJSTART on the “Terms and Categories” Tab.  

A Bidder’s failure to submit the information required by N.J.S.A. 52:25-24.2 will result in the rejection of the Quote as non-responsive and preclude the award of a Contract to said Bidder.

  DISCLOSURE OF INVESTMENT ACTIVITIES IN IRAN FORM
The Bidder should  submit Disclosure of Investment Activities in Iran form to certify that, pursuant to N.J.S.A. 52:32-58, neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates (as defined in N.J.S.A. 52:32-56(e)(3)), is listed on the Department of the Treasury’s List of Persons or Entities Engaging in Prohibited Investment Activities in Iran and that neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates, is involved in any of the investment activities set forth in N.J.S.A. 52:32-56(f).  If the Bidder is unable to so certify, the Bidder shall provide a detailed and precise description of such activities as directed on the form.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  

DISCLOSURE OF INVESTIGATIONS AND OTHER ACTIONS INVOLVING BIDDER FORM
The Bidder should submit the Disclosure of Investigations and Other Actions Involving Bidder Form,  with its Quote, to provide a detailed description of any investigation, litigation, including administrative complaints or other administrative proceedings, involving any public sector clients during the past five (5) years, including the nature and status of the investigation, and, for any litigation, the caption of the action, a brief description of the action, the date of inception, current status, and, if applicable, disposition.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  

MACBRIDE PRINCIPLES FORM
The Bidder should submit the MacBride Principles Form.  Pursuant to N.J.S.A. 52:34-12.2, a Bidder is required to certify  that it either has no ongoing business activities in Northern Ireland and does not maintain a physical presence therein or that it will take lawful steps in good faith to conduct any business operations it has in Northern Ireland in accordance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of their compliance with those principles.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: In lieu of completing and submitting the paper-based form, the Bidder has the option to complete this certification online in NJSTART on the “Terms and Categories” Tab.  

SERVICE PERFORMANCE WITHIN THE UNITED STATES
Not applicable to this procurement.

CONFIDENTIALITY/COMMITMENT TO DEFEND
Pursuant to the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know, Quotes can be released to the public in accordance with N.J.A.C. 17:12-1.2(b) and (c).  

The Bidder should submit a completed and signed Confidentiality/Commitment to Defend Form with the Quote.  In the event that the Bidder does not submit the Confidentiality form with the Quote, the State reserves the right to request that the Bidder submit the form after Quote submission.

After the opening of sealed Quotes, all information submitted by a Bidder in response to a Bid Solicitation is considered public information notwithstanding any disclaimers to the contrary submitted by a Bidder.  Proprietary, financial, security and confidential information may be exempt from public disclosure by OPRA and/or the common law when the Bidder has a good faith, legal/factual basis for such assertion. 

When the Bid Solicitation contains a negotiation component, the Quote will not be subject to public disclosure until a notice of intent to award a Contract is announced. 

As part of its Quote, a Bidder may request that portions of the Quote be exempt from public disclosure under OPRA and/or the common law. The Bidder must provide a detailed statement clearly identifying those sections of the Quote that it claims are exempt from production, and the legal and factual basis that supports said exemption(s) as a matter of law.  The State will not honor any attempts by a Bidder to designate its price sheet, price list/catalog, and/or the entire Quote as proprietary and/or confidential, and/or to claim copyright protection for its entire Quote.  If the State does not agree with a Bidder’s designation of proprietary and/or confidential information, the State will use commercially reasonable efforts to advise the Bidder. Copyright law does not prohibit access to a record which is otherwise available under OPRA.

The State reserves the right to make the determination as to what to disclose in response to an OPRA request.  Any information that the State determines to be exempt from disclosure under OPRA will be redacted.  

In the event of any challenge to the Bidder’s assertion of confidentiality that is contrary to the State’s determination of confidentiality, the Bidder shall be solely responsible for defending its designation, but in doing so, all costs and expenses associated therewith shall be the responsibility of the Bidder. The State assumes no such responsibility or liability.  

In order not to delay consideration of the Quote or the State’s response to a request for documents, the State requires that Bidder respond to any request regarding confidentiality markings within the timeframe designated in the State’s correspondence regarding confidentiality.  If no response is received by the designated date and time, the State will be permitted to release a copy of the Quote with the State making the determination regarding what may be proprietary or confidential.

SUBCONTRACTOR UTILIZATION PLAN
Bidders intending to use Subcontractor(s) shall list all subcontractors on the Subcontractor Utilization Plan form or may list the Subcontractor(s) on the “Subcontractor” Tab in NJSTART. 

For a Quote that does NOT include the use of any Subcontractors, the Bidder is automatically certifying that, if selected for an award, the Bidder will be performing all work required by the Contract. 

If it becomes necessary for the Contractor to substitute a Subcontractor, add a Subcontractor, or substitute its own staff for a Subcontractor, the Contractor will identify the proposed new Subcontractor or staff member(s) and the work to be performed.  The Contractor shall forward a written request to substitute or add a Subcontractor or to substitute its own staff for a Subcontractor to the State Contract Manager for consideration.    The Contractor must provide a completed Subcontractor Utilization Plan, a detailed justification documenting the necessity for the substitution or addition, and resumes of its proposed replacement staff or of the proposed Subcontractor’s management, supervisory, and other key personnel that demonstrate knowledge, ability and experience relevant to that part of the work which the Subcontractor is to undertake. The qualifications and experience of the replacement(s) must equal or exceed those of similar personnel proposed by the Contractor in its Quote.  The State Contract Manager will forward the request to the Director for approval.  

NOTE: No substituted or additional Subcontractors are authorized to begin work until the Contractor has received written approval from the Director.

SMALL BUSINESS AND/OR DISABLED VETERANS’ BUSINESS SUBCONTRACTING SET-ASIDE CONTRACT 
Not applicable to this procurement.

[bookmark: _Toc161300776]RESERVED

AFFIRMATIVE ACTION
The intended Contractor and its named Subcontractor(s) must submit a copy of a New Jersey Certificate of Employee Information Report, or a copy of Federal Letter of Approval verifying it is operating under a federally approved or sanctioned Affirmative Action program.  If the Contractor and/or its named Subcontractor(s) are not in possession of either a New Jersey Certificate of Employee Information Report or a Federal Letter of Approval, it/they must complete and submit the Affirmative Action Employee Information Report (AA-302).  Information, instruction and the application are available at https://www.state.nj.us/treasury/contract_compliance/index.shtml.

[bookmark: _Toc161300778]RESERVED

[bookmark: _Toc161300779]STATE OF NEW JERSEY SECURITY DUE DILIGENCE THIRD-PARTY INFORMATION SECURITY QUESTIONNAIRE 
Not applicable to this procurement.

BUSINESS REGISTRATION
[bookmark: OLE_LINK1]In accordance with N.J.S.A. 52:32-44(b), a Bidder and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Contract.  A Bidder should verify its Business Registration Certification Active status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Bidder’s Business Registration Certification Active status, NJSTART provides a link to take corrective action. 

[bookmark: _Toc99544656][bookmark: _Toc161300781]3.13.14	Certification of Non-Involvement in Prohibited Activities in Russia or Belarus Pursuant to P.L.2022, c.3
The Bidder should submit the Certification of Non-Involvement in Prohibited Activities in Russia or Belarus Form.  Pursuant to P.L.2022, c.3, a person or entity seeking to enter into or renew a contract for the provision of goods or services shall certify that it is not Engaging in Prohibited Activities in Russia or Belarus as defined by P.L.2002, c.3, sec. 1(e).  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
[bookmark: _Toc161300782]TECHNICAL QUOTE 
Not applicable to this procurement.

[bookmark: _Toc161300783]BIDDER QUOTE OVERVIEW FORM
Not applicable to this procurement.

[bookmark: _BIDDER_DATA_SHEET/FORM][bookmark: _Toc161300784]BIDDER DATA SHEET/FORM
The Bidder should submit the Bidder Data Sheet with its Quote.  The Bidder Data Sheet will be used to evaluate the Bidder’s ability to complete the Scope of Work.  

The Bidder should provide in its response to Part I of the Bidder Data Sheet all relevant information regarding its experience in successfully completing contracts of a similar size and scope to the work required by this Bid Solicitation.  

The Bidder must provide, in Part II of the Bidder Data Sheet, details of any negative actions taken by other contracting entities against it in the course of performing these projects including, but not limited to, receipt of letters of potential default, default, cure notices, termination of services for cause, or other similar notifications/processes.  Additionally, the Bidder should provide details, including any negative audits, reports, or findings by any governmental agency for which the Bidder is/was the contractor on any contracts of similar scope.  In the event a Bidder neglects to include this information in its Quote, the Bidder’s omission of necessary disclosure information may be cause for rejection of the Bidder’s Quote by the State.

If proposing to use a Subcontractor, the Bidder should provide as an attachment to the Bidder Data Sheet documented experience to demonstrate that each Subcontractor has successfully performed work on contracts of a similar size and scope to the work that the Subcontractor is designated to perform in the Bidder’s Quote.  The Bidder must provide a detailed description of services to be provided by each Subcontractor.  

AFFIDAVIT OF APPAREL PRODUCTION
Not applicable to this procurement.

[bookmark: _Toc161300786]DISCLOSURE OF PRODUCT COMPOSITION
Not applicable to this procurement.

[bookmark: _Toc161300787]SPECIFICATION DATA SHEETS
Not applicable to this procurement.

[bookmark: _Toc161300788]SAMPLES AND TESTING
Not applicable to this procurement.

[bookmark: _SPECIFICATION_CONFORMANCE_FORM][bookmark: _Toc161300789]SPECIFICATION CONFORMANCE FORM
The Bidder shall submit with its Quote the Specification Conformance Form.  By submitting this form, the Bidders certifies that all items offered in response to this Bid Solicitation conform to the requirements set forth in the Bid Solicitation. 

[bookmark: _Toc161300790]MANUFACTURER’S CERTIFICATION
Upon the State’s request, the Bidder should submit a letter of certification from the manufacturer whose product is supplied, certifying that the Bidder is authorized by the manufacturer to supply the good(s) specified.  The certification must indicate that the Bidder was authorized by the manufacturer to supply the good(s) specified as of the Quote Opening Date. The State reserves the right to request such certification and to require that such certification be provided within five (5) business days from the time it is requested.  

[bookmark: _Toc161300791]MANUFACTURER’S PUBLISHED LIST OF OPTIONS AND ATTACHMENTS/PRICE LIST
Not applicable to this procurement.

[bookmark: _Toc161300792]PRICE LIST AND/OR CATALOG
Not applicable to this procurement.

[bookmark: _Toc161300793]MANAGEMENT OVERVIEW
Not applicable to this procurement.

[bookmark: _Toc161300794]CONTRACT MANAGEMENT
Not applicable to this procurement.

[bookmark: _Toc161300795]CONTRACT SCHEDULE
Not applicable to this procurement.

[bookmark: _Toc161300796]MOBILIZATION PLAN
Not applicable to this procurement.

[bookmark: _Toc161300797]ADDITIONAL PLAN(S)
Not applicable to this procurement.

[bookmark: _Toc161300798]ORGANIZATIONAL EXPERIENCE
Not applicable to this procurement.

[bookmark: _Toc161300799]LOCATION
Not applicable to this procurement.

[bookmark: _Toc161300800]ORGANIZATION CHARTS
Not applicable to this procurement.

[bookmark: _Toc161300801]RESUMES
Not applicable to this procurement.

[bookmark: _Toc161300802]EXPERIENCE WITH CONTRACTS OF SIMILAR SIZE AND SCOPE
Not applicable to this procurement.

[bookmark: _Toc161300803]FINANCIAL CAPABILITY OF THE BIDDER
The Bidder should provide sufficient financial information to enable the State to assess the financial strength and creditworthiness of the Bidder and its ability to undertake and successfully complete the Contract.  In order to provide the State with the ability to evaluate the Bidder’s financial capacity and capability to undertake and successfully complete the Contract, the Bidder should submit the following:
A. For publicly traded companies the Bidder should provide copies or the electronic location of the annual reports filed for the two most recent years; or
B. For privately held companies the Bidder should provide the certified financial statement (audited or reviewed) in accordance with applicable standards by an independent Certified Public Accountant, including a balance sheet, income statement, and statement of cash flow, and all applicable notes for the most recent calendar year or the Bidder’s most recent fiscal year. 

If the information is not supplied with the Quote, the State may still require the Bidder to submit it.  If the Bidder fails to comply with the request within seven (7) business days, the State may deem the Quote non-responsive.

A Bidder may designate specific financial information as not subject to disclosure when the Bidder has a good faith legal/factual basis for such assertion.  The State reserves the right to make the determination to accept the assertion and will so advise the Bidder.

[bookmark: _Toc161300804]STATE-SUPPLIED PRICE SHEET INSTRUCTIONS
The Bidder must submit its pricing using the State-Supplied Price Sheet accompanying this Bid Solicitation and located on the “Attachments” Tab. 

In order for the State to make sound business judgments regarding products and prices offered in response to this Bid Solicitation, the Bidder must supply, with its Quote, the information requested on the Bid Solicitation’s pricing lines in sufficient detail as to allow the State to determine the firm, fixed Quote pricing and the precise product or service being offered, i.e., with no possible misinterpretation of the price or product/service being offered by the Bidder.  A Bidder’s failure to provide, within its Quote, the information deemed by the State to be essential for product identification or price determination shall result in rejection of that Bidder’s Quote.  Notwithstanding the aforementioned material obligation, in order to support the State's decision-making process, the State may require a Bidder to provide additional information or documentation that has been deemed not to be material to product identification or price determination, in which case, the Bidder shall, within the time limit set forth in the written request, comply with said request.  Each Bidder is required to hold its prices firm through issuance of the Contract.

There are sixteen (16) price lines, which are itemized as follows:

	Price Line Number
	Description

	1 
	19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD

	1A
	Vehicle Manufacturer’s Published Options 

	2
	Hook Lift System

	3
	Stainless Steel Dump Body with Tilt/Dump Interlock

	4
	Stake Body

	5
	Landscape Box Body

	6
	Chipper Body

	7
	Enclosed Steel Storage Body

	8
	Platform Body with 300 -Gallon, Gasoline Powered Herbicide Sprayer 

	9
	Platform Body with Toolboxes

	10 
	Dump Body with Multi-Function Tailgate 

	11
	Salt Spreader

	12
	Snow Plow

	13
	In-Cab Controller for Herbicide Sprayer

	14
	In-Cab Controller for Salt Spreader

	15
	One Set of Parts, Service and Operation and Maintenance Manuals

	16
	Technical Support



The State intends to make one (1) Contract award to a responsive Bidder that meet the requirements of the Bid Solicitation.

Price Lines 1 through 16 are grouped to create a single award.  Bidders must bid on Prices Lines 1 through 16 in order to be considered for an award.  If a Bidder does not bid on all price lines, Price Lines 1 through 16, its Quote shall be considered non-responsive.

If a brand/product bid on a price line is deemed non-responsive, the entire Quote will be deemed non-responsive, as these price lines were grouped to create a single award, with the intent that all price lines will be awarded together. 

Price line items are grouped for Quote evaluation purposes only.  Upon Contract award, Using Agencies will be able to order any price lines within the group individually.

Where the State-Supplied Price Sheet includes an estimated quantity column, Bidders are advised that estimated quantities may vary throughout the Contract term resulting from this Bid Solicitation.  The State makes no representation and provides no guarantee as to the minimum, average or maximum volume of purchases to be made under this Contract.

Any price changes including hand written revisions or "white-outs" must be initialed.  Failure to initial price changes shall preclude a Contract award from being made to the Bidder pursuant to N.J.A.C. 17:12-2.2(a)(8).

· Step 1 - The Bidder should enter the Bidder’s name in the field titled “Bidder Name:” located at the top of the State-Supplied Price Sheet.

· Step 2 - The Bidder should enter a cash discount, pursuant to Section 3.36.2, in the space provided on the State-Supplied Price Sheet.  If the Bidder leaves the “Cash Discount” field blank, it shall mean that the Bidder is not offering a cash discount.

· Step 3 – For price lines 1 through 15, the Bidder shall insert a firm, fixed price in US dollars in the column titled “Unit Price” on the State-Supplied Price Sheet.  If a Bidder leaves the “Unit Price” field blank, it shall be considered that the Bidder provided no Quote for that price line item.  

Any additional costs, including freight, must be included in the pricing offered on the State-Supplied Price Sheet.  

The NJSTART system is able to accept Unit Prices containing up to two (2) decimal places to the right of the decimal point. Any price beyond 2 decimal points will be rounded to the second decimal place.  Unit Prices may be offered on the State-supplied Price Sheet up to two (2) decimal places to the right of the decimal point.  Price Sheet formatting will automatically round Unit Prices containing more than two (2) decimal places to the right of the decimal point so as not to exceed this limit.  
· Step 3A – For Price Line 1A, a Bidder shall insert a firm, fixed percentage (%) discount in the “Percentage Discount” column for price lines 1A.

A Percentage discount may be offered on the State-Supplied Price Sheet up to two (2) decimal places to the right of the decimal point.  Price Sheet formatting will automatically round percentage discounts containing more than two (2) decimal places to the right of the decimal point so as not to exceed this limit.

A Bidder's entry in the “Percentage Discount” column shall be considered a percentage (%).  For example, an entry of "50" shall be considered "50%" and that of "0.50" shall be considered "0.50%".  If a Bidder leaves the “Percentage Discount” column/field blank, it shall be considered that the Bidder provided no Quote for that price line item.  A series or a range of discounts or fixed prices (firm dollar amount) on price line 1A shall not be acceptable and shall result in the rejection of the Quote for that price line and the group.
· Step 4 - For price line 16, the Bidder shall insert a firm, fixed hourly rate in the field titled “Unit Price”.  If a Bidder leaves the “Unit Price” field blank, it shall be considered that the Bidder provided no Quote for that price line item and its Quote shall be considered non-responsive.    

The Bidder shall bid firm, fixed hourly rate in the “Unit Price” field, by entering the hourly rate bid in the “Unit Price” field on this specific price line on the State-Supplied Price Sheet.  A Bidder’s entry in the “Unit Price” field for price line 16 shall be considered a firm, fixed price per hour.  For example, entry of “50” shall be considered “$50 per hour”.

Multiple or series or range of hourly rates or a fixed task price on these price lines shall not be accepted and will render the Quote non-responsive for that price line and the Group that price line item is part of.
The NJSTART system is able to accept Unit Prices containing up to two (2) decimal places to the right of the decimal point. Any price beyond 2 decimal points will be rounded to the second decimal place.  Unit Prices may be offered on the State-supplied Price Sheet up to two (2) decimal places to the right of the decimal point.  Price Sheet formatting will automatically round Unit Prices containing more than two (2) decimal places to the right of the decimal point so as not to exceed this limit.  
· Step 5 - For price line 1, the Bidder shall enter the make and model year of the vehicle being offered in the field titled “Make and Model Year”.  For example, 2024 Ford.

· Step 6 – For price line 1, the Bidder shall enter the specific model of the vehicle being offered in the field titled “Model”.  For example, F-550.

· Step 7 – For price line 1, the Bidder shall enter the specific manufacturer’s body code being offered in the field titled “Manufacturer’s Body Code”.  For example, in the case of Ford, a Bidder may enter: Manufacturer’s body code: W5H.

· Step 8 – For price line 1, the Bidder shall enter the specific trim level, trim line, series or package code being offered in the field titled “Trim Level/Trim Line/Package Code”.  For example, in the case of Ford, a Bidder may enter: Trim level: XL, Trim Line: The standard set of features on the particular vehicle, example: seats, tire, wheels, radio, etc., Order Package Code: 660A for example.
· Step 9 – For price line 1, the Bidder shall enter the specific manufacturer’s option code for the engine offered as part of the Quote price in the field titled ‘Option Code for Engine’.  For example, in the case of Ford, 99T.  If a Bidder leaves the field blank, it shall mean that the Bidder is not offering an engine as part of its Quote price, thereby making its Quote non-responsive.

· Step 10 – For price line 1, the Bidder shall enter the specific manufacturer’s option code for the automatic transmission offered as part of the Quote price in the field titled ‘Option Code for Automatic Transmission’.  For example, in the case of Ford, 44G.   If a Bidder leaves the field blank, it shall mean that the Bidder is not offering an automatic transmission as part of its Quote price, thereby making its Quote non-responsive.

· Step 11 – For price line 1, the Bidder shall enter the specific manufacturer’s option code for air conditioning in the field titled ‘Option Code for Air Conditioning’.  If air conditioning is standard with the trim line or package code offered, the Bidder must enter the word ‘included’ in the field provided.  In the example of Ford F-550, the Bidder would enter ‘included’.  If a Bidder leaves the field blank, it shall mean that the Bidder is not offering air conditioning as part of its Quote price, thereby making its Quote non-responsive.

·   Step 12 – For price line 1, the Bidder shall enter any additional option code(s) and a brief description of the option code(s) 
  for each option code offered as part of the Quote price in the field titled “Additional Option Codes Offered as Part of the 
  Quote Price.” For example, in the case of Ford, 67B Alternator.

If no additional option codes are provided, the Bidder should write "none" in the field provided.  If the space is left blank, it shall mean that the Bidder is not offering any additional option codes.  

·   Step 13 – For price lines 2 through 14, the Bidder must enter the make offered in the field titled ‘Make’ on the State- 
  Supplied Price Sheet.  

·   Step 14 – For price lines 2 through 14, the Bidder shall enter the model offered in the field titled ‘Model’ on the State- 
  Supplied Price Sheet.  

The examples listed above are for reference only and may not specifically apply to the vehicle specified in this Bid Solicitation.
Please be advised that the fields listed in Steps 3, 4, 5, 6, 7, 8, 9 10, 11, 13, and 14 are required fields that must be completed on the State-Supplied Price Sheet.  A Bidders failure to provide complete information in these fields on the State-Supplied Price Sheet shall render its Quote non-responsive.
·   Step 15 – For Price Lines 1 throguh 14, the Bidder should enter the days required to make delivery upon receipt of an order  
  into the “Delivery Days After Receipt of Order” field at the bottom of the State-Supplied Price Sheet. If the “Delivery Days 
  ARO” field is left blank, then the delivery days shall default to the delivery days set forth in Bid Solicitation Section 5.6.

[bookmark: _Toc161300805]DELIVERY TIME AND COSTS
Unless otherwise noted elsewhere in the Bid Solicitation or State Price sheet, all delivery times are as noted in Bid Solicitation Section 5.6 Delivery Time and Costs.  Bidder may submit alternate delivery days on the State Price Sheet.  

When there is a discrepancy between the delivery days listed in the General Tab in the Quote in NJSTART and the State Price Sheet, the State Price Sheet delivery days shall govern.  

[bookmark: _Toc161300806]CASH DISCOUNTS
The Bidder is encouraged to offer cash discounts based on expedited payment by the State.  The State will make efforts to take advantage of discounts, but discounts will not be considered in determining the price rankings of Quotes.  Should the Bidder choose to offer cash discounts, the following shall apply:
A. Discount periods shall be calculated starting from the next business day after the Using Agency has accepted the goods or services, received a properly signed and executed invoice and, when required, a properly executed performance security, whichever is latest; and
B. The date on the check issued by the State in payment of that invoice shall be deemed the date of the State's response to that invoice.

[bookmark: _Toc161300807]VOLUME DISCOUNTS
Not applicable to this procurement.

[bookmark: _Toc161300808]USE OF “NO BID” VERSUS “NO CHARGE” ON THE STATE-SUPPLIED PRICE SHEET
All price lines must be filled out in accordance with the instructions above.  If the Bidder is not submitting a price for an item on a price line, the Bidder must indicate “No Bid” on the State-Supplied Price Sheet accompanying this Bid Solicitation. If the Bidder will supply an item on a price line free of charge, the Bidder must indicate “No Charge” on the State-Supplied Price Sheet accompanying this Bid Solicitation.  The use of any other identifier may result in the Bidder’s Quote being deemed non-responsive.

[bookmark: _Toc161300809]ORAL PRESENTATIONS
Not applicable to this procurement.

[bookmark: _Toc161300810]SCOPE OF WORK
[bookmark: _Toc400531507][bookmark: _Toc428533978][bookmark: _Toc32310703]
[bookmark: _Toc161300811]CONTRACT SPECIFIC REQUIREMENTS

4.1.1  The Contractor must be a franchised and/or authorized factory representative, able to furnish the specified Unit.  Dealers or agents submitting a Quote may be required to submit a letter of certification from the manufacturer whose product is supplied, certifying that the dealer or agent is authorized by the manufacturer to supply the Unit specified.  The State reserves the right to request such certification and to require that such certification be delivered within five (5) working days from the time it is requested.  It will be the responsibility of the Contractor to notify the State of New Jersey of any changes in the status of its franchise.
4.1.2  The Unit supplied must be standard manufacturer's product line available to the general public. 
4.1.3 The Contractor shall provide a new Unit only.  A used Unit will not be accepted.  
4.1.4  This Bid Solicitation is for the outright purchase of the Contract Unit only; leasing of the Contract Unit or trade-in against the purchase of the Contract Unit is not permitted.
4.1.5  The Contractor shall ensure that the manufacturer whose product is supplied has a servicing dealer or service location to provide warranty and recall service and/or repair within twenty four (24) hours of notification by the Using Agency. The servicing dealer or location must stock a full range of new spare parts for all units serviced and must be capable of delivering regularly stocked parts within 24 hours of order.  All parts, including special orders, must be delivered within 72 hours of order.  The Contractor may use an aftermarket installer's location to satisfy this requirement, provided this is disclosed in the Quote. As stated in Bid Solicitation Section 4.1.7, any use of aftermarket installer(s) shall not relieve the Contractor of its obligations under the Contract established as a result of this Bid Solicitation.  
4.1.6  All components of each unit supplied under the Contract for the make and model awarded shall be identical, for example, alternators, filters, distributors, etc. 
4.1.7  The Contractor will be permitted to use aftermarket installers.  Any intent to utilize aftermarket installers shall be described in Attachment #5 – List of Aftermarket Installers, with a list of aftermarket installer(s), other than the prime unit manufacturer, who will supply or install all aftermarket options required. 
4.1.7.1  The Contractor is responsible for ensuring aftermarket installer(s)' compliance with all terms and conditions of this Bid Solicitation.  The Contractor will assume sole responsibility for any payments due the aftermarket installer(s).  Nothing contained in the Bid Solicitation shall be construed as creating any contractual relationship between any aftermarket installer(s) and the State.
4.1.7.2  If, subsequent to Contract award, a Contractor desires to substitute any aftermarket installer(s) listed in the Quote, the Contractor will so notify the State and provide the information on the proposed aftermarket installer(s). The State reserves the right to reject any proposed substitute aftermarket installer(s).
4.1.7.3  The State reserves the right to demand from the Contractor the same information regarding any aftermarket installer(s) as is required from the Bidder under this Bid Solicitation.
The Bidder shall provide complete information on aftermarket installer(s) in Attachment #5 – List of Aftermarket Installers.

[bookmark: _Toc161300812]VEHICLE SPECIFICATIONS – GENERAL PROVISIONS

4.2.1  Each Unit and its components shall be completely assembled, serviced and ready for use when delivered to the Using Agency. Unless specified otherwise; any parts, components, equipment, controls, materials, features, performances, capacities, ratings or designs which are standard and/or necessary to form an efficient and complete working unit shall be furnished whether specifically required herein or not.  The Contractor shall supply any item not specified herein but deemed necessary for functional purposes and the item must meet the Industry standards and practices, Federal and New Jersey Safety Standards and Regulations, and SAE and other applicable standards. Unless specified otherwise, the Contractor shall not delete manufacturer’s standard item using any aftermarket option.  No exceptions shall be permitted to this requirement.
4.2.2  Each vehicle shall be delivered with at least a 1/2 tank of fuel.
4.2.3  Each vehicle furnished must be protected to -20° Fahrenheit, with a permanent type anti-freeze.
[bookmark: finish]4.2.4  Vehicles provided shall be manufacturer’s standard vehicles with the necessary upgrades and/or accessories. All accessories shall be supplied and installed by the manufacturer. Dealer installation is permitted only if factory installation is not available. Dealer installation shall be in accordance with the practices recommended by the manufacturer and shall not adversely affect manufacturer's warranty.
4.2.5  Undercoating and Finish: The frame, fenders, underbody, cab, etc., except driveshaft, exhaust system, and other mechanical components must be completely undercoated. Undercoating must be composed of a non-volatile base, grit and abrasive free material, dispersed in a petroleum solvent, which shall provide a homogenous formulation. All undercoating must be applied to a uniform thickness with no bare spots. 
4.2.5.1  DOT Units: 
Unless otherwise indicated in the specification the cab, chassis and bodies shall be finished as indicated below. All stainless steel components shall remain unpainted.
Section 4.3.1 – Cab and Chassis:  The Unit and all its components shall be cleaned and painted with manufacturer’s standard white. All paint must be same shade.
Section 4.3.3 – Stainless Dump Body:  Manufacturer’s standard paint color.
Section 4.3.4 – Stake Body:  Manufacturer’s standard paint color.
Section 4.3.5 – Landscape Box Body:  Manufacturer’s standard paint color.
Section 4.3.6 – Chipper Body:  Manufacturer’s standard paint color.
Section 4.3.7 – Enclosed Steel Storage Body:  Manufacturer’s standard paint color.
Section 4.3.8 – Platform Body with Herbicide Sprayer:  Manufacturer’s standard paint color.
Section 4.3.9 – Platform Body with Toolboxes:  Manufacturer’s standard paint color.
Section 4.3.10 – Dump Body with Multi-Function Tailgate:  Dump body shall be primed and painted white enamel including underside. 
Section 4.3.11 – Salt Spreader:  All stainless steel components shall be left unpainted. Carbon steel components shall be chemically cleaned and coated with a lead free rust inhibitive primer and painted with lead free black enamel. Top screens shall be powder coated.
4.2.5.2  All Other Using Agency Units:  The Using Agency will specify manufacturer's standard one-tone color at the time of ordering.
[bookmark: manuals][bookmark: VEHICLESPECIFICATIONSTECHNICALPROVION]4.2.6  Manuals: If available, the Contractor shall supply one line set sheet for each Unit.  A Unit shall comprise each and every assembly system and/or component.  In addition to any line set sheet, the Contractor shall provide vehicle operation and maintenance manuals for each and every assembly system and/or component that makes up the unit.  The Contractor shall also include any other manuals that the manufacturers provide as standard manuals. 
Examples of assembly systems and/or components include, but are not necessarily limited to:
	A.
	Hydraulic pump and hydraulic systems

	B.
	Engine, drives and chassis

	C.
	Transmission

	D.
	Electrical system

	E.
	Lubrication system


The manuals shall be delivered directly to the Using Agency, upon delivery of the first unit.  Failure to supply these manuals may delay approval of invoices for payment.
Note: These manuals are required as a part of the base Unit purchase (price line 1) and are not part of the “optional manuals” specified in Bid Solicitation Section 4.3.15.
[bookmark: weightchart][bookmark: guaranteewarranty]4.2.7 Training: Complete instructions on the operation and maintenance of each unit and a demonstration of the operation of the unit shall be given by the Contractor, if requested by the Using Agency.  Training must include operator training with instruction on proper operation of the Unit, safety, and basic preventive maintenance.  This demonstration shall be a formal training session and shall be arranged with the Contractor, at the convenience of the Using Agency. The training session shall be conducted at the location of delivery or at a field location within the State of New Jersey, as specified by the Using Agency. 
Note: This training is required as a part of the base Unit purchase (price line 1) and is not part of the technical support specified in Bid Solicitation Section 4.3.16.
4.2.8  Brand Names: Brand names have been kept to a minimum in this Bid Solicitation; but if a brand name is given, the term "or comparable" is considered to follow the brand name.  Wherever a brand name is used, it is meant to denote the minimum level of quality and performance.  Any item supplied as "comparable" must be approved by the State during the Quote evaluation and prior to an award. Specifying a brand name, components and/or equipment in response to this specification shall not relieve the Contractor from its responsibility to produce the Unit in accordance with all specifications and other contractual requirements.
4.2.9  Guarantee/Warranty:  The Contractor must guarantee that the vehicle and all its component parts comply with the current, applicable Federal Motor Vehicle Safety Standards (FMVSS) and New Jersey State Motor Vehicle Code Regulations, perform their functions adequately, and operate successfully without undue wear or vibration. The Contractor shall immediately replace and install free of charge any part that may break or fail by reason of defective material or workmanship within a period of one (1) year from the date of acceptance by the Using Agency.  The Contractor must maintain a supply of component parts for the expected life of the Unit.
4.2.10  The Bidder must provide complete information on warranty coverage as specified in Bid Solicitation Section 4.4.6.
4.2.11 Vehicle manufacturer's options, which includes any compatible options for the cab and chassis specified in Section 4.3.1 shall be offered using the Vehicle Manufacturer’s Published Options percentage discount price line item (Price Line 1A).  Upon Contract award, the State intends to upload the vehicle manufacturer’s published options for the cab and chassis bid/awarded utilizing a third party database.  The vehicle manufacturer’s options for the cab and chassis bid will be based on the vehicle manufacturers MSRP pricing.  As such, the Contractors discount awarded on the Manufacturer’s Options price line (Price Line 1A) will be applied to the vehicle manufacturers MSRP pricing.

4.2.12  Unless specified otherwise, this Bid Solicitation only permits published options offered by a manufacturer for a trim line and manufacturer's body code bid.  No other options that change trim line and/or manufacturer's body code of the cab and chassis bid shall be considered.  No "XLT" trim line options, for example, shall be offered with "XL" trim line vehicle.  No "2WD" option shall be offered, for instance, with a four wheel drive vehicle.  No exceptions shall be permitted*.

*In some special circumstances, the Director may permit a State Agency to purchase a higher trim line than what was awarded as part of the Contract, by using the manufacturers options line.  In those instances, Using Agencies must obtain written approval from the Division prior to the issuance of a purchase order.
[bookmark: _Toc161300813]VEHICLE SPECIFICATIONS – TECHNICAL PROVISIONS

[bookmark: _Toc161300814]19,500 LB. GVWR CREW CAB & CHASSIS, DRW, 4WD (PRICE LINE: 1)

It is the intent of this specification to describe the base model requirements for a 2024 model year or newer 19,500 lb. GVWR crew cab and chassis, DRW, 4WD.  

The following makes and models were considered when developing the specification:   2024 Ford Super Duty F-550 DRW Crew Cab 4WD and 2024 RAM 5500 Chassis Cab DRW Crew Cab 4WD; however, any make and model that meets or exceeds the specifications will be considered.
4.3.1.1  Dimensions and Capacities:

GVWR:	 19,500 lb. minimum     

CA:	 84 inch minimum
WB:	 197 inch minimum 
4.3.1.2  Axles:

Front - Type: 		Manufacturer's standard
            Capacity:		Minimum 7,000 lb. GAWR

Rear - Type: 		Manufacturer’s standard
           Capacity:		Minimum 13,500 lb. GAWR

4.3.1.3  Brakes:

Manufacturer’s 4-wheel disc brakes with anti-lock brake system. 

Note:  Brakes must incorporate manufacturer's standard non-asbestos type brake linings.   

4.3.1.4  Crew Cab:
Capacity:  Minimum Five (5) personnel
Seats:	                                
Front:   Vinyl bucket type seats, or Split Vinyl 40/20/40 bench seat with deleted center seat equipped with safety belts.   
Rear:   Vinyl Bench type equipped with safety belts
Cab must include:  Power front side windows, power door locks with remote keyless entry, tinted windows, minimum of two (2) 12-volt auxiliary power outlets (dash mounted), floor mats and two (2) complete sets of keys.

Air Bags:	  Minimum driver and passenger-side front air bags.

Gauges/Indicators:  Water temperature, fuel, tachometer, speedometer, trip meter and odometer.

Side View Mirror:  Quantity 2, manual telescoping trailer tow type. 
Grab Handles:  Driver and passenger side grab handles.
Running boards and/or steps:   Aluminum tread plate or manufacturer’s optional running boards must be securely attached to the frame of the truck.  They are to extend from the front wheel well to the end of the cab.
Windshield Wipers:  Manufacturer’s standard 	

Heater and Defroster:  Heavy duty fresh air type 

Air conditioning:	Must be provided.
Radio:  AM/FM 
GVWR labeling:  Lower right hand corner, driver’s side door must be labeled in 3 inch high red letters on a while background, for example:  19,500 lb. GVWR Minimum

Curb weight:  Curb weight shall be determined by the Contractor weighing the first completed Unit on each order.

4.3.1.5  Electrical System:

Alternator (volts):  12
Alternator (amps):  Minimum 200 amp. 

Starter (volts):  12

Battery (CCA):  Minimum 12 volt 720 CCA. 

Electronic auxiliary idle/throttle control kit, mounted in cab, must be provided.

Rear Lights:  LED stop lights, taillights, directional signals, 4-way flashers, reflectors, back up lights and license plate light.  

Front Lights:  Manufacturer’s standard headlights, parking lights, directional signals and four-way flashers. 

Fuse panel must be located in a convenient location.  All electrical wires for cab/chassis and bodies, as applicable, must be enclosed in a plastic loom.

Power Distribution:  Any non-OEM accessory such as safety lights and radios must be protected by an appropriately sized fuse or circuit breaker located as close to the battery as practicable. At no time shall an accessory wire pass from the engine compartment through the firewall into the interior of the vehicle or from the engine compartment to any other part of the vehicle (either internally or externally) without the appropriate fuse or circuit breaker.  All wires added shall be automotive type and have an SAE rating. Wires must be properly sized for current draw and length of run per automotive industry standards. All wires passing through the firewall or any metal must be protected by grommets and neatly tied or loomed. Any wiring routed near engine exhaust and exhaust components must be heat shielded.
Accessory Power: From the positive terminal of the battery a two (2) gauge wire shall connect to a high current breaker (Cooper Bussman CB185 Series or comparable), exact rating must be determined by the Vendor {Contractor} and will be subject to Using Agency approval. The breaker shall be mounted as close as practicable to the battery followed by a two (2) gauge wire to a continuous duty solenoid (NAPA, item # ECHST99, continuous duty, 12 volt, 100 amp, or comparable). A two (2) gauge wire connected to the other side of the solenoid should feed the fuse blocks at the console in the cab. The solenoid must engage when the ignition switch is turned on. Any other accessories that are not connected to the fuse blocks at the console must connect to the switched side of the solenoid with appropriate fuse or breaker as close as practicable to the solenoid. Note: All electrical circuits must have a suitable fuse or breaker. Terminals on solenoid and breaker must be shielded from inadvertent shorting.
Electrical system must be guaranteed by the Bidder to be of ample capacity to handle total electrical load with auxiliary lights. All electrical circuits must be equipped with fuses or circuit breakers for protection against overload of wiring and electrically operable devices. Fuses/breakers must be marked as to their function.

All electrical wires shall be heavy duty plastic covered. All exposed electrical junction blocks shall be enclosed with a boot for protection against salt and road chemicals. All electrical wires shall be enclosed in a loom. Any splices in the battery or other electrical cables shall be sealed with heat shrink tubing.
4.3.1.6  Cooling System:

Radiator type:  Heavy duty increased capacity tubular system.

Radiator must be manufacturer’s largest compatible size.  Cooling system must be capable of maintaining safe operating temperatures over extended idling periods.  Cooling system must be protected with long life coolant and shall have a minimum 300,000 mile life with coolant extender. 

4.3.1.7  Engine:

Type:  Diesel, 6.7L 

Rated horsepower:  300 HP or greater

Rated torque:  660 lb.-ft. or greater

Block Heater:  Electrical block heater mounted in engine block, 120-volt with flush mounted NEMA 5-15 configuration body receptacle (male), with spring loaded weather cap.

A 25 ft. grounded extension cord, 12 gauge, UL listed safety extension cord, conforming to OSHA requirements for outdoor use shall be provided. The female connection of the cord must fit the weather cap assembly. Electrical block heater cab connection shall be located on the driver’s side of the vehicle in front of or under the driver’s side door.   

Note:  Engine block heater weatherproof receptacle shall be sealed by spraying the rear wire connecting terminals with Armor #17 (or Krylon or comparable) clear plastic (care shall be taken not to spray the receptacle contact prongs). Rear wire covering boot shall be sealed at both ends with silicone rubber adhesive sealant (MOPAR #4318025 or comparable) or appropriate caulk to seal the boot to the receptacle housing and to the wire lead.

Exhaust:  Horizontal muffler, with horizontal discharge pipe, left or right side of the vehicle.

Low oil pressure and high engine temperature warning light or audible alarm shall be included. 

Air cleaner:  Replaceable; standard.

Oil filter:  Spin-on type

4.3.1.8  Frame:

Frame Type:  Manufacturer’s standard frame.
Front and rear license plate brackets must be provided.
4.3.1.9  Fuel System:
Tank Capacity:  40 gallons or greater  

Fuel tank(s) must have locking fuel fill cap, with two (2) keys included with each unit.  Opening(s) must be labeled "Diesel Only" in 1 inch high black letters.  Locking fuel cap shall be installed prior to delivery.  

4.3.1.10  Steering:

Type:  Power with tilt steering wheel  

4.3.1.11  Suspension:

Front - Capacity:  Minimum 7,000 lbs. GAWR

Rear - Capacity:  Minimum 13,500 lbs. GAWR

Heavy duty front and rear shock absorbers.

4.3.1.12  Transmission:

Type:  Minimum 6-speed automatic with overdrive 

Transmission must be equipped with left or right PTO outlets. 

Transmission must have "hot shift" PTO (Chelsea 276 or comparable) and must include all required hydraulic shift controls.  Engine shall be programmed for over-speed protection while in PTO mode or transmission shall have provision to avoid over-speed occurrence.  A flashing indicator light shall be provided to show when PTO is engaged.  A heavy duty bracket may be required to support the PTO/pump to the transmission.

4.3.1.13  Wheels:
Type:  Steel disc 
Size:  19.5 
Quantity:  Seven (7), including a full size spare.

Fenders must be installed over rear wheels. 

4.3.1.14  Tires:

Type:  Tubeless blackwall, radial, all-season on front and rear.
Quantity:  Seven (7), dual on rear and spare
Size:  LT225 or comparable (sized to meet GVWR)
Tire load rating shall be selected so as to meet or exceed GVWR requirement.

Manufacturer's recommended tire pressure shall be stenciled in black paint over each tire on fender or body in 1 inch high letters. 

Anti-sail mud flaps must be provided behind the rear tires. 

Spare tire must be mounted on spare rim.

4.3.1.15  Trailer Cable Connectors:

Truck must have one (1) A.T.A. and S.A.E. approved, 7-wire trailer connector (female type), Cole Hersee 12080 or comparable.  Connector must be mounted on the rear bumper with cover provided.  Wiring must conform to A.T.A. color code.  All wiring must be protected from salt and corrosion.

4.3.1.16  Combination Ball/Pintle Hook:

A combination ball/pintle hook Buyers Product model #10040 or comparable with pintle hook mounting plate must be provided. Combination ball/pintle hook with 2-5/16 inch ball shall be mounted 18” from ground. A heavy duty 2 inch receiver tube with pin must be provided on a ½ inch thick steel hitch plate. The pintle hook assembly may require an elbow to meet 18 inch height. Two (2) lunettes must be securely fastened to the hitch plate. 

4.3.1.17  Combination Rear Bumper with Receiver Tube:

Full width 4 inch steel channel bumper shall be integrated into the hitch plate with receiver tube and integrated with (FMVSS 108 compliant) LED tail lights, LED backup and amber LED strobes and backup alarm. 

4.3.1.18  Safety Features and Equipment:

Each unit shall include the following:
5 lb. class ABC fire extinguisher and mount. 
Mechanical jack rated to lift vehicles GVWR.
Triangle kit with one set of three triangles in a case, that meets FMVSS 125. 
First aid kit that meets ANSI Z308.1 standards.
Mounting locations for all of the above to be determined at Post-Order/Pre-Production meeting (Bid Solicitation Section 4.4.4.1).
4.3.1.19  Safety Lights and Warning System:
Note:  Safety lighting shall be installed in addition to normal vehicle manufacturer/factory required lighting.  

Vehicle manufacturers/factory lighting shall not be deleted unless specifically noted.  

One emergency light bar, amber, with automatic dimming feature at night shall be mounted on the cab, Whelen Edge Freedom IV F4X2AAAA with PhotoCell F4XPHOTO or comparable. The light bar shall have a raised 55 inch long base and approximately 5” permanent mount, Whelen Model MK8H mount or comparable. The light bar installation shall not interfere with any equipment movement.  

The light bar shall be LED with two (2) LED rear takedown lights, four (4) corner modules with six (6) forward and six (6) rear facing LED modules. 

The light bar shall have sequential or alternating flash capability.

The light bar shall include a weather-proof clear dome and utilize the cab and chassis manufacturer installed upfitter switches. A three-position toggle switch, mounted in the dash, shall allow joint or isolated use of lights. The light bar control switch shall come with a dashboard mounted indicator light.

[image: ]

Two (2) amber LED strobes, Whelen M4 or comparable, must be mounted on the rear of the truck near the taillights.  

[bookmark: _Toc161300815]4.3.1.20   Vehicle Manufacturer’s Published Options (PRICE LINE 1A):
Vehicle manufacturer's options, which includes any compatible options for the cab and chassis specified in Section 4.3.1 shall be offered using the Vehicle Manufacturer’s Published Options percentage discount price line item (Price Line 1A).  Upon Contract award, the State intends to upload the vehicle manufacturer’s published options for the cab and chassis bid/awarded utilizing a third party database.  The vehicle manufacturer’s options for the cab and chassis bid will be based on the vehicle manufacturers MSRP pricing.  As such, the Contractors discount awarded on the Manufacturer’s Options price line (Price Line 1A) will be applied to the vehicle manufacturers MSRP pricing.

[bookmark: _HOOK_LIFT_SYSTEM][bookmark: _Toc161300816]HOOK LIFT SYSTEM (PRICE LINE: 2)

It is the intent of this section to describe the specifications for a hook hoist frame and hook lift, which must be compatible with the various bodies (Sections 4.3.3 through 4.3.10) and salt spreader (Section 4.3.11) specified in this Bid Solicitation. 
The hook lift system specified herein is comparable to an Ampliroll AL90 S-12, Palfinger T12S or Stellar 84-10 Flex 36; however, any hook lift system that meets or exceeds the specifications will be considered.
4.3.2.1  Dimensions and Capacities:
Lifting Capacity:  12,000 lb. or greater
Container Length:  10 feet or greater
Hook Height:  35 inches or greater
Dump Angle:  50° minimum
4.3.2.2  General:
The lifting capacity must be 12,000 lb. or greater and hydraulically adjustable by pressure relief for optimal weight carrying as not to exceed the GVWR and damage the cab and chassis.

The hook lift must have a pivoting type tilt section hook assembly to provide a low degree loading/unloading angle. The pivoting front tilt section must lift the front of the container/body off of the front saddles, then rolling the long sills on the load rollers, eliminating the need for wear pads.  No frame rail wear pads or intermediate rollers are acceptable.

The tilt cylinder must be fully retracted when in transport mode to prevent exposure of the cylinder rod to corrosive road salts. The hook lift must have a positive tilt section safety lock to prevent tilt section operation while in the dump mode.

The hook lift must have two (2) load rollers, one on each side, which the body long sills roll on; wear pads are not acceptable. All rollers must have grease zerks. 

All moving parts shall have grease fittings. Rear pins shall be stainless steel.

The use of wear pads is not acceptable.

4.3.2.3  Frame:

The hook-hoist frame shall be constructed to reduce wear on body understructures. The actual lifting capacity shall be hydraulically limited to not to exceed the chassis manufacturers axle weights.

The frame shall be thoroughly cleaned of welding slag or other by-products prior to applying primer to ensure proper adhesion.
	
The hook lift frame shall have a positive front body lock and keeper system including a hydraulic counterbalance valve.

A positive locking system must be supplied to prevent the body from moving rearward in the event that a hydraulic line fails.

Dual fixed-position hold down devices must be mounted to the dump frame to secure the body to the hook lift through all ranges of the dump mode and transportation. This must be accomplished without the use of springs and/or hydraulic/air cylinders. Slide through hold-down devices are not acceptable. 

A visual indicator (red bars, striping, paint, etc.) that the body has been fully locked in place shall be installed on frame rails. A whisker switch shall also been installed on the frame rails with an indicator light in the cab to ensure that the body has be fully locked in place. The exact layout and configuration of the visual indicator and the whisker switch shall be determined and approved by the Using Agency at the pre-manufacture/pre-production meeting.

4.3.2.4  Hydraulic System:

The hydraulic system shall provide sufficient flow and pressure to maximize hook lift operation as well as provide appropriate hydraulic flow and pressure to power and control the hook lift. 
Hydraulic controls shall be mounted in the cab and must have center lock out on lift/dump function to meet OSHA 1926.601(b) (11), which states: “Operating levers controlling hoisting or dumping devices on haulage bodies shall be equipped with a latch or other device which will prevent accidental starting or tripping of the mechanism.” Hook lift operation shall be controlled from the safety of the chassis cab. 

The hydraulic system shall be sized appropriately to handle all the different body options along with the requirements of the actual hook lift and shall include full hydraulic option. 

A direct coupled pump shall be installed with hot-shift transmission mounted PTO to allow operation in any gear. 
 
[bookmark: _Toc161300817]STAINLESS STEEL DUMP BODY WITH TILT/DUMP INTERLOCK (PRICE LINE: 3)
		
It is the intent of this section to describe the specifications for a hook lift stainless steel dump body, which must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2.  

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

4.3.3.1  Dimensions and Construction:

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black. 

The interior dimensions of the dump body shall be 120 inches to 132 inches long x 84 inches wide with material shedding boxed top rails and 19 inches high 3-panel stainless steel double acting tailgate. The dump body shall carry a minimum of 2.8 yards without sideboards and a maximum of 4.4 yards with sideboards installed.

The dump body and tailgate shall be 304 stainless steel. Dump body shall be of standard single wall construction. The top sides of the body shall have 2 inch x 8 inch hardwood boards and have two intermediate vertical side braces, plus 6 inch front and rear board pocket extension pockets. 

Bulkhead shall be a minimum of 24 inches high, 10-gauge stainless steel, with double bend top.

Cab shield shall be ¼ style, stainless steel. 

Cab shield shall be at a height that does not interfere with equipment movement or the cab safety lighting.

A tarp roller shall be self-contained in the body. Tarp shall be black mesh type and include a tarp roller kit, Buyers Products model DTR with tarp roller kit or comparable. 

The floor shall be 10-gauge thick stainless steel.

The cross members shall be 3 inch structural steel channel spaced on 12 inch centers and full width rear bolster. Cross members shall be painted with corrosion resistant paint.

A two-way gate shall be provided with heavy duty cast or fabricated stainless steel hardware, one (1) set of banjo eyes and chains with abrasion resistant covers

Tailgate control lever shall be located at the front end of the body at the driver’s side. Lever shall  be vertical in latched position and offset as required.  

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

4.3.3.2  Tilt/Dump Interlock:

Dumping must be accomplished through a rear pivot point. Tilt and dump sections must lock into a rigid frame to support the body/container while in the dump mode. This must be accomplished without the use of springs, latches, rods, brackets, air/hydraulic cylinders, and or gravity to change modes of operation. The hook lift must be protected from out-of- sequence operation.

The tilt/dump interlock shall be performed by using the electronic controls of the hook/lift hydraulic system specified in Bid Solicitation Section 4.3.2. 

[bookmark: _Toc161300818]STAKE BODY (PRICE LINE: 4)

It is the intent of this section to describe the specifications for a hook lift stake body, which must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

4.3.4.1  Dimensions and Construction:

The hook lift compatible stake body exterior dimensions shall be 132 inches to 144 inches long x 96 inches wide. 

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black. 

The floor shall be constructed of 3/16 inch diamond plate with a corrosion resistant undercoating. 

The outside edge of deck shall be 3-¼ inches fabricated 10-gauge channel.

The platform shall have a full perimeter 3/8 inch x 2 inch flat bar welded outside the stake pockets.  The stake pockets shall be 2 inches x 4-¼ inch constructed of 3/16 inch steel, 24 inches on center.

The removable slatted stake sides shall be 40 inches to 42 inches high, with 4 rows of 16 gauge corrugated 6-½ inch slats.

The fixed bulkhead shall be 40 inches high and constructed from 10-gauge steel.  Two (2) swivel D rings shall be welded to bulkhead. The bulkhead window shall be 20 inches x 13 inches. 

Key holes or ½ inch D rings, with swivel fittings, shall be located at the four corners of the body floor.

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc161300819]LANDSCAPE BOX BODY (PRICE LINE: 5)

It is the intent of this section to describe the specifications for a hook lift landscape style box body, which must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

4.3.5.1  Dimensions and Construction:

The interior dimensions of the landscape box body shall be 132 inches to 144 inches long x 96 inches wide. 

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black. 

The floor shall be constructed from 10-gauge smooth steel.

The sides shall be constructed from 10-gauge steel.

The cross members shall be 3 inch structural channel spaced on 12 inch centers.

The top rail shall be formed over 10-gauge steel sides.

There shall be 3 side posts per side. Side posts shall be constructed from 12-gauge steel.

The rear corner posts shall be constructed from 7-gauge steel.

The tailgate top shall be formed with 2 inches x 2 inches x 1/8 inch tubular frame work. 

The height of the sides shall be 40 inches high.

On the curb side, there shall be a 48 inch wide door for access.

The back of the box shall have swing open barn doors with a drawer style cam or trailer lock. 

A tarp roller shall be self-contained in the body.  Tarp shall be black mesh type and include a tarp roller kit, Buyers model DTR with tarp roller kit or comparable. 

The body must contain rollers under the body at the rear.  The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc161300820]CHIPPER BODY (PRICE LINE: 6)

It is the intent of this section to describe the specifications for a hook lift chipper body, which must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

4.3.6.1  Dimensions and Construction:

The chipper body’s exterior dimensions shall be 144 inches long x 96 inches wide.

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black. 

The floor shall be constructed from 3/16 inch steel.

The sides shall be constructed from 12 gauge steel. The height of the sides shall be a minimum of 70 inches.

The cross members shall be 3 inch structural channel spaced on 16 inch centers.

The side top rail shall be 3 inches x 3 inches x 1/8 inch box tubing.

The side posts shall be 24 inch centers constructed from 12-gauge steel.

The rear corner posts shall be constructed from 7-gauge steel.

The tailgate top shall be formed with 3 inches x 3 inches x 1/8 inch tubular frame work. 

The tailgate shall consist of a half double barn door style with open top. 

The height of the tailgate to be determined at the time of the prebuild meeting. 

The top supports shall be 2 inches x 2 inches x 3/16 inch angle with mesh vents on both sides.
The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc161300821]ENCLOSED STEEL STORAGE BODY (PRICE LINE: 7)

It is the intent of this section to describe the specifications for a hook lift enclosed steel storage body, which must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

4.3.7.1  Dimensions and Construction:

The storage body exterior dimensions shall be 120 inches to 132 inches long x 96 inches wide with a minimum interior height of 72 inches.  

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudials shall be primed and painted black. 

The floor shall be constructed from 1/8 inch sheet metal with 3 inch cross members on 16 inch to 18 inch centers.

The sides shall be constructed from 12-gauge sheet with 5 inch channel on 36 inch to 48 inch centers. 

The bulkhead shall be 10-gauge sheet with 4 inch channel uprights.

The roof shall be constructed from 12-gauge sheet with a 6 inch peak. 
The top rail shall be 3 inches x 3/16 inch fabricated beam.

The tailgate shall be a lockable trailer type made with 12-gauge sheet and 3 inch channel supports. 

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.
[bookmark: _Toc161300822]PLATFORM BODY WITH 300-GALLON, GASOLINE POWERED HERBICIDE SPRAYER (PRICE LINE: 8)

It is the intent of this section to describe the specifications for a hook lift platform body with minimum 300-gallon, gasoline powered herbicide spreader, AG Spray LS-EL- 300, Reddick 300 Gallon Poly Skid or Reddick RHS-300, Fimco TSSK – 300, or comparable.  The hook lift platform body must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 
All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.
4.3.8.1  Dimensions and Construction:

The platform body exterior dimensions shall be 120 inches long x 96 inches wide. 

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black. 

The floor shall be 3/16 inch diamond plate.

The cross members shall be 3 inch structural channel spaced on 12 inch centers.

The outside edge shall be fabricated of 31/4 inches x 3/16 inch channel.

The bulkhead shall be 40 inches high and shall be constructed from 10-gauge steel.

The stake pockets shall be 24 inches on center.

The rub rail shall be 3/8 inch x 2 inch flat bar.

The bulkhead window shall be minimum 260 square inches. Dimensions to be confirmed at pre-manufacture/pre-production meeting.

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

4.3.8.2  Herbicide Sprayer:

A 300-gallon poly elliptical tank with full length metal cradle shall be mounted to the platform body. 

Metal cradle shall be fabricated from steel or aluminum. 

If steel fabricated cradle is offered it shall be powder coated or painted with corrosion resistant paint.

A 12-volt rewind hose reel with a minimum of 200 foot hose, Hannay model #E1520-17-18-LT or comparable, and an adjustable pattern spray gun, GreenGarde model # JD9 or comparable, shall be mounted to the rear of the tank.

A gasoline powered engine, pump and sprayer shall be properly sized to meet the spray volume of 5 to 125 gallons per acre or more on swath widths of 5 to 40 feet with accuracy.

The cables/hoses from the control unit to the sprayer that control the operation/function of the sprayer shall have quick-disconnect connectors installed. 

Two (2) Radiarc sprayers, or comparable, shall be provided, one mounted on each side (left side and right side) of the platform body, close to the headboard.

Nozzle orifices supplied shall produce uniform droplets from 1000 to 5000 micrometers (microns). 

Ten (10) extra plugs and four (4) extra nozzles shall be included.

The exact layout and configuration shall be determined and approved by the Using Agency at the Post-Order/Pre-Production meeting (Bid Solicitation Section 4.4.4.1). 

4.3.8.2  In-Cab Controls:

NOTE:  The in-cab controls associated with this herbicide sprayer will be ordered utilizing Price line 13.  Please refer to Bid Solicitation Section 4.3.13.

[bookmark: _Toc161300823]PLATFORM BODY WITH TOOLBOXES (PRICE LINE: 9)

It is the intent of this section to describe the specifications for a hook lift platform body with toolboxes, which must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

4.3.9.1  Dimensions and Construction:

The platform body exterior dimensions shall be 132 inches to 144 inches long x 96 inches wide.

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions . Longitudinal shall be primed and painted black. 

The floor shall be 1/8 inch tread plate steel.

The cross members shall be 3 inch x 4.1lb. /ft. structural channel on 12 inch centers.

The side rails shall be fabricated of 3 inch x 4.1lb. /ft. structural channel.

The bulkhead shall be 36 inches high and shall be constructed from 10-gauge steel.

Tailgate shall be 12 inches high x 10 gauge steel, hinged drop down style with retainers on top to secure to steel tubing rear corner posts.
The platform body shall be primed and painted with white enamel including underside.
Both sides of body shall have permanently installed toolboxes: dimensions: 18 inches x 18 inches x 60 inches, Buyers Products model 1702415 or comparable.  Units shall have two (2) toolboxes on each side of the body. Toolboxes shall have a powder coated white finish and must be keyed alike.  
The latch shall be stainless steel “T” handle style.  Any additional space on sides shall be filled with a 10-gauge filler panel at rear.
A removable 2 inch square steel tubing ladder rack shall extend from rear corners posts 6 inches above cab roof height.  This ladder shall be removable with a ½ inch clevis pin on each side.  A permanent 2 inch square tubing ladder rack section shall extend off the front bulkhead.
Hooks shall be installed on all four (4) corners of the ladder rack.
Two 2 inches x 120 inches long retracting ratchet tie downs shall be furnished to secure ladders to rack.
The ladder rack shall support a minimum of 300 lb.
The body must contain rollers under the body at the rear.  The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc161300824]DUMP BODY WITH MULTI-FUNCTION LIFTGATE/TAILGATE (PRICE LINE: 10)

It is the intent of this section to describe the specifications for a hook lift dump body with multi-function liftgate/tailgate, which must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications. 
4.3.10.1  Dimensions and Construction:

The interior dimensions of the platform dump body shall be a minimum of 126 inches long x 84 inches wide. The exterior width dimension shall be 96 inches. 

The hook lift longitudinal shall be of adequate design and strength to ensure proper functioning under normal operating conditions. Longitudinal shall be primed and painted black. 

The floor shall be 10-gauge steel.

The cross members shall be 3 inches x 4.1 lb./ft. structural channel on 12 inch centers.

The body sides shall be 13 inches high 10 gauge steel with 2 vertical ribs and boxed top rail. 

The body front shall be 24 inches high 10 gauge steel. 

The front bulkhead shall be 36 inches high 10 gauge steel. 

The body must contain rollers under the body at the rear with extended brackets, so when the body is off loaded the rear rollers hit the ground before the liftgate.  The rollers must be the first thing to make contact with the ground. 

4.3.10.2  Tailgate:

The liftgate platform shall be 83 inches x 33 inches tread-plate steel with a 6 inch tapered load area, Tommy Gate G2 Series model 92-1650 LD33 Lift-N-Dump or comparable.  The lift gate shall have a dual cylinder, parallel arm design.  The lift and dump feature shall include pins to lock the platform in place when not in dump-trough mode.  A platform latch shall activate the lift gate’s dump trough position.  The lift gate shall have a loading capacity of 1,600 lb. The lift gate shall be powder coated and painted black. 

Power and ground connection shall be run to the front driver’s side bulkhead area of body with a weather resistant, two pole plug connection of adequate amperage rating.  Opposite end of plug shall be wired to battery through high amp resettable circuit breaker.
[bookmark: _Toc161300825]SALT SPREADER (PRICE LINE: 11)

[bookmark: _3.4.11_OPTION:_9’]It is the intent of this section to describe the specifications for a 108 inch- 120 inch, medium duty, 4.0 cubic yard V-box electric salt spreader with single auger, Meyers MDV-A 944 Electric 9’ SS, Part # 64539 or comparable.  The salt spreader must be capable of hauling and spreading free flowing granular materials. The salt spreader and hook lift frame assembly must be compatible with the hook lift system specified in Bid Solicitation Section 4.3.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

The 108 inch to 120 inch stainless steel salt spreader shall be mounted upon the hook lift frame assembly specified in Bid Solicitation  Section 4.3.2.3 that will safely allow the loading and unloading from the chassis mounted hook lift system. 

The unit shall mount on a hook lift frame with 10 gauge stainless steel floor to minimize carry-back onto chassis frame.  Rollers shall be mounted under the rear of the hook lift frame.  The rollers shall be install in such a manner to prevent the spinner from contacting the ground when unloading the body assembly. 

4.3.11.1  Dimensions and Construction:

	Length-----------------------
	108 inch to 120 inch

	Hopper Height-------------
	44 inches

	Hopper Width--------------
	70 inches

	Spread width---------------
	Adjustable from a minimum of 4 feet to a maximum of 30 feet 

	Capacity Load-------------
	 4.0 cubic. yard.



The unit shall consist of a hopper, discharge chute, auger, spinner disc, two independent electric motors and all of the components necessary to make a complete operating system. 
All stainless steel used in the production of this unit shall be 201 or 304 12-gauge corrosion resistant, non-magnetic stainless steel. 
4.3.11.2  Hopper:

Each hopper side shall be constructed from a single piece of 12-gauge stainless steel and shall have a slope of no less than 45° to ensure free flow of material to the conveyor. The side shall have a minimum of six (6) 12-gauge stainless steel (three per side) external body supports for maximum rigidity.

The hopper ends shall be manufactured of 12-gauge stainless steel and be continuously welded to the hopper sides.

The complete hopper top edge shall be double crimped for additional support.

A combination stainless steel lift hook and hold down shall be furnished in each corner of the hopper.

4.3.11.3  Electric Drive:

The spreader must be equipped with two independent industrial grade electric variable speed motors. The motors shall operate at a current of 60 amps. The electric motors shall utilize the vehicle’s existing electrical system. 

One motor shall be used to drive a spiral auger. The other motor shall be used to drive the spinner disc.

Dual speed controller shall be installed in cab of vehicle to provide ultimate spreading. 

The spreader shall include fork pockets and EIS (Electric Inter-Lock System) for safety. 

4.3.11.3  Spinner Assembly:

The distributor disc shall be minimum 12 inches in diameter and made of polyurethane with molded vanes.

The spinner disc shall be directly coupled to spinner motor.  Extension shaft(s) and bearings shall not be used.  

There shall be a minimum of four (4) stainless steel external overlapping baffles, and two (2) internal baffles to control the direction and width of the spread pattern.  Three (3) of the external baffles shall be adjustable without the use of tools; the fourth shall be fixed to protect the truck.  The entire spinner chute and baffles shall be manufactured from 12-gauge stainless steel.
The entire spinner assembly shall swing-up by removing one stainless steel pin and hydraulic quick disconnect.
4.3.11.5  Top Screens:

A two-section center hinged top screen shall be provided. The screen sections shall be manufactured from ¼ inch rod welded to form square openings of 3 inches and framed by J formed channel.

A simple Drop-n-Lock type hinge arrangement shall be provided to eliminate the need for hardware that may vibrate loose.

4.3.11.6  Safety Lighting:

A strobe light system shall be mounted on the rear of spreader wall to ensure visibility. The light system shall include two (2) amber LED strobes, Whelen M6 or comparable. 

4.3.11.7  In-Cab Controls:

The in-cab controls associated with this salt spreader will be ordered utilizing Price line 14.  Please refer to Bid Solicitation Section 4.3.14.

[bookmark: _Toc161300826]SNOW PLOW (PRICE LINE: 12)

It is the intent of this section to describe of the specifications for a 9’ snow plow, Western/Boss/Meyer/Fisher Mount or comparable.

4.3.12.1  Dimensions and Capacities:

Blade Width: 108 inches		
Blade Height: 29 inches or greater		
Plowing Angle: 30˚ right or left, to provide minimum 93 inch swath
Cutting Edge: ½ inch x 6 inches
Type: 11 or 12 gauge steel				

4.3.12.2  Equipment:

Marker Guides:  2 high visibility, flexible marker guides 

Controls – Hand Held type controller:   Boss SmartTouch2 Handheld Controller, Western Cab Command Handheld Controller or comparable.	
Snow Plow Lights.			
Standard Deflector: Rubber with steel backer plate
4.3.12.3  Mounting:

The snow plow must be removable by quick disconnect pins, as one complete unit including blade, lift assemblies and lights. Removal of lift shall also remove lights and electro-hydraulic lift unit.  The vehicle bumper must remain in the same position as originally installed by the vehicle manufacturer.

4.3.12.4  Plow Control System:

Lift, lower and power angle shall be self-contained and consist of an electro-hydraulic pump, reservoir, electric solenoid control valves, lift cylinder, power angle cylinders, hoses, quick disconnects and wire harness.

Please note that the unit must have full hydraulic power for lift, lower and angle functions.  No exceptions.

4.3.12.5  Hydraulically Operated Mechanical Chain Lift System:

The hydraulically operated mechanical chain lift system shall provide float and short chain capabilities to transport the plow in case of inoperable condition.

[bookmark: _IN-CAB_CONTROLLER_FOR][bookmark: _Toc161300827]IN-CAB CONTROLLER FOR HERBICIDE SPRAYER (PRICE LINE: 13)

This section and price line item is for the purchase and installation of an in-cab controller for the herbicide sprayer specified in Bid Solicitation Section 4.3.13.  The in-cab controller shall be compatible with and ensure full functionality of herbicide sprayer and applicable components. Please note that this price line item is for an in-cab control only and not for the actual herbicide sprayer. Since the cab and chassis (Bid Solicitation Section 4.3.1) and Hook Lift System (Bid Solicitation Section 4.3.2) allow for the interchangeability of various bodies between trucks.  Note:  The DOT intends to have this in-cab control installed in most of its trucks. 

[bookmark: _IN-CAB_CONTROLLER_FOR_1][bookmark: _Toc161300828]IN-CAB CONTROLLER FOR SALT SPREADER (PRICE LINE: 14)

This section and price line item is for the purchase and installation of an in-cab controller for the salt spreader specified in Bid Solicitation Section 4.3.14.  The in-cab controller shall be compatible with and ensure full functionality of salt spreader and applicable components. Please note that this price line item is for an in-cab control only and not for the actual salt spreader. Since the cab and chassis (Bid Solicitation Section 4.3.1) and Hook Lift System (Bid Solicitation Section 4.3.2) allow for the interchangeability of various bodies between trucks.  Note:  The DOT intends to have this in-cab control installed in most of its trucks. 

[bookmark: _ONE_SET_OF][bookmark: _Toc161300829]ONE SET OF PARTS, SERVICE AND OPERATION AND MAINTENANCE MANUALS (PRICE LINE: 15)

4.3.15.1  Manuals:
One set of parts, service and operation and maintenance manuals for each and every assembly system and/or component that makes up the unit shall be provided as follows:
1 - set of parts manuals (illustrations and text) bound or with binders, or on CD-ROM, if unavailable bound.
1 - set of complete shop repair (factory service) manuals bound or with binders or on CD-ROM, if unavailable bound.
1 - set of complete operation and routine maintenance manuals
1 - set of electrical schematics
1 - set of troubleshooting manuals for the gas engine on sprayer
Examples of assembly systems and/or components include, but are not necessarily limited to:
	a.
	Hydraulic pump and hydraulic systems

	b.
	Engine, drives and chassis

	c.
	Transmission

	d.
	Electrical system

	e.
	Lubrication system


The manuals shall be delivered directly to the Using Agency upon delivery.  Failure to supply these manuals may delay approval of invoices for payment.
[bookmark: _TECHNICAL_SUPPORT_(PRICE][bookmark: _Toc161300830]TECHNICAL SUPPORT (PRICE LINE: 16)

4.3.16.1  Operator Training:
The Contractor, in cooperation with all aftermarket installers/subcontractors/dealers, shall provide training as described below. 

The Contractor shall collaborate with the Using Agency to provide a four (4) hour operator training session for every completed truck delivered with a maximum of 5 agency personnel.  This training shall be made available throughout the duration of the Contract and any extension(s) thereof.

Complete instructions on the operation and maintenance of each Unit and a demonstration on the operation of the Unit shall be given by the Contractor. 

The training shall consist of, but is not limited to, operator training with instruction on proper operation of the Unit, safety, preventive maintenance and repair.

The Contractor and the Using Agency shall agree on the content of this material, based on the differences between the trucks contained herein and any existing truck in the Using Agency’s fleet. 

This demonstration shall be a formal training session and shall be arranged with the Contractor, conducted within one (1) week of delivery of the first Unit, at the convenience of the Using Agency. 

The training session shall be conducted at the location of delivery or at a field location within the State of New Jersey.

4.3.16.2  Mechanics Training:
The Contractor, in cooperation with aftermarket installers/subcontractors/dealers, shall provide technical training for all components of the complete truck. 
The Contractor shall collaborate with the Using Agency to provide a one (1) eight (8) hour day mechanics training session for every 5 completed trucks delivered with a maximum of 5 agency personnel.
The Contractor shall provide training for the listed critical areas. 
This training shall consist of, but is not limited to, the same training as is provided to technicians employed by dealerships who sell these components, with the following exceptions:
Course content shall be tailored to meet the specific needs of the Using Agency mechanics, and shall not place emphasis on areas or components not specified in these specifications. Course shall also include as much hands-on content as needed to reinforce lecture content.
	Cab and Chassis Systems 
a. Engine diagnostics and repair, including electronic controls, fuel system and emissions system. 
b. Electrical system controllers, operation and diagnostics.
c. Automatic transmission diagnostics and repair.

Body Builder-Installed Components
a. Hydraulic system operation, diagnostics and repair. 
b. Electrical accessories operation, circuits, diagnostics and repair. 
c. Warning light system operation, diagnostics and repair.

This demonstration shall be a formal training session and shall be arranged with the Contractor, conducted within one (1) week of delivery of the first Unit, at the convenience of the Using Agency. 
The training session shall be conducted at the location of delivery or at a field location, within the State of New Jersey.
If additional training is required, it shall be part of the line item for mechanics training and shall cover, but not be limited to the above topics.  The training shall be scheduled with the Using Agency and shall be a one (1) eight (8) hour day mechanics training session with a maximum of 5 Using Agency personnel.  This training shall be made available throughout the duration of the Contract and any extension(s) thereof.
[bookmark: _Toc161300831]CONTRACT IMPLEMENTATION

[bookmark: _Toc161300832]PLACING ORDERS FOR CONTRACT UNITS

4.4.1.1  This term Contract does not permit Using Agencies to order any option that is not specified in this Bid Solicitation.
4.4.1.1.1  The Contractor shall not substitute any item (part, component, equipment, feature, accessory, material, performance, capacity, rating, design or control), which is a part of the Contract Unit, without written authorization to do so from the Procurement Bureau.
4.4.1.2  During the Contract period, no change is permitted in any terms or conditions unless the Contractor receives written approval from the Procurement Bureau.
4.4.1.3  No dealer's accessories or options, or any other purchases which are not specified in this Bid Solicitation shall be offered. 
4.4.1.4  Trade-ins are not permitted under the term Contract established as a result of this Bid Solicitation.
4.4.1.5  Leasing of Units is not permitted under the term Contract resulting from this Bid Solicitation.
[bookmark: _Toc161300833]PRODUCT BROCHURE/VEHICLE MANUFACTURER’S LIST OF PUBLISHED OPTIONS

4.4.2.1  Product Brochure:  The Contractor shall make sales literature and color charts available to Ordering Agencies and New Jersey State inspectors on an as requested basis.

4.4.2.2  Vehicle Manufacturer’s List of Published Options:  The State intends to utilize an independent, third party database for the publication of vehicle manufacturers options and prices.  

In the event that the database does not contain current manufacturers options and prices for the vehicle model year bid, the State may request that the Contractor submit the manufacturer's published list of options with corresponding MSRP (price list) for the vehicle/cab and chassis bid.  The Contractor may provide the price list via e-mail to the Procurement Specialist of record or send the price list through expedited delivery in the form of a CD or thumb drive in MS Excel, PDF or text format.  The State will not release the Contract until this information is received.  

[bookmark: _Toc161300834]CONFIRMATION OF ORDERS

4.4.3.1  Purchase order confirmation must be submitted to each Using Agency for each order accepted, to the attention of the contact person stated in the purchase order.
4.4.3.2  The Contractor must provide the order confirmation promptly following factory order entry.
4.4.3.3  Order confirmation shall mean that the Contractor has received the purchase order, has reviewed it for compatibility with the unit currently on Contract, has resolved any non-compatibility problems with the Using Agency, has entered the order with the manufacturer and that the manufacturer has accepted the order and assigned an order number and anticipated build and delivery dates.
4.4.3.4  The Contractor shall not accept any purchase order after the vehicle manufacturer’s cut-off date, unless instructed otherwise by the Ordering Agency in writing. If an order is not accepted for production by the manufacturer, the Contractor shall return the purchase order with "canceled" marked on the purchase order with an authorized signature next to it. No exception shall be permitted.
[bookmark: _Toc161300835]INSPECTION OF UNITS 

4.4.4.1 Post-Order/Pre-Production/Pre-Installation Meeting and Inspection:  The Contractor shall coordinate and attend a post-order pre-production meeting, if required by the Using Agency, at a location convenient to the Using Agency, to provide all necessary information prior to building any prototype unit or scheduling the production. Only after the post-order pre-production meeting, if required by the Using Agency, and subsequent approval from the Using Agency shall the Contractor begin the production. The Contractor shall coordinate with the Using Agency for a pre-paint inspection for each Unit ordered, if required by the Using Agency.
4.4.4.2 The State reserves the right to inspect the Bidder and/or aftermarket installer(s)' and/or Contractor’s facility. This provision applies during the Quote evaluation period, the Contract term and any extension(s) thereof. 
4.4.4.3 Pre-acceptance Inspections: The State Using Agency reserves the right to inspect the Unit at the Contractor's facility or require that the Contractor make the unit available for inspection at the agency site.  If, during inspection at the agency site, it becomes apparent that corrections/alterations must be made to the Unit to comply with the Contract specifications which cannot be accomplished at the State Using Agency facility, the Unit will be rejected and the Contractor must transport the unit to its facility at no expense to the agency. After the Contractor corrects the deficiencies, the Contractor must re-deliver the unit to the State Using Agency for re-inspection at the expense of the Contractor. 
4.4.4.4 For all inspections performed at the Contractor's site, the Contractor must provide a bay in the repair shop to facilitate the inspection of the Unit.
4.4.4.5 The final inspection and acceptance of the Unit shall occur at the State Using Agency.
4.4.4.6 OEM Equipment/Parts: All of the standard and optional equipment/parts provided shall be original equipment manufacturers items when available.
4.4.4.7 The Contractor must make arrangements for the Using Agency’s inspection of each vehicle prior to the delivery and acceptance of the vehicle by the Using Agency. Prior to presentation for inspection, it shall be the Contractor's responsibility to pre-inspect each Unit.  Each Unit presented for inspection shall be accompanied by an inspection package including, but not limited to, the following: purchase order, line set sheet (when available) - brief list of all features, items and accessories included in the Unit, pre-delivery inspection (PDI), and dealer's pre-inspection prep checklist. The checklist will list the responsible prep mechanic and acknowledge that the vehicle conforms to pre-delivery specifications and that all added equipment and accessories have been properly installed.
4.4.4.8 The Contractor shall notify the State Using Agency by fax and/or e-mail that the Unit is ready for inspection.
4.4.4.9  Delivered Units will be inspected within ten (10) working days. If a Unit has been accepted, the warranty shall commence on the date of final acceptance, or if a Unit has been rejected, the Contractor will be notified. The notice will indicate the reason(s) for rejection. If rejected, the Contractor shall try to rectify the problem(s) at the State Using Agency site. If the problem cannot be corrected at the agency site, the rejected Unit must be removed by the Contractor at its own expense.  The Contractor shall present the corrected Unit for re-inspection within ten (10) working days.  No additional freight or transportation charges are permitted.
4.4.4.10 Within five (5) working days of the Contractor’s notification, the State Using Agency will, if desired, send a team of qualified inspectors to the Contractor's facility to accomplish the inspection of the Unit(s) before delivery to the Using Agency.  The Contractor must properly itemize, organize and segregate all Units.  
4.4.4.11  Non-State Agencies authorized to purchase under this Contract will make arrangements for Unit inspection directly with the Contractor.  All Units must be delivered to each Using Agency’s designated destination at no additional cost.
4.4.4.12  Inspected Units which do not comply with the Contract requirements will be rejected.  The Contractor must correct all rejected Units and the corrected Unit(s) must be presented for re-inspection within ten (10) working days. The Using Agency may cancel the purchase order if the Contractor fails to correct any problem.
4.4.4.13 No additional freight or transportation charges are permitted under this Contract.  
[bookmark: _Toc161300836]DELIVERY AND FINAL ACCEPTANCE  

4.4.5.1  The Contractor must make arrangements for delivery of Unit(s) as instructed by the Using Agency within 15 calendar days of Contractor's receipt of Unit(s) from the manufacturer.  All Units must be delivered within 30 calendar days of Contractor's receipt of Unit(s) from the manufacturer.  For any deliveries that are estimated to exceed 30 calendar days, the Contractor must notify the Using Agency within 14 days of receipt from manufacturer to make further arrangements for delivery with the Using Agency.  All Units must be delivered to each Using Agency's designated destination at no additional cost.
4.4.5.2  All deliveries of Units must be made upon approval and as instructed by the Using Agency, by prior arrangement only, during working hours, except on legal holidays.
Deliveries shall not be made on the following State observed holidays, which may be updated from time to time:
· New Year’s Day;
· Martin Luther King Jr. Day;
· Presidents Day;
· Good Friday;
· Memorial Day;
· Juneteenth;
· Independence Day;
· Labor Day;
· Columbus Day;
· Election Day;
· Veterans Day;
· Thanksgiving Day; and
· Christmas Day.

4.4.5.3  No Unit will be accepted at the final delivery point without all supporting documentation and paperwork completed and delivered with the Unit, which include the certificate of origin, warranty, any specified manuals, invoice and key sets (if applicable).  No Unit will be considered accepted until it has undergone final inspection at the delivery point.
4.4.5.4 For purchases by State Agencies, the manufacturer's certificate of origin must be made out to the State of New Jersey, and presented at the time of delivery.  Purchase order number and requisition number must be indicated on the upper left hand corner. The Contractor shall not furnish the New Jersey Certificate of Title (certificate of ownership).  The State will title the Unit upon receipt of the manufacturer's certificate of origin.  Other governmental entities authorized to purchase under this Contract will make arrangements for titling units directly with the Contractor. 
4.4.5.5  No advertising shall appear on any Unit delivered under the Contract.  Further, the Contractor shall not affix the dealer name to the Unit.  Units delivered to final destinations with dealer's advertising will be rejected.
4.4.5.6  No more than ten (10) Units per day and fifty (50) units per week (based on a 5-day work week) will be accepted at each delivery site.  When necessary, and with the consent of both the Ordering Agency and the Contractor, the number of Units delivered per day may be increased.
4.4.5.7  All vehicles must be delivered with the manufacturer suggested retail price label affixed to the window. The label shall not be removed prior to delivery to the New Jersey agency.
4.4.5.8  All delivered Units must be clean both inside and outside. Manufacturer's standard items, such as hubcaps, floor mats, jack and lug wrench and the like, shall be provided and installed by the Contractor prior to delivery.
4.4.5.9 Complete instructions on the care and maintenance of the unit and a demonstration of its operation shall be given by the Contractor at the time of delivery and acceptance to the agency, if so requested by the Using Agency.
4.4.5.10  The Contractor shall indicate the delivery location of the unit on the factory order, so that recall notices will indicate the delivery location for each Unit.
4.4.5.11 The Contractor must deliver the Units with an index card or other label/card, visible through the windshield, bearing the following information, in typed or printed form:
Vendor's {Contractor’s} name
Purchase order number (if applicable)
Requisition number
Stock number
Serial number
Note: Units without this information will not be accepted.
4.4.5.13  No Unit will be accepted without a New Jersey Motor Vehicle new vehicle inspection sticker in place as prescribed by law, correctly punched to the month of delivery and acceptance or appropriate Diesel Emission Approval Sticker.  Out of State Contractors must comply with this requirement without any additional cost or delay.  Failure to comply with this provision will result in the rejection of the Unit.
[bookmark: _WARRANTIES][bookmark: _Toc161300837]WARRANTIES  

4.4.6.1 The manufacturer's standard warranty must be supplied with each Unit at the time of delivery and shall be in typed form. The warranty commences with the acceptance of the Unit at the delivery site, following the final inspection. 
[bookmark: _Toc161300838]WARRANTIES REQUIREMENTS  

4.4.7.1  The Contractor shall ensure that the manufacturer whose product is supplied has a servicing dealer or service location able to provide warranty and recall service and/or repair within twenty four (24) hours of notification by the Using Agency.  Users of this Contract should contact the Contractor in cases where warranty service/repair is to be performed at a place other than the original place of purchase to arrange for a servicing dealer proximate to their location.
4.4.7.2  The Contractor must perform any warranty service/repair/recall, which will be at Contractor's own expense. Events beyond Contractor's control, such as lack of parts due to strikes and unforeseen acts of God, shall constitute valid reasons for delay in making necessary repairs. However, the State will make such determination.
4.4.7.3 Manufacturer's Warranty Form: The Contractor must provide the appropriate warranty forms.
[bookmark: _Toc161300839]PAYMENT  

4.4.8.1 Invoices will be processed for payment only after final acceptance of the units by the Using Agency and the delivery ticket has been signed off by an authorized representative of the Using Agency. Partial payments may be made for Unit(s) accepted, if billed separately. Timely payment discounts will be taken if offered by the Contractor. The State reserves the right to make payments directly or through a third party.
4.4.8.2 The State reserves the right to order Units through a line of credit.  For these orders, the Contractor will receive a letter from the State in lieu of a purchase order.  Line of credit letters must be accepted by the Contractor on the same basis as regular purchase orders.  All terms and conditions that apply to purchase orders will apply to line of credit letters. 
[bookmark: _Toc161300840]SUBSTITUTION OF DISCONTINUED PRODUCTS 

The Contractor may offer a substitution for any product discontinued by the manufacturer in its Contract. The State may consider substituting the discontinued model with a new model provided that the Unit offered meets or exceeds the Contract specifications.  All substitutions must be approved by the State. 
The Contractor must notify the State immediately in writing to the Division’s assigned Procurement Specialist stating that an item has been discontinued by the manufacturer along with supporting documentation from that manufacturer that the item has been discontinued.  The Contractor must provide in its letter the discontinued model number, model number of the new product being offered, detailed literature for the new product being offered, the price of the discontinued item and the price of the product being offered as a replacement. The State will not approve the substitution of a discontinued item without all of the above information.
The replacement product should be offered to the State at that same price as the discontinued product. 
[bookmark: _Toc161300841]VEHICLE MANUFACTURER’S CUT-OFF DATE  

4.4.10.1  The Contractor must notify the Procurement Bureau of the manufacturer's order cut-off date, as soon as that date is made available by the vehicle manufacturer to the Contractor.  Cut-off Date Notification must be e-mailed to the assigned Procurement Specialist. 
4.4.10.2  Should a potential awardee be notified by a vehicle manufacturer of a cut-off date after the Quote opening and after receiving a letter of intent to award, but before Contract award has been finalized, the awardee must immediately notify the Procurement Bureau in writing. 

4.4.10.3  Failure to fax the cut-off-date notification on time may be considered a violation of the Contract terms and conditions and may result in termination of the Contract for cause.
4.4.10.4  All orders placed by the published cut-off date from either the State or cooperative purchasing program participants must be accepted by the Contractor.  These orders may be hand delivered, or faxed with hard-print purchase orders to follow. The State also reserves the right to order by means of "a letter of intent to purchase" with purchase order to follow.
4.4.10.5  The Contractor is encouraged to offer, during the Contract term and any extension(s) thereof, the contracted or later model year vehicle of configuration meeting or exceeding the Contract specifications at the same Contract terms, conditions and pricing after the manufacturer’s cut-off date. 
4.4.10.6  If a manufacturer is unable to build a vehicle for which an order has been placed by the manufacturer's cut-off date, the Contractor must immediately notify the Procurement Bureau by e-mail.  At a minimum, the letter shall provide the following information:
Purchase order number or line of credit letter date;
The make, model and quantity of vehicles ordered; and
Whether the manufacturer has offered to price-protect and build these vehicles for the next model year.




[bookmark: _Toc161300842]GENERAL CONTRACT TERMS
The Contractor shall have sole responsibility for the complete effort specified in this Contract.  Payment will be made only to the Contractor or to the authorized dealers/distributors, if applicable.  The Contractor is responsible for the professional quality, technical accuracy and timely completion and submission of all deliverables, services or commodities required to be provided under this Contract.  The Contractor shall, without additional compensation, correct or revise any errors, omissions, or other deficiencies in its deliverables and other services.  The approval of deliverables furnished under this Contract shall not in any way relieve the Contractor of responsibility for the technical adequacy of its work.  The review, approval, acceptance or payment for any of the deliverables, goods or services, shall not be construed as a waiver of any rights that the State may have arising out of the Contractor’s performance of this Contract.

[bookmark: _Toc161300843]CONTRACT TERM AND EXTENSION OPTION
The base term of this Contract shall be for a period of three (3) years.  The anticipated Contract effective date is provided on the “Summary” page of the Bid Solicitation in NJSTART.  If delays in the procurement process result in a change to the anticipated Contract effective date, the Contractor agrees to accept a Contract for the full term of this Contract. 

This Contract may be extended up to three (3) years with no single extension exceeding one (1) year, by the mutual written consent of the Contractor and the Director at the same terms, conditions, and pricing at the rates in effect in the last year of this Contract or rates more favorable to the State.  

[bookmark: _Toc400531508][bookmark: _Toc428533979][bookmark: _Toc32310704][bookmark: _Toc161300844]CONTRACT TRANSITION
In the event that a new Contract has not been awarded prior to the expiration date for this Contract, including any extensions exercised, and the State exercises this Contract transition, the Contractor shall continue this Contract under the same terms, conditions, and pricing until a new Contract can be completely operational.  At no time shall this transition period extend more than 180 calendar days beyond the expiration date of this Contract, including any extensions exercised.

[bookmark: _Toc118513795][bookmark: _Toc400531563][bookmark: _Toc428534035][bookmark: _Toc32310758][bookmark: _Toc161300845][bookmark: OLE_LINK3][bookmark: OLE_LINK4]PERFORMANCE SECURITY
Not applicable to this procurement.

[bookmark: _Toc400531513][bookmark: _Toc428533984][bookmark: _Toc32310709][bookmark: _Toc161300846]OWNERSHIP OF MATERIAL
A. State Data – The State owns State Data. Contractor shall not obtain any right, title, or interest in any State Data, or information derived from or based on State Data.  State Data provided to Contractor shall be delivered or returned to the State of New Jersey upon thirty (30) days’ notice by the State or thirty (30) days after the expiration or termination of the Contract.  Except as specifically required by the requirements of the Bid Solicitation, State Data shall not be disclosed, sold, assigned, leased or otherwise disposed of to any person or entity other than the State unless specifically directed to do so in writing by the State Contract Manager.
B. Work Product; Services – The State owns all Deliverables developed for the State in the course of providing Services under the Contract, including but not limited to, all data, technical information, materials gathered, originated, developed, prepared, used or obtained in the performance of the Contract, including but not limited to all reports, surveys, plans, charts, literature, brochures, mailings, recordings (video and/or audio), pictures, drawings, analyses, graphic representations, print-outs, notes and memoranda, written procedures and documents, regardless of the state of completion, which are prepared for or are a result of the Services required under the Contract. 
C. Contractor Intellectual Property; Commercial off the Shelf Software (COTS) and Customized Software – Contractor retains ownership of all Contractor Intellectual Property, and any modifications thereto and derivatives thereof, that the  Contractor supplies to the State pursuant to the Contract, and grants the State a non-exclusive, royalty-free license to use Contractor Intellectual Property delivered to the State for the purposes contemplated by the Contract for the duration of the Contract including all extensions.  In the event Contractor provides its standard license agreement terms with its Quote, such terms and conditions must comply with Bid Solicitation Section 1.4 – Order of Precedence of Contractual Terms.
D. Third Party Intellectual Property – Unless otherwise specified in the Bid Solicitation that the State, on its own, will acquire and obtain a license to Third Party Intellectual Property, Contractor shall secure on the State’s behalf, in the name of the State and subject to the State’s approval, a license to Third Party Intellectual Property sufficient to fulfill the business objectives, requirements and specifications identified in the Contract at no additional cost to the State beyond that in the Quote price.  In the event Contractor is obligated to flow-down commercially standard third party terms and conditions customarily provided to the public associated with Third Party Intellectual Property and such terms and conditions conflict with Bid Solicitation requirements, including the SSTC, the State will accept such terms and conditions with the exception of the following:  indemnification, limitation of liability, choice of law, governing law, jurisdiction, and confidentiality.  The Bid Solicitation including the SSTC shall prevail with respect to such conflicting terms and conditions.  In addition, the State will not accept any provision requiring the State to indemnify a third party or to submit to arbitration.  Such terms are considered void and of no effect.  Third party terms and conditions should be submitted with the Quote. If Contractor uses Third Party Intellectual Property, Contractor must indemnify the State for infringement claims with respect to the Third Party Intellectual Property.   Contractor agrees that its use of Third Party Intellectual Property shall be consistent with the license for the Third Party Intellectual Property, whether supplied by the Contractor, secured by the State as required by the Bid Solicitation, or otherwise supplied by the State. 
E. Work Product; Custom Software – The State owns all Custom Software which shall be considered “work made for hire”, i.e., the State, not the Contractor, subcontractor, or third party, shall have full and complete ownership of all such Custom Software.  To the extent that any Custom Software may not, by operation of the law, be a “work made for hire” in accordance with the terms of the Contract, Contractor, subcontractor, or third party hereby assigns to the State, or Contractor shall cause to be assigned to the State, all right, title and interest in and to any such Custom Software and any copyright thereof, and the State shall have the right to obtain and hold in its own name any copyrights, registrations and any other proprietary rights that may be available. 
F. State Intellectual Property – The State owns all State Intellectual Property provided to Contractor pursuant to the Contract.  State Intellectual Property shall be delivered or returned to the State of New Jersey upon thirty (30) days’ notice by the State or thirty (30) days after the expiration or termination of the Contract.  The State grants Contractor a non-exclusive, royalty-free, license to use State Intellectual Property for the purposes contemplated by the Contract.  Except as specifically required by the requirements of the Bid Solicitation, State Intellectual Property shall not  be disclosed, sold, assigned, leased or otherwise disposed of to any person or entity other than the State unless specifically directed to do so in writing by the State Contract Manager. The State’s license to Contractor is limited by the term of the Contract and the confidentiality obligations set forth in Bid Solicitation Section 6 – Data Security Requirements – Contractor Responsibility.
G. No Rights – Except as expressly set forth in the Contract, nothing in the Contract shall be construed as granting to or conferring upon Contractor any right, title, or interest in State Intellectual Property or any intellectual property that is now owned or licensed to or subsequently owned by or licensed by the State.  Except as expressly set forth in the Contract, nothing in the Contract shall be construed as granting to or conferring upon the State any right, title, or interest in any Contractor Intellectual Property that is now owned or subsequently owned by Contractor.  Except as expressly set forth in the Contract, nothing in the Contract shall be construed as granting to or conferring upon the State any right, title, or interest in any Third Party Intellectual Property that is now owned or subsequently owned by a third party.

[bookmark: _Toc161300847]SUBSTITUTION OF STAFF
Not applicable to this procurement.

[bookmark: _Toc161300848]DELIVERY TIME AND COSTS
Unless otherwise noted in this Bid Solicitation or on the State-Supplied Price Sheet, all delivery times are 350 calendar days after receipt of order (ARO) and prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination (350 calendar days ARO/F.O.B.).  The Contractor shall assume all costs, liability and responsibility for the delivery of merchandise in good condition to the State's Using Agency or designated purchaser.  350 calendar days ARO/F.O.B. does not cover "spotting" but does include delivery on the receiving platform of the Using Agency at any destination in the State of New Jersey unless otherwise specified.  No additional charges will be allowed for any additional transportation costs resulting from partial shipments made at the Contractor’s convenience when a single shipment is ordered.  The weights and measures of the State's Using Agency receiving the shipment shall govern.  Collect on Delivery (C.O.D.) Terms are not permitted.

[bookmark: _Toc161300849]AUTHORIZED DEALER AND/OR DISTRIBUTORS
The Contractor must provide a list of the Dealer(s)/Distributor(s) that will service the Contract.  The Contractor will be required to submit the following forms for each Dealer/Distributor, prior to the Dealer/Distributor being permitted to perform any work on the Contract:
A. Ownership Disclosure (N.J.S.A. 52:25-24.2);
B. Disclosure of Investment Activities in Iran (N.J.S.A. 52:32-55 et. seq.);
C. Disclosure of Investigations and Actions Involving Bidder Form;
D. MacBride Principles  (N.J.S.A. 52:34-12.2);
E. Source Disclosure Certification (N.J.S.A. 52:34-13.2);
F. Vendor Certification (P.L. 2005, c.271);
G. New Jersey Business Registration (N.J.S.A. 52:32-44);
H. Proof of insurance as specified herein;
I. Proof of compliance with New Jersey Affirmative Action requirements (N.J.A.C. 17:27-1.1 et. seq.):
· New Jersey Form AA-302 Affirmative Action Employee Information Report; or 
· New Jersey Affirmative Action Certificate; or 
· Federal Affirmative Action Approval Letter; and
J.	Certification of Non-Involvement of Prohibited Activities in Russia or Belarus Pursuant to P.L.2022, c.3	
A Contractor may submit a request to add or remove Dealers/Distributors at any time during the Contract term, including any extension(s) thereof.  Any such request should be emailed to the Procurement Specialist assigned to this procurement.

[bookmark: _Toc400531525][bookmark: _Toc428533996][bookmark: _Toc32310718][bookmark: _Toc161300850]LIQUIDATED DAMAGES
Not applicable to this procurement.

[bookmark: _Toc400531531][bookmark: _Toc428534002][bookmark: _Toc32310724][bookmark: _Toc161300851]RETAINAGE
Not applicable to this procurement.

[bookmark: _Toc161300852]ELECTRONIC PAYMENTS
With the award of this Contract, the successful Contractor(s) will be required to receive its payment(s) electronically.  In order to receive payments via automatic deposit from the State of New Jersey, the Contractor must complete the EFT information within its NJSTART Vendor Profile.  Please refer to the QRG entitled “Vendor Profile Management – Company Information and User Access” for instructions. 

[bookmark: _Toc161300853]  REPORTING AND SUPPLIER CONVENIENCE FEEPROCUREMENT EFFICIENCY PROGRAM 
A. Quarterly Sales Reporting - The Contractor shall submit a Sales Report documenting all sales made under the Contract.  The Sales Report shall be submitted directly to Periscope no later than thirty (30) calendar days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31. The Sales Report must contain the following information:  
B. Complete and accurate details of all sales, credits, returns, refunds, and the like for the reporting quarter;
C. Purchasing entity;
D. Total of Procurement Efficiency Program Fee amount due for the reporting quarter;
E. Such other information as the State may reasonably request;
F. If no sales were made against this Contract during the reporting quarter, then a report shall be submitted showing zero sales and zero Procurement Efficiency Program Fee due; and
G. Quarterly Sales Reporting and remittance of the Procurement Efficiency Program Fee shall begin on the first calendar quarter starting after the effective date of the Contract.
H. Procurement Efficiency Program Fee - For all purchases made under this Contract, that have been invoiced, the Contractor shall remit the Procurement Efficiency Program Fee in the amount of one percent (1%) of all Purchases to Periscope acting on behalf of the State of New Jersey. 
I. Remittance of the Procurement Efficiency Program Fee - On a quarterly basis, the Contractor shall remit the Procurement Efficiency Program Fee directly to Periscope no later than thirty (30) days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31.  Failure to remit the Procurement Efficiency Program Fee timely and accurately may result in Contract termination as outlined in the “Termination of Contract” clause of the State of New Jersey Standard Terms and Conditions. 
J. NJSTART Marketplace Catalog Enablement - Contractor shall cooperate with State and/or Periscope as requested to upload catalog items and pricing consistent with this Contract. Contractor shall upload catalog within (thirty) 30 calendar days of the date of execution of this Contract. Failure to cooperate will result in the Contractor’s good and/or services not being represented in the NJSTART Marketplace. The Contractor shall ensure that the catalog complies with the scope, and terms and conditions of this Contract. Any identified deviation from the Contract must be corrected immediately. Any catalog that does not comply with the scope and terms and conditions of this Contract can lead to a breach of contract and will be escalated to the Division of Purchase and Property’s Contract Compliance and Audit Unit for review and possible action.  
K. Retention and Inspection of Records and Audit - The Contractor shall keep records of all sales made to all Using Agencies in sufficient detail to enable the State to determine the Procurement Efficiency Program Fee payable by the Contractor. The State and/or Periscope may examine and audit, at its own expense, Contractor’s sales records and Sales Reports for completeness and accuracy. If such examination reveals underpayment of the Procurement Efficiency Program Fee, the Contractor shall immediately pay to Periscope the amount of deficiency. If the examination reveals an underpayment of 5% or more, then the Contractor shall reimburse the State and/or Periscope for the cost of the audit. 
L. Quarterly Sales Reporting - The Contractor shall submit a Sales Report documenting all sales made under the Contract.  The Sales Report shall be submitted directly to Periscope using the NJSTART system no later than thirty (30) calendar days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31. The Sales Report must contain the following information:  
· Complete and accurate details of all sales, credits, returns, refunds, and the like for the reporting quarter;
· Purchasing entity;
· Total of Supplier Convenience Fee amount due for the reporting quarter;
· Such other information as the State may reasonably request; and
· If no sales were made to the State during the reporting quarter, then a report shall be submitted showing zero sales and zero Supplier Convenience Fee due.
Quarterly Sales Reporting and remittance of the Supplier Convenience Fee shall begin on the first calendar quarter starting after the effective date of the Contract.
M. Supplier Convenience Fee - For all purchases made under the Contract, the Contractor shall remit the Supplier Convenience Fee in the amount of one percent (1%) of all Purchases to Periscope Holdings, Inc. (Periscope). 
N. Remittance of the Supplier Convenience Fee - On a quarterly basis, the Contractor shall remit the Supplier Convenience Fee directly to Periscope no later than thirty (30) days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31.  Failure to remit the Supplier Convenience Fee timely and accurately may result in Contractor’s goods and/or services being made ineligible for purchase through the NJSTART Marketplace.
O. Retention and Inspection of Records and Audit - The Contractor shall keep records of all sales made to Using Agencies and Intrastate Cooperative Purchasing Participants in sufficient detail to enable the State to determine the Supplier Convenience Fee payable by the Contractor. The State and/or Periscope may examine and audit, at its own expense, Contractor’s sales records and Sales Reports for completeness and accuracy. If such examination reveals underpayment of the Supplier Convenience Fee, the Contractor shall immediately pay to Periscope the amount of deficiency. If the examination reveals an underpayment of 5% or more, then the Contractor shall reimburse the State and/or Periscope for the cost of the audit.
P. Catalog Enablement - The Contractor shall cooperate with the State and/or Periscope as requested to upload catalog items and pricing consistent with the awarded Contract to the NJSTART Marketplace module within thirty days (30) of the Contract award.



[bookmark: _Toc161300854]DATA SECURITY REQUIREMENTS – CONTRACTOR RESPONSIBILITY 
Not applicable to this procurement.

[bookmark: _4.4.1.1_Ownership_Disclosure][bookmark: _4.4.1.1_Signatory_page][bookmark: _4.4.2.3_Contract_Schedule][bookmark: _4.4.2.4_mobilization_and][bookmark: _Toc161300855]MODIFICATIONS TO THE STATE OF NEW JERSEY STANDARD TERMS AND CONDITIONS
Not applicable to this procurement.

[bookmark: _Toc161300856]QUOTE EVALUATION AND AWARD

[bookmark: _Toc400531542][bookmark: _Toc428534014][bookmark: _Toc32310736][bookmark: _Toc161300857]RIGHT TO WAIVE
Pursuant to N.J.A.C. 17:12-2.7(d) the Director may waive minor irregularities or omissions in a Quote.  The Director reserves the right to waive a requirement provided that the requirement does not materially affect the procurement or the State's interests associated with the procurement.
[bookmark: _Toc400531543][bookmark: _Toc428534015][bookmark: _Toc32310737]
[bookmark: _Toc161300858]DIRECTOR’S RIGHT TO ACCEPT OR REJECT A QUOTE
The Director reserves the right to reject any or all Quotes, or to award in whole or in part if deemed to be in the best interest of the State to do so. The Director shall have authority to award Contracts in accordance with N.J.S.A. 52:34-12. 

[bookmark: _Toc161300859]RECIPROCITY FOR JURISDICTIONAL BIDDER PREFERENCE
In accordance with N.J.S.A. 52:32-1.4 and N.J.A.C. 17:12-2.13, the State of New Jersey will invoke reciprocal action against an out-of-State Bidder whose state or locality maintains a preference practice for its in-state Bidders.  The State of New Jersey will use the annual surveys compiled by the Council of State Governments, National Association of State Procurement Officials, or the National Institute of Governmental Purchasing or a State’s statutes and regulations to identify States having preference laws, regulations, or practices and to invoke reciprocal actions. The State of New Jersey may obtain additional information as it deems appropriate to supplement the stated survey information.

A Bidder may submit information related to preference practices enacted for a State or Local entity outside the State of New Jersey. This information may be submitted in writing as part of the Quote response, including name of the locality having the preference practice, as well as identification of the county and state, and should include a copy of the appropriate documentation, i.e., resolution, regulation, law, notice to Bidder, etc.  It is the responsibility of the Bidder to provide documentation with the Quote or submit it to the Director within five (5) business days after the deadline for Quote submission.  Written evidence for a specific procurement that is not provided to the Director within five (5) business days of the public Quote submission date may not be considered in the evaluation of that procurement, but may be retained and considered in the evaluation of subsequent procurements.

[bookmark: _Toc400531545][bookmark: _Toc428534017][bookmark: _Toc32310739][bookmark: _Toc161300860]CLARIFICATION OF QUOTE
After the Quote Opening Date, unless requested by the State as noted below, Bidder contact with the Procurement Bureau regarding this Bid Solicitation and the submitted Quote is not permitted. 

After the Quotes are reviewed, one (1), some or all of the Bidders may be asked to clarify certain aspects of its Quote.  A request for clarification may be made in order to resolve minor ambiguities, irregularities, informalities or clerical errors.  Clarifications cannot correct any deficiencies, material omissions, or used to revise or modify a Quote.

The Director reserves the right to request that a Bidder to explain, in detail, how the Quote price was determined.

[bookmark: _Toc32310741][bookmark: _Toc161300861][bookmark: _Toc118513837][bookmark: _Toc400531547][bookmark: _Toc428534019]ORAL PRESENTATION 
Not applicable to this procurement.

[bookmark: _Toc161300862]TIE QUOTES
Tie Quotes will be awarded by the Director in accordance with N.J.A.C. 17:12-2.10. 

For the purposes of tie-breaking, any tie-break scenario shall be made utilizing the delivery schedule bid, followed by the criteria set forth in N.J.A.C. 17:12-2.10.  The delivery timeframe will be utilized in any tie-break scenario, and, in the case of a range of delivery days for the product bid, the highest day in the range will be used for the purposes of the tie-break.  For example, if a Bidder offers 10 - 20 days ARO for the product bid, the 20 days will be used for the basis of the tie-break. 

[bookmark: _Toc161300863]STATE'S RIGHT TO INSPECT BIDDER’S FACILITIES
The State reserves the right to inspect the Bidder’s establishment before making an award, for the purposes of ascertaining whether the Bidder has the necessary facilities for performing the Contract.

[bookmark: _Toc161300864]STATE'S RIGHT TO CHECK REFERENCES
The State may also consult with clients of the Bidder during the evaluation of Quotes. Such consultation is intended to assist the State in making a Contract award that is most advantageous to the State.

[bookmark: _Toc161300865]EVALUATION CRITERIA
The following evaluation criteria categories, not necessarily listed in order of significance, will be used to evaluate Quotes received in response to this Bid Solicitation.  The evaluation criteria categories may be used to develop more detailed evaluation criteria to be used in the evaluation process.

[bookmark: _Toc118513839][bookmark: _Toc400531549][bookmark: _Toc428534021][bookmark: _Toc32310743][bookmark: _Toc161300866]TECHNICAL EVALUATION CRITERIA
The following criteria will be used to evaluate Quotes received in response to this Bid Solicitation:  
A. The Bidder’s demonstration in the Quote that the Bidder understands and is able to complete the requirements of the Scope of Work as sought.

[bookmark: _Toc118513840][bookmark: _Toc400531550][bookmark: _Toc428534022][bookmark: _Toc32310744][bookmark: _Toc161300867]PRICE EVALUATION

Group Price Index:

Formula Components:
B1	19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD
B1A	Discount % - Vehicle Manufacturer’s Published Options 
B2	Hook Lift System
B3	Stainless Steel Dump Body with Tilt/Dump Interlock
B4	Stake Body
B5	Landscape Box Body
B6	Chipper Body
B7	Enclosed Steel Storage Body
B8	Platform Body with 300 -Gallon, Gasoline Powered Herbicide Sprayer 
B9	Platform Body with Toolboxes
B10	Dump Body with Multi-Function Tailgate 
B11	Salt Spreader
B12	Snow Plow
B13	In-Cab Controller for Herbicide Sprayer
B14	In-Cab Controller for Salt Spreader
B15	One Set of Parts, Service and Operation and Maintenance Manuals
B16	Technical Support 
Formula:
=B1*((1+U*(1-B1A/100)))+B2+(Average B3:10)+B11+B12+B13+B14+B15+B16
Example:
Chassis Price = $100,000, Discount 10%
Options Utilization Rate = 5%
Hook Lift System = $1500
Stainless Steel Dump BodY with Tilt/Dump Interlock = $15,000
Stake Body = $16,000
Landscape Box Body = $17,000
Chipper Body = $18,000
Enclosed Steel Storage Body = $19,000
Platform Body with 300 -Gallon, Gasoline Powered Herbicide Sprayer = $20,000
Platform Body with Toolboxes = $21,000
Dump Body with Multi-Function Tailgate = $22,000 
Salt Spreader = $250
Snow Plow = $250
In-Cab Controller for Herbicide Sprayer = $100
In-Cab Controller for Salt Spreader = $100
One Set of Parts, Service and Operation and Maintenance Manuals = $300
Technical Support = $95
Formula Explanation:
Chassis Total Price = $100,000 (B1) plus $4500 in options (5% * $100,000 = $5000, discounted 10%, = $4500) = $104,500
Average Price of various body types (B3-B10): $18,500 = $123,000
Combined Value of Hook Lift, Salt Spreader, Snow Plow, In Cab Controllers (2), Manuals, 1 Hour of Tech Support = $2,595
Grand Total = $125,695
The figures utilized above are only listed as an example to calculate how the group price index final cost is achieved and are not meant to be utilized as a benchmark for the actual Unit Prices or Options discount offered by the Bidder in its Quote.

In the event that no Quote offers a reasonable discount for the vehicle manufacturer's published options, the Director may determine to award the cab and chassis only (Price Line 1), if deemed in the best interest of the State.  In such a case, the manufacturer's options price line (Price Line 1A) shall be removed from the Quote evaluation criteria and award shall be made based upon, among other Quote evaluation criteria, a total price bid for the group (sum of the total prices on Price Lines 1 through 16). 

The State intends to utilize an independent, third party database for the publication of vehicle manufacturers options and prices.  
If a Bidder does not bid on all price lines, Price Lines 1 through 16, its Quote shall be considered non-responsive.

If a product bid on a price line within the group is deemed non-responsive, the entire group will be deemed non-responsive, as these price lines were grouped to create a single award, with the intent that all price lines in the group will be awarded.  

Price line items are grouped for Quote evaluation purposes only.  Upon Contract award, Using Agencies will be able to order any price lines within the group individually.

[bookmark: _Toc118513841][bookmark: _Toc400531551][bookmark: _Toc428534023][bookmark: _Toc32310745][bookmark: _Toc161300868]QUOTE DISCREPANCIES
In evaluating Quotes, discrepancies between words and figures will be resolved in favor of words.  Discrepancies between Unit Prices and totals of Unit Prices will be resolved in favor of Unit Prices.  Discrepancies in the multiplication of units of work and Unit Prices will be resolved in favor of the Unit Prices.  Discrepancies between the indicated total of multiplied Unit Prices and units of work and the actual total will be resolved in favor of the actual total.  Discrepancies between the indicated sum of any column of figures and the correct sum thereof will be resolved in favor of the correct sum of the column of figures.

[bookmark: _Toc118513842][bookmark: _Toc400531553][bookmark: _Toc428534025][bookmark: _Toc32310747][bookmark: _Toc161300869]NEGOTIATION
Not applicable to this procurement.

[bookmark: _Toc161300870]BEST AND FINAL OFFER (BAFO) 
The Procurement Bureau may invite one (1) Bidder or multiple Bidders to submit a Best and Final Offer (BAFO). Said invitation will establish the time and place for submission of the BAFO. Any BAFO that does not result in more advantageous pricing to the State will not be considered, and the State will evaluate the Bidder’s most advantageous previously submitted pricing.

The Division may conduct more than one (1) round of BAFO in order to attain the best value for the State. 

BAFOs will be conducted only in those circumstances where it is deemed by the Procurement Bureau or Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Bidder is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Contract award based on the content of the initial submission 

If the Procurement Bureau contemplates BAFOs, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Bidder will be publicly announced at the Quote opening.

[bookmark: _Toc32310748][bookmark: _Toc161300871]“REQUEST FOR REVISION” WITHIN NJSTART
The State may request a revision of the Bidder’s Quote within NJSTART. The Bidder shall respond to the “Request for Revision” only for the reason(s) identified by the State. Any changes made by a Bidder to the Quote other than as requested by the State shall be considered null and void. 

[bookmark: _Toc400531554][bookmark: _Toc428534026][bookmark: _Toc32310749][bookmark: _Toc161300872]POOR PERFORMANCE
A Bidder with a history of performance problems may be bypassed for consideration of an award issued as a result of this Bid Solicitation. The following materials may be reviewed to determine Bidder performance:  
A. Contract cancellations for cause pursuant to State of New Jersey Standard Terms and Conditions Section 5.7(B); 
B. Information contained in Contractor performance records; 
C. Information obtained from audits or investigations conducted by a local, state or federal agency of the Bidder’s work experience; 
D. Current licensure, registration, and/or certification status and relevant history thereof; or 
E. Bidder’s status or rating with established business/financial reporting services, as applicable.  

Bidders should note that this list is not exhaustive.

[bookmark: _Toc161300873]RECOMMENDATION FOR AWARD 
After the evaluation of the submitted Quotes is complete, the Procurement Bureau will recommend to the Director for award, the responsible Bidder(s) whose Quote, conforming to this Bid Solicitation, is most advantageous to the State, price and other factors considered.  The Director may accept, reject or modify the recommendation of the Procurement Bureau.

[bookmark: _Toc400531561][bookmark: _Toc428534033][bookmark: _Toc32310756][bookmark: _Toc161300874]CONTRACT AWARD
A Contract award will be made with reasonable promptness by written notice to that responsible Bidder, whose Quote, conforming to this Bid Solicitation, is most advantageous to the State, price, and other factors considered.  Any or all Quotes may be rejected when the State Treasurer or the Director determines that it is in the public interest to do so.  Contract awards will be publicly posted under the relevant contract number and available on NJSTART.

The State intends to make one (1) Statewide Contract award.
As stated in Bid Solicitation Section 8.9.2, the State intends to utilize an independent, third party database for the publication of vehicle manufacturers options and prices.  Upon Contract award, the vehicle manufacturers options price list will be uploaded to NJSTART under the Contract for the Ordering Agencies to utilize when creating a purchase order that includes vehicle manufacturers options.

[bookmark: _Toc161300875]GLOSSARY

[bookmark: _Toc161300876]CROSSWALK

	Current DPP Template Term
	Equivalent Statutory, Regulatory NJSTART and/or Legacy Term

	Bid Solicitation 
	Request For Proposal (RFP)/Solicitation

	Bid Amendment 
	Addendum

	Contract 
	Master Blanket Purchase Order (Blanket/Blanket P.O.)

	Contract Amendment 
	Change Order

	Administrative Change Order
	Change Order

	Quote
	Proposal/Bid

	Contractor
	Vendor/Contractor

	Bidder
	Bidder/Contractor



[bookmark: _Toc161300877]DEFINITIONS
Unless otherwise specified in the Bid Solicitation, the following definitions will be part of any Contract awarded, or order placed, as a result of this Bid Solicitation.  Note that not all definitions included here apply to all Bid Solicitations.
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Acceptance – The written confirmation by the Using Agency that Contractor has completed a Deliverable according to the specified requirements.

Administrative Change Order – A unilateral administrative modification to the Contract in the NJSTART system by the Division. Administrative Change Orders are not to be considered formal Contract Amendments.
All-Inclusive Hourly Rate – An hourly rate comprised of all direct and indirect costs including, but not limited to: labor costs, overhead, fee or profit, clerical support, travel expenses, per diem, safety equipment, materials, supplies, managerial support and all documents, forms, and reproductions thereof.  This rate also includes portal-to-portal expenses as well as per diem expenses such as food.

Apparel – means any clothing, headwear, linens or fabric.  

Apparel Contracts – include all purchases, rentals or other acquisition of apparel products by the State of New Jersey, including authorizations by the State of New Jersey for contractors to sell apparel products through cash allowances or vouchers issued by the State of New Jersey, and license agreements with a public body.

Apparel Production – includes the cutting and manufacturing of apparel products performed by the contractor or by any subcontractors, but not including the production of supplies or sundries such as buttons, zippers, and thread.

Approved Products – Those products that have been identified in Bid Solicitation as meeting Using Agency needs and confirmed as meeting product specifications.

Best and Final Offer or BAFO – Pricing timely submitted by a Bidder upon invitation by the Procurement Bureau after Quote opening, with or without prior discussion or negotiation.

Bid or Bid Solicitation – The documents which establish the bidding and Contract requirements and solicits Quotes to meet the needs of the Using Agencies as identified herein, and includes the Bid Solicitation, State of New Jersey Standard Terms and Conditions (SSTC), State-Supplied Price Sheet, Attachments, and Bid Amendments.

Bid Amendment – Written clarification or revision to this Bid Solicitation issued by the Division. Bid Amendments, if any, will be issued prior to Quote opening.

Bid Opening Date – The date Quotes will be opened for evaluation and closed to further Quote submissions.

Bid Security - means a guarantee, in a form acceptable to the Division, that the bidder, if selected, will accept the contract as bid; otherwise, the bidder or, as applicable, its guarantor will be liable for the amount of the loss suffered by the State, which loss may be partially or completely recovered by the State in exercising its rights against the instrument of bid security.

Bidder – An entity offering a Quote in response to the Division’s Bid Solicitation.

Breach of Security – as defined by N.J.S.A. 56:8-161, means unauthorized access to electronic files, media, or data containing Personal Data that compromises the security, confidentiality, or integrity of Personal Data when access to the Personal Data has not been secured by encryption or by any other method or technology that renders the Personal Data unreadable or unusable.  Good faith acquisition of Personal Data by an employee or agent of the Provider for a legitimate business purpose is not a Breach of Security, provided that the Personal Data is not used for a purposes unrelated to the business or subject to further unauthorized disclosure.  

Business Day – Any weekday, excluding Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Calendar Day – Any day, including Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Commercial off the Shelf Software or COTS – Software provided by Provider that is commercially available and that can be used with little or no modification.

Customized Software – COTS that is adapted or configured by Provider to meet specific requirements of the Authorized Purchaser that differ from the standard requirements of the base product. For the avoidance of doubt, “Customized Software” is not permitted to be sold to the State under the scope of this Contract.

Contract – The Contract consists of the State of NJ Standard Terms and Conditions (SSTC), the Bid Solicitation, the responsive Quote submitted by a responsible Bidder as accepted by the State, the notice of award, any Best and Final Offer, any subsequent written document memorializing the agreement, any modifications to any of these documents approved by the State and any attachments, Bid Amendment or other supporting documents, or post-award documents including Contract Amendments agreed to by the State and the Contractor, in writing.

Contract Amendment – An amendment, alteration, or modification of the terms of a Contract between the State and the Contractor(s). A Contract Amendment is not effective until it is signed and approved in writing by the person with the appropriate signing authority.  Contract Amendments are tracked using Change Orders in NJSTART. Please note that Administrative Change Orders (see definition above) are not considered Contract Amendments.  

Contractor – The Bidder awarded a Contract resulting from this Bid Solicitation.

Contractor Intellectual Property – Any intellectual property that is owned by Contractor and contained in or necessary for the use of the Deliverables or which the Contractor makes available for the State to use as part of the work under the Contract.  Contractor Intellectual Property includes COTS or Customized Software owned by Contractor, Contractor’s technical documentation, and derivative works and compilations of any Contractor Intellectual Property.

Cooperative Purchasing Program – The Division’s intrastate program that provides procurement-related assistance to New Jersey local governmental entities and boards of education, State and county colleges and other public entities having statutory authority to utilize select State Contract s issued by the Division, pursuant to the provisions of N.J.S.A. 52:25-16.1 et seq.
Cooperative Purchasing Participants – These participants include quasi-State entities, counties, municipalities, school districts, volunteer fire departments, first aid squads, independent institutions of higher learning, County colleges, and State colleges.

Days After Receipt of Order (ARO) – The number of calendar days ‘After Receipt of Order’ in which the Using Agency will receive the ordered materials and/or services.

Dealer/Distributor – A Company authorized by a Bidder or Contractor as having the contractual ability to accept and fulfill orders and receive payments directly on behalf of the Contractor that is awarded a Contract.  Any authorized Dealer/Distributor must agree to all terms and conditions contained within the Bid Solicitation and must agree to provide all products and services in accordance with the Contract specifications, terms, conditions and pricing.  

Deliverable – Goods, products, Services and Work Product that Contractor is required to deliver to the State under the Contract.

Director – Director, Division of Purchase and Property, Department of the Treasury, who by statutory authority is the Chief Contracting Officer for the State of New Jersey; or the Director’s designee.

Disabled Veterans’ Business - means a business which has its principal place of business in the State, is independently owned and operated and at least 51% of which is owned and controlled by persons who are disabled veterans or a business which has its principal place of business in this State and has been officially verified by the United States Department of Veterans Affairs as a service disabled veteran-owned business for the purposes of department contracts pursuant to federal law.  N.J.S.A. 52:32-31.2.

Disabled Veterans’ Business Set-Aside Contract – means a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from disabled veterans’ businesses, or a portion of a Contract when that portion has been so designated.  N.J.S.A. 52:32-31.2.

Discount – The standard price reduction applied by the Bidder to all items.

Division – The Division of Purchase and Property.

Equivalent Products – Products offered other than those identified as an Approved Product in this Bid Solicitation that meet the specifications herein. Equivalent Products will be evaluated to ensure that they meet all technical, nutritional, and packaging specifications herein as part of the Quote evaluation process.

Evaluation Committee – A group of individuals or a Division staff member assigned by the Director to review and evaluate Quotes submitted in response to this Bid Solicitation and recommend a Contract award to the Director.

Firm Fixed Price – A price that is all-inclusive of direct cost and indirect costs, including, but not limited to, direct labor costs, overhead, fee or profit, clerical support, equipment, materials, supplies, managerial (administrative) support, all documents, reports, forms, travel, reproduction and any other costs.

Hardware – Includes computer equipment and any Software provided with the Hardware that is necessary for the Hardware to operate.

Internet of Things (IoT) – the network of physical devices, vehicles, home appliances and other items embedded with electronics, software, sensors, actuators, and network connectivity which enables these objects to connect and exchange data.

Intrastate cooperative purchasing participants – refers to political subdivisions, volunteer fire departments and first aid squads, and independent institutions of higher education and school districts pursuant to N.J.S.A. 52:25-16.1 et seq., State and county colleges pursuant to N.J.S.A. 18A:64-60 and 18A:64A-25.9, quasi-State agencies and independent authorities pursuant to N.J.S.A. 52:27B-56.1, and other New Jersey public entities having statutory authority to utilize select State contracts issued by the Division.

Joint Venture – A business undertaking by two (2) or more entities to share risk and responsibility for a specific project.

Life cycle assessment – The comprehensive examination of a product’s environmental and economic aspects and potential impacts throughout its lifetime, including raw material extraction, transportation, manufacturing, use and disposal.

Life cycle cost – The amortized total cost of a product, including capital costs, installation costs, operating costs, maintenance costs, and disposal costs discounted over the lifetime of the product.

Master Blanket Purchase Order (Blanket/Blanket P.O.) – A Term Contract that allows repeated purchases from an awarded contract.

Materials in Solid Waste – Material found in the various components of the solid waste stream. General, solid waste has several components, such as municipal solid waste (MSW), construction and demolition debris (C&D), and nonhazardous industrial waste.  Under RCRA Section 6002, EPA considers materials recovered from any component of the solid waste stream when designating items containing Recovered Materials.

May – Denotes that which is permissible or recommended, not mandatory.

Mobile Device – means any device used by Provider that can move or transmit data, including but not limited to laptops, hard drives, and flash drives.

Must – Denotes that which is a mandatory requirement.  

Net Purchases – means the total gross purchases, less credits, taxes, regulatory fees and separately stated shipping charges not included in unit prices, made by Intrastate Cooperative Purchasing Participants, regardless of whether or not NJSTART is used as part of the purchase process.

No Bid – The Bidder is not submitting a price Quote for an item on a price line.

No Charge – The Bidder will supply an item on a price line free of charge.

Non-Public Data – means data, other than Personal Data, that is not subject to distribution to the public as public information. Non-Public Data is data that is identified by the State as non-public information or otherwise deemed to be sensitive and confidential by the State because it contains information that is exempt by statute, ordinance or administrative rule from access by the general public as public information.

Percentage Discount or Markup – The percentage bid applied as a Markup or a Discount to a firm, fixed price contained within a price list/catalog. 

Performance Security – means a guarantee, executed subsequent to award, in a form acceptable to the Division, that the successful bidder will complete the contract as agreed and that the State will be protected from loss in the event the contractor fails to complete the contract as agreed.

Personal Data means – 
“Personal Information” as defined in N.J.S.A. 56:8-161, means an individual’s first name or first initial and last name linked with any one or more of the following data elements: (1) Social Security number, (2) driver’s license number or State identification card number or (3) account number or credit or debit card number, in combination with any required security code, access code, or password that would permit access to an individual’s financial account.  Dissociated data that, if linked would constitute Personal Information is Personal Information if the means to link the dissociated were accessed in connection with access to the dissociated data.  Personal Information shall not include publicly available information that is lawfully made available to the general public from federal, state or local government records, or widely distributed media; and/or 

Data, either alone or in combination with other data, that includes information relating to an individual that identifies the person or entity by name, identifying number, mark or description that can be readily associated with a particular individual and which is not a public record, including but not limited to, Personally Identifiable Information (PII); government-issued identification numbers (e.g., Social Security, driver’s license, passport); Protected Health Information (PHI) as that term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and defined below; and Education Records, as that term is defined in the Family Educational Rights and Privacy Act (FERPA), 20 U.S.C. § 1232g.

Personally Identifiable Information or PII - as defined by the U.S. Department of Commerce, National Institute of Standards and Technology, means any information about an individual maintained by an agency, including (1) any information that can be used to distinguish or trace an individual’s identity, such as name, social security number, date and place of birth, mother’s maiden name, or biometric records; and (2) any other information that is linked or linkable to an individual, such as medical, educational, financial, and employment information.

Post-Consumer Material – Material or finished product that has served its intended use and has been diverted or recovered from waste destined for disposal, having completed its life as a consumer item.  Post-Consumer Materials are part of the broader category of Recovered Materials.

Pre-Consumer Material – Materials generated in manufacturing and converting processes, such as manufacturing scrap and trimmings/cuttings.

Price List/Catalog – A document published by a manufacturer, resellers, Dealers, or Distributors that typically contains product descriptions, a list of products with fixed prices to which a Bidder’s percentage discount or markup bid is applied. 

Procurement Bureau (Bureau) – The Division unit responsible for the preparation, advertisement, and issuance of Bid Solicitations, for the tabulation of Quotes and for recommending award(s) of Contract(s) to the Director and the Deputy Director.

Project – The undertakings or services that are the subject of this Bid Solicitation.

Protected Health Information or PHI – has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 means Individually Identifiable Health Information (as defined below) transmitted by electronic media, maintained in electronic media, or transmitted or maintained in any other form or medium. PHI excludes education records covered by the Family Educational Rights and Privacy Act (FERPA), as amended, 20 U.S.C. 1232g, records described at 20 U.S.C. 1232g(a)(4)(B)(iv) and employment records held by a covered entity in its role as employer. The term “Individually Identifiable Health Information” has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and means information that is a subset of Protected Health Information, including demographic information collected from an individual, and (1) is created or received by a health care provider, health plan, employer or health care clearinghouse; and (2) relates to the past, present or future physical or mental health or condition of an individual; the provision of health care to an individual; or the past, present or future payment for the provision of health care to an individual; and (a) that identifies the individual; or (b) with respect to which there is a reasonable basis to believe the information can be used to identify the individual.

Purchases - means the total gross purchases, less credits, taxes, regulatory fees and separately stated shipping charges not included in unit prices, made regardless of whether or not NJSTART is used as part of the purchase process.

Quasi-State Agency – is any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member, as defined in N.J.S.A. 52:27B-56.1, provided that any sale to any such bi-state governmental entity is for use solely within the State of New Jersey.

Quick Reference Guides (QRGs) – Informational documents which provide Vendors with step-by-step instructions to navigate the NJSTART eProcurement System. QRGs are available on the NJSTART Vendor Support Page.

Quote – Bidder’s timely response to the Bid Solicitation including, but not limited to, technical Quote, price Quote including Best and Final Offer, any licenses, forms, certifications, clarifications, negotiated documents, and/or other documentation required by the Bid Solicitation.

Quote Opening Date – The date Quotes will be opened for evaluation and closed to further Quote submissions.

Recovered Material – Waste material and byproduct that have been recovered or diverted from solid waste, but does not include materials and byproducts generated from, and commonly reused within, an original manufacturing process.

Recycling – The series of activities, including collection, separation, and processing, by which products or other materials are recovered from the solid waste stream for use in the form of raw materials in the manufacture of new products other than fuel for producing heat or power by combustion.
Recyclability – The ability of a product or material to be recovered from, or otherwise diverted from, the solid waste stream for the purpose of recycling.

Retainage – The amount withheld from the Contractor payment that is retained and subsequently released upon satisfactory completion of performance milestones by the Contractor.

Revision – A response to a BAFO request or a requested clarification of the Bidder’s Quote. 

RMAN – Recovered Materials Advisory Notices provide purchasing guidance and recommendations for Recovered and Post-Consumer Material content levels for designated items. 

Security Incident – means the potential access by non-authorized person(s) to Personal Data or Non-Public Data that the Provider believes could reasonably result in the use, disclosure, or access or theft of State’s unencrypted Personal Data or Non-Public Data within the possession or control of the Provider. A Security Incident may or may not turn into a Breach of Security.

Services – Includes, without limitation (i) Information Technology (IT) professional services, (ii) Software and Hardware-related services, including without limitation, installation, configuration, and training, and (iii) Software and Hardware maintenance and support and/or Software and Hardware technical support services. 

Shall – Denotes that which is a mandatory requirement.  

Should – Denotes that which is permissible or recommended, not mandatory.

Small Business – Pursuant to N.J.S.A. 52:32-19, N.J.A.C. 17:13-1.2, and N.J.A.C. 17:13-2.1, “small business” means a business that meets the requirements and definitions of “small business” and has applied for and been approved by the New Jersey Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit as (i) independently owned and operated, (ii) incorporated or registered in and has its principal place of business in the State of New Jersey; (iii)  has 100 or fewer full-time employees; and has gross revenues falling in one (1) of the six (6) following categories:  
For goods and services - (A) 0 to $500,000 (Category I); (B) $500,001 to $5,000,000 (Category II); and (C) $5,000,001 to $12,000,000, or the applicable federal revenue standards established at 13 CFR 121.201, whichever is higher (Category III). 
For construction services: (A) 0 to $3,000,000 (Category IV); (B) gross revenues that do not exceed 50 percent of the applicable annual revenue standards established at 13 CFR 121.201 (Category V); and (C) gross revenues that do not exceed the applicable annual revenue standards established at CFR 121.201, (Category VI).

Small Business Set-Aside Contract – means (1) a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from small businesses, or (2) a portion of a Contract when that portion has been so designated.”  N.J.S.A. 52:32-19.

Software – means, without limitation, computer programs, source codes, routines, or subroutines supplied by Provider, including operating software, programming aids, application programs, application programming interfaces and software products, and includes COTS, unless the context indicates otherwise.  

Software as a Service or SaaS – means the capability provided to a purchaser to use the Provider’s applications running on a cloud infrastructure. The applications are accessible from various client devices through a thin client interface such as a Web browser (e.g., Web-based email) or a program interface. The purchaser does not manage or control the underlying cloud infrastructure, including network, servers, operating systems, storage or even individual application capabilities, with the possible exception of limited user-specific application configuration settings.

State – The State of New Jersey.

State Confidential Information – shall consist of State Data and State Intellectual Property  supplied by the State, any information or data gathered by the Contractor in fulfillment of the Contract and any analysis thereof (whether in fulfillment of the Contract or not).

State Contract Manager or SCM – The individual, responsible for the approval of all deliverables, i.e., tasks, sub-tasks or other work elements in the Scope of Work.  The SCM cannot direct or approve a Contract Amendment.

State Data – means all data and metadata created or in any way originating with the State, and all data that is the output of computer processing of or other electronic manipulation of any data that was created by or in any way originated with the State, whether such data or output is stored on the State’s hardware, the Provider’s hardware or exists in any system owned, maintained or otherwise controlled by the State or by the Provider.  State Data includes Personal Data and Non-Public Data.

State Intellectual Property – Any intellectual property that is owned by the State.  State Intellectual Property includes any derivative works and compilations of any State Intellectual Property.

State Price Sheet or State-Supplied Price Sheet – the bidding document created by the State and attached to this Bid Solicitation on which the Bidder submits its Quote pricing as is referenced and described in the Bid Solicitation.   

Subtasks – Detailed activities that comprise the actual performance of a task.

Subcontractor – An entity having an arrangement with a Contractor, whereby the Contractor uses the products and/or services of that entity to fulfill some of its obligations under its State Contract, while retaining full responsibility for the performance of all  Contractor's obligations under the Contract, including payment to the Subcontractor.  The Subcontractor has no legal relationship with the State, only with the Contractor.

Task – A discrete unit of work to be performed.

Third Party Intellectual Property – Any intellectual property owned by parties other than the State or Contractor and contained in or necessary for the use of the Deliverables.  Third Party Intellectual Property includes COTS owned by Third Parties, and derivative works and compilations of any Third Party Intellectual Property. 

Unit Cost or Unit Price – All-inclusive, firm fixed price charged by the Bidder for a single unit identified on a price line.

US CERT – United States Computer Emergency Readiness Team.

USEPA – United States Environmental Protection Agency.

Using Agency[ies] – A State department or agency, a quasi-State governmental entity, or an Intrastate Cooperative Purchasing participant, authorized to purchase products and/or services under a Contract procured by the Division. 

Vendor – Either the Bidder or the Contractor.

Work Product – Every invention, modification, discovery, design, development, customization, configuration, improvement, process, Software program, work of authorship, documentation, formula, datum, technique, know how, secret, or intellectual property right whatsoever or any interest therein (whether patentable or not patentable or registerable under copyright or similar statutes or subject to analogous protection) that is specifically made, conceived, discovered, or reduced to practice by Contractor or Contractor’s subcontractors or a third party engaged by Contractor or its subcontractor pursuant to the Contract Notwithstanding anything to the contrary in the preceding sentence, Work Product does not include State Intellectual Property, Contractor Intellectual Property or Third Party Intellectual Property. 









[bookmark: _Toc161300878]CONTRACT-SPECIFIC DEFINITIONS
Unless otherwise specified in the Bid Solicitation, the following Contract-specific definitions will be part of any Contract awarded, or order placed, as a result of this Bid Solicitation.  

AF – Rear axle to end of frame.

Aftermarket Component - Any component - utility body, snow plow, crane, liftgate or the like - installed on the vehicle chassis (prime unit) by manufacturer or installer (aftermarket installer) other than the chassis manufacturer (prime unit manufacturer).

ANSI – American National Standards Institute: https://www.ansi.org/#:~:text=American%20National%20Standards%20Institute%20%2D%20ANSI%20Home

A.T.A – American Trucking Association.   Trade association in the trucking industry that develops innovative research-based policies that promote highway safety, security, and environmental sustainability.
ASTM - American Society for Testing Materials.
BBC – Bumper-to-back-of-cab, the distance from the front-most edge of the front bumper to the back of cab.

BL - Body length, overall length minus BBC.

CA - Cab-to-axle, the distance from the back of cab to the centerline of rear axle.

DRW – Dual Rear Wheel.

Dry Weight - Curb weight or tare weight of a vehicle - weight of an empty vehicle, without any payload, driver and passenger, with fluids filled to half capacity.

FMVSS - Federal Motor Vehicle Safety Standards, as established by National Highway Traffic Safety Administration.

GAWR - Gross Axle Weight Rating; the maximum legal weight carrying capacity of axle components, including their own dry weights, as published by the vehicle/chassis manufacturer.  GAWR shall not exceed the capacity of the least rated axle component.

GVWR - Gross Vehicle Weight Rating; the maximum legal weight carrying capacity of a vehicle, including its own weight, as published by the vehicle/chassis manufacturer.  GVWR shall not exceed the sum of front and rear GAWRs.

NEMA – National Electrical Manufacturers Association.  The National Electrical Manufacturers Association (NEMA) is an organization that forms the standards for the manufacturing of medical imaging equipment and electrical equipment. The purpose is to provide the safety, environment, and marketing enhancement of the industry.
NJMVC or NJDMV - New Jersey Motor Vehicle Commission, formerly known as Division of Motor Vehicles.

OEM – Original Equipment Manufacturer.  OEM parts are new parts, which are designed, manufactured and/or approved by the original equipment (prime unit) manufacturer.

Ordering Agency - Any using agency placing a purchase order based upon the Contract resulting from this Bid Solicitation.

OSHA – Occupational Safety and Health Administration - https://www.osha.gov/

Payload - Weight carrying capacity of a vehicle, excluding its dry weight, driver and passenger.  Payload, when added to dry weight and weight of driver, passenger and half fluids, shall not exceed the GVWR.  Payload is limited by the front or rear GAWR.

PTO – Power Take Off.  Power take-off (PTO) is a device that transfers an engine's mechanical power to another piece of equipment.  A PTO allows the hosting energy source to transmit power to additional equipment that does not have its own engine or motor. 

RBM - Resisting bending moment, a measure of chassis frame stiffness.

S.A.E - Society of Automotive Engineers.

SRW – Single Rear Wheel.

UL – Underwriters Laboratories.  Underwriters Laboratories are most widely known for standards in electrical products.

Unit - Vehicle ("truck", "product", "commodity" or "item"), Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Optional Hook Lift System, Various Bodies, Salt Spreader, Snow Plow & Accessories, as specified herein, made available for outright purchase as a new, unused unit under a Contract established as a result of this Bid Solicitation.  

WB - Wheelbase, the distance between the centerlines of front and rear axles. 
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