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	Bid Solicitation #
	22DPP00728

	[bookmark: _GoBack]T2877- Large Platform Truck, 33, 000 L.B. GVWR Heavy Duty Truck Chassis, With Utility Body, Hydraulic Platform and Accessories.



	
	Date
	Time

	Due Date For Electronic Questions
Refer to Bid Solicitation Section 2.1 for more information.
	June 14, 2022
	2:00 PM

	Mandatory/Optional Pre-Quote Submission Conference 
Refer to Bid Solicitation Section 2.5 for more information.
	Not Applicable
	Not Applicable

	Mandatory/Optional Site Visit
Refer to Bid Solicitation Section 2.4 for more information.
	Not Applicable
	Not Applicable

	Quote Opening Date
Refer to Bid Solicitation Section 3 for more information.
	July 20, 2022 July 27, 2022
	2:00 PM



Dates are subject to change.  All times contained in the Bid Solicitation refer to Eastern Time. 
All changes will be reflected in Bid Amendments to the Bid Solicitation posted on www.njstart.gov.

	SET-ASIDES

	     Small Business Set-Aside
For Goods and Services:
☐  I          ☐  II          ☐  III
For Construction:
☐  IV          ☐  V          ☐  VI
	☒  Not Applicable
☐  Entire Contract 
☐  Partial Contract 
☐  Subcontracting Only
☐  Preference

	     Disabled Veteran-Owned Business Set-Aside
	☒  Not Applicable
☐  Entire Contract 
☐  Partial Contract 
☐  Subcontracting Only
☐  Preference



	Bid Solicitation Issued By:
State of New Jersey
Department of the Treasury
Division of Purchase and Property
Trenton, New Jersey 08625‑0230
	On Behalf of:
State of New Jersey
Using Agency/Agencies
Cooperative Purchasing Participants



Date:  July 15, 2022
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[bookmark: _Toc108770310]INTRODUCTION AND SUMMARY OF THE BID SOLICITATION
This Bid Solicitation is issued by the Department of Treasury, Division of Purchase and Property (Division), Procurement Bureau, on behalf of New Jersey Department of Transportation (NJDOT). Quotes submitted in response to this Bid Solicitation shall be through the State of New Jersey’s eProcurement system, NJSTART.  Bidders are advised to thoroughly read all sections of this Bid Solicitation and follow all instructions.  

Bidders are strongly encouraged to visit the NJSTART Vendor Support Page, which contains Quick Reference Guides (QRGs), supporting videos, a glossary of NJSTART terms, and helpdesk contact information.  Bidders should utilize the QRGs before attempting to submit a Quote through NJSTART.   It is the Bidder’s responsibility to ensure that the Quote and attachments have been properly submitted.  Inquiries concerning the use of NJSTART may be directed to njstart@treas.nj.gov. The Division will not respond to substantive questions related to the Bid Solicitation or any other Contract via this email address.

[bookmark: _Toc400531467][bookmark: _Toc428533937][bookmark: _Toc32310614][bookmark: _Toc108770311]PURPOSE AND INTENT
The purpose of this Bid Solicitation is to solicit Quotes for a Large Platform Truck, 33, 000 L.B. GVWR Heavy Duty Truck Chassis, With Utility Body, Hydraulic Platform and Accessories.

It is the intent of the Procurement Bureau to award a Contract(s) to that/those responsible Bidder(s) whose Quote(s), conforming to this Bid Solicitation is/are most advantageous to the State of New Jersey (State), price and other factors considered.  The Procurement Bureau may award any or all price lines.  The State, however, reserves the right to separately procure individual requirements that are the subject of the Contract during the Contract term, when deemed by the Director of the Division (Director) to be in the State’s best interest.

There are 11 price lines, itemized as follows:

	Price Line
	Description

	1
	33,000 LB. GVWR Heavy Duty Truck Chassis, 

	2
	Vehicle Manufacturer’s Options

	3
	Utility Body

	4
	Utility Body Manufacturer’s Options

	5
	Hydraulic Platform Lift

	6
	Hydraulic Platform Lift Manufacturer’s Options

	7
	Hydraulic Generator

	8
	Chassis Mounted Air Compressor

	9
	One Additional Set of Parts, Service And Operation & Maintenance Manuals

	10
	Special Monotone Paint Color In Lieu Of Manufacturer’s Standard Paint Color

	11
	Technical Support



The State intends to make one (1) Statewide Contract award per cab and chassis on which the utility body, hydraulic platform lift, hydraulic generator and air compressor shall be mounted, in accordance with Bid Solicitation Section 8.16. For example:

· One (1) award for a Large Platform Truck mounted on a 2022 Model Year Kenworth T370  Cab and Chassis
· One (1) award for a Large Platform Truck mounted on a 2022 Model Year International MV 43100 Cab and Chassis
· One (1) award for a Large Platform Truck mounted on a 2022 Model Year Freightliner M2-106 Cab and Chassis

Bidders may offer any equivalent makes and models that meet the technical requirements of the Bid Solicitation. Please refer to Bid Solicitation Section 3.19 for submission of Specification Data Sheets.

Bidders must bid on all price lines (one (1) through eleven (11)) in order for its Quote to be considered responsive. If a Bidder does not bid on all price lines within the group, its Quote may be considered non-responsive.

Price line items are grouped for Quote evaluation purposes only.  Upon Contract award, Using Agencies will be able to order any price lines within the group individually.

Bidders offering more than one make/model should submit a separate State-Supplied Price Sheet for each combination offered.  In the alternative, Bidders may add tabs to the bottom of the State-Supplied Price Sheet for additional makes and models bid (by copying the text and information from the original Price Sheet). 

The State makes no representation and provides no guarantee as to the minimum, average or maximum volume of purchases to be made under this Contract. 

This procurement is not a Small Business or Disabled Veteran-Owned Business set aside procurement.

The State of New Jersey Standard Terms and Conditions (SSTCs) included with this Bid Solicitation will apply to all Contracts made with the State.  These terms are in addition to the terms and conditions set forth in this Bid Solicitation and should be read in conjunction with them unless the Bid Solicitation specifically indicates otherwise. 
 
[bookmark: _Toc400531468][bookmark: _Toc428533938][bookmark: _Toc32310615][bookmark: _Toc108770312]BACKGROUND 
This is a reprocurement of the product under T2877 - UTILITY TRUCK, 29,000 LB. GVWR C&C W/11'BODY, 41' W.H. HYD. PLATFORM LIFT & ACC.  Bidders interested in reviewing the current Contract/Master Blanket Purchase Order specifications and pricing information may do so by following the instruction below.  Bidders should not rely upon or use data or information from the Contract when preparing a response to this Bid Solicitation as this Bid Solicitation addresses the State’s current requirements.

· Go to: www.njstart.gov 
· Select “Active Blankets”
· In the search bar, select “Blankets” from the drop down menu
· Enter the T2877 and click “[image: ]”
· The current Contract list will appear under “Results”

[bookmark: _Toc108770313]CONTRACT AMOUNT
The estimated amount of the Contract, if stated, shall not be construed as either the maximum or minimum amount which the State shall be obliged to order.

[bookmark: _Toc400531506][bookmark: _Toc428533977][bookmark: _Toc32310702][bookmark: _Toc108770314]ORDER OF PRECEDENCE OF CONTRACTUAL TERMS
The Contract awarded, and the entire agreement between the parties, as a result of this Bid Solicitation shall consist of:  (1) the final Bid Solicitation, (2) the State of New Jersey Standard Terms and Conditions, (3) the Quote, and if applicable (4) any Bidder responses to clarifications; (5) a Bidder’s Best and Final Offer, (6) other negotiated document, and/or (7) third party document.  In the event of a conflict in the terms and conditions among the documents comprising this Contract, the order of precedence, for purposes of interpretation thereof, listed from highest ranking to lowest ranking as noted above. 

Any other terms or conditions, not included with the Bidder’s Quote and accepted by the State, shall not be incorporated into the Contract awarded.  Any references to external documentation, included those documents referenced by a URL, including without limitation, technical reference manuals, technical support policies, copyright notices, additional license terms, etc., are subject to the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Condition.  In the event of any conflict between the terms of a document incorporated by reference the terms and conditions of the Bid Solicitation and the State of New Jersey Standard Terms and Condition shall prevail.

[bookmark: _Toc108770315]INTRASTATE COOPERATIVE PURCHASING
The State intends to extend the Contracts awarded to the State's Intrastate Cooperative Purchasing Participants.  Although the State is making the use of any Contract resulting from this Bid Solicitation available to Intrastate Cooperative Purchasing Participants, the State makes no representation as to the acceptability of the Bid Solicitation’s terms and conditions to any Intrastate Cooperative Purchasing Participants.

If a Contractor makes any sales to Intrastate Cooperative Purchasing Participants pursuant to the awarded Contract, the Contractor agrees to the remit the Supplier Convenience Fee in the amount of one percent (1%) of all Net Purchases made by Intrastate Cooperative Purchasing Participants to the Division’s eProcurement administrator, Periscope Holdings, Inc. (Periscope).  
A. Supplier Convenience Fee - For all purchases made by Intrastate Cooperative Purchasing Participants under the Contract, the Vendor shall remit the Supplier Convenience Fee in the amount of one percent (1%) of all Net Purchases to Periscope Holdings, Inc. (Periscope). 
B. Remittance of the Supplier Convenience Fee - On a quarterly basis, the Vendor shall remit the Supplier Convenience Fee via Automated Clearing House (ACH) transactions directly to Periscope using the NJSTART Reconciler module. The remittance shall be made no later than thirty (30) calendar days after the end of each calendar quarter.  The calendar quarters will end March 31, June 30, September 30, and December 31.  Failure to remit the Supplier Convenience Fee timely and accurately may result in Vendor’s goods and services being made ineligible for purchase through the NJSTART Marketplace module by Intrastate Cooperative Purchasing Participants.
C. Catalog Enablement - The Vendor shall cooperate with the State and/or Periscope as requested to upload catalog items and pricing consistent with the awarded Contract to the NJSTART Marketplace module. Vendor shall only upload a catalog containing items awarded.
D. Quarterly Sales Reporting - The Vendor shall submit a Sales Report documenting all sales made to Intrastate Cooperative Purchasing Participants. The Sales Report shall be submitted directly to Periscope using the NJSTART Reconciler module no later than thirty (30) calendar days after the end of each calendar quarter. The calendar quarters will end March 31, June 30, September 30, and December 31. The Sales Report must contain the following information:  
· Complete and accurate details of all sales, credits, returns, refunds, and the like for the reporting quarter;
· Purchasing entity;
· Total of Supplier Convenience Fee amount due for the reporting quarter;
· Such other information as the State may reasonably request; and
· If no sales were made to State during the reporting quarter, then a report shall be submitted showing zero sales and zero Supplier Convenience Fee due.
E. Retention and Inspection of Records and Audit - The Vendor shall keep records of sales made to Intrastate Cooperative Purchasing Participants in sufficient detail to enable the State to determine the Supplier Convenience Fee payable by the Vendor. The State and/or Periscope may examine and audit, at its own expense, Vendor’s sales records and Sales Reports for completeness and accuracy. If such examination reveals underpayment of the Supplier Convenience Fee, the Vendor shall immediately pay to Periscope the amount of deficiency. If the examination reveals an underpayment of 5% or more, then the Vendor shall reimburse the State and/or Periscope for the cost of the audit.


[bookmark: _Toc108770316]PRE-QUOTE SUBMISSION INFORMATION
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote and for reviewing the Quote submission requirements and the Scope of Work requirements.  

[bookmark: _Toc428533940][bookmark: _Toc32310617][bookmark: _Toc108770317]ELECTRONIC QUESTION AND ANSWER PERIOD
The Division will electronically accept questions and inquiries from all potential Bidders via the “Q&A” Tab of the Bid Solicitation in NJSTART.  Questions should be directly tied to a Bid Solicitation Section, the Price Sheet, Form or Attachment; and should reference the specific Bid Solicitation Section or document to which it relates.

The cut-off date for electronic questions and inquiries relating to this Bid Solicitation is indicated on the Bid Solicitation cover page.  In the event that questions are posed by Bidders, answers to such questions will be issued by Bid Amendment.  
[bookmark: _1.3.3__Mandatory_Pre-Bid_Conference][bookmark: _1.3.5__SUBMISSION_OF_BID_PROPOSAL][bookmark: _1.3.2_SUBMISSION_OF_BID_PROPOSAL]
A Bidder shall not contact the Using Agency and/or the Procurement Specialist directly, in person, by telephone or by e-mail, concerning this Bid Solicitation, prior to Contract award.

[bookmark: _Toc108770318]EXCEPTIONS TO THE STATE OF NJ STANDARD TERMS AND CONDITIONS (SSTC)
Questions regarding the State of New Jersey Standard Terms and Conditions and exceptions to mandatory requirements MUST be posed during the Electronic Question and Answer period and shall contain the Bidder’s suggested changes and the reason(s) for the suggested change(s).

[bookmark: _Toc108770319]BID AMENDMENTS
In the event that it becomes necessary to clarify or revise this Bid Solicitation, such clarification or revision will be by Bid Amendment.  Any Bid Amendment will become part of this Bid Solicitation and part of any Contract awarded. Bid Amendments will be posted as a file attachment on the “Summary” page of the Bid Solicitation in NJSTART after the cut-off date.  

There are no designated dates for release of Bid Amendments.  Those Bidders who are on the bid holder list either through commodity code registration in NJSTART or by acknowledging the bid in NJSTART should receive notification of any Bid Amendment(s). If a Bidder is not on the bid holder list, Bid Amendments are still viewable on the “Summary” page of the Bid Solicitation in NJSTART.

It is the sole responsibility of the Bidder to be knowledgeable of all Bid Amendments related to this procurement. An interested Bidder should check the NJSTART “Open Bids” Tab on a daily basis to ensure review of the most updated information.

[bookmark: _1.3.4_MANDATORY/OPTIONAL_SITE][bookmark: _1.3.45_MANDATORY/OPTIONAL_SITE][bookmark: _Toc224543885][bookmark: _Toc238623352][bookmark: _Toc400531474][bookmark: _Toc428533944][bookmark: _Toc32310620][bookmark: _Toc108770320]MANDATORY/OPTIONAL SITE VISIT
Not applicable to this procurement.
[bookmark: _1.3.5__MANDATORY/OPTIONAL][bookmark: _1.3.6__MANDATORY/OPTIONAL][bookmark: _Toc224543888][bookmark: _Toc238623354][bookmark: _Toc428533945][bookmark: _Toc32310621][bookmark: _Toc108770321]MANDATORY/OPTIONAL PRE-QUOTE CONFERENCE
Not applicable to this procurement.
[bookmark: _Toc95619434][bookmark: _Toc109701220][bookmark: _Toc225321579][bookmark: _Toc400531476][bookmark: _Toc428533946][bookmark: _Toc32310622][bookmark: _Toc108770322][bookmark: _Toc94946029][bookmark: _Toc72744593]PRE-QUOTE DOCUMENT REVIEW 
Not applicable to this procurement.



[bookmark: _Toc108770323]QUOTE SUBMISSION REQUIREMENTS

[bookmark: _Toc108770324]QUOTE SUBMISSION 
In order to be considered for award, the Quote must be received electronically by the Division’s Proposal Review Unit, through NJSTART, by the required date and time. 

The date and time of the Quote opening are indicated on the Bid Solicitation cover sheet and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  If the Quote opening deadline has been revised, the new Quote opening deadline will be shown on the posted Bid Amendment and on the “Summary” Tab of the Bid Solicitation webpage within NJSTART.  Quotes not received prior to the Quote opening deadline shall be rejected.

Quotes will be publicly opened and announced by telephone conference on the date and time of the quote opening. 
(Dial-in phone number: 888-204-5984 / Access code: 2602305)

When submitting a Quote through NJSTART, do not use any symbols (i.e., #, @, $, &, *) in the filename as this may prevent the Quote from being properly uploaded.  Uploaded files must be compatible with Microsoft Office and/or Adobe software applications. DO NOT UPLOAD files with extensions such as .zip, .numbers, or .pages.

When uploading the documents to NJSTART, the Bidder should select the “Confidential” option in NJSTART for attachments on the “Attachments” Tab to request that the documents not be displayed publicly through NJSTART. Marking an attachment as "Confidential" in NJSTART shall not constitute the Bidder's designation of the attachment as exempt from public disclosure under the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know.

[bookmark: _Toc108770325]BIDDER RESPONSIBILITY
The Bidder assumes sole responsibility for the complete effort required in submitting a Quote in response to this Bid Solicitation.  No special consideration will be given after Quotes are opened because of a Bidder’s failure to be knowledgeable as to all of the requirements of this Bid Solicitation.  The State assumes no responsibility and bears no liability for costs incurred by a Bidder in the preparation and submittal of a Quote in response to this Bid Solicitation or any pre-contract award costs incurred.

[bookmark: _Toc108770326]ANNOUNCEMENT OF QUOTE INFORMATION
On the date and time Quotes are due under the Bid Solicitation, all information concerning the Quotes submitted may be publicly announced and shall be available for inspection and copying except otherwise noted:  
A. Information appropriately designated as proprietary and/or confidential in a Bidder’s Quote shall not be available for inspection and copying; and
B. Where negotiation is contemplated, only the names and addresses of the Bidders submitting Quotes will be announced, and the contents of the Quotes shall not be available for inspection and copying until the Notice of Intent to Award is issued by the Director. 

[bookmark: _Toc108770327]QUOTE ERRORS
In accordance with N.J.A.C. 17:12-2.11 “Proposal errors,” a Bidder may withdraw its Quote as described below.

[bookmark: _Toc108770328]QUOTE WITHDRAWAL PRIOR TO QUOTE OPENING
A Bidder may withdraw its Quote submission in NJSTART prior to the Quote opening; however, Bidders should note that while withdrawn NJSTART Quotes remain viewable by the Bidder on its Vendor Profile Homepage, they are removed from the Division’s view and cannot be considered for Contract award. The Bidder may submit a revised Quote as long as the Quote is received prior to the announced date and time for Quote submission. Bidders may refer to the QRG “Submit a Quote” for additional instructions.

[bookmark: _Toc108770329]QUOTE WITHDRAWAL AFTER QUOTE OPENING, BUT PRIOR TO CONTRACT AWARD
If, after the Quote opening, but before Contract award, a Bidder discovers an error in its Quote, the Bidder may make a written request to the Procurement Bureau to withdraw its Quote, from consideration for award.  If the Bidder’s request to withdraw is made in good faith, and the State will not be significantly prejudiced by granting the withdrawal of the Quote beyond the loss of the benefit of the bargain to the State of the withdrawing Bidder’s offer, the request shall be granted.  Evidence of the Bidder’s good faith in making this request can be demonstrated by one (1) or more of the following factors: A mistake is so significant that to enforce the Contract resulting from the Quote would be unconscionable; that the mistake relates to a material feature or term of the Contract; and that the mistake occurred notwithstanding the Bidder’s exercise of reasonable care.  After Quote opening, while pursuant to the provisions of this section a Bidder may request to withdraw its Quote and the Director may in his/her discretion allow said Bidder to withdraw it, the Division also may take notice of repeated or unusual requests to withdraw by a Bidder and take those prior requests to withdraw into consideration when evaluating the Bidder’s future Quotes.

The Quote withdrawal request must include the Bid Solicitation Number, Bid Solicitation Title, and the Quote submission date and should be sent to Procurement.Bureau@treas.nj.gov.

If, during a Quote evaluation process, an obvious pricing error made by a potential Contract awardee is found, the Director or his/her designee shall issue written notice to the Bidder.  The Bidder will have up to five (5) business days after receipt of the notice to confirm its pricing.  If the Bidder fails to respond, its Quote shall be considered withdrawn, and no further consideration shall be given to it.

[bookmark: _Toc108770330]JOINT VENTURE
If a Joint Venture is submitting a Quote, the agreement between the parties relating to such Joint Venture should be submitted with the Joint Venture’s Quote.  Authorized signatories from each party comprising the Joint Venture must sign the Offer and Acceptance Page.  Each party to the Joint Venture must individually complete and comply with all the forms and certification requirements in Bid Solicitation Section 3 – Quote Submission Requirements. 

[bookmark: _Toc108770331]SMALL BUSINESS SET-ASIDE CONTRACTS
Not applicable to this procurement.

[bookmark: _Toc108770332]DISABLED VETERANS’ BUSINESS SET-ASIDE CONTRACT 
Not applicable to this procurement.

[bookmark: _Toc108770333]BID SECURITY
Not applicable to this procurement.

[bookmark: _Toc108770334]BIDDER ADDITIONAL TERMS SUBMITTED WITH THE QUOTE
A Bidder may submit additional terms as part of its Quote.  Additional terms are Bidder-proposed terms or conditions that do not conflict with the scope of work required in this Bid Solicitation, the terms and conditions of this Bid Solicitation, or the State of New Jersey Standard Terms and Conditions.  Bidder proposed terms or conditions that conflict with those contained the State of New Jersey Standard Terms and Conditions will render a Quote non-responsive.  It is incumbent upon the Bidder to identify and remove its conflicting proposed terms and conditions prior to Quote submission.  

Quotes including Bidder proposed additional terms may be accepted, rejected, or negotiated, in whole or in part, at the State’s sole discretion. 

If Bidder intends to propose terms and conditions that conflict with the State of New Jersey Standard Terms and Conditions, those Bidder proposed terms and conditions shall only be considered if submitted and agreed to pursuant to the electronic question and answer procedure.  Bidders shall not submit exceptions or modifications as part of the Quote or on the “Terms and Conditions” Tab through NJSTART. 

[bookmark: _Toc108770335]QUOTE CONTENT
The Quote should be submitted with the attachments organized in following manner:
· Forms
· Technical Quote
· State-Supplied Price Sheet

A Bidder should not password protect any submitted documents. Use of URLs in a Quote should be kept to a minimum and shall not be used to satisfy any material term of a Bid Solicitation. If a preprinted or other document included as part of the Quote contains a URL, a printed copy of the information should be provided and will be considered as part of the Quote. 

[bookmark: _Toc108770336]FORMS, REGISTRATIONS AND CERTIFICATIONS TO BE SUBMITTED WITH QUOTE 
A Bidder is required to complete and submit the following forms.  As an alternative to uploading forms with the submitted Quote, a Bidder may complete the appropriate certifications in NJSTART on the “Terms and Categories” Tab within the Vendor Profile.  Those forms that may be completed on the NJSTART “Terms and Categories” Tab noted below. Additionally, a Bidder may attach completed forms to the Vendor Profile.  Refer to QRGs “Vendor Forms” and “Attaching Files” for additional instructions.  



OFFER AND ACCEPTANCE PAGE 
The Bidder should complete and submit the Offer and Acceptance Page with the Quote.  The Offer and Acceptance Page must be signed by an authorized representative of the Bidder.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.    

OWNERSHIP DISCLOSURE FORM 
Pursuant to N.J.S.A. 52:25-24.2, in the event the Bidder is a corporation, partnership or limited liability company, the Bidder must disclose all 10% or greater owners by (a) completing and submitting the Ownership Disclosure Form with the Quote; (b) if the Bidder has submitted a signed and accurate Ownership Disclosure Form dated and received no more than six (6) months prior to the Quote submission deadline for this procurement, the Division may rely upon that form; however, if there has been a change in ownership within the last six (6) months, a new Ownership Disclosure Form must be completed, signed and submitted with the Quote; or, (c) a Bidder with any direct or indirect parent entity which is publicly traded may submit the name and address of each publicly traded entity and the name and address of each person that holds a 10 percent or greater beneficial interest in the publicly traded entity as of the last annual filing with the federal Securities and Exchange Commission or the foreign equivalent, and, if there is any person that holds a 10 percent or greater beneficial interest, also shall submit links to the websites containing the last annual filings with the federal Securities and Exchange Commission or the foreign equivalent and the relevant page numbers of the filings that contain the information on each person that holds a 10 percent or greater beneficial interest. N.J.S.A. 52:25-24.2.
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab. 

A Bidder’s failure to submit the information required by N.J.S.A. 52:25-24.2 will result in the rejection of the Quote as non-responsive and preclude the award of a Contract to said Bidder.

  DISCLOSURE OF INVESTMENT ACTIVITIES IN IRAN FORM
The Bidder should  submit Disclosure of Investment Activities in Iran form to certify that, pursuant to N.J.S.A. 52:32-58, neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates (as defined in N.J.S.A. 52:32-56(e)(3)), is listed on the Department of the Treasury’s List of Persons or Entities Engaging in Prohibited Investment Activities in Iran and that neither the Bidder, nor one (1) of its parents, subsidiaries, and/or affiliates, is involved in any of the investment activities set forth in N.J.S.A. 52:32-56(f).  If the Bidder is unable to so certify, the Bidder shall provide a detailed and precise description of such activities as directed on the form.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab. 

DISCLOSURE OF INVESTIGATIONS AND OTHER ACTIONS INVOLVING BIDDER FORM
The Bidder should submit the Disclosure of Investigations and Other Actions Involving Bidder Form,  with its Quote, to provide a detailed description of any investigation, litigation, including administrative complaints or other administrative proceedings, involving any public sector clients during the past five (5) years, including the nature and status of the investigation, and, for any litigation, the caption of the action, a brief description of the action, the date of inception, current status, and, if applicable, disposition.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab. 

MACBRIDE PRINCIPLES FORM
The Bidder should submit the MacBride Principles Form.  Pursuant to N.J.S.A. 52:34-12.2, a Bidder is required to certify  that it either has no ongoing business activities in Northern Ireland and does not maintain a physical presence therein or that it will take lawful steps in good faith to conduct any business operations it has in Northern Ireland in accordance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of their compliance with those principles.  If a Bidder does not submit the form with the Quote, the Bidder must comply within seven (7) business days of the State’s request or the State may deem the Quote non-responsive.
NOTE: Also available on the NJSTART on the “Terms and Categories” Tab.

SERVICE PERFORMANCE WITHIN THE UNITED STATES
Not applicable to this procurement.

CONFIDENTIALITY/COMMITMENT TO DEFEND
Pursuant to the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know, Quotes can be released to the public in accordance with N.J.A.C. 17:12-1.2(b) and (c).  

The Bidder should submit a completed and signed Confidentiality /Commitment to Defend Form with the Quote.  In the event that the Bidder does not submit the Confidentiality form with the Quote, the State reserves the right to request that the Bidder submit the form after Quote submission.

After the opening of sealed Quotes, all information submitted by a Bidder in response to a Bid Solicitation is considered public information notwithstanding any disclaimers to the contrary submitted by a Bidder.  Proprietary, financial, security and confidential information may be exempt from public disclosure by OPRA and/or the common law when the Bidder has a good faith, legal/factual basis for such assertion. 

When the Bid Solicitation contains a negotiation component, the Quote will not be subject to public disclosure until a notice of intent to award a Contract is announced. 

As part of its Quote, a Bidder may request that portions of the Quote be exempt from public disclosure under OPRA and/or the common law. The Bidder must provide a detailed statement clearly identifying those sections of the Quote that it claims are exempt from production, and the legal and factual basis that supports said exemption(s) as a matter of law.  The State will not honor any attempts by a Bidder to designate its price sheet, price list/catalog, and/or the entire Quote as proprietary and/or confidential, and/or to claim copyright protection for its entire Quote.  If the State does not agree with a Bidder’s designation of proprietary and/or confidential information, the State will use commercially reasonable efforts to advise the Bidder. Copyright law does not prohibit access to a record which is otherwise available under OPRA.

The State reserves the right to make the determination as to what to disclose in response to an OPRA request.  Any information that the State determines to be exempt from disclosure under OPRA will be redacted.  

In the event of any challenge to the Bidder’s assertion of confidentiality that is contrary to the State’s determination of confidentiality, the Bidder shall be solely responsible for defending its designation, but in doing so, all costs and expenses associated therewith shall be the responsibility of the Bidder. The State assumes no such responsibility or liability.  

In order not to delay consideration of the Quote or the State’s response to a request for documents, the State requires that Bidder respond to any request regarding confidentiality markings within the timeframe designated in the State’s correspondence regarding confidentiality.  If no response is received by the designated date and time, the State will be permitted to release a copy of the Quote with the State making the determination regarding what may be proprietary or confidential.

SUBCONTRACTOR UTILIZATION PLAN
Bidders intending to use Subcontractor(s) shall list all subcontractors on the Subcontractor Utilization Plan form or may list the Subcontractor(s) on the “Subcontractor” Tab in NJSTART. 

For a Quote that does NOT include the use of any Subcontractors, the Bidder is automatically certifying that, if selected for an award, the Bidder will be performing all work required by the Contract. 

If it becomes necessary for the Contractor to substitute a Subcontractor, add a Subcontractor, or substitute its own staff for a Subcontractor, the Contractor will identify the proposed new Subcontractor or staff member(s) and the work to be performed.  The Contractor shall forward a written request to substitute or add a Subcontractor or to substitute its own staff for a Subcontractor to the State Contract Manager for consideration.    The Contractor must provide a completed Subcontractor Utilization Plan, a detailed justification documenting the necessity for the substitution or addition, and resumes of its proposed replacement staff or of the proposed Subcontractor’s management, supervisory, and other key personnel that demonstrate knowledge, ability and experience relevant to that part of the work which the Subcontractor is to undertake. The qualifications and experience of the replacement(s) must equal or exceed those of similar personnel proposed by the Contractor in its Quote.  The State Contract Manager will forward the request to the Director for approval.  

NOTE: No substituted or additional Subcontractors are authorized to begin work until the Contractor has received written approval from the Director.

SMALL BUSINESS AND/OR DISABLED VETERANS’ BUSINESS SUBCONTRACTING SET-ASIDE CONTRACT 
Not applicable to this procurement.

PAY TO PLAY PROHIBITIONS
Pursuant to N.J.S.A. 19:44A-20.13 et seq. (P.L. 2005, c. 51), the State shall not enter into a Contract to procure services or any material, supplies or equipment, or to acquire, sell, or lease any land or building from any Business Entity, where the value of the transaction exceeds $17,500, if that Business Entity has solicited or made any contribution of money, or pledge of contribution, including in-kind contributions, to a candidate committee and/or election fund of any candidate for or holder of the public office of Governor or Lieutenant Governor, to any State, county, municipal political party committee, or to any legislative leadership committee during certain specified time periods.  

Prior to awarding any Contract or agreement to any Business Entity, the Business Entity proposed as the intended Contractor of the Contract shall submit the Two-Year Chapter 51/Executive Order 117 Vendor Certification and Disclosure of Political Contributions form, certifying that no contributions prohibited by either Chapter 51 or Executive Order No. 117 have been made by the Business Entity and reporting all qualifying contributions made by the Business Entity or any person or entity whose contributions are attributable to the Business Entity.  Failure to submit the required forms will preclude award of a Contract under this Bid Solicitation.

Further, the Contractor is required, on a continuing basis, to report any contributions it makes during the term of the Contract, and any extension(s) thereof, at the time any such contribution is made. 

AFFIRMATIVE ACTION
The intended Contractor and its named Subcontractor(s) must submit a copy of a New Jersey Certificate of Employee Information Report, or a copy of Federal Letter of Approval verifying it is operating under a federally approved or sanctioned Affirmative Action program.  If the Contractor and/or its named Subcontractor(s) are not in possession of either a New Jersey Certificate of Employee Information Report or a Federal Letter of Approval, it/they must complete and submit the Affirmative Action Employee Information Report (AA-302).  Information, instruction and the application are available at https://www.state.nj.us/treasury/contract_compliance/index.shtml.

EXECUTIVE ORDER 271
Not applicable to this procurement.

[bookmark: _Toc108770348]STATE OF NEW JERSEY SECURITY DUE DILIGENCE THIRD-PARTY INFORMATION SECURITY QUESTIONNAIRE 
Not applicable to this procurement.

BUSINESS REGISTRATION
[bookmark: OLE_LINK1]In accordance with N.J.S.A. 52:32-44(b), a Bidder and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Contract.  A Bidder should verify its Business Registration Certification Active status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Bidder’s Business Registration Certification Active status, NJSTART provides a link to take corrective action. 

[bookmark: _Toc108770350]Certification Regarding Prohibited Activities with Russia or Belarus

The Bidder should submit the Disclosure of Prohibited Activities in Russia / Belarus Form.  Pursuant to P.L.2022, c. 3, a person or entity seeking to enter into or renew a contract for the provision of goods or services shall certify that it is not Engaging in Prohibited Activities in Russia or Belarus as defined by P.L.2002, c. 3, sec. 1(e).    If the Contractor is unable to so certify, the Contractor shall provide a detailed and precise description of such activities. 

If you certify that the bidder is engaged in activities prohibited by P.L. 2022, c. 3, the bidder shall have 90 days to cease engaging in any prohibited activities and on or before the 90th day after this certification, shall provide an updated certification.  If the bidder does not provide the updated certification or at that time cannot certify on behalf of the entity that it is not engaged in prohibited activities, the State shall not award the business entity any contracts, renew any contracts, and shall be required to terminate any contract(s) the business entity holds with the State that were issued on or after the effective date of P.L. 2022, c. 3.

[bookmark: _Toc108770351]TECHNICAL QUOTE 
Not applicable to this procurement.

[bookmark: _Toc108770352]BIDDER QUOTE OVERVIEW FORM
Not applicable to this procurement.

[bookmark: _Toc108770353]BIDDER DATA SHEET/FORM
The Bidder should submit the Bidder Data Sheet with its Quote.  The Bidder Data Sheet will be used to evaluate the Bidder’s ability to complete the Scope of Work.  See the “Attachments” tab in NJSTART.

The Bidder should provide in its response to Part I of the Bidder Data Sheet all relevant information regarding its experience in successfully completing contracts of a similar size and scope to the work required by this Bid Solicitation.  

The Bidder must provide, in Part II of the Bidder Data Sheet, details of any negative actions taken by other contracting entities against it in the course of performing these projects including, but not limited to, receipt of letters of potential default, default, cure notices, termination of services for cause, or other similar notifications/processes.  Additionally, the Bidder should provide details, including any negative audits, reports, or findings by any governmental agency for which the Bidder is/was the contractor on any contracts of similar scope.  In the event a Bidder neglects to include this information in its Quote, the Bidder’s omission of necessary disclosure information may be cause for rejection of the Bidder’s Quote by the State.

If proposing to use a Subcontractor, the Bidder should provide as an attachment to the Bidder Data Sheet documented experience to demonstrate that each Subcontractor has successfully performed work on contracts of a similar size and scope to the work that the Subcontractor is designated to perform in the Bidder’s Quote.  The Bidder must provide a detailed description of services to be provided by each Subcontractor.  

AFFIDAVIT OF APPAREL PRODUCTION
Not applicable to this procurement.

[bookmark: _Toc108770355]DISCLOSURE OF PRODUCT COMPOSITION
Not applicable to this procurement.

[bookmark: _SPECIFICATION_DATA_SHEETS][bookmark: _Toc108770356]SPECIFICATION DATA SHEETS
Bidders should submit with its Quote specification data sheets for all Equivalent Products bid. The specification data sheets must document that its product bid meets or exceeds the requirements of the Bid Solicitation specifications.

Bidders offering Approved Products identified in this Bid Solicitation are not required to submit specification data sheets for those Approved Products only.  However, all required information identified on the State-Supplied Price Sheet and outlined in Bid Solicitation Section 4.0 as necessary to confirm specification conformance must be provided.  

In the event that the specification data sheets are not provided with a Bidder’s Quote, the Bidder must provide the specification data sheets within 48 hours following a written request from the State. Failure to comply with the written request within the allotted timeframe will result in a Bidder’s Quote non-responsive for the requested item(s).  

[bookmark: _Toc108770357]SAMPLES AND TESTING
Not applicable to this procurement.

[bookmark: _SPECIFICATION_CONFORMANCE_FORM][bookmark: _Toc108770358]SPECIFICATION CONFORMANCE FORM
The Bidder shall submit with its Quote the Specification Conformance Form.  By submitting this form, the Bidders certifies that all items offered in response to this Bid Solicitation conform to the requirements set forth in the Bid Solicitation. 

[bookmark: _Toc108770359]MANUFACTURER’S CERTIFICATION
The Bidder should submit a letter of certification from the manufacturer whose product is supplied, certifying that the Bidder is authorized by the manufacturer to supply the good(s) and/or services specified.  The certification must indicate that the Bidder was authorized by the manufacturer to supply the good(s) and/or services specified as of the Quote Opening Date. 

The State reserves the right to request such certification and to require that such certification be provided within five (5) business days from the time it is requested.  

[bookmark: _MANUFACTURER’S_PUBLISHED_LIST][bookmark: _Toc108770360]MANUFACTURER’S PUBLISHED LIST OF OPTIONS AND ATTACHMENTS/PRICE LIST
The Bidder should submit a manufacturer's published list of options and attachments, compatible with the goods offered, with corresponding pricing for the Unit bid with its Quote.  The Bidder should upload the price list as an attachment through NJSTART.  Upon establishment of a Contract, the manufacturers published list of options shall become a part of the Contract and will be uploaded to NJSTART.

If a Bidder does not provide the manufacturer's published list of options and attachments with corresponding pricing for the price line item(s) bid with its Quote, the State reserves the right to request such information from the Bidder.  The Bidder must respond to such request by providing all requested information within forty-eight (48) hours.  If the information requested is not received within forty-eight (48) hours, the Quote may be deemed non-responsive.
[bookmark: _Toc108770361]PRICE LIST AND/OR CATALOG
Not applicable for this procurement.

[bookmark: _Toc108770362]FINANCIAL CAPABILITY OF THE BIDDER
The Bidder should provide sufficient financial information to enable the State to assess the financial strength and creditworthiness of the Bidder and its ability to undertake and successfully complete the Contract.  In order to provide the State with the ability to evaluate the Bidder’s financial capacity and capability to undertake and successfully complete the Contract, the Bidder should submit the following:
A. For publicly traded companies the Bidder should provide copies or the electronic location of the annual reports filed for the two most recent years; or
B. For privately held companies the Bidder should provide the certified financial statement (audited or reviewed) in accordance with applicable standards by an independent Certified Public Accountant which include a balance sheet, income statement, and statement of cash flow, and all applicable notes for the most recent calendar year or the Bidder’s most recent fiscal year. 

If the information is not supplied with the Quote, the State may still require the Bidder to submit it.  If the Bidder fails to comply with the request within seven (7) business days, the State may deem the Quote non-responsive.

A Bidder may designate specific financial information as not subject to disclosure when the Bidder has a good faith legal/factual basis for such assertion.  The State reserves the right to make the determination to accept the assertion and shall so advise the Bidder.

[bookmark: _Toc108770363]STATE PRICE SHEET INSTRUCTIONS
The Bidder must submit its pricing using the State Price Sheet accompanying this Bid Solicitation and located on the “Attachments” Tab. 

Any price changes including hand written revisions or "white-outs" must be initialed.  Failure to initial price changes shall preclude a Contract award from being made to the Bidder pursuant to N.J.A.C. 17:12-2.2(a)(8).

In order for the State to make sound business judgments regarding products and prices offered in response to this Bid Solicitation, the Bidder must supply, with its Quote, the information requested on the Bid Solicitation’s pricing lines in sufficient detail as to allow the State to determine the firm, fixed Quote pricing and the precise product or service being offered, i.e., with no possible misinterpretation of the price or product/service being offered by the Bidder.  A Bidder’s failure to provide, within its Quote, the information deemed by the State to be essential for product identification or price determination shall result in rejection of that Bidder’s Quote.  Notwithstanding the aforementioned material obligation, in order to support the State's decision-making process, the State may require a Bidder to provide additional information or documentation that has been deemed not to be material to product identification or price determination, in which case, the Bidder shall, within the time limit set forth in the written request, comply with said request.  Each Bidder is required to hold its prices firm through issuance of the Contract.

	Price Line
	Description

	1
	33,000 LB. GVWR Heavy Duty Truck Chassis, 

	2
	Vehicle Manufacturer’s Options

	3
	Utility Body

	4
	Utility Body Manufacturer’s Options

	5
	Hydraulic Platform Lift

	6
	Hydraulic Platform Lift Manufacturer’s Options

	7
	Hydraulic Generator

	8
	Chassis Mounted Air Compressor

	9
	One Additional Set of Parts, Service And Operation & Maintenance Manuals

	10
	Special Monotone Paint Color In Lieu Of Manufacturer’s Standard Paint Color

	11
	Technical Support



The State intends to make one (1) Statewide Contract award per cab and chassis on which the utility body, hydraulic platform lift, hydraulic generator and air compressor shall be mounted, in accordance with Bid Solicitation Section 8.16.  For example:  

· One (1) award for a Large Platform Truck mounted on a 2022 Model Year Kenworth T370  Cab and Chassis
· One (1) award for a Large Platform Truck mounted on a 2022 Model Year International MV 43100 Cab and Chassis
· One (1) award for a Large Platform Truck mounted on a 2022 Model Year Freightliner M2-106 Cab and Chassis

Bidders may offer any Equivalent Products that meet the technical requirements of the Bid Solicitation. Please refer to Bid Solicitation Section 3.19 for submission of Specification Data Sheets.

Bidders must bid on all price lines (Price Lines 1 through 11) within the group in order for its Quote to be considered responsive. If a Bidder does not bid on all price lines within the group, its Quote may be considered non-responsive.

If a brand/product bid on a price line within the group is deemed non-responsive, the entire group that price line item is part of will be deemed non-responsive, as these price lines were grouped to create a single award, with the intent that all price lines in the group will be awarded.

Price line items are grouped for Quote evaluation purposes only.  Upon Contract award, Using Agencies will be able to order any price lines within the group individually.

Bidders offering more than one make/model should submit a separate State-Supplied Price Sheet for each combination offered.  In the alternative, Bidders may add tabs to the bottom of the State-Supplied Price Sheet for additional makes and models bid (by copying the text and information from the original Price Sheet).  

Step 1 - The Bidder should enter the Bidder’s name in the field titled “Bidder Name:” located at the top of the State-Supplied Price Sheet.

Step 2 –The Bidder should enter the days required to make delivery of a completed Unit upon receipt of an order into the field titled “Delivery Days ARO” on the State-Supplied Price Sheet. If the “Delivery Days ARO” field is left blank, then the delivery days shall default to the delivery days set forth in Bid Solicitation Section 5.6.

Step 3 – For Price Lines 1, 3, 5, 7, 8, 9 and 10 the Bidder shall insert a firm, fixed price in US dollars in the field titled “Unit Price” on the State-Supplied Price Sheet. If a Bidder leaves the “Unit Price” field blank, it’s Quote shall be deemed non-responsive.
Any additional costs, including freight, must be included in the pricing offered on the State-Supplied Price Sheet.  

Step 4 – For Price Line 2 the Bidder shall insert a firm, fixed percentage (%) discount only in the “Unit Price” field.

For Price Lines 4 and 6 the Bidder shall insert a firm, fixed percentage (%) discount or markup in the “Unit Price” field.  

A Bidder’s entry in the “Unit Price" for price lines 2, 4, and 6 shall be considered a percentage (%). For example, an entry of "50" shall be considered "50%" and that of "0.50" shall be considered "0.50%". If a Bidder leaves the “Unit Price” field blank on Price Lines 2, 4, and 6,  it shall be considered that the Bidder is offering no markup or discount to the price list. it shall be considered that the Bidder is offering the list price (i.e no markup or discount) for that price line item.” 

A series or a range of discounts or markups or fixed prices (firm dollar amount) on Price Lines 2, 4, and 6 shall not be acceptable, and shall result in rejection of the Quote.

The Bidder is permitted to bid a % markup (by entering “+5%” or “5% markup”, for example) on the manufacturers options price list in the "Unit Price” column on Price Lines 4 and 6.

If a Bidder fails to insert the “+” or term “markup” on the price line, the State will assume that the percentage offered is a discount.

The NJSTART system is able to accept Unit Prices containing up to two (2) decimal places to the right of the decimal point. Any price beyond 2 decimal points will be rounded to the second decimal place.  Unit Prices may be offered on the State-supplied Price Sheet up to two (2) decimal places to the right of the decimal point.  Price Sheet formatting will automatically round Unit Prices containing more than two (2) decimal places to the right of the decimal point so as not to exceed this limit.  The State will only consider pricing offered up to two (2) decimal places to the right of the decimal point and will not round any figures beyond two (2) decimal places to the right of the decimal point.

The following is an example of an acceptable submission of a Discount (Price Line #2 and #6 highlighted in yellow) and a Markup (Price Line #4 highlighted in yellow) on the State-Supplied Price Sheet:

[image: ]

Step 5 – For Price Line 11 the Bidder shall insert a firm, fixed hourly rate in the “Unit Price” field.  If a Bidder leaves the “Unit Price” field blank, it’s Quote shall be deemed non-responsive. 

The Bidder shall bid a firm, fixed hourly rate in the “Unit Price” field, by entering the hourly rate bid in the “Unit Price” field on this specific price line on the State-Supplied Price Sheet.  A Bidder’s entry in the “Unit Price” field for Price Line 11 shall be considered a firm, fixed price per hour.  For example, entry of “50” shall be considered “$50 per hour”.  

Multiple or series or range of hourly rates or a fixed task price on this price line shall not be accepted and will render the Quote non-responsive.

If a Bidder leaves the “Unit Price” field blank on any price line, it shall be considered that the Bidder provided no Quote for that price line item.  Failure to bid on all price lines shall result in rejection of the Bidders Quote.  

Step 6 – For Price Line 1, the Bidder shall enter the make of the item being offered in the field titled “Make”. (e.g. Kenworth), the model of the item being offered in the field titled “Model” (e.g. T370), and the model year of the item being offered in the field titled “Model Year” (e.g. 2022) on the State Supplied Price Sheet.

Step 7 - For Price Lines 3, 5, 7 and 8, the Bidder shall enter the make of the item being offered in the field titled “Make”, and the model of the item being offered in the field titled “Model” on the State-Supplied Price Sheet.

Step 8 - The Bidder should enter the cash discount for expedited payments, pursuant to Section 3.36.2, into the “Cash Discount Terms” field located at the top of the State-Supplied Price Sheet.  If the Bidder leaves the “Cash Discount Terms” field blank, it shall mean that the Bidder is not offering a cash discount.

Where the State-Supplied Price Sheet includes an estimate quantity column, Bidders are advised that estimated quantities may vary throughout the Contract term resulting from this Bid Solicitation.  There is no guaranteed minimum or maximum volume for these price lines. 

Please be advised that Steps 3, 4, 5, 6 and 7 are required fields that must be completed on the State-Supplied Price Sheet.  A Bidder’s failure to complete these fields on the State-Supplied Price Sheet shall render the Bidder’s Quote non-responsive.

[bookmark: _Toc108770364]DELIVERY TIME AND COSTS
Unless otherwise noted elsewhere in the Bid Solicitation or price sheet, all delivery times are as noted in Bid Solicitation Section 5.6 Delivery Time and Costs.  Bidder may submit alternate delivery days on the State Price Sheet.  Alternate delivery times shall not exceed the delivery days noted in Bid Solicitation Section 4.5.5 Delivery and Final Acceptance, as applicable.  Quotes that exceed the delivery days of Bid Solicitation Section 4.5.5 Delivery and Final Acceptance may be deemed non-responsive.  

[bookmark: _Toc108770365]CASH DISCOUNTS
The Bidder is encouraged to offer cash discounts based on expedited payment by the State.  The State will make efforts to take advantage of discounts, but discounts will not be considered in determining the price rankings of Quotes.  Should the Bidder choose to offer cash discounts, the following shall apply:
A. Discount periods shall be calculated starting from the next business day after the Using Agency has accepted the goods or services, received a properly signed and executed invoice and, when required, a properly executed performance security, whichever is latest; and
B. The date on the check issued by the State in payment of that invoice shall be deemed the date of the State's response to that invoice.

[bookmark: _Toc108770366]VOLUME DISCOUNTS
Not applicable to this procurement.

[bookmark: _Toc108770367]USE OF “NO BID” VERSUS “NO CHARGE” ON THE STATE-SUPPLIED PRICE SHEET
All price lines must be filled out in accordance with the instructions above.  If the Bidder will supply an item on a price line free of charge, the Bidder must indicate “No Charge” on the State-Supplied Price Sheet accompanying this Bid Solicitation. The use of any other identifier may result in the Bidder’s Quote being deemed non-responsive.
 
[bookmark: _Toc108770368]ORAL PRESENTATIONS
Not applicable to this procurement.





























[bookmark: _Toc108770369]SCOPE OF WORK
[bookmark: _Toc400531507][bookmark: _Toc428533978][bookmark: _Toc32310703]
[bookmark: _Toc108770370]CONTRACT UTILIZATION
This Bid Solicitation has been developed to establish a term Contract to procure the specified Large Platform Truck for the New Jersey Department of Transportation (NJDOT), other State agencies, and the Cooperative Purchasing Program participants.  

The State guarantees neither any minimum nor average or maximum quantity per order nor total quantity during Contract term, including any extension(s) thereof.

[bookmark: _Toc172392760][bookmark: _Toc424044872][bookmark: _Toc455130500][bookmark: _Toc475965612][bookmark: _Toc482353332][bookmark: _Toc493254936][bookmark: _Toc9499248][bookmark: _Toc15908063][bookmark: _Toc70515792][bookmark: _Toc99962163][bookmark: _Toc108770371]CONTRACT SPECIFIC REQUIREMENTS
4.2.1 The Contractor must be a franchised and/or authorized factory representative, able to furnish the specified Unit. Dealers or agents submitting a Quote may be required to submit a letter of certification from the manufacturer whose product is supplied, certifying that the dealer or agent is authorized by the manufacturer to supply the Unit specified. The State reserves the right to request such certification and to require that such certification be provided within five (5) business days from the time it is requested.  The Contractor must notify the State of New Jersey of any changes in the status of its franchise with the manufacturer.
4.2.2 The Unit supplied must be the manufacturer's product line available to the general public.  
4.2.3 The Contractor shall provide a new Unit of latest design and is current in production.  No used Unit shall be accepted.
4.2.4 This Bid Solicitation is for the outright purchase of the Contract Unit only; leasing of the Contract Unit or trade-in against the purchase of the Contract Unit is not permitted.
4.2.5 All components of each Unit supplied under the Contract established shall be identical, for example, alternators, filters, distributors, etc. 
4.2.6 Aftermarket installation is permitted. The Contractor is responsible for assuring aftermarket installer(s)' compliance with all terms and conditions of the Bid Solicitation.  The Contractor will assume sole responsibility for any payments due the aftermarket installer(s).  Nothing contained in the Bid Solicitation shall be construed as creating any contractual relationship between any aftermarket installer(s) and the State. 
4.2.7 OEM Equipment/Parts:  All of the standard and optional equipment/parts provided shall be original equipment manufacturers items when available.
4.2.8 Manufacturer's options, which includes any compatible options for each Unit specified in Section 4.4, shall be offered using the Manufacturer’s Options percentage discount or markup price line item. Upon Contract award, the State intends to upload the Unit manufacturer’s published options for the Unit bid.  The manufacturer’s options for the Unit bid shall be based on the manufacturer’s pricing.  As such, the Contractor’s discount or markup awarded on each Manufacturer’s Options price line shall be applied to the manufacturer’s pricing.
[bookmark: _Toc172392761][bookmark: _Toc448401100][bookmark: _Toc467160934][bookmark: _Toc475622011][bookmark: _Toc478734468][bookmark: _Toc5608562][bookmark: _Toc15908064][bookmark: _Toc70515793][bookmark: _Toc99962164][bookmark: _Toc108770372]VEHICLE SPECIFICATIONS – GENERAL PROVISIONS
4.3.1 Each Unit and its components shall be completely assembled, serviced and ready for use when delivered to the Using Agency.  Unless specified otherwise, any parts, components, equipment, controls, materials, features, performances, capacities, ratings or designs which are standard and/or necessary to form an efficient and complete working Unit shall be furnished whether specifically required herein or not.  The Contractor shall supply any item not specified herein but deemed necessary for the application and the item must meet the Industry standards and practices, Federal and New Jersey Safety Standards and Regulations, and SAE and other applicable standards.  

4.3.2 Each Unit shall be delivered with at least a 1/2 tank of fuel.

4.3.3 Each Unit must be protected to -20° F, with a permanent type anti-freeze.

4.3.4 The Unit provided shall be manufacturer’s standard Units with the necessary options, upgrades, customization and/or accessories required to conform to the specifications set forth in Section 4.0 of this Bid Solicitation. All options, upgrades, customization and/or accessories shall be supplied and installed by the manufacturer. Dealer installation is permitted only if factory installation is not available.  Dealer installation shall be in accordance with the practices recommended by the manufacturer and shall not adversely affect manufacturer's warranty.

[bookmark: finish]4.3.5 Undercoating and Finish:  The frame, fenders, underbody, cab, etc., except driveshaft, exhaust system, and other mechanical components must be completely undercoated.  Undercoating must be composed of a non-volatile base, grit and abrasive free material, dispersed in a petroleum solvent, which shall provide a homogenous formulation.  All undercoating must be applied to a uniform thickness with no bare spots.  

4.3.5.1 NJDOT Units: The Unit and all its components shall be cleaned and painted in accordance with Section 4.4.10.1.  All paint must be same shade.

4.3.5.2 All Other State Using Agency and Non-State Using Agency Units:  Using Agencies will specify manufacturer's standard one-tone color at the time of ordering.

In some cases, vehicle manufacturers’ special colors may be offered at a charge.  The Using Agency shall be able to order these special colors utilizing the vehicle manufacturer’s published options price line (discount line).

[bookmark: manuals][bookmark: VEHICLESPECIFICATIONSTECHNICALPROVION]4.3.6  Manuals:  If available, the Contractor shall supply one line set sheet for each Unit.  A Unit shall comprise each and every assembly system and/or component.  In addition to any line set sheet, the Contractor shall provide Unit operation and maintenance manuals for each and every assembly system and/or component that makes up the Unit.  The Contractor shall also include any other manuals that the manufacturers provide as standard manuals.  

Examples of assembly systems and/or components include, but are not necessarily limited to:

	A.
	Hydraulic pump and hydraulic systems

	B.
	Engine, drives and chassis

	C.
	Transmission

	D.
	Electrical system

	E.
	Lubrication system



The manuals shall be delivered directly to the Using Agency, upon delivery of the first Unit.  Failure to supply these manuals may delay approval of invoices for payment.

Note:  These manuals are required as a part of the Unit purchase and are not part of the “optional manuals” specified in Section 4.4.9. 

[bookmark: weightchart][bookmark: guaranteewarranty]4.3.7 Training: Complete instructions on the operation and maintenance of each Unit and a demonstration of the operation of the Unit shall be given by the Contractor, if requested by the Using Agency. Training must include operator training with instruction on proper operation of the Unit, safety, and basic preventive maintenance. This demonstration shall be a formal training session and shall be arranged with the Contractor, at the convenience of the Using Agency. The training session shall be conducted at the location of delivery or at a field location within the State of New Jersey, as specified by the Using Agency.

Note:  This training is required as a part of the Unit purchase and is not part of the “technical support specified in Section 4.4.11.

4.3.8  Guarantee/Warranty:  The Contractor must guarantee that the vehicle and all its component parts comply with the current, applicable Federal Motor Vehicle Safety Standards (FMVSS) and New Jersey State Motor Vehicle Code Regulations, perform their functions adequately, and operate successfully without undue wear or vibration.  The Contractor shall immediately replace and install free of charge any part that may break or fail by reason of defective material or workmanship within a period of one (1) year from the date of acceptance by the agency.  The Contractor must maintain a supply of component parts for the expected life of the Unit.

4.3.9 The Bidder must provide complete information on warranty coverage as specified in Section 4.5.6. 
[bookmark: _Toc448401101][bookmark: _Toc467160935][bookmark: _Toc475622012][bookmark: _Toc478734469][bookmark: _Toc5608563][bookmark: _Toc15908065][bookmark: _Toc70515794][bookmark: _Toc99962165] 
[bookmark: _Toc108770373][bookmark: vehiclespecstechnicalprovisions]UNIT SPECIFICATION – TECHNICAL PROVISIONS
[bookmark: _Toc62453702][bookmark: _Toc72994024][bookmark: _Toc99962166][bookmark: _Toc108770374]33,000 lb. GVWR Heavy Duty Truck Chassis, (PRICE LINE: 1)

It is the intent of this specification to describe the base model requirements for a 2022 model year or newer 33,300 GVWR heavy duty truck chassis.

The following cab and chassis makes and models shall be considered Approved Products and responsive to the technical requirements in Bid Solicitation Section 4.4.1:

· 2022 Model Year Kenworth T370 Cab and Chassis
· 2022 Model Year International MV 43100 Cab and Chassis
· 2022 Model Year Freightliner M2-106 Cab and Chassis

Bidders may also offer Equivalent Products that meet the technical requirements of this section of the Bid Solicitation. 

Please refer to Bid Solicitation Section 3.19 for submission of Specification Data Sheets.

NOTE: Bidders offering one of the above pre-approved cab chassis must still provide a Specification Conformance Certification for Bid Solicitation Sections 4.4.1.10, 4.4.1.11, and 4.4.1.12. 

Please refer to Bid Solicitation Section 3.21 for submission of Specification Conformance Certification.

1.1.1.1 DIMENSIONS & CAPACITIES 

GVWR:			33,000 lbs. minimum.

CA:			119 inch minimum. 

WB:			182 inch minimum.

AF:			96 inches maximum 

Drivetrain:		Rear Wheel Drive

Driver Seat: 		Air suspension type, bucket seats with high back shall be provided.

Passenger Seat: 		Fixed passenger type seat.

Heater, Defroster and Air Conditioning: 	Manufacturer’s standard fresh air type shall be provided. 

Windshield wipers:                 The Unit shall have left and right windshield wipers with intermittent control.

Radio: 			Manufacturer's standard AM/FM radio with wireless connection shall be provided. 

Air Horn: 		An air horn shall be provided.

Gauges and indicators:	Manufacturer's standard gauge package shall be provided.

PTO Indicator:		PTO engagement shall be dash mounted and shall be clearly and permanently labeled.

Rearview Mirrors:		The Unit shall have two (2) heated auxiliary convex mirrors.

1.1.1.2 ENGINE 

Type: 				Minimum six (6)-cylinder diesel engine. 

Horsepower: 			320 HP minimum.

Torque:				650 lb. /ft. torque minimum.

Electronic Throttle:		Manufacturer's standard.

Exhaust: 	The Unit shall have a horizontal muffler on the driver side or passenger side of the vehicle. Note: An underbody vertical exhaust will not be accepted.
 
Engine Shutdown:	Automatic engine shutdown with automatic override for low oil pressure and high water temperature shall be provided.

Alternator: 			160 amp alternator shall be provided. 

Transmission 

Type: 				Automatic transmission with hot shift PTO shall be provided.

Speed: 				Minimum five (5) speed forward & one (1) speed reverse. 

Transmission shall be equipped with a heavy duty oil cooler.

Fuel System

Fuel Tank: 			50 gallon minimum corrosion resistant fuel tank shall be provided.
 
Fuel Filter: 			Manufacturer’s standard fuel filter with fuel/water separator. 

Diesel Exhaust Fluid (Def) Tank: 	Def tank shall have a minimum capacity of 4.7 gallons, and shall have a screw-on locking type DEF tank cap with minimum of 2 keys.
Cooling System 

Coolant:				Manufacturer’s standard.

All coolant lines shall have constant torque clamps to eliminate potential leakage.

Radiator Type: 			Manufacturer’s standard.

Fan Clutch: 			Manufacturer’s standard.

Electrical System 

Starter:				The Unit’s starter shall be 12 volts and shall have thermal over crank/circuit protection.

Battery:				Manufacturer’s standard.

Axles 

Front Axle Type: 			Single front type axle shall be provided.

Front Axle Load: 			Shall be suitable for vehicle configuration.

Rear Axle Type: 			Single or double reaction rear axle shall be provided.

Rear Axle Load: 			Shall be suitable for vehicle configuration.

Front Suspension: 	The Unit’s front suspension shall be taper leaf spring type. Shock absorbers shall be provided. 

Rear Suspension:			The Unit’s rear suspension shall be steel leaf spring type.

Stabilizing Bar/ Auxiliary Springs: 	Manufacturer’s standard stabilizing bar or auxiliary springs shall be provided.

Brakes

Brake System:	The Unit shall have an air brake system, and shall be manufacturer’s standard anti – lock brakes. Dust shields for both front and rear brakes shall be provided.

Air Dryer: 			Air dryer with automatic moisture ejector shall be provided. Dryer shall have heater. Heater for after 
cooler shall be wired separate fuse.

Parking Brake:			Manufacturer’s standard parking brake.

Service Brake:			Shall be heavy duty air breaks with automatic slack adjusters for front and rear drum brakes.

Air (Service) Tank:			The Unit shall include an automatic drain valve with heater on wet tank.

Wheels/ Tires

Front: 				Manufacturer’s standard.

Rear: 				Manufacturer’s standard.

Chassis Equipment 

Backup Alarm:			The Unit shall have a waterproof and weatherproof back up alarm.

Emergency Warning Triangles:	One (1) set of three emergency warning triangles packed in a storage case shall be provided in accordance with FMVSS No. 125. The storage case shall be mounted in the cab. Exact mounting location shall be provided by the Using Agency during the pre-build meeting.

Fire Extinguisher: 			One (1) Type ABC Fire Extinguisher shall be provided.

Combination Ball/Pintle hook:	A 20,000 lb. capacity combination ball/pintle hook shall be installed at a height of 20 inches on the pintle hook structure. The ball/pintle hook shall be supported to the frame as necessary and shall be capable of pulling a 4,000 lb. trailer at highway speeds. Two (2) 1-inch lunettes securely mounted to the horizontal channel supporting the pintle hook shall be provided. 
	
Safety chain anchors size, type and location shall be specified.  A snap hook for the trailer safety brakes cable snap shall be provided. Require a "Tractor Package" or equivalent on the chassis, with minimum a tractor protection valve, hand control valve, and trailer brakes hoses extended to the rear of the chassis frame.

Trailer Cable Connector:	The Unit shall have an A.T.A. approved, 7-wire trailer connector, round pin, receptacle, and factory wired, to S.A. E. and 7-wire A.T.A. color code and standards and mounted near center of truck and shall be easily accessible. Center pin of trailer connector shall be wired to the truck’s back-up light circuit. The connector shall be flush mounted on a plate welded to the pintle hook structure. Final location is subject to approval of Using Agency.

Mud Flaps: 	Front and rear mud flaps shall be provided. The mud flaps shall be rubber, anti-sail, spray suppression type with no advertising permitted. 

Muffler/Tail Pipe Guards:		Stainless steel muffler/tail pipe guards shall be provided.

Wheel Wells:			Corrosion resistant metallic wheel wells shall be provided. 

Frame 

Main Rail:			The main rail shall be heat treated alloy steel.

Reinforcement Type:		Outer steel channel, "C" channel or inverted "L" reinforcement shall be continuous to the rear of frame

Section Modulus (SM) Per Side:	Reinforced frame minimum section modulus and RBM shall meet or exceed aerial lift manufacturer requirements, per rail, for aerial lift, outriggers, and all associated equipment during all conditions of equipment operation.

Resisting bending moment (RBM):	Reinforced frame minimum section modulus and RBM shall meet or exceed aerial lift manufacturer requirements, per rail, for aerial lift, outriggers, and all associated equipment during all conditions of equipment operation.


Safety Lighting and Labeling

Rear Lighting:	Combination LED stoplight, back up lights, taillights, directional lights, and 4 way flashers, all in one housing shall be provided. Lights shall comply with Federal Motor Carrier Safety (FMCSA 393) Administration guidelines.

Light Wiring: 	All electrical wires shall be heavy duty plastic covered. All exposed electrical junction blocks shall be enclosed with a boot for protection against salt and road chemicals.

GVWR Labeling:	Lower right hand corner, driver’s side door shall be labeled in 3 inch high red letters on a white background: “Must be 33,000 lbs.”

Dry Weight Decal:			Shall be weather proof and permanently mounted on driver’s side door post.

Note: The State will utilize the manufacturer’s option line to order a front license plate bracket, if offered by the vehicle manufacturer as a cost option.  If the license plate bracket option is listed as a no charge option by the vehicle manufacturer, it will automatically be included as part of the base vehicle upon ordering.

[bookmark: _Toc5608569][bookmark: _Toc18397137][bookmark: _Toc70515796][bookmark: _Toc99962167][bookmark: _Toc108770375]Vehicle’s Manufacturer’s OPTIONS (PRICE LINE: 2)

Manufacturer's attachments and options, which includes any compatible options and attachments for the Vehicle specified in Section 4.4.1, shall be offered using this percentage discount.

Please refer to Section 3.23 for submission of manufacturer’s options and attachments price list.

[bookmark: _Toc99962168][bookmark: _Toc108770376]Utility Body (PRICE LINE: 3)

It is the intent of this specification to describe a utility body that shall be mounted on the chassis described in Sections 4.4.1.

The following utility body make and model shall be considered an Approved Product and responsive to the technical requirements in Bid Solicitation Section 4.4.3:

· Knapheide 6133H-1 Customized To Meet The Specification

· Dakota Utility Body For A Large Platform Truck Customized To Meet The Specification

Bidders may also offer Equivalent Products that meet the technical requirements of this section of the Bid Solicitation. 

NOTE: Bidders offering one of the above pre-approved utility body must still provide a Specification Conformance Certification.

Please refer to Bid Solicitation Section 3.21 for submission of Specification Conformance Certification.

Body Dimensions

Material:				The Unit’s body shall be minimum two sided 14 gauge galvanized steel.

Outer Length (Overall): 		132 inches minimum.

Outer Width (Overall): 		102 inches maximum.

Inner Width:			58 inches maximum.	

Inner Height:			28 inches minimum height above floor level.

Compartments

The utility body shall have eight (8) compartments with outward opening doors, four (4) compartments on each side of the Unit, configured as follows:

· Two (2) front vertical compartment on the Unit’s driver side.
· Two (2) front vertical compartment on the Unit’s passenger side.
· One (1) horizontal compartment over wheel housing on the Unit’s driver side.
· One (1) horizontal side compartment over wheel housing on the Unit’s passenger side.
· One (1) rear vertical compartment on the Unit’s driver side.
· One (1) rear vertical compartment on the Unit’s passenger side.

Tread Plates:	Compartment top and floor shall be minimum 12 gauge or 1/8 inch steel tread steel tread plate. Compartment tread plates shall include a 1 inch overlap to form outside drip edge.		

Drain Holes and Splash Guards:	Drain holes shall be included on all vertical compartments and shall be shielded to prevent exterior water entry from road travel.
		
All compartments shall be completely water tight with automotive type non-porous door seals fastened on all doors. Rain guards for weather protection shall be included. Glue on type door seals are not acceptable. Door seals shall be replaceable.

Doors shall be double shell 18 gauge or 20-gauge panels for rigidity. Hinges shall be continuous with a stainless steel pin. All door latches shall be recessed slam-type with tumbler locks on each vehicle keyed adjustable to compensate for wear. All vertical doors shall have double spring over center door closure.

A master locking system shall be supplied, which shall consist of two (2) master locking system assemblies, one for driver side and one for the passenger side. The system shall be fully independent of the standard individual door locks. There shall be a provision for a padlock on the rear of the body which will lock the handle and hence the three full length compartments. Two (2) padlocks with keys shall be supplied for each unit.

Locking bar handles shall be designed to prevent handle rotation when padlocks are removed.

[bookmark: _Driver_Side_Front]Driver Side Front Vertical Compartments

The first front vertical compartment on the driver’s side of the Unit should be approximately 30 inches wide, 48 inches high, and 18 inches deep.

The second front vertical compartment on the driver’s side of the Unit should be approximately 24 inches wide, 48 inches high, and 18 inches deep.

Please refer to Section 4.13.1 of the Bid Solicitation for picture examples of the compartment locations.  

Each front compartment shall be equipped with two (2) adjustable trays with adjustable dividers. Exact location of the hooks shall be determined at pre-build meeting.

Each compartment door shall be vertically hinged along the forward edge and rearward edge.

[bookmark: _Passenger_Side_Front]Passenger Side Front Vertical Compartments

The first front vertical compartment on the passenger’s side of the Unit should be approximately 30 inches wide, 48 inches high, and 18 inches deep.

The second front vertical compartment on the passenger’s side of the Unit should be approximately 24 inches wide, 48 inches high, and 18 inches deep.

Please refer to Section 4.13.2 of the Bid Solicitation for picture example of the compartment locations.

Each front compartment shall be equipped with two (2) adjustable trays with adjustable dividers. Exact location of the hooks shall be determined at pre-build meeting.

Each compartment door shall be vertically hinged along the forward edge and rearward edge.

[bookmark: _Driver_Side_Horizontal]Driver Side Horizontal Compartment

The horizontal compartment on the driver’s side of the Unit should be approximately 52 inches long, 22 inches high, and 18 inches deep.

Please refer to Section 4.13.1 of the Bid Solicitation for picture examples of the compartment locations.

Driver side horizontal compartment shall be an open type compartment and shall be equipped with two chains at the door for opening door either upward or downward. Exact location of the hinges to be determined at pre-build meeting.

[bookmark: _Passenger_Side_Horizontal]Passenger Side Horizontal Compartment

The rear horizontal compartment on the passenger’s side of the Unit should be approximately 52 inches long, 22 inches high, and 18 inches deep.

Please refer to Section 4.13.2 of the Bid Solicitation for picture example of the compartment locations.

Passenger side horizontal compartment shall have adjustable dividers installed in the compartment’s bottom on 6 inch centers.

Doors shall be vertically hinged along the forward edge of the compartment. Exact location of the hinges to be determined at pre-build meeting.

[bookmark: _Driver_Side_Rear]Driver Side Rear Vertical Compartment

The rear vertical compartment on the driver’s side of the Unit should be approximately 25 inches wide, 48 inches high, and 18 inches deep.

Please refer to Section 4.13.1 of the Bid Solicitation for picture examples of the compartment locations.

Driver side vertical compartment shall be equipped with one (1) adjustable trays with adjustable dividers. 

Driver side vertical compartment doors shall be vertically hinged along the forward edge of the compartment.

[bookmark: _Passenger_Side_Rear]Passenger Side Rear Vertical Compartment

The rear horizontal compartment on the passenger’s side of the Unit should be approximately 25 inches wide, 48 inches high, and 18 inches deep.

Please refer to Section 4.13.2 of the Bid Solicitation for picture example of the compartment locations.

Doors shall be vertically hinged along the forward edge of the compartment.

1.1.1.3 FLOOR AREA

Weather Protection:	The floor shall have 3/16 inch thick tread plate, turned up to the side walls of the compartment (approximately 1-3 inches high).  Seams shall be continuous welding with caulking for additional protection.

Drain Holes:		Drain holes shall be shielded on the bottom side to prevent water entry on floor.

U-Channel:	A U-channel, 6 inches high, shall be installed at the rear of the body on each side. This will accommodate a 6 inch composite tail board (included) to serve as a removable tailgate.

Holder

Chocks:	Triangular rubber wheel chocks, approximately 6 inches high x 7-1/2 inch face width x 10 inches in length, with handle shall be provided.

Chock Holders:	Two (2) chock holders shall be installed in wheel panel on driver side, or below tail shelf. Exact location shall be determined at pre-build meeting. A retainer device to prevent chocks from bouncing out during road travel shall be provided.

Outrigger Pad Holder: 	Outrigger pad holder and pads shall be mounted under the body on each side. Pad holders shall be made of aluminum and pads have handles made of ½ inch diameter nylon rope. Outrigger pad size and type shall be determined at pre-build meeting.

[bookmark: _Accessibility]Accessibility

Tail Shelf:	The tail shelf shall be minimum 36 inches long, full width of the body, and all surfaces shall be constructed of steel tread plate (all surfaces).  If needed the tail shelf may be longer to extend past the end of the stored aerial lift bucket to prevent bucket damage when backing the truck. Tail shelf shall be continuous welded on all corners and shall be capable of carrying two (2) personnel and material. The Unit shall require an ICC type bumper at the end of the tail shelf for underride protection per Federal Motor Carrier Safety Regulations 393.86. Please refer to Section 4.13.3 of the Bid Solicitation for picture example of the tail shelf location.

Hand Rails:	Tail shelf shall include hand rails on each side and shall be designed for optimal operator safety.

Tail Shelf Cables:	Two (2) heavy duty cable steps with traction tread shall be installed to the tail shelf, with grab handles to permit entrance onto rear surface. Each step shall consist of two (2) sets of parallel cables.

Access Step: 	An additional step shall be required to gain access onto the top of the utility body compartment for entry onto the platform. This step shall be securely mounted either to the vertical surface of the utility body compartment or the deck of the utility body and shall have an open tread design, measuring approximately 6 inches x 12 inches. Grip-strut or equivalent safety grating for step surface shall be provided.

Safety Lighting

Flush Mount:		In addition to the FMVSS108 compliant lighting the following lighting shall be included:
	
· Two (2) 7 inch diameter LED lights shall be mounted on the rear of the body one on each side and shall function as taillights, directional signals, brake lights and 4-way flashers.

Warning Bar:	One (1) low profile LED dominator plus, Whelen model DP800800 or approved equal, should be flush mounted within or just below the recessed framework of the tail shelf. The traffic advisor should be capable of only one non – directional pattern. Controls and indicator light shall be clearly and permanently labeled.

Light Bar:	One (1) Whelen LED Freedom light bar or approved equal shall be mounted level on the truck cab. Light bar cannot interfere with the operation of the platform lift. Light bar shall incorporate an internal automatic dimming feature.

Light heads:	Two (2) Whelen LED M9 or approved equal light head shall be mounted on the rear of the utility body. Exact location shall be determined at the pre-build meeting.

Light Switches:	Lights shall be controlled by heavy duty switches with indicator lights installed on or under dash. One switch is to control the safety lights the other switch is to control the take down lights.

Strobe Light:	Both front fenders and rear fenders shall be equipped with a LED strobe lights. Four (4) interchangeable amber strobe lights in total.

Compartment Lights: 	Each compartment shall have sealed, weatherproof light strips. Location of master switch shall be determined at pre-build meeting.

Light Mount:		Four (4) light mounts shall be on each corner of the platform.

Telescopic light:	A bottom raising telescoping pole with (120-volt) light shall be supplied. The lamp head shall be LED type. A removable protective lens cover shall be included on the light housing. The light shall rotate 360°. The pole shall be corrosion resistant and shall feature a quick release latch. Pole shall have pigtail wiring with a three prong plug.

Light Assembly Brackets:	The brackets shall be mounted near the aforementioned outlets so that the light/pole assembly can be removed and utilized at the front or back of the vehicle. Also, the light assembly shall be capable of being used in the platform on brackets.

Wiring:	All wiring shall be protected in heavy duty loom, be supported and tied with no hanging loops. No wire splicing butt connections are permitted inside wiring harnesses. Wiring must be shielded from exhaust heat. Wire in loom must pass through grommets into body compartments. No "Scotch-Lock" type parallel connectors shall be allowed. Wiring connectors shall have a heat-shrink insulator sleeve with a heat activated bonding material inside the sleeve. Protect exposed terminations with a corrosion preventive compound. Perhaps require a sealed junction box.

Reflective Striping: 	The Unit shall be striped for use in night operations with 3M grade 2 inch wide, red/white conspicuity tape per the following:

A. On the interior lower section of cab door, one section of red/white tape with white facing door hinge at the bottom of the door, typically all doors.
B. Interior of cabinet/accessory door, stripe shall be visible when doors are open, typically all doors.
C. On top of the body side, full length of body from the front of body to the rear, horizontal stripe with white edge forward, typically both sides.
D. On each side of the aerial boom.
E. On the rear face of body, vertical stripe on the outer edge of the body, from bottom to top, typically both sides.
Equipment	

Receptacles:	Two (2) duplex weatherproof electrical GFI receptacles (20 amp) with weather caps shall be provided. One shall be installed at the passenger rear vertical compartment for operating 110 VAC tools. The other shall be mounted on the front face of the utility body’s passenger side. They shall be hard-wired into the circuit from the hydraulic generator.

Pole Holder:	A pole holder (for carrying a 300 lb., 20 foot long pole) shall be featured. Exact location of pole holder shall be determined at pre-build meeting. Each front and rear pole holder mount shall be removable. Each carrier shall consist of a reinforced "U" or "V" steel bracket at the top of each stanchion to hold various diameter metal poles. Each bracket is to include 2 inch thick, dense rubber, bolt-on pads.

[bookmark: _Toc99962169][bookmark: _Toc108770377]Utility Body MANUFACTURER’S OPTIONS (PRICE LINE: 4)

Manufacturer's attachments and options, which includes any compatible options and attachments for the Unit specified in Section 4.4.3, 
shall be offered using this percentage discount or markup price line item.

Please refer to Section 3.23 for submission of manufacturer’s options and attachments price list.

[bookmark: _Hydraulic_Platform_Lift][bookmark: _Toc99962170][bookmark: _Toc108770378]Hydraulic Platform Lift (Price Line: 5)

It is the intent of this specification to describe the base model requirements for a hydraulic platform lift.

The following hydraulic platform lift shall be considered an Approved Product and responsive to the technical requirements in Bid Solicitation Section 4.4.5: 

· Aero-Lift 3TP

Bidders may also offer Equivalent Products that meet the technical requirements in this section of this Bid Solicitation. Please refer to Bid Solicitation Section 3.19 for submission of Specification Data Sheets.

NOTE: Bidders offering the above pre-approved hydraulic platform lift must still provide a Specification Conformance Certification for Bid Solicitation Sections 4.4.5.5, 4.4.5.9, 4.4.5.10, 4.4.5.11 and 4.4.5.12. 

Please refer to Bid Solicitation Section 3.21 for submission of Specification Conformance Certification.

1.1.1.4 GENERAL

Type:	The Unit shall have a hydraulic, telescopic, three stage lift and is non-insulated.	

Height from Bottom of Platform:  	55 feet maximum

Working Side Reach:	32 feet minimum from the centerline of rotation to the center of the platform (fully extended).

1.1.1.5 TURRET AND BOOM

Boom Assembly:	The boom assembly shall include an outer boom, telescopic inner boom(s), extension system and hose. Boom assembly shall consist of stationary main boom attached to the turret and one (1) outer movable boom.

Outer Boom:	The outer boom shall slide onto wear pads. A non-skid step surface shall be located on the boom near the platform entrance.

Inner Boom:	The inner boom shall be telescopic and shall be easily removable and disassembly for service and inspection.

Extension System:	The Unit’s extension system shall consist of hydraulic cylinder(s) and holding valves.

Rotation:	The Unit shall be able to rotate 360 degrees continuously in both directions.

Boom Elevation:	20 degrees below horizon to 75 degrees

Turret:	Turret weldment shall be bolted to a ball bearing gear on top of the pedestal. It shall form a strong rigid framework, incorporating a base plate and two (2) side plates. Boom assembly and elevation cylinder shall be mounted between the turret side plates.

Hoses: 	The hydraulic hoses shall be routed through the boom and contained within the assembly.

Pins:	Manufacturer’s standard.

Manlift Requirements

Cylinders:	Boom elevation, extension and retraction shall be made by double-acting cylinders.

Check Valves:	The aerial device shall be equipped with cylinder mounted holding valves on all cylinders.

Cat Track System:	Cat track system for the control harness at the platform shall be incorporated within the boom assembly.

Boom Support	

Stanchion:	A steel boom stanchion with rubber pads shall be furnished, at the rear of the truck, for support of the boom in the stowed or travel position. The boom support is to extend from the tail shelf to the boom and is to cradle the boom at a position directly over it.

Boom Cradle:	The boom cradle shall be positioned over the centerline of the vehicle or at a location so that an operator can easily step from the top of the utility body to the boom step area. Boom cradle is to present minimal obstruction to loading vehicle body from the tailgate.

Rigging:	Rigging shall strap the boom down during transport (if required by manufacturer).

1.1.1.6 PEDESTAL

The Unit’s pedestal shall consist of a base plate, bolted to the cab and chassis frame. The pedestal incorporate gussets to prevent the unit from 
side movements on the truck chassis (if required by manufacture). 

The pedestal shall be mounted directly behind the cab with the platform resting at the rear of utility body above the rear extended step. 
Oriented with platform resting above cab is also acceptable.


[bookmark: _Two-Man_Rotating_Platform]Two-Man Rotating Platform

Material:	Steel

Floor Material: 	Non-skid steel

Hinges:	The hinges shall be a corrosion resistant metallic material.

Lift Capacity:	600 lbs. minimum

Width:	48 inches minimum

Length:	60 inches minimum

Height:	42 inches minimum

Rotation:	The platform shall be hydraulically driven and rotate a minimum of 180 degrees.

Self-Leveling:	The Unit shall have self-leveling capabilities.

Kick Plate:	The platform shall have a 4 inch high kick plate at the base of the railings.

Accessibility:	Manufacturers standard.

Stowed Position: 	Platform shall be secured during transport.

Please refer to Section 4.13.3 of the Bid Solicitation for picture example of the platform location.

Controls

The Unit shall have lowering controls and platform controls.

Emergency Stop/ Lowering:  	Emergency stop/ lowering feature shall be included with both the lowering controls and the platform controls.

Wireless Remote:		The remote for both controls shall be wireless.

1.1.1.6.1 LOWERING CONTROLS

[bookmark: _Hlk82527619]The lowering controls shall rotate turret/boom assembly, as well as boom extension/retraction. Exact locations of controls shall be determined 
at pre-build meeting. 

Manually activated controls for winch operation and platform leveling shall be included. The lowering control shall be equipped with a 
selector valve to override the platform controls.  All controls shall be fully metered, permitting feathering of all hydraulic operations, and shall 
be the dead man fail-safe type.

All lower controls location and configuration must meet the requirements of ANSI A92.2 latest revision.

Platform Controls

[bookmark: _Hlk82527820]The platform controls shall be full-pressure single-stick type for operating the turret/boom assembly’s rotation, raising, lowering, and 
extension. Remote re-leveling and winch controls shall also be included. 

A truck engine start/kill switch shall be mounted on the platform. The Unit shall shut down automatically if shifted into any other gear when 
the platform is in the "up" position. A two-speed throttle control shall be provided at the platform. 

All hydraulic and electrical controls at the platform shall be mounted inside a protective, weatherproof enclosure with hinged cover. All control 
functions associated with the aerial lift shall be properly identified. Engraved plates are preferred where possible.

All upper controls location and configuration must meet the requirements of ANSI A92.2 latest revision.

1.1.1.7 HYDRAULIC SYSTEM

Power Source:	Transmission PTO.

Pump:	The hydraulic system pump shall be able to produce the pressure and flow to run the hydraulic generator.

Operating Pressure:	Manufacturer's standard.

Filter:	A removable suction screen of minimum 100 mesh shall be installed at the pump inlet while a minimum 6 micron removable filter shall be installed in the return line above the hydraulic oil level so that it can be changed without draining the reservoir.

System Type:	Manufacturer’s Standard

Reservoir:	Must be of sufficient size to provide the hydraulic system needs of the aerial device and the hydraulic generator without the addition of an oil cooler. Reservoir shall include a full line size opening gate or ball valve in the suction line between the reservoir and the pump, which will shut off the oil for pump replacement or service. The reservoir shall be mounted and readily accessible for servicing without removing structural components.

Pressure Lines:	All pressure lines shall be either seamless metal hydraulic tubing or minimum two-wire braid with the applicable burst and working pressure ratings.

Return Lines:	All return lines shall be single wire braid with the applicable burst and working pressure ratings.

Service Lines:	There shall be provisions to dump, adjust and bleed the hydraulic system at the turret control station. A sight gauge, drain and shut off valves shall be included for servicing of the Unit.

1.1.1.8 BACK UP POWER SYSTEM

In the event of primary power source failure, a DC powered motor operated off of the truck engine battery will provide backup power to the 
hydraulic pump. This emergency provision will provide all hydraulic functions in order to move aerial platform to rest position if operator 
becomes incapacitated in the raised position. The system shall be connected in parallel with the main hydraulic pump and be designed for non-
continuous operation.

Outriggers

Primary:	Two (2) "H" type outriggers, independently controlled by separate control valves mounted on each side of the utility body. Spread shall meet or exceed stability requirements of A92.2.

 Ground penetration: 	6 inch minimum and shall be connected with a full length sub frame structure to protect the truck frame from being over stressed from side material handling.

Secondary:	Shall be connected with a full length sub frame structure to protect the truck frame from being over stressed from side material handling.

Location:	The primary outriggers shall be fastened to the truck’s frame behind the cab or to the pedestal. Outrigger spread should be maximum 12 feet 6 inches (to prevent interference with traffic).

Check Valves:	A pilot operated check valve on each outrigger shall lock and prevent any sudden tipping due to broken hoses.

Interlock System:	Outrigger system shall be equipped with an outrigger/boom interlock system to prevent operator from using lift until outriggers are extended. Each outrigger leg shall be visible to the operator when operating the valves. There also must be an outrigger leg motion alarm to sound when any outrigger is extending.

Outrigger Pads: 	Shall be provided for each outrigger.
1.1.1.9 WINCH

Type:	The winch shall be a boom tip type for load lifting. Winch shall have a load locking capability to hold the load at any position of the load line.

Material:	Minimum 90 feet of polyester, double braid rope that exceeds weight rating on main winch and jib combination.

Working Capacity:	1,000 lb. minimum

Safety:	Safety hook shall be securely mounted on the boom. It shall have sheave head on the boom tip (under the platform) with double sheaves, two (2) quick disconnect guides to allow an operator to install or remove the safety hook at the boom tip without special tools.

Routing:	Rope shall be routed so there is no interference with other components.

Fastening:	Winch shall incorporate a fastening device near the end of the primary boom. This device is to serve as a point for securing the free end of the winch cable when not in use. The device is to use spring loaded hardware which will relieve slack in the cable.

Equipment/Lighting/Wiring

Receiver:	One (1) receiver shall be permanently mounted on the rail of the platform for the pole mounted floodlight noted previously. Receiver should be able to lock in the pole and the electrical outlet in platform should be located near it.

Light Mount:	Two (2) light mounts shall be on the top rear corners of the platform.

Hydraulic Oil Marking:	At the fill cap area, in 1 inch high letters the following shall be stated "hydraulic oil only".

Dash Warning Lights:    	For non-insulated Units only, the following red warning lights shall be installed on truck dash and shall be clearly marked:

	- To indicate when power take off is engaged.
	- To indicate whenever the outriggers are in the lowered position.
	- To indicate when upper boom or lower boom is out of its stored position.	

Wiring and Receptacles:	For non-insulated Units only one (1) duplex weatherproof electrical receptacle (20 amp) with weather caps shall be provided for operating 110 VAC tools. The circuit is to incorporate a ground fault protection device. The wiring is to terminate at a weatherproof box containing a flush mount 110V NEMA 5-20 configuration receptacle (male) with spring-loaded weather proof cover. This shall be used to provide power from hydraulic generator. Wiring from the generator to the platform shall be routed internally or external to the boom assembly without interfering with other components.

[bookmark: _Toc99962171][bookmark: _Toc108770379]Hydraulic Platform Manufacturer’s Options (PRICE LINE: 6)

Manufacturer's attachments and options, which includes any compatible options and attachments for the Unit specified in Section 4.4.5, shall be offered using this percentage discount or markup price line item.

Please refer to Section 3.23 for submission of manufacturer’s options and attachments price list.

[bookmark: _Toc99962172][bookmark: _Toc108770380]Hydraulic Generator (Price Line: 7)

It is the intent of this specification to describe the base model requirements for a Hydraulic Generator.

The following hydraulic generators  shall be considered Approved Products and responsive to the technical requirements in Bid Solicitation Section 4.4.7: 

· Getec HM-480
· Vanair XCITE
· Vanair Genair
· MTE Hydraulics Inc. G Series 1 PH

Bidders may also offer Equivalent Products that meet the technical requirements in this section of this Bid Solicitation.

Please refer to Bid Solicitation Section 3.19 for submission of Specification Data Sheets.

NOTE: Bidders offering one the above pre-approved hydraulic generators must still provide a Specification Conformance Certification for Bid Solicitation Sections 4.4.7.2.

Please refer to Bid Solicitation Section 3.21 for submission of Specification Conformance Certification.

General

In the event of primary power source failure, a DC powered motor operated off of the truck engine battery will provide backup power to the hydraulic pump. This emergency provision will provide all hydraulic functions in order to move aerial platform to rest position if operator becomes incapacitated in the raised position. The system shall be connected in parallel with the main hydraulic pump and be designed for non-continuous operation.

Generator Mounting and Location

The hydraulic generator size & location shall be determined at pre-build. Bidder to state dimensions of the generator package. Shall be installed without cutting any of the interior walls. A main hydraulic power valve (2-position) to divert flow to the tank when not in use shall be installed at the curb side front of the body.  Floor shall be reinforced with 1/8 inch steel plate.

Venting:			Adequate venting on the wall and door to cool the generator shall be provided.
		
Voltage:			The primary outriggers shall be fastened to the truck’s frame behind the cab or to the pedestal.

Receptacles:	The generator’s electrical 120V duplex receptacles shall be positioned front facing within the compartment for accessibility.

Routing:			Hydraulic supply and return hoses shall be routed to prevent chafing.

Hydraulic Power Valve:	A main hydraulic power valve (2-position) to divert flow to the tank when not in use shall be provided. Exact location of hydraulic power valve shall be determined at pre-build. Valve shall be labeled according to operation.

Labeling:			Valves shall be labeled according to operation.

[bookmark: _Toc99962173][bookmark: _Toc108770381]Chassis Mounted Air Compressor (Price Line: 8) 

It is the intent of this specification to describe the base model requirements for a Chassis Mounted Air Compressor.

The following chassis mounted air compressors shall be considered Approved Products and responsive to the technical requirements in Bid Solicitation Section 4.4.8: 

· Boss 8060-UBI
· Vanair UDSM
· Vanair Genair

Bidders may also offer Equivalent Products that meet the technical requirements in this section of this Bid Solicitation.

Please refer to Bid Solicitation Section 3.19 for submission of Specification Data Sheets.

NOTE: Bidders offering one the above pre-approved hydraulic generators must still provide a Specification Conformance Certification for Bid Solicitation Sections 4.4.8.2.

 Please refer to Bid Solicitation Section 3.21 for submission of Specification Conformance Certification.

1.1.1.10 GENERAL

Type:			A complete truck mounted air power system with under-deck PTO type air compressor, shall be provided.

Air power System:	The system shall consist of an air compressor that will produce no less than 90 CFM @ up to 200 PSI continuously.

1.1.1.11 ACCESSORIES

The chassis mounted air compressor shall include:

· ASME approved air/oil receiver tank 
· Engine speed control to modulate speed and match air demand 
· Oil cooler package
· Automatic injection oiler
· Dry type air intake filter
· Replaceable 25 micron compressor lubricant filter
· Hoses and fittings, 
· Remote final separator element 
· Mounting brackets.

Safety Device: 		Safety devices shall include, compressor lube high temperature and high pressure safety system, high pressure 
relief valve, automatic blow-down device.

High pressure and high temperature system shall automatically disengage clutch on PTO. Oil cooler lines shall be routed to oil cooler at front of engine ahead of radiator. Thermal bypass valve shall regulate oil temperature to oil cooler from compressor. Control panel shall be mounted in an accessible location and shall have an hour meter, lubricant temperature and air pressure gauges, with an over-temperature/over-pressure reset switch. The air discharge connector shall be conveniently located under the utility body or on the tail shelf deck.

Hose Reels:	A hose reel shall be mounted at the rear of the utility body. Exact placement of the reel shall be determined by the using agency. It shall be a manually operated reel with crank-rewind.

[bookmark: _Hlk82591016][bookmark: _Hlk82591000]Hoses:	50 feet of 2-ply, ¾ inch air hose (Gates #19B or approved equal) shall be supplied on the hose reel. Hose shall be resistant to sunlight, weathering, ozone and abrasion. Inner tube and cover shall be oil resistant. Air hose shall be 250 PSI working pressure, temperature range of -40° to -212° F.

Fittings:			The tool end of the hose and the compressor outlet end are to have type "A" Ingersoll-Rand or approved equal 
couplings, male end. The hose reel-to-compressor coupling shall be female. Couplings shall be held in place with two-piece, bolt together hose clamps. A method of securing the free end of the hose at the hose reel, when not in use, shall be supplied. A safety excess flow check valve shall be installed in the outlet line (Dixon part#-SCVJ6 or approved equal).

[bookmark: _One_Additional_Set][bookmark: _Toc475622019][bookmark: _Toc478734476][bookmark: _Toc5608570][bookmark: _Toc15908072][bookmark: _Toc70515797][bookmark: _Toc99962174][bookmark: _Toc108770382]One Additional Set Of Parts, Service And O&M Manuals (Price Line: 9)

Optional Manuals: One set of parts, service and operation and maintenance manuals for each assembly system and/or component that makes up the Unit shall be provided as follows: 

1 - Set of parts manuals (illustrations and text) bound or with binders, and on CD-ROM or Flash Drive. 

1 - Set of complete shop repair (factory service) manuals bound or with binders and on CD-ROM or Flash Drive. 

1 - Set of complete operation & routine maintenance manuals 

1 - Set of electrical schematics 

1 - Set of troubleshooting manuals for the diesel engine 
	
Examples of assembly systems and/or components include, but are not necessarily limited to: 

A. Hydraulic Pump and Hydraulic Systems
	

	B. Engine, Drives and Chassis
	

	C. Automatic Transmission
	

	D. Utility Body and Components
	

	E. Hydraulic Platform
	 



The manuals shall be delivered directly to the Using Agency, upon delivery of the first Unit. 

[bookmark: _Toc70515798][bookmark: _Toc99962175][bookmark: _Toc108770383]Special Monotone Paint Color In Lieu of Manufacturer’s Standard Paint Color (Price Line 10) 

1.1.1.12 NJDOT UNIT 

The Unit’s cab fenders and hood, turret, inner and outer boom assembly, rotating platform and compartments  shall be cleaned and painted with Manufacturer’s standard paint and primer and finished with DuPont Centari color, in lieu of manufacturer's standard paint color (“Undercoating and Finish”, see item 4.3.5). All paint shall be same shade. 
 
Note:  Other components requiring paint such as the sub frame, bumper, fuel tank and additional module components shall be painted with two coats of primer and two coats of gloss black.  Aluminum and stainless-steel components do not require paint.

1.1.1.13 OTHER USING AGENCY UNITS 
Other Using Agency Units shall be manufacturer's standard one-tone colors available. Using Agency shall select color at time of order.

Note:  Other components requiring paint such as the frame, bumper, fuel tank and any accessory housings must be painted with two coats of primer and two coats of gloss black.  Aluminum and   stainless-steel components do not require paint. 

[bookmark: _Technical_Support_(Hourly][bookmark: _Toc19520363][bookmark: _Toc53748379][bookmark: _Toc54703921][bookmark: _Toc70515799][bookmark: _Toc99962176][bookmark: _Toc108770384]Technical Support (Hourly Rate)  – Operators and Mechanics Training (PRICE LINE: 11)

Operator Training:

The Contractor, shall provide training for the Unit specified in Section 4.4.1, as described below.  

The Contractor shall coordinate with the Using Agency to provide an operator training session for a maximum of ten (10) personnel.

Complete instructions on the operation and maintenance of each Unit and a demonstration on the operation of the Unit shall be given by the Contractor. 

The training shall consist of, but is not limited to, operator training with instruction on proper operation of the Unit, safety, and basic preventive maintenance. 

This demonstration shall be a formal training session and shall be arranged with the Contractor. 

The training session shall be conducted at a specific location or a field location, within the State of New Jersey as agreed upon between the Contractor and the Using Agency.

Mechanics Training:

The Contractor, shall provide technical training for all components of the complete Unit specified in Section 4.4.1.  

The Contractor shall coordinate with the Using Agency to provide a mechanics training session for a maximum of five (5) personnel.

Course content shall be tailored to meet the specific needs of the Using Agency mechanics, and shall not place emphasis on areas or components not specified in the Bid Solicitation. The course shall also include hands-on instruction and content to reinforce lecture content.

The training session shall be conducted at a specific location or a field location, within the State of New Jersey as agreed upon between the Contractor and the Using Agency.

[bookmark: _Toc99962177][bookmark: _Toc108770385]CONTRACT IMPLEMENTATION
[bookmark: _Toc99962178][bookmark: _Toc108770386]Placing orders for Contract Units
4.5.1.1. The Contractor shall not substitute any item (part, component, equipment, feature, accessory, material, performance, capacity, rating, design or control), which is a part of the Contract Unit, without written authorization to do so from the Procurement Bureau.
4.5.1.2 During the Contract period, no change is permitted in any terms or conditions unless the Contractor receives written approval from the Procurement Bureau.
4.5.1.3 An offer to sell a non-Contract Unit against two or more purchase orders, one for the Contract Unit and one or more for non-Contract items, constitutes a serious violation of the Contract and may be the basis for termination of the Contract and may disqualify the Contractor from award of future State Contracts.
[bookmark: _Toc99962179][bookmark: _Toc108770387]Product Brochures
The Contractor shall make sales literature and color charts available to Using Agencies and NJ State inspectors on an "as requested" basis. 
[bookmark: _Toc99962180][bookmark: _Toc108770388]confirmation of orders
4.5.3.1 Purchase order confirmation shall be submitted to each Using Agency for each order accepted, to the attention of the contact person stated in the purchase order.
4.5.3.2 The Contractor must provide the order confirmation promptly following factory order entry.
4.5.3.3 Order confirmation shall mean that the Contractor has received the purchase order, has reviewed it for compatibility with the Unit currently on Contract, has resolved any non-compatibility problems with the Using Agency, has entered the order with the manufacturer and that the manufacturer has accepted the order and assigned an order number and anticipated build and delivery dates.
4.5.3.4 A Contractor shall not accept any purchase order on "will try" basis, unless instructed otherwise by the Using Agency in writing. If an order is not accepted for production by the manufacturer, the Contractor shall return the purchase order with "canceled" marked on the purchase order with authorized signature next to it, unless instructed to accept on "will try" basis by the Using Agency in writing. No exception shall be permitted.
[bookmark: _Toc99962181][bookmark: _Toc108770389]POST-ORDER PRE-PRODUCTION MEETING AND INSPECTION
4.5.4.1 Pre-production/pre-installation meeting and inspection: The Contractor shall coordinate and attend a post-order pre-production meeting, if required by the Using Agency, at a location convenient to the Using Agency, to provide all necessary information prior to building any prototype Unit or scheduling the production. Only after the post-order pre-production meeting, if required by the Using Agency, and subsequent approval from the Using Agency shall the Contractor begin the production. The Contractor shall coordinate with the Using Agency for a pre-paint inspection for each Unit ordered, if required by the Using Agency.
Contractor shall prepare and submit schematic drawings of all components as required by the Using Agency prior to the post order/pre-production meeting.
4.5.4.2 The State reserves the right to inspect the Bidder and/or aftermarket installer(s)' and/or Contractor’s facility. This provision applies during the Quote  evaluation period, the Contract term and any extension(s) thereof. 
4.5.4.3 Pre-acceptance Inspections: The State Using Agency reserves the right to inspect the Unit at the Contractor’s facility or require that the Contractor make the Unit available for inspection at the Using Agency site. If, during inspection at the agency site, it becomes apparent that corrections/alterations shall be made to the Unit to comply with the Contract specifications which cannot be accomplished at the State Using Agency facility, the Unit will be rejected and the Contractor must transport the Unit to its facility at no expense to the agency. After the Contractor corrects the deficiencies, the Contractor must re-deliver the Unit to the State Using Agency for re-inspection at the expense of the Contractor. 
4.5.4.4 For all inspections performed at the Contractor’s site, the Contractor must provide a bay in the repair shop to facilitate the inspection of the Unit.
4.5.4.5 The final inspection and acceptance of the Unit shall occur at the State Using Agency.
4.5.4.6 OEM Equipment/Parts: All of the standard and optional equipment/parts provided shall be original equipment manufacturers items when available.
4.5.4.7 The Contractor must make arrangements for the Using Agency’s inspection of each Unit prior to the delivery and acceptance of the Unit by the Using Agency. Prior to presentation for inspection, it shall be the Contractor’s responsibility to pre-inspect each Unit. Each Unit presented for inspection shall be accompanied by an inspection package including, but not limited to, the following: purchase order, line set sheet (when available) - brief list of all features, items and accessories included in the Unit, pre-delivery inspection (PDI), and dealer's pre-inspection prep checklist. The checklist will list the responsible prep mechanic and acknowledge that the Unit conforms to pre-delivery specifications and that all added equipment and accessories have been properly installed.
4.5.4.8 The Contractor shall notify the State Using Agency by fax and e-mail that the Unit is ready for inspection.
4.5.4.9 Delivered Units will be inspected within ten (10) working days. If a Unit has been accepted, the warranty shall commence on the date of final acceptance, or if a Unit has been rejected, the Contractor will be notified. The notice will indicate the reason(s) for rejection. If rejected, the Contractor shall try to rectify the problem(s) at the State Using Agency site. If the problem cannot be corrected at the agency site, the rejected Unit shall be removed by the Contractor at its own expense. The Contractor shall present the corrected Unit for re-inspection within ten (10) working days. No additional freight or transportation charges are permitted.
4.5.4.10 Within five (5) working days of the Contractor’s notification, the State Using Agency will, if desired, send a team of qualified inspectors to the Contractor’s facility to accomplish the inspection of the Unit(s) before delivery to the Using Agency. The Contractor must properly itemize, organize, and segregate all Units.  
4.5.4.11 Non-State Agencies authorized to purchase under this Contract will make arrangements for Unit inspection directly with the Contractor. All Units shall be delivered to each Using Agency’s designated destination at no additional cost.
4.5.4.12 Inspected Units which do not comply with the Contract requirements will be rejected. The Contractor must correct all rejected Units and the corrected Unit(s) shall be presented for re-inspection within ten (10) working days. The Using Agency may cancel the purchase order if the Contractor fails to correct any problem.
4.5.4.13 No additional freight or transportation charges are permitted under this Contract  

[bookmark: _Toc475717209][bookmark: _Toc493254948][bookmark: _Toc8647929][bookmark: _Toc19520376][bookmark: _Toc53748402][bookmark: _Toc54703944][bookmark: _Toc62549439][bookmark: _Toc72994038][bookmark: _Toc99962182][bookmark: _Toc108770390]DELIVERY AND FINAL ACCEPTANCE

4.5.5.1 Contractor deliveries for all items shall be made within the delivery timeframe noted on the price sheet and in strict accordance with the instructions from the Using Agency.  When there is a discrepancy between the delivery days listed in the General Tab in NJSTART and the Price Sheet, the Price Sheet delivery days shall govern.  Prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination.
4.5.5.2 All deliveries of Units shall be made upon approval and as instructed by the Using Agency, by prior arrangement only, during working hours, except on legal holidays.
Deliveries shall not be made on the following State observed holidays, which may be updated from time to time:
· New Year’s Day;
· Martin Luther King Jr. Day;
· Presidents Day;
· Good Friday;
· Memorial Day;
· Juneteenth;
· Independence Day;
· Labor Day;
· Columbus Day;
· Election Day;
· Veterans Day;
· Thanksgiving Day; and
· Christmas Day.

For NJDOT deliveries Only: Deliveries will be accepted from Monday through Friday, excluding weekends and all State holidays, as noted above, from 8:00 am to 2:30 pm.  No deliveries will be accepted after 2:30 pm.  Twenty-four (24) hour advanced notice must be given prior to delivery.
For All Other Using Agencies: Deliveries must be made in accordance with the delivery timeframe noted on the purchase order. 
4.5.5.3 No Unit will be accepted at the final delivery point without all supporting documentation and paperwork completed and delivered with the Unit, which include the warranty, any specified manuals, and invoice. No Unit will be considered accepted until it has undergone final inspection at the delivery point.
4.5.5.4 For purchases by State Agencies, the manufacturer's certificate of origin must be made out to the State of New Jersey, and presented at the time of delivery. Purchase order number and requisition number must be indicated on the upper left hand corner. The Contractor shall not furnish the New Jersey Certificate of Title (certificate of ownership). The State will title the Unit upon receipt of the manufacturer's certificate of origin. Other governmental entities authorized to purchase under this Contract will make arrangements for titling Units directly with the Contractor.
4.5.5.5 No advertising shall appear on any Unit delivered under the terms of the Contract. Further, the Contractor shall not affix the dealer name to the Unit. Units delivered to final destinations with dealer's advertising will be rejected.
4.5.5.6 No more than ten (10) Units per day and fifty (50) Units per week (based on a 5-day work week) will be accepted at each delivery site. When necessary, and with the consent of both the agency and the Contractor, the number of Units delivered per day may be increased.
4.5.5.7 All vehicles must be delivered with the manufacturer suggested retail price label affixed to the window. The label shall not be removed prior to delivery to the New Jersey agency.
4.5.5.8 All delivered Units must be clean both inside and outside. Manufacturer's standard items, such as hubcaps, floor mats, jack and lug wrench and the like, shall be provided and installed by the Contractor prior to delivery.
4.5.5.9 Complete instructions on the care and maintenance of the unit and a demonstration of its operation shall be given by the Contractor at the time of delivery and acceptance to the agency, if so requested by the Using Agency.
4.5.5.10 The Contractor shall indicate the delivery location of the unit on the factory order, so that recall notices will indicate the delivery location for each unit.
4.5.5.11 The Contractor must deliver the Units with an index card or other label/card, visible through the windshield, bearing the following information, in typed or printed form:
Contractor’s name
Purchase order number (if applicable)
Requisition number
Stock number
Serial number
Note: Units without this information will not be accepted.
4.5.5.12 No Unit will be accepted without a New Jersey Motor Vehicle new vehicle inspection sticker in place as prescribed by law, correctly punched to the month of delivery and acceptance or appropriate Diesel Emission Approval Sticker. Out of State Contractors must comply with this requirement without any additional cost or delay. Failure to comply with this provision will result in the rejection of the Unit.
[bookmark: _WARRANTIES][bookmark: _Toc493254949][bookmark: _Toc8647930][bookmark: _Toc19520377][bookmark: _Toc53748403][bookmark: _Toc54703945][bookmark: _Toc62549440][bookmark: _Toc72994039][bookmark: _Toc99962183][bookmark: _Toc108770391]WARRANTIES
The manufacturer's standard warranty must be supplied with each Unit at the time of delivery and shall be in typed form.  The warranty commences with the acceptance of the Unit at the delivery site, following the final inspection. 
The Contractor must guarantee that the Unit and all its component parts comply with the current, applicable safety standards, Federal Motor Vehicle Safety Standards (FMVSS) and New Jersey State Motor Vehicle Code Regulations, perform their functions adequately, and operate successfully without undue wear or failure.  The Contractor shall immediately replace and install free of charge any part that may fail by reason of defective material or workmanship.
[bookmark: _Toc475717211][bookmark: _Toc493254950][bookmark: _Toc8647931][bookmark: _Toc19520378][bookmark: _Toc53748404][bookmark: _Toc54703946][bookmark: _Toc62549441][bookmark: _Toc72994040][bookmark: _Toc99962184][bookmark: _Toc108770392]WARRANTY REQUIREMENTS
4.5.7.1 The Contractor shall ensure that the manufacturer whose product is supplied has a servicing dealer or service location to provide warranty and recall service and/or repair within twenty four (24) hours of notification by the Using Agency. 
4.5.7.2 The Contractor must perform any warranty service/repair/recall, which will be at Contractor’s own expense. Events beyond Contractor’s control, such as lack of parts due to strikes and unforeseen acts of God, shall constitute valid reasons for delay in making necessary repairs. However, the State will make such determination.
[bookmark: _Toc493254951][bookmark: _Toc8647932][bookmark: _Toc19520379][bookmark: _Toc53748405][bookmark: _Toc54703947][bookmark: _Toc62549442][bookmark: _Toc72994041][bookmark: _Toc99962185][bookmark: _Toc108770393]PAYMENT
Invoices will be processed for payment only after final acceptance of the Units by the Using Agency and the delivery ticket has been signed off by an authorized representative of the Using Agency. Partial payments may be made for Unit(s) accepted, if billed separately. Timely payment discounts will be taken if offered by the Contractor. 
[bookmark: _Toc99962186][bookmark: _Toc108770394]RECYCLED PRODUCTS
Not applicable for this procurement.

[bookmark: _Toc99962187][bookmark: _Toc108770395]DISCLOSURE OF PRODUCT COMPOSITION
At the request of the Using Agency, the Contractor must furnish material safety data sheets (MSDS) or an equivalent manufacturer’s information sheet for the goods provided under the Contract awarded.

[bookmark: _Toc99962188][bookmark: _Toc108770396]REPLACEMENT OF UNSATISFACTORY PRODUCT
In the event the product delivered does not meet the approved product specifications or is damaged prior to or at the time of delivery, as determined by the Using Agency, the Contractor shall immediately remove and replace the unsatisfactory product, at no cost to the Using Agency. The timeframe for the replacement shall not exceed the delivery days ARO listed on the State-Supplied Price Sheet.  Failure to comply may result in the product being removed from the Contract and a similar product obtained from another Contractor with any additional costs assumed by the original Contractor.

[bookmark: _Toc99962189][bookmark: _Toc108770397]SUBSTITUTION OF DISCONTINUED OR REFORMULATED PRODUCTS
The Contractor may offer a substitution for any product discontinued or reformulated by the manufacturer in its Contract.  The State may consider substituting the discontinued or reformulated model with a new model provided that the unit offered meets or exceeds the Contract specifications.  All substitutions must be approved by the State. 

The Contractor must notify the State immediately in writing to the Division’s assigned Procurement Specialist stating that an item has been discontinued or reformulated by the manufacturer along with supporting documentation from that manufacturer that the item has been discontinued or reformulated.  The Contractor must provide in its letter the discontinued or reformulated model number, model number of the new product being offered, detailed literature for the new product being offered, the price of the discontinued or reformulated item and the price of the product being offered as a replacement.  The State will not approve the substitution of a discontinued or reformulated item without all of the above information.

The replacement product should be offered to the State at that same price as the discontinued or reformulated product.

[bookmark: _Toc99962190][bookmark: _Toc108770398]SUBSTITUTION OF PRODUCTS ON A TEMPORARY BASIS
Not applicable to this procurement.

[bookmark: _Toc99962191][bookmark: _Toc108770399]PRICE LIST UPDATES
A Contractor must only provide the options and attachments that are applicable to the makes and models awarded..  This will require the Contractor to redact the products which do not apply to the makes and models awarded.  In lieu of redacting a price list, a Contractor may choose to offer only the pages of the price list that correspond with the category awarded.

The State reserves the right to redact all products which do not apply to the Group identified in this Bid Solicitation.

The Contractor may request a price list update once during a rolling twelve (12) month period.  

Requests for price list updates shall be limited to the makes and models that a Contractor is awarded.  The file name should contain the Contract number and date of the revised price list. The Contractor must provide the revised price list for the specific category awarded to the procurement via email, in pdf or Excel format.  The correspondence to the Division with the revised price list shall reference the location of the specific price line that has been revised. The revised price list will not be considered valid until it has been reviewed and approved by the Procurement Bureau and published in NJSTART.

[bookmark: _Toc513012259][bookmark: _Toc3904830][bookmark: _Toc18397151][bookmark: _Toc72994046][bookmark: _Toc99962192][bookmark: _Toc108770400]MANUFACTURER’S CUT-OFF DATE
Passage of the vehicle manufacturer's cut-off date will render the Contract unusable unless the Contractor agrees to a roll-over to the next model year. 
4.12.1 The Contractor must notify the Procurement Bureau of the manufacturer's order cut-off date, as soon as that date is made available by the vehicle manufacturer to the Contractor, but no later than two weeks prior to the cut-off date.  Cut-off date notification can be e-mailed to the Contract’s assigned Procurement Specialist.  The Procurement Bureau will post all vehicle order cut-off dates (Master Notification - Vehicle Manufacturers' Cut-off Dates), to its website and NJSTART (http://www.state.nj.us/treasury/purchase/mnmaster.pdf).   
4.12.2 Should a potential awardee be notified by a vehicle manufacturer of a cut-off date after the Quote opening and after receiving a letter of intent to award, but before Contract award has been finalized, the awardee must immediately notify the Procurement Bureau in writing.
4.12.3 Failure to fax or e-mail the cut-off date notification on time may be considered a violation of the Contract terms and conditions and may result in termination of the Contract for cause.
4.12.4 All orders placed by the published cut-off date from either the State or cooperative purchasing participants (if the Contract is so extended) must be accepted by the Contractor. These orders may be generated through the NJSTART system, hand delivered, e-mailed or faxed and may be followed by a hard-print purchase order. The State also reserves the right to order by means of "a letter of intent to purchase" with purchase order to follow.
 4.12.5 The State will consider any request for a Contract roll-over to the next model year after the passing of the vehicle manufacturer's cut-off date, at the same Contract specifications, terms and conditions or better. Vendor requests for price increases at time of rollover will be considered in accordance with State of NJ Standard Terms and Conditions (SSTC) Section 6.1. If a roll-over is agreed upon by the Contractor and approved by the Director, the Contract affected by the roll-over will be amended to the newest model year information and the manufacturer’s order cut-off date will revised to reflect the newest model year information.
4.12.6 In the absence of such roll-over, after the passage of the vehicle manufacturer's cut-off date, the State reserves the right to terminate any unusable Contract(s), in accordance with Section 5.7a (Contract Termination for Convenience) of the Standard Terms and Conditions, to facilitate the reprocurement process to establish new model year vehicle Contract(s). Such Contract termination will not affect the Contractor’s standing with the State. 
4.12.7 If a manufacturer is unable to build a vehicle for which an order has been placed by the manufacturer's cut-off date, the Contractor must immediately notify the Procurement Bureau by fax or e-mail.  At a minimum, the letter shall provide the following information: 
Purchase order number or line of credit letter date;
The make, model and quantity of vehicles ordered; and
Whether the manufacturer has offered to price protect and build these vehicles for the next model year.
4.12.8 A new Contract established for the next model year will automatically terminate any existing unusable current model year Contract, but will not relieve the Contractor of the obligation to fulfill orders placed prior to the cut-off date.







[bookmark: _Toc108770401][bookmark: _Toc37223625]EXAMPLES AND EXHIBITS
[bookmark: _Pictured_Driver_sIde][bookmark: _Toc108770402]Pictured Driver sIde Compartment Configuration – Example Only

[image: C:\Users\TYQWARR\AppData\Local\Microsoft\Windows\INetCache\Content.Outlook\85KT8SAQ\20220510_120535.jpg]

	The arrows below indicate the approximate locations of the two (2) front vertical compartments on the driver side of the Unit for example purposes ONLY. Please refer to Section 4.4.3.2.1 of the Bid Solicitation for specification details.

	The arrow below indicates the approximate locations of the horizontal compartment on the driver side of the Unit for example purposes ONLY. Please refer to Section 4.4.3.2.3 of the Bid Solicitation for specification details.

	The arrow below indicates the approximate locations of the rear vertical compartments on the driver side of the Unit for example purposes ONLY. Please refer to Section 4.4.3.2.4 of the Bid Solicitation for specification details.
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[bookmark: _Pictured_Passenger_sIde]
[bookmark: _Toc108770403]Pictured Passenger sIde Comparement Configuration – Example Only

[image: C:\Users\TYQWARR\AppData\Local\Microsoft\Windows\INetCache\Content.Outlook\85KT8SAQ\20220510_120422.jpg]


	The arrow below indicates the approximate locations of the rear vertical compartments on the passenger side of the Unit for example purposes ONLY. Please refer to Section 4.4.3.2.6 of the Bid Solicitation for specification details.

	The arrow below indicates the approximate locations of the horizontal compartment on the passenger side of the Unit for example purposes ONLY. Please refer to Section 4.4.3.2.4 of the Bid Solicitation for specification details.

	The arrows below indicate the approximate locations of the two (2) front vertical compartments on the passenger side of the Unit for example purposes ONLY. Please refer to Section 4.4.3.2.2 of the Bid Solicitation for specification details.
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[bookmark: _Pictured_Rear_View][bookmark: _Toc108770404]Pictured Rear View – Example only

The image below indicated the approximate location of the rear tail shelf described in Section 4.4.3.5 and the platform described in Section 4.4.5.6 for example purposes Only. Please refer to in Section 4.4.3.5 and Section 4.4.5.6 of the Bid Solicitation for specification details.

[image: C:\Users\TYQWARR\AppData\Local\Microsoft\Windows\INetCache\Content.Outlook\85KT8SAQ\20220510_120624.jpg]


1.2 CONTRACT SPECIFIC DEFINITIONS/ACRONYMS
AF- Axle to Frame 
Approved Products – Those products that have been identified in the Bid Solicitation as meeting Using Agency needs and confirmed as meeting product specifications.
ASTM - American Society for Testing Materials (http://www.astm.org/).
Drivetrain – The system in a motor vehicle which connects the transmission to the drive axles.  
Dry Weight - Curb weight or tare weight of a vehicle - weight of an empty vehicle, without any payload, driver and passenger, with fluids filled to half capacity.
Equivalent Products – Products offered, other than those identified as an Approved Product, in the Bid Solicitation that meet the specifications herein.
Factory Order Entry Confirmation – When a Contractor enters the purchase order in the manufacturer’s order bank successfully, it receives this confirmation.
Fleet Identification Number – An identification number assigned by the vehicle manufacturer, which is a requirement when placing a vehicle order.  The Contractor will be responsible for assisting an Ordering Agency in securing the fleet identification number from the vehicle manufacturer.
FMVSS - Federal Motor Vehicle Safety Standards, as established by National Highway Traffic Safety Administration (http://www.nhtsa.gov/cars/rules/import/FMVSS/).
GAWR - Gross Axle Weight Rating; the maximum legal weight carrying capacity of axle components, including their own dry weights, as published by the vehicle/chassis manufacturer.  GAWR shall not exceed the capacity of the least rated axle component.
GVWR - Gross Vehicle Weight Rating; the maximum legal weight carrying capacity of a vehicle, including its own weight, as published by the vehicle/chassis manufacturer.  GVWR shall not exceed the sum of front and rear GAWRs.
NJMVC or NJDMV - New Jersey Motor Vehicle Commission, formerly known as Division of Motor Vehicles (http://www.state.nj.us/mvc/).
OEM - Original Equipment Manufacturer.
Ordering Agency - Any Using Agency placing a purchase order based upon the Contracts resulting from this Bid Solicitation.
Payload - Weight carrying capacity of a vehicle, excluding its dry weight, driver and passenger.  Payload, when added to dry weight and weight of driver, passenger and half fluids, shall not exceed the GVWR.  Payload is limited by the front or rear GAWR.
Roll-over – Agreement by the Contractor to offer a later model year vehicle than the one currently under the Contract  Such an event could occur only after the manufacturer’s order cut-off date for the current model has passed.
SAE - Society of Automotive Engineers (http://www.sae.org/
Unit - (“Large Platform Truck” or "Vehicle" or “Large Platform Truck, 33, 000 L.B. GVWR Heavy Duty Truck Chassis, With Utility  Body, Hydraulic Platform and Accessories”), as specified herein, made available for outright purchase as a new, unused unit under a Contract established as a result of this Bid Solicitation. 
WB - Wheelbase, the distance between the centerlines of front and rear axles


[bookmark: _Toc108770405]GENERAL CONTRACT TERMS
The Contractor shall have sole responsibility for the complete effort specified in this Contract.  Payment will be made only to the Contractor or to the authorized dealers/distributors, if applicable.  The Contractor is responsible for the professional quality, technical accuracy and timely completion and submission of all deliverables, services or commodities required to be provided under this Contract.  The Contractor shall, without additional compensation, correct or revise any errors, omissions, or other deficiencies in its deliverables and other services.  The approval of deliverables furnished under this Contract shall not in any way relieve the Contractor of responsibility for the technical adequacy of its work.  The review, approval, acceptance or payment for any of the deliverables, goods or services, shall not be construed as a waiver of any rights that the State may have arising out of the Contractor’s performance of this Contract.

[bookmark: _Toc108770406]CONTRACT TERM AND EXTENSION OPTION
The base term of this Contract shall be for a period of three (3) years.  The anticipated Contract effective date is provided on the “Summary” page the Bid Solicitation in NJSTART.  If delays in the procurement process result in a change to the anticipated Contract effective date, the Contractor agrees to accept a Contract for the full term of this Contract 

This Contract may be extended up to three (3) years with no single extension exceeding one (1) year, by the mutual written consent of the Contractor and the Director at the same terms, conditions, and pricing at the rates in effect in the last year of this Contract or rates more favorable to the State.  

[bookmark: _Toc400531508][bookmark: _Toc428533979][bookmark: _Toc32310704][bookmark: _Toc108770407]CONTRACT TRANSITION
In the event that a new Contract has not been awarded prior to the expiration date for this Contract, including any extensions exercised, and the State exercises this Contract transition, the Contractor shall continue this Contract under the same terms, conditions, and pricing until a new Contract can be completely operational.  At no time shall this transition period extend more than one hundred eighty (180) days calendar days beyond the expiration date of this Contract, including any extensions exercised.

[bookmark: _Toc118513795][bookmark: _Toc400531563][bookmark: _Toc428534035][bookmark: _Toc32310758][bookmark: _Toc108770408][bookmark: OLE_LINK3][bookmark: OLE_LINK4]PERFORMANCE SECURITY
Not applicable to this procurement.

[bookmark: _Toc400531513][bookmark: _Toc428533984][bookmark: _Toc32310709][bookmark: _Toc108770409]OWNERSHIP OF MATERIAL
Not applicable to this procurement.

[bookmark: _Toc108770410]SUBSTITUTION OF STAFF
Not applicable to this procurement.

[bookmark: _Toc108770411]DELIVERY TIME AND COSTS
Unless otherwise noted elsewhere in the Bid Solicitation or price sheet, all delivery times are three hundred and sixty five days (365) calendar days after receipt of order (ARO) and prices for items in Quotes shall be submitted Freight On Board (F.O.B.) Destination (365 calendar days ARO/F.O.B.).  The Contractor shall assume all costs, liability and responsibility for the delivery of merchandise in good condition to the State's Using Agency or designated purchaser.  three hundred and sixty five days (365) calendar days ARO/F.O.B. does not cover "spotting" but does include delivery on the receiving platform of the Using Agency at any destination in the State of New Jersey unless otherwise specified.  No additional charges will be allowed for any additional transportation costs resulting from partial shipments made at the Contractor’s convenience when a single shipment is ordered.  The weights and measures of the State's Using Agency receiving the shipment shall govern.  Collect on Delivery (C.O.D.) Terms are not permitted.

[bookmark: _Toc108770412]AUTHORIZED DEALER AND/OR DISTRIBUTORS
The Contractor must provide a list of the Dealer(s)/Distributor(s) that will service the Contract.  The Contractor will be required to submit the following forms for each Dealer/Distributor, prior to the Dealer/Distributor being permitted to perform any work on the Contract:
A. Ownership Disclosure (N.J.S.A. 52:25-24.2);
B. Disclosure of Investment Activities in Iran (N.J.S.A. 52:32-55 et. seq.);
C. Disclosure of Investigations and Actions Involving Bidder Form;
D. MacBride Principles  (N.J.S.A. 52:34-12.2);
E. Completed Contractor Certification and Disclosure of Political Contributions (N.J.S.A. 19:44A-20:13 et. seq.);
F. Vendor Certification (P.L. 2005, c.271);
G. New Jersey Business Registration  (N.J.S.A. 52:32-44);
H. Proof of insurance as specified herein;
I. Proof of compliance with New Jersey Affirmative Action requirements (N.J.A.C. 17:27-1.1 et. seq.):
· New Jersey Form AA-302 Affirmative Action Employee Information Report; or 
· New Jersey Affirmative Action Certificate; or 
· Federal Affirmative Action Approval Letter.
J. Disclosure of Prohibited Activities in Russia / Belarus Form  

A Contractor may submit a request to add or remove Dealers/Distributors at any time during the Contract term, including any extension(s) thereof.  Any such request should be emailed to the Procurement Specialist assigned to this procurement.

[bookmark: _Toc400531525][bookmark: _Toc428533996][bookmark: _Toc32310718][bookmark: _Toc108770413]LIQUIDATED DAMAGES
Not applicable to this procurement.  

[bookmark: _Toc400531531][bookmark: _Toc428534002][bookmark: _Toc32310724][bookmark: _Toc108770414]RETAINAGE
Not applicable to this procurement.  

[bookmark: _Toc108770415]ELECTRONIC PAYMENTS
With the award of this Contract, the successful Contractor(s) will be required to receive its payment(s) electronically.  In order to receive your payments via automatic deposit from the State of New Jersey, you must complete the EFT information within your NJSTART Vendor Profile.  Please refer to the QRG entitled “Vendor Profile Management – Company Information and User Access” for instructions. 

[bookmark: _Toc108770416]CONTRACT ACTIVITY REPORT
The Contractor must provide, on a quarterly basis, a record of all purchases made under this Contract.  The calendar quarters will end March 31, June 30, September 30, and December 31 with the required reports due no later than thirty (30) days after the calendar quarter.  The Contractor must submit the required information in Microsoft Excel format to NJSupplierReports@treas.nj.gov. 

This reporting requirement includes sales to State Using Agencies, political sub-divisions thereof and, if permitted under the terms of this Contract, sales to counties, municipalities, school districts, volunteer fire departments, first aid squads and rescue squads, independent institutions of higher education, state and county colleges and quasi-State entities.  Quasi-State entities include any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member.

This information must be provided in Microsoft Excel such that an analysis can be made to determine the following:
A. Contractor’s total sales volume, with line item detail, to each purchaser under this Contract;
B. Subtotals by product, including, if applicable, catalog number and description, price list with appropriate page reference, and/or Contract, discount applied; and
C. Total dollars paid to Subcontractors.

Submission of purchase orders, confirmations, and/or invoices do not fulfill this Contract requirement for information.  Failure to report this mandated information may be a factor in future award decisions.


[bookmark: _Toc108770417]DATA SECURITY REQUIREMENTS – CONTRACTOR RESPONSIBILITY 
Not applicable to this procurement.  

[bookmark: _4.4.1.1_Ownership_Disclosure][bookmark: _4.4.1.1_Signatory_page][bookmark: _4.4.2.3_Contract_Schedule][bookmark: _4.4.2.4_mobilization_and][bookmark: _Toc108770418]MODIFICATIONS TO THE STATE OF NEW JERSEY STANDARD TERMS AND CONDITIONS
Not applicable to this procurement. 
 
[bookmark: _Toc108770419]QUOTE EVALUATION AND AWARD

[bookmark: _Toc400531542][bookmark: _Toc428534014][bookmark: _Toc32310736][bookmark: _Toc108770420]RIGHT TO WAIVE
Pursuant to N.J.A.C. 17:12-2.7(d) the Director may waive minor irregularities or omissions in a Quote.  The Director reserves the right to waive a requirement provided that the requirement does not materially affect the procurement or the State's interests associated with the procurement.
[bookmark: _Toc400531543][bookmark: _Toc428534015][bookmark: _Toc32310737]
[bookmark: _Toc108770421]DIRECTOR’S RIGHT TO ACCEPT OR REJECT A QUOTE
The Director reserves the right to reject any or all Quotes, or to award in whole or in part if deemed to be in the best interest of the State to do so. The Director shall have authority to award Contracts in accordance with N.J.S.A. 52:34-12. 

[bookmark: _Toc108770422]RECIPROCITY FOR JURISDICTIONAL BIDDER PREFERENCE
In accordance with N.J.S.A. 52:32-1.4 and N.J.A.C. 17:12-2.13, the State of New Jersey will invoke reciprocal action against an out-of-State Bidder whose state or locality maintains a preference practice for its in-state Bidders.  The State of New Jersey will use the annual surveys compiled by the Council of State Governments, National Association of State Procurement Officials, or the National Institute of Governmental Purchasing or a State’s statutes and regulations to identify States having preference laws, regulations, or practices and to invoke reciprocal actions. The State of New Jersey may obtain additional information as it deems appropriate to supplement the stated survey information.

A Bidder may submit information related to preference practices enacted for a State or Local entity outside the State of New Jersey. This information may be submitted in writing as part of the Quote response, including name of the locality having the preference practice, as well as identification of the county and state, and should include a copy of the appropriate documentation, i.e., resolution, regulation, law, notice to Bidder, etc.  It is the responsibility of the Bidder to provide documentation with the Quote or submit it to the Director within five (5) business days after the deadline for Quote submission.  Written evidence for a specific procurement that is not provided to the Director within five (5) business days of the public Quote submission date may not be considered in the evaluation of that procurement, but may be retained and considered in the evaluation of subsequent procurements.

[bookmark: _Toc400531545][bookmark: _Toc428534017][bookmark: _Toc32310739][bookmark: _Toc108770423]CLARIFICATION OF QUOTE
After the Quote Opening Date, unless requested by the State as noted below, Bidder contact with the Procurement Bureau regarding this Bid Solicitation and the submitted Quote is not permitted. 

After the Quotes are reviewed, one (1), some or all of the Bidders may be asked to clarify certain aspects of its Quote.  A request for clarification may be made in order to resolve minor ambiguities, irregularities, informalities or clerical errors.  Clarifications cannot correct any deficiencies, material omissions, or used to revise or modify a Quote.

The Director reserves the right to request that a Bidder to explain, in detail, how the Quote price was determined.

[bookmark: _Toc32310741][bookmark: _Toc108770424][bookmark: _Toc118513837][bookmark: _Toc400531547][bookmark: _Toc428534019]ORAL PRESENTATION 
Not applicable to this procurement. 
 
[bookmark: _Toc108770425]TIE QUOTES
Tie Quotes will be awarded by the Director in accordance with N.J.A.C. 17:12-2.10. 

[bookmark: _Toc108770426]STATE'S RIGHT TO INSPECT BIDDER’S FACILITIES
The State reserves the right to inspect the Bidder’s establishment before making an award, for the purposes of ascertaining whether the Bidder has the necessary facilities for performing the Contract.

[bookmark: _Toc108770427]STATE'S RIGHT TO CHECK REFERENCES
The State may also consult with clients of the Bidder during the evaluation of Quotes. Such consultation is intended to assist the State in making a Contract award that is most advantageous to the State.


[bookmark: _Toc108770428]EVALUATION CRITERIA
The following evaluation criteria categories, not necessarily listed in order of significance, will be used to evaluate Quotes received in response to this Bid Solicitation.  The evaluation criteria categories may be used to develop more detailed evaluation criteria to be used in the evaluation process.

[bookmark: _Toc118513839][bookmark: _Toc400531549][bookmark: _Toc428534021][bookmark: _Toc32310743][bookmark: _Toc108770429]TECHNICAL EVALUATION CRITERIA
The following criteria will be used to evaluate Quotes received in response to this Bid Solicitation:  

A. The Bidder’s demonstration in the Quote that the Bidder understands and is able to complete the requirements of the Scope of Work as sought.

[bookmark: _Toc118513840][bookmark: _Toc400531550][bookmark: _Toc428534022][bookmark: _Toc32310744][bookmark: _Toc108770430]PRICE EVALUATION
For evaluation purposes, Bidders will be ranked from lowest to highest according to the total Quote price located on the State-Supplied Price Sheet accompanying this Bid Solicitation, utilizing the Group Price Index as follows: 

Group Price Index Components:

BP1= Bid Price Chassis
D1 = Options Discount Chassis
BP2= Bid Price Utility Body
D2 = Options Discount Body
BP3 = Bid Price Hydraulic Platform Lift
D3 = Options Discount Hydraulic Platform Lift
BP4 = Bid Price Hydraulic Generator
BP5 = Bid Price Chassis Mounted Air Compressor
BP6 = Manuals
BP7 = Paint 
BP8= Technical Support
U = Projected Options Utilization Rate 

(Note: Based upon the consumption statistics, and the input provided by major Using Agencies, an educated and calculated assumption is made that an average purchaser, in an average purchase, will buy manufacturer's options worth 5% of the base Unit price. For example, a purchase that includes base Unit price of $20,000 is expected to also include $1000 worth of total manufacturer's options.)

Group Price Index Formula:

BP1*((1+U*(1-D1/100)))+BP2*((1+U*(1-D2/100)))+BP3*((1+U*(1-D3/100)))+BP4+BP5+BP6+BP7+BP8

Example:

Chassis Price = $100,000, Discount 10%
Utility Body Price = $10,000, Discount 10%
Hydraulic Platform Lift Price = $10,000, Discount 10%
$100 each for; Generator, Air Compressor, Manuals, Paint, Tech Support.

Formula Explanation:

Chassis Total Price = $100,000 (BP1) plus $4500 in options (5% * $100,000 = $5000, discounted 10%, = $4500) = $104,500
Stake Body Total Price = $10,000 (BP2) plus $450 in options (5% * $10,000 = $500, discounted 10%, = $4500) = $10,450
Hydraulic Platform Lift Total Price = $10,000 (BP3) plus $450 in options (5% * $10,000 = $500, discounted 10%, = $4500) = $10,450
Total Price of Other Options = $500

Grand Total = $125,900




[bookmark: _Toc118513841][bookmark: _Toc400531551][bookmark: _Toc428534023][bookmark: _Toc32310745][bookmark: _Toc108770431]QUOTE DISCREPANCIES
In evaluating Quotes, discrepancies between words and figures will be resolved in favor of words.  Discrepancies between Unit Prices and totals of Unit Prices will be resolved in favor of Unit Prices.  Discrepancies in the multiplication of units of work and Unit Prices will be resolved in favor of the Unit Prices.  Discrepancies between the indicated total of multiplied Unit Prices and units of work and the actual total will be resolved in favor of the actual total.  Discrepancies between the indicated sum of any column of figures and the correct sum thereof will be resolved in favor of the correct sum of the column of figures.

[bookmark: _Toc118513842][bookmark: _Toc400531553][bookmark: _Toc428534025][bookmark: _Toc32310747][bookmark: _Toc108770432]NEGOTIATION
In accordance with N.J.S.A. 52:34-12(f) and N.J.A.C. 17:12-2-7, after evaluating Quotes, the Procurement Bureau may establish a competitive range and enter into negotiations with one (1) Bidder or multiple Bidders within this competitive range.  The primary purpose of negotiations is to maximize the State’s ability to obtain the best value based on the mandatory requirements, evaluation criteria, and cost.  Multiple rounds of negotiations may be conducted with one (1) Bidder or multiple Bidders.  Negotiations will be structured by the Procurement Bureau to safeguard information and ensure that all Bidders are treated fairly.

Negotiations will be conducted only in those circumstances where it is deemed by the Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Bidder is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Contract award based on the content of the initial submission.  

If the Procurement Bureau contemplates negotiation, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Bidder will be publicly announced at the Quote opening.

[bookmark: _Toc108770433]BEST AND FINAL OFFER (BAFO) 
The Procurement Bureau may invite one (1) Bidder or multiple Bidders to submit a Best and Final Offer (BAFO). Said invitation will establish the time and place for submission of the BAFO. Any BAFO that does not result in more advantageous pricing to the State will not be considered, and the State will evaluate the Bidder’s most advantageous previously submitted pricing.

The Division may conduct more than one (1) round of BAFO in order to attain the best value for the State. 

BAFOs will be conducted only in those circumstances where it is deemed by the Procurement Bureau or Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Bidder is advised to submit its best technical and price Quote in response to this Bid Solicitation since the State may, after evaluation, make a Contract award based on the content of the initial submission 

If the Procurement Bureau contemplates BAFOs, Quote prices will not be publicly read at the Quote opening.  Only the name and address of each Bidder will be publicly announced at the Quote opening.

[bookmark: _Toc32310748][bookmark: _Toc108770434]“REQUEST FOR REVISION” WITHIN NJSTART
The State may request a revision of the Bidder’s Quote within NJSTART. The Bidder shall respond to the “Request for Revision” only for the reason(s) identified by the State. Any changes made by a Bidder to the Quote other than as requested by the State shall be considered null and void. 

[bookmark: _Toc400531554][bookmark: _Toc428534026][bookmark: _Toc32310749][bookmark: _Toc108770435]POOR PERFORMANCE
A Bidder with a history of performance problems may be bypassed for consideration of an award issued as a result of this Bid Solicitation. The following materials may be reviewed to determine Bidder performance:  
A. Contract cancellations for cause pursuant to State of New Jersey Standard Terms and Conditions Section 5.7(B); 
B. information contained in Vendor performance records; 
C. information obtained from audits or investigations conducted by a local, state or federal agency of the Bidder’s work experience; 
D. current licensure, registration, and/or certification status and relevant history thereof; or 
E. Bidder’s status or rating with established business/financial reporting services, as applicable.  

Bidders should note that this list is not exhaustive.

[bookmark: _Toc108770436]RECOMMENDATION FOR AWARD 
After the evaluation of the submitted Quotes is complete, the Procurement Bureau will recommend to the Director for award, the responsible Bidder(s) whose Quote, conforming to this Bid Solicitation, is most advantageous to the State, price and other factors considered.  The Director may accept, reject or modify the recommendation of the Procurement Bureau.
[bookmark: _Toc400531561][bookmark: _Toc428534033][bookmark: _Toc32310756][bookmark: _Toc108770437]CONTRACT AWARD
Contract award(s) will be made with reasonable promptness by written notice to those responsible Bidders, whose Quotes, conforming to this Bid Solicitation, is(are) most advantageous to the State, price, and other factors considered.  Any or all Quotes may be rejected when the State Treasurer or the Director determines that it is in the public interest to do so.

The State intends to make one (1) Statewide Contract award per cab and chassis on which the utility body, hydraulic platform lift, hydraulic generator and air compressor will be mounted, in accordance with Bid Solicitation Section 8.16. Example:  

· One (1) award for a Large Platform Truck mounted on a 2022 Model Year Kenworth T370  Cab and Chassis
· One (1) award for a Large Platform Truck mounted on a 2022 Model Year International MV 43100 Cab and Chassis
· One (1) award for a Large Platform Truck mounted on a 2022 Model Year Freightliner M2-106 Cab and Chassis



[bookmark: _Toc108770438]GLOSSARY
[bookmark: _CROSSWALK]
	NJSTART Term
	Equivalent Statutory, Regulatory and/or Legacy Term

	Bid/Bid Solicitation 
	Request For Proposal (RFP)/Solicitation

	Bid Amendment 
	Addendum

	Change Order 
	Contract Amendment

	Master Blanket Purchase Order (Blanket/Blanket P.O.) 
	Contract

	Offer and Acceptance Page
	Signatory Page

	Quote
	Proposal

	Vendor 
	Bidder/Contractor



Unless otherwise specified in the Bid Solicitation, the following definitions will be part of any Contract awarded, or order placed, as a result of this Bid Solicitation.  Note that not all definitions included here apply to all Bid Solicitations.
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Acceptance – The written confirmation by the Using Agency that Contractor has completed a Deliverable according to the specified requirements.

All-Inclusive Hourly Rate – An hourly rate comprised of all direct and indirect costs including, but not limited to: labor costs, overhead, fee or profit, clerical support, travel expenses, per diem, safety equipment, materials, supplies, managerial support and all documents, forms, and reproductions thereof.  This rate also includes portal-to-portal expenses as well as per diem expenses such as food.

Apparel - means any clothing, headwear, linens or fabric.  

Apparel Contracts - include all purchases, rentals or other acquisition of apparel products by the State of New Jersey, including authorizations by the State of New Jersey for vendors to sell apparel products through cash allowances or vouchers issued by the State of New Jersey, and license agreements with a public body.

Apparel Production - includes the cutting and manufacturing of apparel products performed by the vendor or by any subcontractors, but not including the production of supplies or sundries such as buttons, zippers, and thread.

Best and Final Offer or BAFO – Pricing timely submitted by a Bidder upon invitation by the Procurement Bureau after Quote opening, with or without prior discussion or negotiation.

Bid or Bid Solicitation – The documents which establish the bidding and Contract requirements and solicits Quotes to meet the needs of the Using Agencies as identified herein, and includes the Bid Solicitation, State of New Jersey Standard Terms and Conditions (SSTC), State Price Sheet, Attachments, and Bid Amendments.

Bid Amendment – Written clarification or revision to this Bid Solicitation issued by the Division. Bid Amendments, if any, will be issued prior to Quote opening.

Bid Opening Date – The date Quotes will be opened for evaluation and closed to further Quote submissions.
Bid Security - means a guarantee, in a form acceptable to the Division, that the bidder, if selected, will accept the contract as bid; otherwise, the bidder or, as applicable, its guarantor will be liable for the amount of the loss suffered by the State, which loss may be partially or completely recovered by the State in exercising its rights against the instrument of bid security.

Bidder – An entity offering a Quote in response to the Division’s Bid Solicitation.

Breach of Security – as defined by N.J.S.A. 56:8-161, means unauthorized access to electronic files, media, or data containing Personal Data that compromises the security, confidentiality, or integrity of Personal Data when access to the Personal Data has not been secured by encryption or by any other method or technology that renders the Personal Data unreadable or unusable.  Good faith acquisition of Personal Data by an employee or agent of the Provider for a legitimate business purpose is not a Breach of Security, provided that the Personal Data is not used for a purposes unrelated to the business or subject to further unauthorized disclosure.  

Business Day – Any weekday, excluding Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Calendar Day – Any day, including Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Change Order – An amendment, alteration, or modification of the terms of a Contract between the State and the Contractor(s). A Change Order is not effective until it is signed and approved in writing by the Director or Deputy Director, Division of Purchase and Property.

Commercial off the Shelf Software or COTS - Software provided by Provider that is commercially available and that can be used with little or no modification.


Customized Software - COTS that is adapted or configured by Provider to meet specific requirements of the Authorized Purchaser that differ from the standard requirements of the base product. For the avoidance of doubt, “Customized Software” is not permitted to be sold to the State under the scope of this Contract.

Contract – The Contract consists of the State of NJ Standard Terms and Conditions (SSTC), the Bid Solicitation, the responsive Quote submitted by a responsible Bidder as accepted by the State, the notice of award, any Best and Final Offer, any subsequent written document memorializing the agreement, any modifications to any of these documents approved by the State and any attachments, Bid Amendment or other supporting documents, or post-award documents including Change Orders agreed to by the State and the Contractor, in writing.

Contractor – The Bidder awarded a Contract resulting from this Bid Solicitation.

Cooperative Purchasing Program – The Division’s intrastate program that provides procurement-related assistance to New Jersey local governmental entities and boards of education, State and county colleges and other public entities having statutory authority to utilize select State Contract s issued by the Division, pursuant to the provisions of N.J.S.A. 52:25-16.1 et seq.

Cooperative Purchasing Participants - These participants include quasi-State entities, counties, municipalities, school districts, volunteer fire departments, first aid squads, independent institutions of higher learning, County colleges, and State colleges

Days After Receipt of Order (ARO) – The number of calendar days ‘After Receipt of Order’ in which the Using Agency will receive the ordered materials and/or services.

Dealer/Distributor – A Company authorized by a Bidder or Contractor as having the contractual ability to accept and fulfill orders and receive payments directly on behalf of the Contractor that is awarded a Contract.  Any authorized Dealer/Distributor must agree to all terms and conditions contained within the Bid Solicitation and must agree to provide all products and services in accordance with the Contract specifications, terms, conditions and pricing.  

Deliverable – Goods, products, Services and Work Product that Contractor is required to deliver to the State under the Contract.

Director – Director, Division of Purchase and Property, Department of the Treasury, who by statutory authority is the Chief Contracting Officer for the State of New Jersey; or the Director’s designee.

Disabled Veterans’ Business - means a business which has its principal place of business in the State, is independently owned and operated and at least 51% of which is owned and controlled by persons who are disabled veterans or a business which has its principal place of business in this State and has been officially verified by the United States Department of Veterans Affairs as a service disabled veteran-owned business for the purposes of department contracts pursuant to federal law.  N.J.S.A. 52:32-31.2.

Disabled Veterans’ Business Set-Aside Contract - means a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from disabled veterans’ businesses, or a portion of a Contract when that portion has been so designated.  N.J.S.A. 52:32-31.2.

Discount – The standard price reduction applied by the Bidder to all items.

Division – The Division of Purchase and Property.

Evaluation Committee – A group of individuals or a Division staff member assigned by the Director to review and evaluate Quotes submitted in response to this Bid Solicitation and recommend a Contract award to the Director.

Firm Fixed Price – A price that is all-inclusive of direct cost and indirect costs, including, but not limited to, direct labor costs, overhead, fee or profit, clerical support, equipment, materials, supplies, managerial (administrative) support, all documents, reports, forms, travel, reproduction and any other costs.

Hardware – Includes computer equipment and any Software provided with the Hardware that is necessary for the Hardware to operate.

Internet of Things (IoT) - the network of physical devices, vehicles, home appliances and other items embedded with electronics, software, sensors, actuators, and network connectivity which enables these objects to connect and exchange data.

Intrastate cooperative purchasing participants - refers to political subdivisions, volunteer fire departments and first aid squads, and independent institutions of higher education and school districts pursuant to N.J.S.A. 52:25-16.1 et seq., State and county colleges pursuant to N.J.S.A. 18A:64-60 and 18A:64A-25.9, quasi-State agencies and independent authorities pursuant to N.J.S.A. 52:27B-56.1, and other New Jersey public entities having statutory authority to utilize select State contracts issued by the Division

Joint Venture – A business undertaking by two (2) or more entities to share risk and responsibility for a specific project.


Life cycle assessment – The comprehensive examination of a product’s environmental and economic aspects and potential impacts throughout its lifetime, including raw material extraction, transportation, manufacturing, use and disposal.

Life cycle cost – The amortized total cost of a product, including capital costs, installation costs, operating costs, maintenance costs, and disposal costs discounted over the lifetime of the product.

Master Blanket Purchase Order (Blanket/Blanket P.O.) – A Term Contract that allows repeated purchases from an awarded contract.

Materials in Solid Waste – Material found in the various components of the solid waste stream. General, solid waste has several components, such as municipal solid waste (MSW), construction and demolition debris (C&D), and nonhazardous industrial waste.  Under RCRA Section 6002, EPA considers materials recovered from any component of the solid waste stream when designating items containing Recovered Materials.

May – Denotes that which is permissible or recommended, not mandatory.

Mobile Device - means any device used by Provider that can move or transmit data, including but not limited to laptops, hard drives, and flash drives.

Must – Denotes that which is a mandatory requirement.  

Net Purchases - means the total gross purchases, less credits, taxes, regulatory fees and separately stated shipping charges not included in unit prices, made by Intrastate Cooperative Purchasing Participants, regardless of whether or not NJSTART is used as part of the purchase process.

No Bid – The Bidder is not submitting a price Quote for an item on a price line.

No Charge – The Bidder will supply an item on a price line free of charge.

Non-Public Data - means data, other than Personal Data, that is not subject to distribution to the public as public information. Non-Public Data is data that is identified by the State as non-public information or otherwise deemed to be sensitive and confidential by the State because it contains information that is exempt by statute, ordinance or administrative rule from access by the general public as public information.

Percentage Discount or Markup - The percentage bid applied as a Markup or a Discount to a firm, fixed price contained within a price list/catalog. 

Performance Security - means a guarantee, executed subsequent to award, in a form acceptable to the Division, that the successful bidder will complete the contract as agreed and that the State will be protected from loss in the event the contractor fails to complete the contract as agreed.

Personal Data means – 
“Personal Information” as defined in N.J.S.A. 56:8-161, means an individual’s first name or first initial and last name linked with any one or more of the following data elements: (1) Social Security number, (2) driver’s license number or State identification card number or (3) account number or credit or debit card number, in combination with any required security code, access code, or password that would permit access to an individual’s financial account.  Dissociated data that, if linked would constitute Personal Information is Personal Information if the means to link the dissociated were accessed in connection with access to the dissociated data.  Personal Information shall not include publicly available information that is lawfully made available to the general public from federal, state or local government records, or widely distributed media; and/or 

Data, either alone or in combination with other data, that includes information relating to an individual that identifies the person or entity by name, identifying number, mark or description that can be readily associated with a particular individual and which is not a public record, including but not limited to, Personally Identifiable Information (PII); government-issued identification numbers (e.g., Social Security, driver’s license, passport); Protected Health Information (PHI) as that term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and defined below; and Education Records, as that term is defined in the Family Educational Rights and Privacy Act (FERPA), 20 U.S.C. § 1232g.

Personally Identifiable Information or PII - as defined by the U.S. Department of Commerce, National Institute of Standards and Technology, means any information about an individual maintained by an agency, including (1) any information that can be used to distinguish or trace an individual’s identity, such as name, social security number, date and place of birth, mother’s maiden name, or biometric records; and (2) any other information that is linked or linkable to an individual, such as medical, educational, financial, and employment information.

Post-Consumer Material – Material or finished product that has served its intended use and has been diverted or recovered from waste destined for disposal, having completed its life as a consumer item.  Post-Consumer Materials are part of the broader category of Recovered Materials.

Pre-Consumer Material – Materials generated in manufacturing and converting processes, such as manufacturing scrap and trimmings/cuttings.

Price List/Catalog – A document published by a manufacturer, resellers, Dealers, or Distributors that typically contains product descriptions, a list of products with fixed prices to which a Bidder’s percentage discount or markup bid is applied. 

Primary Form – An electronic form contained within a Vendor’s NJSTART profile designated by the Vendor as the primary or principal version of the required form.

Procurement Bureau (Bureau) – The Division unit responsible for the preparation, advertisement, and issuance of Bid Solicitations, for the tabulation of Quotes and for recommending award(s) of Contract(s) to the Director and the Deputy Director.

Project – The undertakings or services that are the subject of this Bid Solicitation.

Protected Health Information or PHI - has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 means Individually Identifiable Health Information (as defined below) transmitted by electronic media, maintained in electronic media, or transmitted or maintained in any other form or medium. PHI excludes education records covered by the Family Educational Rights and Privacy Act (FERPA), as amended, 20 U.S.C. 1232g, records described at 20 U.S.C. 1232g(a)(4)(B)(iv) and employment records held by a covered entity in its role as employer. The term “Individually Identifiable Health Information” has the same meaning as the term is defined in the regulations adopted pursuant to the Health Insurance Portability and Accountability Act of 1996, P.L. No. 104-191 (1996) and found in 45 CFR Parts 160 to 164 and means information that is a subset of Protected Health Information, including demographic information collected from an individual, and (1) is created or received by a health care provider, health plan, employer or health care clearinghouse; and (2) relates to the past, present or future physical or mental health or condition of an individual; the provision of health care to an individual; or the past, present or future payment for the provision of health care to an individual; and (a) that identifies the individual; or (b) with respect to which there is a reasonable basis to believe the information can be used to identify the individual.

Quasi-State Agency - is any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member, as defined in N.J.S.A. 52:27B-56.1, provided that any sale to any such bi-state governmental entity is for use solely within the State of New Jersey.

Quick Reference Guides (QRGs) – Informational documents which provide Vendors with step-by-step instructions to navigate the NJSTART eProcurement System. QRGs are available on the NJSTART Vendor Support Page.

Quote – Bidder’s timely response to the Bid Solicitation including, but not limited to, technical Quote, price Quote including Best and Final Offer, any licenses, forms, certifications, clarifications, negotiated documents, and/or other documentation required by the Bid Solicitation.

Quote Opening Date - The date Quotes will be opened for evaluation and closed to further Quote submissions.

Recovered Material – Waste material and byproduct that have been recovered or diverted from solid waste, but does not include materials and byproducts generated from, and commonly reused within, an original manufacturing process.

Recycling – The series of activities, including collection, separation, and processing, by which products or other materials are recovered from the solid waste stream for use in the form of raw materials in the manufacture of new products other than fuel for producing heat or power by combustion.
Recyclability – The ability of a product or material to be recovered from, or otherwise diverted from, the solid waste stream for the purpose of recycling.

Retainage – The amount withheld from the Contractor payment that is retained and subsequently released upon satisfactory completion of performance milestones by the Contractor.

Revision – A response to a BAFO request or a requested clarification of the Bidder’s Quote. 

RMAN – Recovered Materials Advisory Notices provide purchasing guidance and recommendations for Recovered and Post-Consumer Material content levels for designated items. 

Security Incident - means the potential access by non-authorized person(s) to Personal Data or Non-Public Data that the Provider believes could reasonably result in the use, disclosure, or access or theft of State’s unencrypted Personal Data or Non-Public Data within the possession or control of the Provider. A Security Incident may or may not turn into a Breach of Security.

Services – Includes, without limitation (i) Information Technology (IT) professional services, (ii) Software and Hardware-related services, including without limitation, installation, configuration, and training, and (iii) Software and Hardware maintenance and support and/or Software and Hardware technical support services. 




Shall – Denotes that which is a mandatory requirement.  

Should – Denotes that which is permissible or recommended, not mandatory.

Small Business – Pursuant to N.J.S.A. 52:32-19, N.J.A.C. 17:13-1.2, and N.J.A.C. 17:13-2.1, “small business” means a business that meets the requirements and definitions of “small business” and has applied for and been approved by the New Jersey Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit as (i) independently owned and operated, (ii) incorporated or registered in and has its principal place of business in the State of New Jersey; (iii)  has 100 or fewer full-time employees; and has gross revenues falling in one (1) of the six (6) following categories:  
For goods and services - (A) 0 to $500,000 (Category I); (B) $500,001 to $5,000,000 (Category II); and (C) $5,000,001 to $12,000,000, or the applicable federal revenue standards established at 13 CFR 121.201, whichever is higher (Category III). 
For construction services: (A) 0 to $3,000,000 (Category IV); (B) gross revenues that do not exceed 50 percent of the applicable annual revenue standards established at 13 CFR 121.201 (Category V); and (C) gross revenues that do not exceed the applicable annual revenue standards established at CFR 121.201, (Category VI).

Small Business Set-Aside Contract – means (1) a Contract for goods, equipment, construction or services which is designated as a Contract with respect to which bids are invited and accepted only from small businesses, or (2) a portion of a Contract when that portion has been so designated.”  N.J.S.A. 52:32-19.

Software - means, without limitation, computer programs, source codes, routines, or subroutines supplied by Provider, including operating software, programming aids, application programs, application programming interfaces and software products, and includes COTS, unless the context indicates otherwise.  

Software as a Service or SaaS - means the capability provided to a purchaser to use the Provider’s applications running on a cloud infrastructure. The applications are accessible from various client devices through a thin client interface such as a Web browser (e.g., Web-based email) or a program interface. The purchaser does not manage or control the underlying cloud infrastructure, including network, servers, operating systems, storage or even individual application capabilities, with the possible exception of limited user-specific application configuration settings.

State – The State of New Jersey.

State Confidential Information - shall consist of State Data and State Intellectual Property  supplied by the State, any information or data gathered by the Contractor in fulfillment of the Contract and any analysis thereof (whether in fulfillment of the Contract or not);

State Contract Manager or SCM – The individual, responsible for the approval of all deliverables, i.e., tasks, sub-tasks or other work elements in the Scope of Work.  The SCM cannot direct or approve a Change Order.

State Data - means all data and metadata created or in any way originating with the State, and all data that is the output of computer processing of or other electronic manipulation of any data that was created by or in any way originated with the State, whether such data or output is stored on the State’s hardware, the Provider’s hardware or exists in any system owned, maintained or otherwise controlled by the State or by the Provider.  State Data includes Personal Data and Non-Public Data.

State Intellectual Property – Any intellectual property that is owned by the State.  State Intellectual Property includes any derivative works and compilations of any State Intellectual Property.

State-Supplied Price Sheet – the bidding document created by the State and attached to this Bid Solicitation on which the Bidder submits its Quote pricing as is referenced and described in the Bid Solicitation.   

Subtasks – Detailed activities that comprise the actual performance of a task.

Subcontractor – An entity having an arrangement with a Contractor, whereby the Contractor uses the products and/or services of that entity to fulfill some of its obligations under its State Contract, while retaining full responsibility for the performance of all  Contractor's obligations under the Contract, including payment to the Subcontractor.  The Subcontractor has no legal relationship with the State, only with the Contractor.

Task – A discrete unit of work to be performed.

Third Party Intellectual Property – Any intellectual property owned by parties other than the State or Contractor and contained in or necessary for the use of the Deliverables.  Third Party Intellectual Property includes COTS owned by Third Parties, and derivative works and compilations of any Third Party Intellectual Property. 

Unit Cost or Unit Price – All-inclusive, firm fixed price charged by the Bidder for a single unit identified on a price line.

US CERT – United States Computer Emergency Readiness Team.

USEPA – United States Environmental Protection Agency

Using Agency[ies] – A State department or agency, a quasi-State governmental entity, or an Intrastate Cooperative Purchasing participant, authorized to purchase products and/or services under a Contract procured by the Division. 

Vendor – Either the Bidder or the Contractor.

Vendor Intellectual Property – Any intellectual property that is owned by Contractor and contained in or necessary for the use of the Deliverables or which the Contractor makes available for the State to use as part of the work under the Contract Vendor Intellectual Property includes COTS or Customized Software owned by Contractor, Contractor’s technical documentation, and derivative works and compilations of any Vendor Intellectual Property.

Work Product – Every invention, modification, discovery, design, development, customization, configuration, improvement, process, Software program, work of authorship, documentation, formula, datum, technique, know how, secret, or intellectual property right whatsoever or any interest therein (whether patentable or not patentable or registerable under copyright or similar statutes or subject to analogous protection) that is specifically made, conceived, discovered, or reduced to practice by Contractor or Contractor’s subcontractors or a third party engaged by Contractor or its subcontractor pursuant to the Contract Notwithstanding anything to the contrary in the preceding sentence, Work Product does not include State Intellectual Property, Vendor  Intellectual Property or Third Party Intellectual Property. 
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Price 

Line

Item Description Quantity

Unit of 

Measure

Unit Price                          

(Required)

Make                                 

(Required)

1

 33,000 LB. GVWR Heavy Duty 

Truck Chassis, 4WD, as 

specified in Section 4.4.1 of 

the Bid Solicitation.

1 Each

$50,000.00 Kenworth

2

Vehicle Manufacturer’s 

Options (Discount Only), as 

specified in Section 4.4.2 of 

the Bid Solicitation. 

1 Percent

-5%

3

Utility Body, as specified in 

Section 4.4.3 of the Bid 

Solicitation. 

1 Each

$20,000.00

Utility Body of 

America

4

Utility Body Manufacturer’s 

Options (Discount or Markup), 

as specified in Section 4.4.4 of 

the Bid Solicitation. 

1 Percent

+10%

5

Hydraulic Platform Lift, as 

specified in Section 4.4.5 of 

the Bid Solicitation. 

1 Each

$10,000.00 Aero-Lift

6

Hydraulic Platform Lift 

Manufacturer’s Options 

(Discount or Markup), as 

specified in Section 4.4.6 of 

the Bid Solicitation. 

1 Percent

-15%



22DPP00728 STATE-SUPPLIED PRICE SHEET 

T2877- Large Platform Truck, 33, 000 L.B. GVWR Heavy Duty Truck Chassis, 4WD With Service Body, Hydraulic Platform and Accessories.

We Sell Trucks LLC. Vendor {Bidder} Name:



Model                                        

(Required)

365 Calendar Days ARO

Delivery Days ARO (Completed Unit):

Model Year                          

(Required)

T370



2022



UTB-2022
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