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March 22, 2017


To: All Interested Vendors {Bidders} 


Re:  Bid Solicitation {RFP} # 17DPP00116
        Heavy Duty Regenerative Air Street Sweeper With Twin Brooms, Mounted on 
        Truck Chassis (T-3074)

       Quote {Proposal} Submission Due Date: March 29, 2017 (2:00 p.m. ET)
       Revised: Quote {Proposal} Submission Due Date: April 11, 2017 (2:00 p.m. ET)


Bid Amendment {Addendum} #01


The following constitutes Bid Amendment {Addendum} #01 to the above referenced Bid Solicitation {RFP}:
  
· This Bid Amendment {Addendum} includes answers to questions and revisions to the Bid Solicitation {RFP}. 

· Please note that the {Proposal} Submission Due Date has been changed from March 29, 2017 to April 4, 2017.

It is the sole responsibility of the Vendor {Bidder} to be knowledgeable of all of the additions, deletions, clarifications, and modifications to the Bid Solicitation {RFP} and/or the New Jersey Standard Terms and Conditions relative to this Bid Solicitation {RFP} as set forth in all Bid Amendments {Addenda}. 

All other instructions, terms, and conditions of the Bid Solicitation {RFP} shall remain the same.



Heavy Duty Regenerative Air Street Sweeper with Twin Brooms, Mounted on Truck Chassis 
Bid Solicitation {RFP} Number: 17DPP00116

Answers to Questions

Note: Some of the questions have been paraphrased in the interest of readability and clarity.  Each question is referenced by the appropriate Bid Solicitation {RFP} page number(s) and section where applicable.  

	#
	Page #
	RFP Section Reference
	Question (Bolded) and Answer

	1
	
	
	Submitting No Bid: Could you please provide us with information on how to submit a “No Bid Letter” for this bid”

A No-Bid Letter is not required. A Bidder can simply opt not to bid on this procurement.

	2
	18
	Section 3.3.5.1 Finish:
	Is white to be the required color?

Yes, for NJDOT Units only.

	3
	19
	Section 3.4.1
	Can parking garage be changed to " Highways, Interstates, Etc? Due to height of sweeper.

See the revised Bid Solicitation {RFP} specification  Section 3.4.1.


	4
	19
	Section 3.4.1.1 Wheel Base
	Can the wheelbase be changed to read "158 to 185"? To allow our standard engineered chassis design be acceptable.

See the revised Bid Solicitation {RFP} specification  Section 3.4.1.1.

	5
	20
	Section 3.4.1.1 Rear Suspension
	Can the specifications be modified to detail air ride suspension as required to add stability and safety when driving and dumping?

See the revised Bid Solicitation {RFP}  specification  Section 3.4.1.1.

	6
	19
	Section 3.4.1.1 Cab: Seats
	We recommend dual air ride seats be required to assure safe, comfortable,operations. Will you modify specifications to require air ride seats of all bidders.

See the revised Bid Solicitation {RFP} specification  Section 3.4.1.1.

	7
	19
	Section 3.4.1.1. Horn
	We recommend an air horn be required for operator and pedestrian safety. Will the NJDOT modify the specifications to require all bidders supply air horn on chassis.

See the revised Bid Solicitation {RFP} specification Section  3.4.1.1.

	8
	19
	Section 3.4.1.1 Cab: Mirrors
	We recommend the power/heated mirrors be specified for increased visibility from either side of sweeper for improved safety and operation. Will be NJDOT modify specifications to require power/heated mirrors of all bidders.

See the revised Bid Solicitation {RFP} specification  Section 3.4.1.1.



	9
	20
	Section 3.4.1.1 Cab Tilt Steering Wheel
	We recommend tilt steering wheels be required for comfortable, efficient, safe operation of sweeper from either side  for operators of different sizes. Will be NJDOT modify specifications for all bidders to require dual tilt steering wheels.

See the revised Bid Solicitation {RFP} specification  Section 3.4.1.1

	10
	19
	Section 3.4.1.1 Cab: Windows
	We recommend that power windows and door locks be specified to enhance safe communication. Will the NJDOT modify specifications to require power windows and door locks from all bidders.

See the revised  Bid Solicitation {RFP} specification  Section 3.4.1.1.

	11
	20
	Section 3.4.1.1 Cab & Chassis
	We recommend the requirement of a master battery disconnect switch. Will the NJDOT modify specifications to require a master electrical disconnect switch from all bidders.

See the revised Bid Solicitation {RFP} specification  Section 3.4.1.1.

	12
	20
	Section 3.4.1.2 Cab & Chassis Engine
	We recommend the requirement of a higher horse power diesel engine for highway speeds when loaded. Will the NJDOT modify specifications to require 260 HP from all bidders.

The specification will not be revised. 

	13
	24
	Section 3.4.1.8 Puck up Head
	Our demonstration unit had pickup head front curtain lifter on it to enhance operation when sweeping bulky materials. Will the NJDOT modify specifications to require curtain head lifter from all bidders.

The specification will not be revised.  Optional equipment may be offered.  See Section 3.4.5 of the Bid Solicitation {RFP}.

	14
	25
	Section 3.4.1.11 Hopper
	We recommend the inclusion of a hopper screen vibrator to keep sweeper screens clear of material while production sweeping. Will the NJDOT modify specifications to require hopper screen vibrator from all bidders.

The specification will not be revised. Optional equipment may be offered.  See Section 3.4.5 of the Bid Solicitation {RFP}.

	15
	25
	Section 3.4.1.11 Hopper
	We recommend the use of a free floating dump chute to reduce damage and down time caused by rigid dump chute contacting dump target. Will the NJDOT modify specifications to require floating stainless steel dump chute from all bidders.

The specification will not be revised. Optional equipment may be offered.  See Section 3.4.5 of the Bid Solicitation {RFP}.

	16
	25
	Section 3.4.1.11 Hopper
	We recommend the mandatory use of dual stabilizers before hopper raises to dump for added stability and safety. Will the NJDOT modify specifications to require dual stabilizers to deploy prior to hopper raising from all bidders.

The specification will not be revised. Optional equipment may be offered.  See specification Section 3.4.5.

	17
	25
	Section 3.4.1.12 Blower
	We recommend the blower shut off when dumping to eliminate exposed blower wheel and blowing dust during dump cycle for safety. This shall be accomplished utilizing diesel powered hydraulics not electric hydraulic system. Will NJDOT modify specifications to require all bidders to provide a blower disengage system during dump cycles to ensure safety of anyone around sweeper when dumping.

The specification will not be revised. Optional equipment may be offered.  See Section 3.4.5 of the Bid Solicitation {RFP}..

	18
	25
	Section 3.4.1.11 Hopper
	We recommend the use of a free floating dump chute to reduce damage and down time caused by rigid dump chute contacting dump target. Will the NJDOT modify specifications to require floating stainless steel dump chute from all bidders.

See answer to question #15.

	19
	25
	Section 3.4.1.11 Hopper
	We recommend the mandatory use of dual stabilizers before hopper raises to dump for added stability and safety. Will the NJDOT modify specifications to require dual stabilizers to deploy prior to hopper raising from all bidders.

See answer to question #16.

	20
	25
	Section 3.4.1.12 Blower
	We recommend the blower shut off when dumping to eliminate exposed blower wheel and blowing dust during dump cycle for safety. This shall be accomplished utilizing diesel powered hydraulics not electric hydraulic system. Will NJDOT modify specifications to require all bidders to provide a blower disengage system during dump cycles to ensure safety of anyone around sweeper when dumping.

See answer to question  #17.

	21
	25 and 56
	Section 1.1 
and Section 7.2 
	How many awards will be made?

The State intends to make one Blanket P.O. {Contract} award for each Make/Model  that meets the specifications. 
















	#
	Page #
	RFP Section Reference
	Question (Bolded) and Answer

	22     
	
	4.4.1.2.1
Ownership Disclosure Form
	Are limited liability companies required to comply with the ownership disclosure requirements?

Yes.  Section 4.4.1.2.1 has been revised as follows:

“Pursuant to N.J.S.A. 52:25-24.2, in the event the Vendor {Bidder} is a corporation, partnership or sole proprietorship limited liability company, the Vendor {Bidder} must complete an Ownership Disclosure Form.”  

Please see the revised RFP entitled “T3074 17DPP00116 Sweeper Rev RFP March 23, 2017.”

Please note that a revised Ownership Disclosure Form has been uploaded to the Division’s Website.

	23
	
	4.4.1.2.1
Ownership Disclosure Form
	Are there any other methods by which a publically traded entity may comply with the ownership disclosure requirements?

Yes.  The following language has been added to the RFP Section 4.4.1.2.1:

“In the alternative, to comply with this section, a Vendor {Bidder} with any direct or indirect parent entity which is publicly traded may submit the name and address of each publicly traded entity and the name and address of each person that holds a 10 percent or greater beneficial interest in the publicly traded entity as of the last annual filing with the federal Securities and Exchange Commission or the foreign equivalent, and, if there is any person that holds a 10 percent or greater beneficial interest, also shall submit links to the websites containing the last annual filings with the federal Securities and Exchange Commission or the foreign equivalent and the relevant page numbers of the filings that contain the information on each person that holds a 10 percent or greater beneficial interest. N.J.S.A. 52:25-24.2.”

Please see the revised RFP entitled “T3074 17DPP00116 Sweeper Rev RFP March 23, 2017.”

Please note that a revised Ownership Disclosure Form has been uploaded to the Division’s Website.

	24
	
	9.0
State of NJ Terms & Conditions

Section 2.3
Prevailing Wage Act
	Is the citation of the New Jersey Prevailing Wage Act in Section 2.3 of the Standard Terms and Conditions correct?

The citation in Section 2.3 of the Standard Terms and Conditions has been revised as follows:

“The New Jersey Prevailing Wage Act, N.J.S.A. 34: 11-56.265 et seq. is hereby made part of every contract entered into on behalf of the State of New Jersey through the Division of Purchase and Property, except those contracts which are not within the contemplation of the Act. The bidder's signature on [this proposal] is his guarantee that neither he nor any subcontractors he might employ to perform the work covered by [this proposal] has been suspended or debarred by the Commissioner, Department of Labor and Workforce Development for violation of the provisions of the Prevailing Wage Act and/or the Public Works Contractor Registration Acts; the bidder’s signature on the proposal is also his guarantee that he and any subcontractors he might employ to perform the work covered by [this proposal] shall comply with the provisions of the Prevailing Wage and Public Works Contractor Registration Acts, where required.” 

[bookmark: _GoBack]Please see the revised RFP entitled “T3074 17DPP00116 Sweeper Rev RFP March 23, 2017.”
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