



                                                          




Bid Solicitation/Request for Proposal
Bid #	17DPP00105
	For:
	T-3063 - Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Optional Hook Lift System, Various Bodies, Salt Spreader, Snow Plow & Accessories 


                                                                                                        
	Event
	Date
	Time

	Vendor’s {Bidder’s} Electronic Question Due Date
(Refer to Bid Solicitation {RFP} Section 1.3.1 for more information.)
	3/16/17
	2:00 PM

	Mandatory/Optional Pre-Quote {Proposal} Conference 
(Refer to Bid Solicitation {RFP} Section 1.3.6 for more information.)
	N/A
	N/A

	Mandatory/Optional Site Visit
(Refer to Bid Solicitation {RFP} Section 1.3.5 for more information.)
	
N/A
	
N/A

	Quote {Proposal} Submission Date
(Refer to Bid Solicitation {RFP} Section 1.3.2 for more information.)
	3/30/17
	2:00 PM



Dates are subject to change.  All times contained in the Bid Solicitation {RFP} refer to Eastern Time. All changes will be reflected in Bid Amendments {Addenda} to the Bid Solicitation {RFP} posted on the Division of Purchase and Property website and on www.njstart.gov.

	Small Business
Set-Aside
	Status
[bookmark: Check1]|X|  Not Applicable

|_|  Entire Blanket P.O. {Contract}

[bookmark: Check7]|_|  Partial Blanket P.O. {Contract}

|_|  Subcontracting Only
	Category

 |_|   I     

 |_|   II    

 |_|   III   




Bid Solicitation {RFP} Issued By			Using Agency/Agencies

State of New Jersey				State of New Jersey
Department of the Treasury			Cooperative Purchasing Program Participants 
Division of Purchase and Property		
Trenton, New Jersey 08625‑0230 			

Date:  2/24/17
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[bookmark: _Toc428533936][bookmark: _Toc475717156] INFORMATION FOR VENDORS {BIDDERS}

NOTICE: This Bid Solicitation {Request for Proposal (RFP)} is part of the NJSTART Procurement Program. The Vendor {Bidder} is advised to thoroughly read all sections, as many have been revised, and follow all instructions contained in this Bid Solicitation {RFP}, including the instructions on the Bid Solicitation’s {RFP’s} Offer and Acceptance Page {Signatory Page} and read through all Quick Reference Guides (QRGs) located on the NJSTART Vendor Support Page (http://www.state.nj.us/treasury/purchase/njstart/vendor.shtml), in preparing and submitting its Quote {Proposal}.

Terminology is listed by new NJSTART term; {existing term} appears in braces.

0. [bookmark: _Toc400531467][bookmark: _Toc428533937][bookmark: _Toc475717157]PURPOSE AND INTENT

This Bid Solicitation {RFP} is issued by the Procurement Bureau, Division of Purchase and Property (Division), Department of the Treasury on behalf of the Department of Transportation (DOT), the State Agencies and Cooperative Purchasing Program participants. The purpose of this Bid Solicitation {RFP} is to solicit Quotes {Proposals} for the purchase of a new specified unit. (See Section 2.0 Definitions.)  

The intent of this Bid Solicitation {RFP} is to award a Master Blanket Purchase Order (Blanket P.O.) {Contract} to that responsible Vendor {Bidder} whose Quote {Proposal}, conforming to this Bid Solicitation {RFP} is most advantageous to the State, price and other factors considered. The State may award any and all price lines. The State, however, reserves the right to separately procure individual requirements that are the subject of the Blanket P.O. {Contract} during the Blanket P.O. {Contract} term, when deemed by the the Director of the Division of Purchase and Property (Director) to be in the State’s best interest.

There are sixteen (16) price lines, which are itemized in Section 3.4 Vehicle Specification of this Bid Solicitation {RFP}.  Price lines 1 through 16 are grouped to create a single award.  Vendors {Bidders} must bid on all price line items in the group (price lines 1 through 16) to be eligible for a Blanket P.O. {Contract} award. 

The State of NJ Standard Terms and Conditions (SSTC) accompanying this Bid Solicitation {RFP} will apply to all Blanket P.O.s {Contracts} made with the State of New Jersey.  These terms are in addition to the terms and conditions set forth in this Bid Solicitation {RFP} and should be read in conjunction with them unless the Bid Solicitation {RFP} specifically indicates otherwise.  

The State of New Jersey (State) intends to extend the Blanket P.O. {Contract} awarded to the Division's Cooperative Purchasing Program participants.  These participants include quasi-state agencies, counties, municipalities, school districts, volunteer fire departments, first aid squads, independent institutions of higher learning, County colleges and State colleges.  In order for the State Blanket P.O. {Contract} to be extended to Cooperative Purchasing Program participants, the Vendor {Bidder} must agree to the extension by executing the Cooperative Purchase Form.  Also refer to Section 4.4.6 of this Bid Solicitation {RFP}. Although the State, with the consent of the Vendor(s) {Bidder(s)}, is making the use of any Blanket P.O. {Contract} resulting from this Bid Solicitation {RFP} available to non-State Agencies, the State makes no representation as to the acceptability of any State Bid Solicitation {RFP} terms and conditions under the Local Public Contracts Law or any other enabling statute or regulation.




[bookmark: _Toc400531468][bookmark: _Toc428533938][bookmark: _Toc475717158]BACKGROUND 

This is the first time that a Bid Solicitation {RFP} has been developed to establish a term Blanket P.O. {Contract} for the specified unit.
 
[bookmark: _Toc428533939][bookmark: _Toc475717159]Key Events

[bookmark: _1.3.1_ELECTRONIC_QUESTION_AND_ANSWE][bookmark: _Toc428533940][bookmark: _Toc475717160]ELECTRONIC QUESTION AND ANSWER PERIOD

The Division will electronically accept questions and inquiries from all potential Vendors {Bidders} via the “Q&A” Tab of the Bid Solicitation {RFP} in NJSTART. 

a. Questions should be directly tied to the Bid Solicitation {RFP} and asked in consecutive order, from beginning to end, following the organization of the Bid Solicitation {RFP}; and  

b. Each question should begin by referencing the Bid Solicitation {RFP} page number and section number to which it relates.

Vendors {Bidders} may refer to the QRG “Submit a Quote” for additional instruction. QRGs are located on the NJSTART Vendor Support Page.  

A Vendor {Bidder} must not contact the Using Agency and/or the Procurement Specialist directly, in person, by telephone or by e-mail, concerning this Bid Solicitation {RFP}.

The cut-off date for electronic questions and inquiries relating to this Bid Solicitation {RFP} is indicated on the Bid Solicitation {RFP} cover sheet.  In the event that questions are posed by Vendors {Bidders}, answers to such questions will be issued by Bid Amendment {Addendum}.  Any Bid Amendment {Addendum} to this Bid Solicitation {RFP} will become part of this Bid Solicitation {RFP} and part of any Blanket P.O. {Contract} awarded as a result of this Bid Solicitation {RFP}. Bid Amendments {Addenda} to this Bid Solicitation {RFP}, if any, will be posted as a File Attachment on the “Summary” page of the Bid Solicitation {RFP} in NJSTART after the cut-off date.  (See Bid Solicitation {RFP} Section 1.4.1 for further information.)
[bookmark: _1.3.3__Mandatory_Pre-Bid_Conference][bookmark: _1.3.5__SUBMISSION_OF_BID_PROPOSAL][bookmark: _1.3.2_SUBMISSION_OF_BID_PROPOSAL]
EXCEPTIONS TO THE STATE OF NJ STANDARD TERMS AND CONDITIONS (SSTC)

Questions regarding the SSTC and exceptions to mandatory requirements must be posed during this Electronic Question and Answer period and shall contain the Vendor’s {Bidder’s} suggested changes and the reason(s) for the suggested changes.

[bookmark: _Toc428533941][bookmark: _Toc475717161]SUBMISSION OF QUOTES {PROPOSALS}

In order to be considered for award, the Quote {Proposal} must be received by the Procurement Bureau of the Division at the appropriate location by the required time.  Vendors {Bidders} shall submit a Quote {Proposal} either electronically through NJSTART or via hard copy. 

Hard copy Quote {Proposal} must be submitted to the physical location noted below: 

PROPOSAL RECEIVING ROOM – 9TH FLOOR
DIVISION OF PURCHASE AND PROPERTY
DEPARTMENT OF THE TREASURY
33 WEST STATE STREET, P.O. BOX 230
TRENTON, NJ 08625-0230

Directions to the Division are available on the web at http://www.state.nj.us/treasury/purchase/directions.shtml.

QUOTES {PROPOSALS} NOT RECEIVED PRIOR TO THE QUOTE {PROPOSAL} OPENING DEADLINE SHALL BE REJECTED.  THE DATE AND TIME OF THE QUOTE {PROPOSAL} OPENING ARE INDICATED ON THE BID SOLICITATION {RFP} COVER SHEET AND IN THE “SUMMARY” PAGE OF THE BID SOLICITATION {RFP} IN NJSTART. 

Note:  A Vendor {Bidder} using U.S. Postal Service regular or express mail services should allow additional time since the U.S. Postal Service does not deliver directly to the Quote {Proposal}  Receiving Room. A Vendor {Bidder} should make every effort to submit its Quote {Proposal} well ahead of the Quote {Proposal} submission deadline to mitigate unforeseen delays or issues.  The Vendor {Bidder} is solely responsible for the timely submission of its Quote {Proposal} in response to this Bid Solicitation {RFP}.

Procedural inquiries concerning this Bid Solicitation {RFP} may be directed to njstart@treas.nj.gov and/or (609) 341-3500.  The State will not respond to substantive questions related to the Bid Solicitation {RFP} or any other Blanket P.O. {Contract} via this e-mail address or phone number.

[bookmark: _Toc428533942][bookmark: _Toc475717162]NJSTART

The Division is pleased to announce its new eProcurement solution “[image: cid:image001.jpg@01CF740E.F15E7FA0] .” 

Vendor {Bidder} Support:

Vendors {Bidders} are strongly encouraged to visit the NJSTART Vendor Support Page, which contains Quick Reference Guides (QRGs), supporting videos, a glossary of NJSTART terms, and helpdesk contact information.  

The Vendor {Bidder} should utilize the QRGs before attempting to submit its Quote {Proposal} using the NJSTART process.   It is the Vendor’s {Bidder’s} responsibility to ensure that the NJSTART Quote {Proposal} and attachments have been properly submitted.

[bookmark: _Toc428533943][bookmark: _Toc475717163]ELECTRONIC SIGNATURES

Vendors {Bidders} submitting Quotes {Proposals} through NJSTART may sign the forms listed in Section 4.4.1 (Forms, Registrations and Certifications Required with Quote {Proposal}) and Section 4.4.2 (Forms, Registrations and Certifications Required Before Blanket P.O. {Contract} Award and That Should Be Submitted with the Quote {Proposal}) of this Bid Solicitation {RFP} electronically by typing the name of the authorized signatory in the “Signature” block, or as an alternative downloading, physically signing the form, scanning the form, and uploading the form to NJSTART. 

Vendors {Bidders} submitting Quotes {Proposals} in hard copy format, must provide forms with original, physical signatures, otherwise its Quote {Proposal} may be deemed non-responsive.

[bookmark: _1.3.4_MANDATORY/OPTIONAL_SITE][bookmark: _1.3.45_MANDATORY/OPTIONAL_SITE][bookmark: _Toc224543885][bookmark: _Toc238623352][bookmark: _Toc400531474][bookmark: _Toc428533944][bookmark: _Toc475717164]MANDATORY/OPTIONAL SITE VISIT

Not applicable to this procurement.

[bookmark: _1.3.5__MANDATORY/OPTIONAL][bookmark: _1.3.6__MANDATORY/OPTIONAL][bookmark: _Toc224543888][bookmark: _Toc238623354][bookmark: _Toc428533945][bookmark: _Toc475717165]MANDATORY/OPTIONAL PRE-QUOTE {PROPOSAL} CONFERENCE

[bookmark: _Toc95619434][bookmark: _Toc109701220][bookmark: _Toc225321579][bookmark: _Toc94946029][bookmark: _Toc72744593]Not applicable to this procurement.





[bookmark: _Toc400531476][bookmark: _Toc428533946][bookmark: _Toc475717166]PRE-QUOTE {PROPOSAL} DOCUMENT REVIEW 

Not applicable to this procurement.

[bookmark: _Toc428533947][bookmark: _Toc475717167]ADDITIONAL Information

[bookmark: _Toc428533948][bookmark: _Toc475717168]BID AMENDMENTS {ADDENDA}: Revisions to this BID SOLICITATION {RFP}

In the event that it becomes necessary to clarify or revise this Bid Solicitation {RFP}, such clarification or revision will be by Bid Amendment {Addendum}.  Any Bid Amendment {Addendum} to this Bid Solicitation {RFP} will become part of this Bid Solicitation {RFP} and part of any Blanket P.O. {Contract} awarded as a result of this Bid Solicitation {RFP}.

There are no designated dates for release of Bid Amendments {Addenda}.  Those Vendors {Bidders} who are on the bidholder list either through commodity code registration in NJSTART or by acknowledging the bid in NJSTART should receive notification of any Bid Amendment(s) {Addenda}. If a Vendor {Bidder} is not on the bidholder list to receive notifications related to a Bid Solicitation {RFP}, Bid Amendments {Addenda} are still viewable on the “Summary” page of the Bid Solicitation {RFP} in NJSTART.

BID AMENDMENTS {ADDENDA} WILL BE ISSUED AS FILE ATTACHMENTS, AND ARE VIEWABLE ON THE “SUMMARY” PAGE OF THE BID SOLICITATION {RFP} IN NJSTART.  Vendors {Bidders} may refer to the QRG “Submit a Quote” for additional instruction. QRGs are located on the NJSTART Vendor Support Page.  

It is the sole responsibility of the Vendor {Bidder} to be knowledgeable of all Bid Amendments {Addenda} related to this procurement. An interested Vendor {Bidder} should check the NJSTART “Open Bids” Tab on a daily basis to ensure review of the most updated information.

[bookmark: _Toc400531479][bookmark: _Toc428533949][bookmark: _Toc475717169]VENDOR {BIDDER} Responsibility

The Vendor {Bidder} assumes sole responsibility for the complete effort required in submitting a Quote {Proposal} in response to this Bid Solicitation {RFP}.  No special consideration will be given after Quotes {Proposals} are opened because of a Vendor’s {Bidder’s} failure to be knowledgeable as to all of the requirements of this Bid Solicitation {RFP}.

[bookmark: _Toc400531480][bookmark: _Toc428533950][bookmark: _Toc475717170]COST Liability

The State assumes no responsibility and bears no liability for costs incurred by a Vendor {Bidder} in the preparation and submittal of a Quote {Proposal} in response to this Bid Solicitation {RFP}.

[bookmark: _Toc400531481][bookmark: _Toc428533951][bookmark: _Toc475717171]CONTENTS of QUOTE {Proposal}

Quotes {Proposals} can be released to the public pursuant to N.J.A.C. 17:12-1.2(b) and (c), or under the New Jersey Open Public Records Act (OPRA), N.J.S.A. 47:1A-1 et seq., or the common law right to know.  

After the opening of sealed Quotes {Proposals}, including Quotes {Proposals} submitted through the NJSTART electronic process, all information submitted by a Vendor {Bidder} in response to a Bid Solicitation {RFP} is considered public information notwithstanding any disclaimers to the contrary submitted by a Vendor {Bidder}. Proprietary and confidential information may be exempted from public disclosure by OPRA and/or the common law. When the Bid Solicitation {RFP} contains a negotiation component, the Quote {Proposal} will not be subject to public disclosure until a notice of intent to award a Blanket P.O. {Contract} is announced. 

As part of its Quote {Proposal}, a Vendor {Bidder} may designate any data or materials it asserts are exempt from public disclosure under OPRA and/or the common law, explaining the basis for such assertion. The location in the Quote {Proposal} of any such designation should be clearly stated in a cover letter. The State reserves the right to make the determination as to what is proprietary or confidential, and will advise the Vendor {Bidder} accordingly. Any proprietary and/or confidential information in a Quote {Proposal} will be redacted by the State.   The State will not honor any attempt by a Vendor {Bidder} to designate its entire Quote {Proposal} and/or prices as proprietary, confidential and/or to claim copyright protection for its entire Quote {Proposal}.  Copyright law does not prohibit access to a record which is otherwise available under OPRA.  In the event of any challenge to the Vendor’s {Bidder’s} assertion of confidentiality with which the State does not concur, the Vendor {Bidder} shall be solely responsible for defending its designation, but in doing so, all costs and expenses associated therewith shall be the responsibility of the Vendor {Bidder}. The State assumes no such responsibility or liability.  

A Vendor {Bidder} shall not designate any price lists and/or catalogs submitted as exempt from public disclosure as the same must be accessible to State Using Agencies and Cooperative Purchasing Program participants (if the Bid Solicitation {Contract} has been extended to these participants) and thus must be made public to allow all eligible purchasing entities access to the pricing information.

[bookmark: _Toc400531482][bookmark: _Toc428533952][bookmark: _Toc475717172] ANNOUNCEMENT OF QUOTE {PROPOSAL} INFORMATION

On the date and time Quotes {Proposals} are due under the Bid Solicitation {RFP}, all information concerning the Quotes {Proposals} submitted may be publicly announced and shall be available for inspection and copying except as noted below:

a. Information appropriately designated as proprietary and/or confidential shall not be available for inspection and copying; and
b. Where negotiation is contemplated, only the names and addresses of the 
Vendors {Bidders} submitting Quotes {Proposals} will be announced, and the contents of the Quotes {Proposals} shall not be available for inspection until the Notice of Intent to Award is issued by the Director. 

[bookmark: _Toc400531483][bookmark: _Toc428533953][bookmark: _Toc475717173]PRICE Alteration In Hard copy QUOTES {Proposals}

Hard copy Quote {Proposal} prices must be typed or written in ink. Any price change (including "white-outs") must be initialed. Failure to initial price changes shall preclude a Blanket P.O. {Contract} award from being made to the Vendor {Bidder}.

[bookmark: _Toc400531484][bookmark: _Toc428533954][bookmark: _Toc475717174]QUOTE {Proposal} ERRORS

In accordance with N.J.A.C. 17:12-2.11, “Quote {Proposal} errors,” a Vendor {Bidder} may withdraw its Quote {Proposal} as described below.

QUOTE {PROPOSAL} WITHDRAWAL PRIOR TO QUOTE {PROPOSAL} OPENING

NJSTART: A Vendor {Bidder} may withdraw its Quote {Proposal} submission in NJSTART prior to the Quote {Proposal} opening; however, Vendors {Bidders} should note that while withdrawn NJSTART Quotes {Proposals} remain viewable by the Vendor {Bidder} on its Vendor Profile Homepage, they are removed from the Division’s view and cannot be considered for Blanket P.O. {Contract} award. The Vendor {Bidder} may submit a revised Quote {Proposal} as long as the Quote {Proposal} is received prior to the announced date and time for Quote {Proposal} submission. Vendors {Bidders} may refer to the QRG “Submit a Quote” for additional instruction. QRGs are located on the NJSTART Vendor Support Page.  

Hard Copy: A Vendor {Bidder} may request that its hard copy Quote {Proposal} be withdrawn prior to the Quote {Proposal} opening. Such request must be made, in writing, to the Supervisor of the Quote {Proposal} Review Unit at the address provided in Section 1.4.7.2 below. The Vendor {Bidder} may submit a revised Quote {Proposal} as long as the Quote {Proposal} is received prior to the announced date and time for Quote {Proposal} submission and at the place specified. 

QUOTE {PROPOSAL} WITHDRAWAL AFTER QUOTE {PROPOSAL} OPENING, BUT PRIOR TO BLANKET P.O. {CONTRACT} AWARD

NJSTART and Hard Copy: If, after the Quote {Proposal} opening, but before Blanket P.O. {Contract} award, a Vendor {Bidder} discovers an error in its Quote {Proposal}, the Vendor {Bidder} may make a written request to the Supervisor of the Quote {Proposal} Review Unit to withdraw its Quote {Proposal}, or a portion thereof, from consideration for award. If the Vendor’s {Bidder’s} request to withdraw is made in good faith, and the State will not be significantly prejudiced by granting the withdrawal of the Quote {Proposal} beyond the loss of the benefit of the bargain to the State of the withdrawing Vendor’s {Bidder’s} offer, the request shall be granted. Evidence of the Vendor’s {Bidder’s} good faith in making this request can be demonstrated by one or more of the following factors: A mistake is so significant that to enforce the Blanket P.O. {Contract} resulting from the Quote {Proposal} would be unconscionable; that the mistake relates to a material feature or term of the Blanket P.O. {Contract}; and that the mistake occurred notwithstanding the Vendor’s {Bidder’s} exercise of reasonable care. After Quote {Proposal} opening, while pursuant to the provisions of this section a Vendor {Bidder} may request to withdraw its Quote {Proposal} and the Director may in her discretion allow said Vendor {Bidder} to withdraw it, the Division also may take notice of repeated or unusual requests to withdraw by a Vendor {Bidder} and take those prior requests to withdraw into consideration when evaluating the Vendor’s {Bidder’s} future Quotes {Proposals}.

All Quote {Proposal} withdrawal requests must include the Bid Solicitation {RFP} identification number and the final Quote {Proposal} submission date and be sent to the following address:

Department of the Treasury
Division of Purchase and Property
PO Box 039
33 West State Street – 9th Floor
Trenton, New Jersey 08625-0039
Attention:  Supervisor, Quote {Proposal}  Review Unit

If during a Quote {Proposal} evaluation process, an obvious pricing error made by a potential Blanket P.O. {Contract} awardee is found, the Director or her designee shall issue written notice to the Vendor {Bidder}. The Vendor {Bidder} will have up to five (5) business days after receipt of the notice to confirm its pricing. If the Vendor {Bidder} fails to respond, its Quote {Proposal} shall be considered withdrawn, and no further consideration shall be given to it.

If it is discovered that there is an arithmetic disparity between the unit price and the total extended price, the unit price shall prevail. If there is any other ambiguity in the pricing, other than a disparity between the unit price and extended price and the Vendor’s {Bidder’s} intention is not readily discernible from other parts of the Quote {Proposal}, the Director may seek clarification from the Vendor {Bidder} to ascertain the true intent of the Quote {Proposal}. If the Vendor {Bidder} inadvertently completes the “Discount” field and the “Unit Cost” field, the Discounted Unit Cost will prevail. 





[bookmark: _Toc400531485][bookmark: _Toc428533955][bookmark: _Toc475717175]JOINT Venture

If a Joint Venture is submitting a Quote {Proposal}, the agreement between the parties relating to such Joint Venture should be submitted with the Joint Venture’s Quote {Proposal}. Authorized signatories from each party comprising the Joint Venture must sign the Offer and Acceptance Page {Signatory Page}.  Each party to the Joint Venture must individually comply with all the forms and certification requirements in Sections 4.4.1 and 4.4.2 of this Bid Solicitation {RFP}. 
 
[bookmark: _Toc400531486][bookmark: _Toc428533956][bookmark: _Toc475717176]Reciprocity for Jurisdictional Vendor {Bidder} Preference

In accordance with N.J.S.A. 52:32-1.4 and N.J.A.C. 17:12-2.13, the State of New Jersey will invoke reciprocal action against an out-of-State Vendor {Bidder} whose state or locality maintains a preference practice for its in-state Vendors {Bidders}. New Jersey will use the annual surveys compiled by the Council of State Governments, National Association of State Procurement Officials, or the National Institute of Governmental Purchasing to identify States having preference laws, regulations, or practices and to invoke reciprocal actions. The State may obtain additional information as it deems appropriate to supplement the stated survey information.

A Vendor {Bidder} may submit information related to preference practices enacted for a State or Local entity outside the State of New Jersey. This information may be submitted in writing as part of the Quote {Proposal} response, including name of the locality having the preference practice, as well as identification of the county and state, and should include a copy of the appropriate documentation, i.e., resolution, regulation, law, notice to Vendor {Bidder}, etc. It is the responsibility of the Vendor {Bidder} to provide documentation with the Quote {Proposal} or submit it to the Director within five (5) business days after the deadline for Quote {Proposal} submission. Written evidence for a specific procurement that is not provided to the Director within five (5) business days of the public Quote {Proposal} submission date may not be considered in the evaluation of that procurement, but may be retained and considered in the evaluation of subsequent procurements.

[bookmark: _Toc294607267][bookmark: _Toc294680428][bookmark: _Toc400531487][bookmark: _Toc428533957][bookmark: _Toc475717177]QUOTE {PROPOSAL} ACCEPTANCES AND REJECTIONS

N.J.A.C. 17:12-2.7(d), the Director’s right to waive minor irregularities or omissions in a Quote {Proposal} and N.J.A.C. 17:12-2.2 which defines causes for Quote {Proposal} rejection, apply to all Quotes {Proposals}. In addition, pursuant to N.J.S.A. 52:34-12, the Director retains the right to reject all Quotes {Proposals} if it is in the public interest. 

[bookmark: _Toc473528310][bookmark: _Toc475717178]PRICE List and/or catalog pricing

Not applicable to this procurement.


[bookmark: _Toc400531488][bookmark: _Toc428533958][bookmark: _Toc475717179] DEFINITIONS

0. [bookmark: _Toc428533959][bookmark: _Toc475717180]CROSSWALK

	NJSTART Term
	Equivalent Existing New Jersey Term

	Bid/Bid Solicitation 
	RFP/Solicitation

	Bid Amendment 
	Addendum

	Change Order 
	Contract Amendment

	Master Blanket Purchase Order (Blanket P.O.) 
	Contract

	Offer and Acceptance Page
	Signatory Page

	Quote
	Proposal

	Vendor 
	Bidder/Contractor



0. [bookmark: _Toc428533960][bookmark: _Toc475717181]General Definitions

The following definitions will be part of any Blanket P.O. {Contract} awarded or order placed as a result of this Bid Solicitation {RFP}.

Definitions are listed by new NJSTART terminology; {existing terminology} appears in braces.

All-Inclusive Hourly Rate – An hourly rate comprised of all direct and indirect costs including, but not limited to:  labor costs, overhead, fee or profit, clerical support, travel expenses, per diem, safety equipment, materials, supplies, managerial support and all documents, forms, and reproductions thereof. This rate also includes portal-to-portal expenses as well as per diem expenses such as food.

Best and Final Offer or BAFO – Pricing timely submitted by a Vendor {Bidder} upon invitation by the Division after Quote {Proposal} opening, with or without prior discussion or negotiation.

Bid or Bid Solicitation {RFP or Solicitation} – This series of documents, which establish the bidding and Blanket P.O. {Contract} requirements and solicits Quotes {Proposals} to meet the needs of the Using Agencies as identified herein, and includes the Bid Solicitation {RFP}, State of NJ Standard Terms and Conditions (SSTC), price schedule, attachments, and Bid Amendments {Addenda}.

Bid Amendment {Addendum} – Written clarification or revision to this Bid Solicitation {RFP} issued by the Division of Purchase and Property. Bid Amendments {Addendum}, if any, will be issued prior to Quote {Proposal} opening.

Business Day - Any weekday, excluding Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Calendar Day – Any day, including Saturdays, Sundays, State legal holidays, and State-mandated closings unless otherwise indicated.

Change Order {Contract Amendment} – An alteration or modification of the terms of a Blanket P.O. {Contract} between the State and the Vendor(s) {Contractor(s)}. A Change Order {Contract Amendment} is not effective until it is signed and approved in writing by the Director or Deputy Director, Division of Purchase and Property.

Cooperative Purchasing Program – The Division’s intrastate program that provides procurement-related assistance to New Jersey local governmental entities and boards of education, State and county colleges and other public entities having statutory authority to utilize select State Blanket P.O.s {Contracts} issued by the Division, pursuant to the provisions of N.J.S.A. 52:25-16.1 et seq.

Days After Receipt of Order (ARO) - The number of calendar days ‘After Receipt of Order’ in which the Using Agency will receive the ordered materials and/or services.

Director – Director, Division of Purchase and Property, Department of the Treasury, who by statutory authority is the Chief Contracting Officer for the State of New Jersey.

Discount - Means the standard discount applied by the Vendor {Bidder} to all items.

Discounted Unit Cost – Means “Unit Cost” field multiplied by (100 percent minus the “Discount” field percentage).

Division – The Division of Purchase and Property.

Evaluation Committee – A committee established or Division staff member assigned by the Director to review and evaluate Quotes {Proposals} submitted in response to this Bid Solicitation {RFP} and recommend a Blanket P.O. {Contract} award to the Director.

Firm Fixed Price – A price that is all-inclusive of direct cost and indirect costs, including, but not limited to, direct labor costs, overhead, fee or profit, clerical support, equipment, materials, supplies, managerial (administrative) support, all documents, reports, forms, travel, reproduction and any other costs.

Freight - Means Freight on Board (FOB) Destination.

Joint Venture – A business undertaking by two or more entities to share risk and responsibility for a specific project.

Master Blanket Purchase Order (“Blanket P.O.”) {Contract} – The Blanket P.O. {Contract} consists of the State of NJ Standard Terms and Conditions (SSTC), the Bid Solicitation {RFP}, the responsive Quote {Proposal} submitted by a responsible Vendor {Bidder} as accepted by the State, the notice of award, any Best and Final Offer, any subsequent written document memorializing the agreement, any modifications to any of these documents approved by the State and any attachments, Bid Amendment {Addendum} or other supporting documents, or post-award documents including Change Orders {Contract Amendments} agreed to by the State and the Vendor {Contractor}, in writing.

May – Denotes that which is permissible or recommended, not mandatory.

No Bid – The Vendor {Bidder} is not submitting a price Quote {Proposal} for an item on a price line.

No Charge – The Vendor {Bidder} will supply an item on a price line free of charge.

Ownership Disclosure Form – Refers to the Statement of Bidder/Vendor Ownership as utilized in NJSTART.

Primary Form – An electronic form contained within a Vendor’s {Bidder’s} NJSTART profile designated by the Vendor {Bidder} as the primary or principal version of the required form.

Procurement Bureau - The Division unit responsible for the preparation, advertisement, and issuance of Bid Solicitations {RFPs}, for the tabulation of Quotes {Proposals} and for recommending award(s) of Blanket P.O. (s) {Contract(s)} to the Director and the Deputy Director.

Project – The undertakings or services that are the subject of this Bid Solicitation {RFP}.

QRGs – Quick Reference Guides.

Quote {Proposal} – Vendor’s {Bidder’s} timely response to the Bid Solicitation {RFP} including, but not limited to, technical Quote {Proposal}, price Quote {Proposal}, and any licenses, forms, certifications, or other documentation required by the Bid Solicitation {RFP}.

Retainage - The amount withheld from the Vendor {Contractor} payment that is retained and subsequently released upon satisfactory completion of performance milestones by the Vendor {Contractor}.

Revision – A response to a BAFO request or a requested clarification of the Vendors {Bidders} Quote {Proposal}. 

Shall or Must – Denotes that which is a mandatory requirement. Failure to meet a mandatory material requirement will result in the rejection of a Quote {Proposal} as non-responsive.

Should – Denotes that which is permissible or recommended, not mandatory.

Small Business – Pursuant to N.J.A.C. 17:13-1.2, “small business” means a business that meets the requirements and definitions of “small business” and has applied for and been approved by the New Jersey Division of Revenue and Enterprise Services, Small Business Registration and M/WBE Certification Services Unit as (i) independently owned and operated, (ii) incorporated or registered in and has its principal place of business in the State of New Jersey; (iii)  has 100 or fewer full-time employees; and has gross revenues falling in one of the three following categories: (A) 0 to $500,000 (Category I); (B) $500,001 to $5,000,000 (Category II); and (C) $5,000,001 to $12,000,000, or the applicable federal revenue standards established at 13 CFR 121.201, whichever is higher (Category III).

State – State of New Jersey.

State Contract Manager or SCM – The individual, as set forth in Section 8.0, responsible for the approval of all deliverables, i.e., tasks, sub-tasks or other work elements in the Scope of Work.  The SCM cannot direct or approve a Change Order {Contract Amendment}.

Subtasks – Detailed activities that comprise the actual performance of a task.

Subcontractor – An entity having an arrangement with a Vendor {Contractor}, whereby the Vendor {Contractor} uses the products and/or services of that entity to fulfill some of its obligations under its State Blanket P.O. {Contract}, while retaining full responsibility for the performance of all [the Vendor’s {Contractor's}] obligations under the Blanket P.O. {Contract}, including payment to the Subcontractor. The Subcontractor has no legal relationship with the State, only with the Vendor {Contractor}.

Task – A discrete unit of work to be performed.

Unit Cost – All-inclusive, firm fixed price charged by the Vendor {Bidder} for a single unit identified on a price line.

Using Agency[ies] – A State department or agency, a quasi-State governmental entity, or a Cooperative Purchasing Program participant, authorized to purchase products and/or services under a Blanket P.O. {Contract} procured by the Division. This Blanket P.O. {Contract} may be used by the Using Agencies or quasi-governmental agencies specifically identified in the Bid Solicitation {RFP}. In addition, with the approval of the Director of the Division of Purchase and Property and the agreement of the Vendor {Contractor}, the Blanket P.O. {Contract} may be used by any Using Agency or quasi-governmental agency. 

Vendor {Bidder} – An entity offering a Quote {Proposal} in response to the Division’s Bid Solicitation {RFP}.

Vendor {Contractor} – The Vendor {Bidder} awarded a Blanket P.O. {Contract} resulting from this Bid Solicitation {RFP}.

[bookmark: _Toc355709006][bookmark: _Toc400531490][bookmark: _Toc428533961][bookmark: _Toc475717182]BLANKET P.O. {contract}-specific definitions/ACRONYMS

AF – Rear axle to end of frame.

Aftermarket Component - Any component - utility body, snow plow, crane, liftgate or the like - installed on the vehicle chassis (prime unit) by manufacturer or installer (aftermarket installer) other than the chassis manufacturer (prime unit manufacturer).

Aftermarket Installer – An entity modifying a unit with or without installation of an accessory equipment after the vehicle is manufactured by the original vehicle manufacturer (primary unit manufacturer), where the Vendor {Contractor} uses the products and/or services of that entity to fulfill some of its obligations under its Blanket P.O. {Contract}, while retaining full responsibility for the performance of all of its (Vendor’s {Contractor’s}) obligations under the Blanket P.O. {Contract}, including payment to the aftermarket installer and prime unit manufacturer.  The aftermarket installer and prime unit manufacturer have no legal relationship with the State, only with the Vendor {Contractor}.

ANSI – American National Standards Institute (http://www.ansi.org/).

ASTM - American Society for Testing Materials (http://www.astm.org/). 

BBC – Bumper-to-back-of-cab, the distance from the front-most edge of the front bumper to the back of cab.

BL - Body length, overall length minus BBC.

CA - Cab-to-axle, the distance from the back of cab to the centerline of rear axle.

DRW – Dual Rear Wheel.

Dry Weight - Curb weight or tare weight of a vehicle - weight of an empty vehicle, without any payload, driver and passenger, with fluids filled to half capacity.

FMVSS - Federal Motor Vehicle Safety Standards, as established by National Highway Traffic Safety Administration (http://www.nhtsa.gov/).

GAWR - Gross Axle Weight Rating; the maximum legal weight carrying capacity of axle components, including their own dry weights, as published by the vehicle/chassis manufacturer.  GAWR shall not exceed the capacity of the least rated axle component.

GVWR - Gross Vehicle Weight Rating; the maximum legal weight carrying capacity of a vehicle, including its own weight, as published by the vehicle/chassis manufacturer. GVWR shall not exceed the sum of front and rear GAWRs.

NJMVC or NJDMV - New Jersey Motor Vehicle Commission, formerly known as Division of Motor Vehicles.

Non-State Agency - Any Using Agency other than the State agencies. Any quasi-State Agency (New Jersey Turnpike, for example) or political sub-division is a non-State Agency. Quasi-State Agencies include any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-State governmental entity of which the State of New Jersey is a member.

OEM – Original Equipment Manufacturer. OEM parts are new parts, which are designed, manufactured and/or approved by the original equipment (prime unit) manufacturer.

OSHA – Occupational Safety and Health Administration (https://www.osha.gov/). 

Payload - Weight carrying capacity of a vehicle, excluding its dry weight, driver and passenger.  Payload, when added to dry weight and weight of driver, passenger and half fluids, shall not exceed the GVWR. Payload is limited by the front or rear GAWR.

RBM - Resisting bending moment, a measure of chassis frame stiffness.

SAE - Society of Automotive Engineers (https://www.sae.org/).

State Agency - Any department or agency, which is a part of the New Jersey State government, such as the Department of Transportation, Department of Environmental Protection, Department of Corrections, Department of Human Services, Department of Law and Public Safety and Department of the Treasury. For a complete list of all State agencies, visit the State website at (lowercase): www.state.nj.us.

Unit - Vehicle ("truck", "product", "commodity" or "item"), Universal Truck, 19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD, with Optional Hook lift System, Various Bodies, Salt Spreader, Snow Plow & Accessories, as specified herein, made available for outright purchase as a new, unused unit under a Blanket P.O. {Contract} established as a result of this Bid Solicitation {RFP}.  

WB - Wheelbase, the distance between the centerlines of front and rear axles. 

Pre-Consumer Material - materials generated in manufacturing and converting processes, such as manufacturing scrap and trimmings/cuttings.

Post-Consumer Material - material or finished product that has served its intended use and has been diverted or recovered from waste destined for disposal, having completed its life as a consumer item. Post-consumer materials are part of the broader category of recovered materials.                                                                                                                                                                                                                                     

Recovered Material - Waste material and byproduct that have been recovered or diverted from solid waste, but does not include materials and byproducts generated from, and commonly reused within, an original manufacturing process.

Materials in Solid Waste - Material found in the various components of the solid waste stream. General, solid waste has several components, such as municipal solid waste (MSW), construction and demolition debris (C&D), and nonhazardous industrial waste. Under RCRA Section 6002, EPA considers materials recovered from any component of the solid waste stream when designating items containing recovered materials. 

Recycling - The series of activities, including collection, separation, and processing, by which products or other materials are recovered from the solid waste stream for use in the form of raw materials in the manufacture of new products other than fuel for producing heat or power by combustion.

Recyclability - The ability of a product or material to be recovered from, or otherwise diverted from, the solid waste stream for the purpose of recycling.

RMAN - Recovered Materials Advisory Notices provide purchasing guidance and recommendations for recovered and post-consumer material content levels for designated items. 

USEPA - United States Environmental Protection Agency


[bookmark: _2.2_contract_specific][bookmark: _3.0_Scope_of][bookmark: _Ref37485783][bookmark: _Toc400531491][bookmark: _Toc428533962][bookmark: _Toc475717183]
 SCOPE OF WORK

0. [bookmark: _Toc475717184]BLANKET P.O. {CONTRACT} UTILIZATION

3.1.1 This Bid Solicitation {RFP} has been developed to establish a Blanket P.O. {Contract} to procure the specified unit for the DOT and other State agencies and Cooperative Purchasing Program participants. It is anticipated that the DOT will purchase approximately 134 units during the term of the Blanket P.O. {Contract} (Agency Reference # 15-DCN-0176). 

3.1.2 The State makes no representation and provides no guarantee as to the minimum, average or maximum volume of purchases to be made under this Blanket P.O. {Contract}. 

[bookmark: _Toc475717185]BLANKET P.O. {CONTRACT} SPECIFIC REQUIREMENTS

[bookmark: listofaftermarketinstallers][bookmark: TechnicalComplianceDeclaration][bookmark: deviationsubstitution][bookmark: postorderpreproductionmeeting]3.2.1 The Vendor {Contractor} must be a franchised and/or authorized factory representative, able to furnish the specified unit. Dealers or agents submitting a Quote {Proposal} may be required to submit a letter of certification from the manufacturer whose product is supplied, certifying that the dealer or agent is authorized by the manufacturer to supply the unit specified. The State reserves the right to request such certification and to require that such certification be delivered within five (5) working days from the time it is requested. It will be the responsibility of the Vendor {Contractor} to notify the State of New Jersey of any changes in the status of its franchise.

3.2.2 The unit supplied must be standard manufacturer's product line available to the general public. 

3.2.3 The Vendor {Contractor} shall provide a new unit only.  A used unit will not be accepted.

3.2.4 This Bid Solicitation {RFP} is for the outright purchase of the Blanket P.O. {Contract} unit only; leasing of the Blanket P.O. {Contract} unit or trade-in against the purchase of the Blanket P.O. {Contract} unit is not permitted.

3.2.5 The Vendor {Contractor} shall ensure that the manufacturer whose product is supplied has a servicing dealer or service location to provide warranty and recall service and/or repair within twenty four (24) hours of notification by the Using Agency. The servicing dealer or location must stock a full range of new spare parts for all units serviced and must be capable of delivering regularly stocked parts within 24 hours of order. All parts, including special orders, must be delivered within 72 hours of order. The Vendor {Contractor} may use an aftermarket installer's location to satisfy this requirement, provided this is disclosed in the Quote {Proposal}. As stated in 3.2.7, any use of aftermarket installer(s) shall not relieve the Vendor {Contractor} of its obligations under the Blanket P.O. {Contract} established as a result of this Bid Solicitation {RFP}.  

3.2.6 All components of each unit supplied under the Blanket P.O. {Contract} established shall be identical, for example, alternators, filters, distributors, etc. 

3.2.7 The Vendor {Contractor} will be permitted to use aftermarket installers. Any intent to utilize aftermarket installers shall be described in Attachment #1 – List of Aftermarket Installers, with a list of aftermarket installer(s), other than the prime unit manufacturer, who will supply or install all aftermarket options required. 

3.2.7.1 The Vendor {Contractor} is responsible for ensuring aftermarket installer(s)' compliance with all terms and conditions of this Bid Solicitation {RFP}. The Vendor {Contractor} will assume sole responsibility for any payments due the aftermarket installer(s). Nothing contained in the Bid Solicitation {RFP} shall be construed as creating any contractual relationship between any aftermarket installer(s) and the State.

3.2.7.2  If, subsequent to Blanket P.O. {Contract} award, a Vendor {Contractor} desires to substitute any aftermarket installer(s) listed in the Quote {Proposal}, the Vendor {Contractor} will so notify the State and provide the information on the proposed aftermarket installer(s). The State reserves the right to reject any proposed substitute aftermarket installer(s).

3.2.7.3 The State reserves the right to demand from the Vendor {Contractor} the same information regarding any aftermarket installer(s) as is required from the bidder under this Bid Solicitation {RFP}.

The Vendor {Bidder} shall provide complete information on aftermarket installer(s) in Attachment #1 – List of Aftermarket Installers.
 
[bookmark: _Toc172392761][bookmark: _Toc448401100][bookmark: _Toc467160934][bookmark: _Toc475717186]VEHICLE SPECIFICATIONS – GENERAL PROVISIONS

3.3.1 Each unit and its components shall be completely assembled, serviced and ready for use when delivered to the Using Agency. Unless specified otherwise; any parts, components, equipment, controls, materials, features, performances, capacities, ratings or designs which are standard and/or necessary to form an efficient and complete working unit shall be furnished whether specifically required herein or not. The Vendor {Contractor} shall supply any item not specified herein but deemed necessary for functional purposes and the item must meet the Industry standards and practices, Federal and New Jersey Safety Standards and Regulations, and SAE and other applicable standards. Unless specified otherwise, the Vendor {Contractor} shall not delete manufacturer’s standard item using any aftermarket option. No exceptions shall be permitted to this requirement.

3.3.2 Each vehicle shall be delivered with at least a 1/2 tank of fuel.

3.3.3 Each vehicle furnished must be protected to -20° F, with a permanent type anti-freeze.

3.3.4 Vehicles provided shall be manufacturer’s standard vehicles with the necessary upgrades and/or accessories. All accessories shall be supplied and installed by the manufacturer. Dealer installation is permitted only if factory installation is not available. Dealer installation shall be in accordance with the practices recommended by the manufacturer and shall not adversely affect manufacturer's warranty.

[bookmark: finish]3.3.5 Undercoating and Finish: The frame, fenders, underbody, cab, etc., except driveshaft, exhaust system, and other mechanical components must be completely undercoated. Undercoating must be composed of a non-volatile base, grit and abrasive free material, dispersed in a petroleum solvent, which shall provide a homogenous formulation. All undercoating must be applied to a uniform thickness with no bare spots. 

3.3.5.1    DOT Units: 

Cab, chassis and bodies shall be finished as indicated below. All stainless steel components shall remain unpainted.

Section 3.4.1 – Cab and Chassis: The unit and all its components shall be cleaned and painted with manufacturer’s standard white. All paint must be same shade.
Section 3.4.3 – Stainless Dump Body: Manufacturer’s standard paint color.
Section 3.4.4 – Stake Body: Manufacturer’s standard paint color.
Section 3.4.5 – Landscape Box Body: Manufacturer’s standard paint color.
Section 3.4.6 – Chipper Body: Manufacturer’s standard paint color.
Section 3.4.7 – Enclosed Steel Storage Body: Manufacturer’s standard paint color.
Section 3.4.8 – Platform Body with Sprayer: Manufacturer’s standard paint color.
Section 3.4.9 – Platform Body with Toolboxes: Manufacturer’s standard paint color.
Section 3.4.10 – Dump Body with Multi-Function Tailgate: Dump body shall be primed and painted white enamel including underside. 
Section 3.4.11 – Salt Spreader: All stainless steel components shall be left unpainted. Carbon steel components shall be chemically cleaned and coated with a lead free rust inhibitive primer and painted with lead free black enamel. Top screens shall be powder coated.

3.3.5.2  All Other State Agency and Non-State Agency Units: Using Agency will specify manufacturer's standard one-tone color at the time of ordering.

[bookmark: manuals][bookmark: VEHICLESPECIFICATIONSTECHNICALPROVION]3.3.6 Manuals: If available, the Vendor {Contractor} shall supply one line set sheet for each unit. A unit shall comprise each and every assembly system and/or component. In addition to any line set sheet, the Vendor {Contractor} shall provide vehicle operation and maintenance manuals for each and every assembly system and/or component that makes up the unit. The Vendor {Contractor} shall also include any other manuals that the manufacturers provide as standard manuals. 

Examples of assembly systems and/or components include, but are not necessarily limited to:

	A.
	Hydraulic pump and hydraulic systems

	B.
	Engine, drives and chassis

	C.
	Transmission

	D.
	Electrical system

	E.
	Lubrication system



The manuals shall be delivered directly to the Using Agency, upon delivery of the first unit. Failure to supply these manuals may delay approval of invoices for payment.

Note: These manuals are required as a part of the base unit purchase (price line 1) and are not part of the “optional manuals” specified in Section 3.4.15.

[bookmark: weightchart][bookmark: guaranteewarranty][bookmark: _Toc172392762]3.3.7 Training: Complete instructions on the operation and maintenance of each unit and a demonstration of the operation of the unit shall be given by the Vendor {Contractor}, if requested by the Using Agency. Training must include operator training with instruction on proper operation of the unit, safety, and basic preventive maintenance. This demonstration shall be a formal training session and shall be arranged with the Vendor {Contractor}, at the convenience of the Using Agency. The training session shall be conducted at the location of delivery or at a field location within the State of New Jersey, as specified by the Using Agency. 

Note: This training is required as a part of the base unit purchase (price line 1) and is not part of the technical support specified in Section 3.4.16.

3.3.8 Brand Names: Brand names have been kept to a minimum in this Bid Solicitation {RFP}; but if a brand name is given, the term "or comparable" is considered to follow the brand name. Wherever a brand name is used, it is meant to denote the minimum level of quality and performance. Any item supplied as "comparable" must be approved by the State during the Quote {Proposal} evaluation and prior to an award. Specifying a brand name, components and/or equipment in response to this specification shall not relieve the Vendor {Contractor} from its responsibility to produce the unit in accordance with all specifications and other contractual requirements.

3.3.9 Guarantee/Warranty: The Vendor {Contractor} must guarantee that the vehicle and all its component parts comply with the current, applicable Federal Motor Vehicle Safety Standards (FMVSS) and New Jersey State Motor Vehicle Code Regulations, perform their functions adequately, and operate successfully without undue wear or vibration. The Vendor {Contractor} shall immediately replace and install free of charge any part that may break or fail by reason of defective material or workmanship within a period of one (1) year from the date of acceptance by the agency. The Vendor {Contractor} must maintain a supply of component parts for the expected life of the unit.

3.3.10 The Vendor {Bidder} must provide complete information on warranty coverage as specified in Section 3.5.6.

[bookmark: _Toc448401101][bookmark: _Toc467160935][bookmark: _Toc475717187][bookmark: _Toc172392768]VEHICLE SPECIFICATIONS – TECHNICAL PROVISIONS

[bookmark: vehiclespecstechnicalprovisions][bookmark: _Toc448401102][bookmark: _Toc467160936][bookmark: _Toc475717188]3.4.1    19,500 LB. GVWR CREW CAB & CHASSIS, DRW, 4WD (PRICE LINE: 1)

It is the intent of this specification to describe the base model requirements for a 2017 model year or newer 19,500 lb. GVWR crew cab and chassis, DRW, 4WD.

Dimensions and Capacities: 

GVWR:	 19,500 lb. minimum     

CA:	             84 inch minimum

WB:	             197 inch minimum 

Axles:

Front - Type: 		Manufacturer's standard
            Capacity:	Minimum 7,200 lbs. GAWR

Rear - Type: 		Manufacturer’s standard
           Capacity:	Minimum 13,500 lbs. GAWR


Brakes:

Manufacturer’s 4-wheel disc brakes with anti-lock brake system. 

Note:  Brakes are to incorporate manufacturer's standard non-asbestos type brake linings.   

Crew Cab: 

Capacity:		Minimum Five (5) personnel

Seats-	Type:              Front:   Vinyl bucket type seats, or Split Vinyl 40/20/40 bench     
     	                                    seat with deleted center seat equipped with safety belts.   
Rear:   Vinyl Bench type equipped with safety belts

Cab must include:       Power front side windows, power door locks with remote keyless entry,   
tinted windows, minimum of two (2) 12-volt auxiliary power outlets (dash mounted), floor mats and two (2) complete sets of keys.

Air Bags:		Minimum driver and passenger-side front air bags.

Gauges/Indicators:      Water temperature, fuel, tachometer, speedometer, trip meter and odometer.

Side View Mirror assembly: 	 Quantity 2, heated, manual telescoping trailer tow type. 

Grab Handles:         		 Driver and passenger side grab handles.
 
Running boards and/or steps:   Aluminum tread plate or manufacturer’s optional running boards
   must be securely attached to the frame of the truck and shall.     
   They are to extend from the front wheel well to the end of the cab.

Windshield Wipers: 	            Manufacturer’s standard 	

Heater and Defroster:	 	Heavy duty fresh air type 

Air conditioning:		Manufacturer’s standard

Radio:          			AM/FM with clock

GVWR labeling:                      Lower right hand corner, driver’s side door must be labeled in 3 
 inch” high red letters on a white background, for example: 
 GVWR 19,500 lb. Minimum

Curb weight:  			 Curb weight shall be determined by the Vendor {Contractor} 
 				 weighing the first completed unit on each order.

Electrical System:

Alternator (volts):		12
Alternator (amps): 		Minimum 200 amp. 


Starter (volts):			12

Battery (CCA):			Minimum 12 volt 720 CCA. 

Electronic auxiliary idle/throttle control kit, mounted in cab, must be provided.

Rear Lights:                            LED stop lights, taillights, directional signals, 4-way flashers,
reflectors, back up lights and license plate light.  

Front Lights:                         Manufacturer’s standard headlights, parking lights, directional signals 
and four-way flashers. 

Fuse panel must be located in a convenient location. All electrical wires for cab/chassis and body (ies) as applicable must be enclosed in a plastic loom.

Power Distribution: Any non-OEM accessory such as safety lights and radios must be protected by an appropriately sized fuse or circuit breaker located as close to the battery as practicable. At no time shall an accessory wire pass from the engine compartment through the firewall into the interior of the vehicle or from the engine compartment to any other part of the vehicle (either internally or externally) without the appropriate fuse or circuit breaker.  All wires added shall be automotive type and have an SAE rating. Wires must be properly sized for current draw and length of run per automotive industry standards. All wires passing through the firewall or any metal must be protected by grommets and neatly tied or loomed. Any wiring routed near engine exhaust and exhaust components must be heat shielded.

Accessory Power: From the positive terminal of the battery a two (2) gauge wire shall connect to a high current breaker (Cooper Bussman CB185 Series or comparable), exact rating must be determined by the Vendor {Contractor} and will be subject to Using Agency approval. The breaker shall be mounted as close as practicable to the battery followed by a two (2) gauge wire to a continuous duty solenoid (NAPA, item # ECHST99, continuous duty, 12 volt, 100 amp, or comparable). A two (2) gauge wire connected to the other side of the solenoid should feed the fuse blocks at the console in the cab. The solenoid must engage when the ignition switch is turned on. Any other accessories that are not connected to the fuse blocks at the console must connect to the switched side of the solenoid with appropriate fuse or breaker as close as practicable to the solenoid. Note: All electrical circuits must have a suitable fuse or breaker. Terminals on solenoid and breaker must be shielded from inadvertent shorting.

Electrical system must be guaranteed by the Vendor {Bidder} to be of ample capacity to handle total electrical load with auxiliary lights. All electrical circuits must be equipped with fuses or circuit breakers for protection against overload of wiring and electrically operable devices. Fuses/breakers must be marked as to their function.

All electrical wires shall be heavy duty plastic covered. All exposed electrical junction blocks shall be enclosed with a boot for protection against salt and road chemicals. All electrical wires shall be enclosed in a loom. Any splices in the battery or other electrical cables shall be sealed with heat shrink tubing.

Cooling System:

Radiator type:          Heavy duty increased capacity tubular system.

Radiator must be manufacturer’s largest compatible size. Cooling system must be capable of maintaining safe operating temperatures over extended idling periods. Cooling system must be protected with long life coolant and shall have a minimum 300,000 mile life with coolant extender. 

Engine:

Type: 	   		 Diesel, 6.7L 

Rated horsepower: 	 300 HP or greater

Rated torque:       	 660 lb.-ft. or greater

Block Heater:	 Electrical block heater mounted in engine block, 120 volt with flush mounted NEMA 5-15 configuration body receptacle (male), with spring loaded weather cap.  

A 25 ft. grounded extension cord, 12 gauge, UL listed safety extension cord, conforming to OSHA requirements for outdoor use shall be provided. The female connection of the cord must fit the weather cap assembly. Electrical block heater cab connection shall be located on the driver’s side of the vehicle in front of or under the driver’s side door.   

Note:  Engine block heater weatherproof receptacle shall be sealed by spraying the rear wire connecting terminals with Armor #17 (or Krylon or comparable) clear plastic (care shall be taken not to spray the receptacle contact prongs). Rear wire covering boot shall be sealed at both ends with silicone rubber adhesive sealant (MOPAR #4318025 or comparable) or appropriate caulk to seal the boot to the receptacle housing and to the wire lead.

Exhaust:             Horizontal muffler, with horizontal discharge pipe, left or right side of the vehicle.
                                             
Low oil pressure and high engine temperature warning light or audible alarm shall be included. 

Air cleaner: 	      Replaceable; standard

Oil filter:   	      Spin-on type
     
Frame:

Frame Type:         Manufacturer’s standard frame 

Front and rear license plate brackets must be provided.

Fuel System:

Tank Capacity:      40 gallons or greater  

Fuel tank(s) must have locking fuel fill cap, with two (2) keys included with each unit.  Opening(s) must be labeled "Diesel Only" in 1 inch high black letters.  Locking fuel cap shall be installed prior to delivery.  

Steering:

Type:	Power with tilt steering wheel  

Suspension:

Front - Capacity: 	Minimum 7,200 lbs. GAWR

Rear - Capacity: 	Minimum 13,500 lbs. GAWR

Heavy duty front and rear shock absorbers.

Transmission:

Type:			Minimum 6-speed automatic with overdrive 

Transmission must be equipped with left or right PTO outlets. 

Transmission must have "hot shift" PTO (Chelsea 276 or comparable) and must include all required hydraulic shift controls. Engine shall be programmed for over-speed protection while in PTO mode or transmission shall have provision to avoid over-speed occurrence. A flashing indicator light shall be provided to show when PTO is engaged. A heavy duty bracket may be required to support the PTO/pump to the transmission.
  
Wheels:

Type:		Steel disc 
Size:		19.5 
Quantity:	7, including a full size spare

Fenders must be installed over rear wheels. 




Tires: 

Type:    	Tubeless blackwall, radial, all-season on front and rear.
Quantity:	7, dual on rear and spare
Size:	            LT225 or comparable (sized to meet GVWR)

Tire load rating shall be selected so as to meet or exceed GVWR requirement.

Manufacturer's recommended tire pressure shall be stenciled in black paint over each tire on fender or body in 1 inch high letters. 

Anti-sail mud flaps must be provided behind the rear tires. 

Spare tire must be mounted on spare rim.

Trailer Cable Connectors: 

Truck must have two (2) A.T.A. and S.A.E. approved, 7-wire trailer connectors (female type), Cole Hersee 12080 or comparable.  Connectors must be mounted on the rear bumper with cover provided.  Wiring must conform to A.T.A. color code.  All wiring must be protected from salt and corrosion.

Combination Ball/Pintle Hook:

A combination pintle hook Buyers Product model #10040 or comparable with pintle hook mounting plate must be provided. Combination pintle hook shall be mounted 18” from ground. A heavy duty 2 inch receiver tube with pin must be provided on a ½ inch thick steel hitch plate. The pintle hook assembly may require an elbow to meet 18 inch height. Two (2) lunettes must be securely fastened to the hitch plate. 
 
Combination Rear Bumper with Receiver Tube:

Full width 4 inch steel channel bumper shall be integrated into the hitch plate with receiver tube and integrated with (FMVSS108 compliant) LED tail lights, LED backup and amber LED strobes and backup alarm. 
 
Safety Features and Equipment:  

Each unit shall include the following:

5 lb. fire extinguisher and mount 

Mechanical jack

Triangle kit

First aid kit 

Safety Lights and Warning System:

Note:  Safety lighting shall be installed in addition to normal vehicle manufacturer/factory required lighting.  

Vehicle manufacturers/factory lighting shall not be deleted unless specifically noted.  

One emergency light bar, amber, with automatic dimming feature at night shall be mounted on the cab, Whelen Edge Freedom IV F4X2AAAA with PhotoCell F4XPHOTO or comparable. The light bar shall have a raised 55 inch long base and approximately 5” permanent mount, Whelen Model MK8H mount or comparable. The light bar installation shall not interfere with any equipment movement.  

The light bar shall be LED with two (2) LED rear takedown lights, four (4) corner modules with six (6) forward and six (6) rear facing LED modules. 

The light bar shall have sequential or alternating flash capability.

The light bar shall include a weather-proof clear dome and utilize the cab and chassis manufacturer installed upfitter switches. A three-position toggle switch, mounted in the dash, shall allow joint or isolated use of lights. The light bar control switch shall come with a dashboard mounted indicator light.


[image: ]

Two (2) amber LED strobes, Whelen M4 or comparable, must be mounted on the rear of the truck near the taillights.  

[bookmark: _3.4.2_OPTION:_HOOK][bookmark: _3.4.2__HOOK][bookmark: _Toc448401103][bookmark: _Toc467160937][bookmark: _Toc475717189]3.4.2    HOOK LIFT SYSTEM (PRICE LINE: 2)

It is the intent of this section to describe the specifications for a hook hoist frame and hook lift, which must be compatible with the various bodies (Sections 3.4.3 through 3.4.10) and salt spreader (Section 3.4.11) specified in this Bid Solicitation {RFP}. 

The hook lift system specified herein is comparable to an Ampliroll AL90 S-12, Palfinger T12S or Stellar 84-10 Flex 36; however, any hook lift system that meets or exceeds the specifications will be considered.

3.4.2.1    Dimensions and Capacities:

Lifting Capacity:	12,000 lb. or greater
Container Length:	10 feet or greater
Hook Height:		35 inches or greater
Dump Angle:		50° minimum

3.4.2.2    General:

The lifting capacity must be 12,000 lb. or greater and hydraulically adjustable by pressure relief for optimal weight carrying as not to exceed the GVWR and damage the cab and chassis.

The hook lift must have a pivoting type tilt section hook assembly to provide a low degree loading/unloading angle. The pivoting front tilt section must lift the front of the container/body off of the front saddles, then rolling the long sills on the load rollers, eliminating the need for wear pads.  No frame rail wear pads or intermediate rollers are acceptable.

The tilt cylinder must be fully retracted when in transport mode to prevent exposure of the cylinder rod to corrosive road salts. The hook lift must have a positive tilt section safety lock to prevent tilt section operation while in the dump mode.

The hook lift must have two (2) load rollers, one on each side, which the body long sills roll on; wear pads are not acceptable. All rollers must have grease zerks. 

All moving parts shall have grease fittings. Rear pins shall be stainless steel.

The use of wear pads is not acceptable.

[bookmark: _3.4.2.3_Frame:]3.4.2.3    Frame:

The hook-hoist frame shall be constructed to reduce wear on body understructures. The actual lifting capacity shall be hydraulically limited to not to exceed the chassis manufacturers axle weights.

The frame shall be thoroughly cleaned of welding slag or other by-products prior to applying primer to ensure proper adhesion.
	
The hook lift frame shall have a positive front body lock and keeper system including a hydraulic counterbalance valve.

Dual fixed-position hold down devices must be mounted to the dump frame to secure the body to the hook lift through all ranges of the dump mode and transportation. This must be accomplished without the use of springs and/or hydraulic/air cylinders. Slide through hold-down devices are not acceptable. 

A visual indicator (red bars, striping, paint, etc.) that the body has been fully locked in place shall be installed on frame rails. A whisker switch shall also been installed on the frame rails with an indicator light in the cab to ensure that the body has be fully locked in place. The exact layout and configuration of the visual indicator and the whisker switch shall be determined and approved by the Using Agency at the pre-manufacture/pre-production meeting.

[bookmark: _3.4.2.4__]    3.4.2.3   Hydraulic System:

The hydraulic system shall provide sufficient flow and pressure to maximize hook lift operation as well as provide appropriate hydraulic flow and pressure to power and control the hook lift. 

Hydraulic controls shall be mounted in the cab and must have center lock out on lift/dump function to meet OSHA 1926.601(b) (11), which states: “Operating levers controlling hoisting or dumping devices on haulage bodies shall be equipped with a latch or other device which will prevent accidental starting or tripping of the mechanism.” Hook lift operation shall be controlled from the safety of the chassis cab. 

The hydraulic system shall be sized appropriately to handle all the different body options along with the requirements of the actual hook lift and shall include full hydraulic option. 

A direct coupled pump shall be installed with hot-shift transmission mounted PTO to allow operation in any gear. 
 
			
[bookmark: _Toc448401104][bookmark: _Toc467160938][bookmark: _Toc475717190]3.4.3    STAINLESS STEEL DUMP BODY WITH TILT/DUMP INTERLOCK (PRICE LINE: 3)

It is the intent of this section to describe the specifications for a hook lift stainless steel dump body, which must be compatible with the hook lift system specified in Section 3.4.2.  

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

3.4.3.1    Dimensions and Construction: 

The hook lift longitudinal shall be 6 inches x 224 inches x ¼ inch thick steel, primed and painted black. 

The interior dimensions of the dump body shall be 120 inches to 132 inches long x 84 inches wide with material shedding boxed top rails and 19 inches high 3-panel stainless steel double acting tailgate. The dump body shall carry a minimum of 2.8 yards without sideboards and a maximum of 4.4 yards with sideboards installed.

The dump body and tailgate shall be stainless steel. Dump body shall be of standard single wall construction. The top sides of the body shall have 24 inch x 8 inch hardwood boards and have two intermediate vertical side braces, plus 6 inch front and rear board pocket extension pockets. 

Bulkhead shall be a minimum of 24 inches high, 10-gauge stainless steel, with double bend top.

Cab shield shall be ¼ inch stainless steel. 

A tarp roller shall be self-contained in the body. Tarp shall be black mesh type and include a tarp roller kit, Buyers Products model DTR with tarp roller kit or comparable. 

The floor shall be 10-gauge thick.

The cross members shall be 3 inch structural steel channel spaced on 12 inch centers and full width rear bolster.

A two-way gate shall be provided with heavy duty cast stainless steel hardware, one (1) set of banjo eyes and chains with abrasion resistant covers

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.
[bookmark: _3.4.3.2__Tilt/Dump]
3.4.3.2    Tilt/Dump Interlock:

Dumping must be accomplished through a rear pivot point. Tilt and dump sections must lock into a rigid frame to support the body/container while in the dump mode. This must be accomplished without the use of springs, latches, rods, brackets, air/hydraulic cylinders, and or gravity to change modes of operation. The hook lift must be protected from out-of- sequence operation.

The tilt/dump interlock shall be performed by using the electronic controls of the hook/lift hydraulic system specified in Section 3.4.2.4

[bookmark: _Toc448401105][bookmark: _Toc467160939][bookmark: _Toc475717191]3.4.4    STAKE BODY (PRICE LINE: 4)

It is the intent of this section to describe the specifications for a hook lift stake body, which must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

3.4.4.1    Dimensions and Construction: 

The hook lift compatible stake body exterior dimensions shall be 132 inches to 144 inches long x 96 inches wide. 

The hook lift longitudinal shall be 6 inches x 224 inches x ¼ inch thick steel, primed and painted black. 

The floor shall be constructed of 3/16 inch diamond plate with a corrosion resistant undercoating. 

The outside edge of deck shall be 3-¼ inches fabricated 10-gauge channel.

The platform shall have a full perimeter 3/8 inch x 2 inch flat bar welded outside the stake pockets. The stake pockets shall be 2 inches x 4-¼ inch constructed of 3/16 inch steel, 24 inches on center.

The removable slatted stake sides shall be 40 inches to 42 inches high, with 4 rows of 16 gauge corrugated 6-½ inch slats.

The fixed bulkhead shall be 40 inches high and constructed from 10-gauge steel. Two (2) swivel D rings shall be welded to bulkhead. The bulkhead window shall be 20 inches x 13 inches. 

Key holes or ½ inch D rings, with swivel fittings, shall be located at the four corners of the body floor.

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc448401106][bookmark: _Toc467160940][bookmark: _Toc475717192]3.4.5    LANDSCAPE BOX BODY (PRICE LINE: 5)

It is the intent of this section to describe the specifications for a hook lift landscape style box body, which must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

3.4.5.1    Dimensions and Construction: 

The interior dimensions of the landscape box body shall be 132 inches to 144 inches long x 96 inches wide. 

The hook lift longitudinal shall be 6 inches x 224 inches x 3/16 inch thick steel, primed and painted black. 

The floor shall be constructed from 10-gauge smooth steel.

The sides shall be constructed from 10-gauge steel.

The cross members shall be 3 inch structural channel spaced on 12 inch centers.

The top rail shall be formed over 10-gauge steel sides.

There shall be 3 side posts per side. Side posts shall be constructed from 12-gauge steel.

The rear corner posts shall be constructed from 7-gauge steel.

The tailgate top shall be formed with 2 inches x 2 inches x 1/8 inch tubular frame work. 

The height of the sides shall be 40 inches high.

On the curb side, there shall be a 48 inch wide door for access.

The back of the box shall have swing open barn doors with a drawer style cam or trailer lock. 

A tarp roller shall be self-contained in the body. Tarp shall be black mesh type and include a tarp roller kit, Buyers model DTR with tarp roller kit or comparable. 

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc448401107][bookmark: _Toc467160941][bookmark: _Toc475717193]3.4.6    CHIPPER BODY (PRICE LINE: 6)

It is the intent of this section to describe the specifications for a hook lift chipper body, which must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

3.4.6.1    Dimensions and Construction: 

The chipper body’s exterior dimensions shall be 144 inches long x 96 inches wide.

The hook lift longitudinal shall be 6 inches x 224 inches x 3/16 inch thick steel, primed and painted black. 

The floor shall be constructed from 3/16 inch steel.

The sides shall be constructed from 12 gauge steel. The height of the sides shall be a minimum of 70 inches.

The cross members shall be 3 inch structural channel spaced on 16 inch centers.

The side top rail shall be 3 inches x 3 inches x 1/8 inch box tubing.

The side posts shall be 24 inch centers constructed from 12-gauge steel.

The rear corner posts shall be constructed from 7-gauge steel.

The tailgate top shall be formed with 3 inches x 3 inches x 1/8 inch tubular frame work. 

The tailgate shall consist of a half double barn door style with open top. 

The height of the tailgate to be determined at the time of the prebuild meeting. 

The top supports shall be 2 inches x 2 inches x 3/16 inch angle with mesh vents on both sides.

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc448401108][bookmark: _Toc467160942][bookmark: _Toc475717194]3.4.7    ENCLOSED STEEL STORAGE BODY (PRICE LINE: 7)

It is the intent of this section to describe the specifications for a hook lift enclosed steel storage body, which must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

3.4.7.1    Dimensions and Construction: 

The storage body exterior dimensions shall be 120 inches to 132 inches long x 96 inches wide with a minimum interior height of 72 inches.  

The hook lift longitudinal shall be 6 inches x 224 inches x 3/16 inch thick steel, primed and painted black. 

The floor shall be constructed from 1/8 inch sheet metal with 3 inch cross members on 16 inch to 18 inch centers.

The sides shall be constructed from 12-gauge sheet with 5 inch channel on 36 inch to 48 inch centers. 

The bulkhead shall be 10-gauge sheet with 4 inch channel uprights.

The roof shall be constructed from 12-gauge sheet with a 6 inch peak. 

The top rail shall be 3 inches x 3/16 inch fabricated beam.

The tailgate shall be a lockable trailer type made with 12-gauge sheet and 3 inch channel supports. 

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

[bookmark: _3.4.8_OPTION:_PLATFORM][bookmark: _Toc448401109][bookmark: _Toc467160943][bookmark: _Toc475717195]3.4.8    PLATFORM BODY WITH 300 -GALLON, GASOLINE POWERED HERBICIDE SPRAYER (PRICE LINE: 8)

It is the intent of this section to describe the specifications for a hook lift platform body with minimum 300-gallon, gasoline powered herbicide spreader, AG Spray LS-EL- 300, Reddick 300 Gallon Poly Skid, Fimco TSSK – 300, or comparable. The hook lift platform body must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

3.4.8.1    Dimensions and Construction: 

The platform body exterior dimensions shall be 120 inches long x 96 inches wide. 

The hook lift longitudinal shall be 6 inches x 224 inches x 3/16 inch thick steel, primed and painted black. 

The floor shall be 3/16 inch diamond plate.

The cross members shall be 3 inch structural channel spaced on 12 inch centers.

The outside edge shall be fabricated of 31/4 inches x 3/16 inch channel.

The bulkhead shall be 40 inches high and shall be constructed from 10-gauge steel.

The stake pockets shall be 24 inches on center.

The rub rail shall be 3/8 inch x 2 inch flat bar.

The bulkhead window shall be minimum 260 square inches. Dimensions to be confirmed at pre-manufacture/pre-production meeting.

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

3.4.8.2    Herbicide Sprayer:

A 300-gallon poly elliptical tank with full length metal cradle shall be mounted to the platform body. 

A 12-volt rewind hose reel with a minimum of 200 foot hose, Hannay model #E1520-17-18-LT or comparable, and an adjustable pattern spray gun, GreenGarde model # JD9 or comparable, shall be mounted to the rear of the tank.

A gasoline powered engine and pump shall be properly sized to meet the spray volume of 5 to 125 gallons per acre or more on swath widths of 5 to 40 feet with accuracy.

The cables/hoses from the control unit to the sprayer that control the operation/function of the sprayer shall have quick-disconnect connectors installed. 

Two (2) Radiarc sprayers, or comparable, shall be provided, one mounted on each side (left side and right side) of the platform body, close to the headboard.

Nozzle orifices supplied shall produce uniform droplets from 1000 to 5000 micrometers (microns). 

Ten (10) extra plugs and four (4) extra nozzles shall be included.

The exact layout and configuration shall be determined and approved by the Using Agency at pre-manufacture/pre-production meeting. 
 
3.4.8.3    In-Cab Controls: 

NOTE: The in-cab controls associated with this herbicide sprayer will be ordered utilizing Price line 13. Please refer to Section 3.4.13 of the Bid Solicitation {RFP}.

[bookmark: _Toc448401110][bookmark: _Toc467160944][bookmark: _Toc475717196]3.4.9    PLATFORM BODY WITH TOOLBOXES (PRICE LINE: 9)

It is the intent of this section to describe the specifications for a hook lift platform body with toolboxes, which must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

3.4.9.1    Dimensions and Construction:

The platform body exterior dimensions shall be 132 inches to 144 inches long x 96 inches wide.

The hook lift longitudinal shall be 6 inches x 224 inches x ¼ inch thick steel, primed and painted black. 

The floor shall be 1/8 inch tread plate steel.

The cross members shall be 3 inch x 4.1lb. /ft. structural channel on 12 inch centers.

The side rails shall be fabricated of 3 inch x 4.1lb. /ft. structural channel.

The bulkhead shall be 36 inches high and shall be constructed from 10-gauge steel.

Tailgate shall be 12 inches high x 10 gauge steel, hinged drop down style with retainers on top to secure to steel tubing rear corner posts.

The platform body shall be primed and painted withwhite enamel including underside.

Both sides of body shall have permanently installed toolboxes: dimensions: 18 inches x 18 inches x 60 inches, Buyers Products model 1702415 or comparable. Units shall have two (2) toolboxes on each side of the body. Toolboxes shall have a powder coated white finish and must be keyed alike.  

The latch shall be stainless steel “T” handle style. Any additional space on sides shall be filled with a 10-gauge filler panel at rear.

A removable 2 inch square steel tubing ladder rack shall extend from rear corners posts 6 inches above cab roof height. This ladder shall be removable with a ½ inch clevis pin on each side. A permanent 2 inch square tubing ladder rack section shall extend off the front bulkhead.

Hooks shall be installed on all four (4) corners of the ladder rack.

Two 2 inches x 120 inches long retracting ratchet tie downs shall be furnished to secure ladders to rack.

The ladder rack shall support a minimum of 300 lb.

The body must contain rollers under the body at the rear. The rollers must be the first thing to make contact with the ground.

[bookmark: _Toc448401111][bookmark: _Toc467160945][bookmark: _Toc475717197]3.4.10   DUMP BODY WITH MULTI-FUNCTION LIFTGATE/TAILGATE (PRICE LINE: 10)

It is the intent of this section to describe the specifications for a hook lift dump body with multi-function liftgate/tailgate, which must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications. 

3.4.10.1    Dimensions and Construction: 

The interior dimensions of the platform dump body shall be a minimum of 126 inches long x 84 inches wide. The exterior width dimension shall be 96 inches. 

The hook lift longitudinal shall be 6 inches x 224 inches x ¼ inch thick steel, primed and painted black. 

The floor shall be 10-gauge steel.

The cross members shall be 3 inches x 4.1lb. /ft. structural channel on 12 inch centers

The body sides shall be 13 inches high 10 gauge steel with 2 vertical ribs and boxed top rail.

The body front shall be 24 inches high 10 gauge steel.

The front bulkhead shall be 36 inches high 10 gauge steel. 

The body must contain rollers under the body at the rear with extended brackets, so when the body is off loaded the rear rollers hit the ground before the liftgate. The rollers must be the first thing to make contact with the ground. 

3.4.10.2    Tailgate:

The liftgate platform shall be 83 inches x 33 inches tread-plate steel with a 6 inch tapered load area, Tommy Gate G2 Series model 92-1650 LD33 Lift-N-Dump or comparable. The lift gate shall have a dual cylinder, parallel arm design. The lift and dump feature shall include pins to lock the platform in place when not in dump-trough mode. A platform latch shall activate the lift gate’s dump trough position. The lift gate shall have a loading capacity of 1,600 lb. The lift gate shall be powder coated and painted black. 

Steel hinged drop down tailgate shall be 12 inches high x 10-gauge with retainers on top to secure to rear corner posts.

Power and ground connection shall be run to the front driver’s side bulkhead area of body with a weather resistant, two pole plug connection of adequate amperage rating. Opposite end of plug shall be wired to battery through high amp resettable circuit breaker.

[bookmark: _3.4.11_OPTION:_9’][bookmark: _Toc448401112][bookmark: _Toc467160946][bookmark: _Toc475717198]3.4.11    SALT SPREADER (PRICE LINE: 11)

It is the intent of this section to describe the specifications for a 108 inch- 120 inch, medium duty, 3.5 cubic yard V-box electric salt spreader with single auger, Meyers MDV-A 844 Electric 8’ SS, Part #64451 or comparable. The salt spreader must be capable of hauling and spreading free flowing granular materials. The salt spreader and hook lift frame assembly must be compatible with the hook lift system specified in Section 3.4.2. 

All components specified in this section, as applicable, shall be fabricated and/or perform to within +/- five (5) percent of specifications.

The 108 inch to 120 inch stainless steel salt spreader shall be mounted upon the hook lift frame assembly specified in Section 3.4.2.3 that will safely allow the loading and unloading from the chassis mounted hook lift system. 

The unit shall mount on a hook lift frame with 10 gauge stainless steel floor to minimize carry-back onto chassis frame. Rollers shall be mounted under the rear of the hook lift frame. The rollers shall be install in such a manner to prevent the spinner from contacting the ground when unloading the body assembly. 

3.4.11.1    Dimensions and Construction: 

	Length-----------------------
	108 inch to 120 inch

	Hopper Height-------------
	44 inches

	Hopper Width--------------
	70 inches

	Spread width---------------
	Adjustable from a minimum of 4 feet to a maximum of 30 feet 

	Capacity Load-------------
	3.5 cu. yd.



The unit shall consist of a hopper, discharge chute, auger, spinner disc, two independent electric motors and all of the components necessary to make a complete operating system. 

All stainless steel used in the production of this unit shall be 12-gauge corrosion resistant, non-magnetic stainless steel. 

3.4.11.2    Hopper:

Each hopper side shall be constructed from a single piece of 12-gauge stainless steel and shall have a slope of no less than 45° to ensure free flow of material to the conveyor. The side shall have a minimum of six (6) 12-gauge stainless steel (three per side) external body supports for maximum rigidity.

The hopper ends shall be manufactured of 12-gauge stainless steel and be continuously welded to the hopper sides.

The complete hopper top edge shall be double crimped for additional support.

A combination stainless steel lift hook and hold down shall be furnished in each corner of the hopper.

A lever action style stainless steel feed gate shall be provided in the rear wall of the hopper. The feed gate shall have a maximum opening of 70 square inches, and a clamp to allow for a positive gate setting.

3.4.11.3    Electric Drive:

The spreader must be equipped with two independent industrial grade electric variable speed motors. The motors shall operate at a current of 60 amps. The electric motors shall utilize the vehicle’s existing electrical system. 

One motor shall be used to drive a spiral auger. The other motor shall be used to drive the spinner disc.

Dual speed controller shall be installed in cab of vehicle to provide ultimate spreading. 
 
The spreader shall include fork pockets and EIS (Electric Inter-Lock System) for safety. 

3.4.11.4    Spinner Assembly:

The distributor disc shall be minimum 12 inches in diameter and made of polyurethane with molded vanes.

The spinner disc shall be directly coupled to spinner motor. Extension shaft(s) and bearings shall not be used.  

There shall be a minimum of four (4) stainless steel external overlapping baffles, and two (2) internal baffles to control the direction and width of the spread pattern.  Three (3) of the external baffles shall be adjustable without the use of tools; the fourth shall be fixed to protect the truck. The entire spinner chute and baffles shall be manufactured from 12-gauge stainless steel.

The entire spinner assembly shall swing-up by removing one stainless steel pin and hydraulic quick disconnect.

3.4.11.5    Top Screens:
 
A two-section center hinged top screen shall be provided. The screen sections shall be manufactured from ¼ inch rod welded to form square openings of 3 inches and framed by J formed channel.

A simple Drop-n-Lock type hinge arrangement shall be provided to eliminate the need for hardware that may vibrate loose.

3.4.11.6    Safety Lighting:

A strobe light system shall be mounted on the rear of spreader wall to ensure visibility. The light system shall include two (2) amber LED strobes, Whelen M6 or comparable. 

3.4.11.7    In-Cab Controls: 

The in-cab controls associated with this salt spreader will be ordered utilizing Price line 14. Please refer to Section 3.4.14 of the Bid Solicitation {RFP}.


[bookmark: _Toc448401113][bookmark: _Toc467160947][bookmark: _Toc475717199]3.4.12    SNOW PLOW (PRICE LINE: 12)

It is the intent of this section to describe of the specifications for a 9’ snow plow, Western/Boss/Meyer/Fisher Mount or comparable.

3.4.12.1     Dimensions and Capacities: 

Blade Width: 108 inches		
Blade Height: 29 inches or greater		
Plowing Angle: 30˚ right or left, to provide minimum 93 inch swath
Cutting Edge: ½ inch x 6 inches
Type: 11 or 12 gauge steel				

3.4.12.2    Equipment:

Marker Guides: 2 high visibility, flexible marker guides 
Controls – Hand Held type controller	: Boss SmartTouch2 Handheld Controller, Western Cab Command Handheld Controller or comparable.	
Snow Plow Lights			
Standard Deflector: Rubber with steel backer plate

3.4.12.3    Mounting:

The snow plow must be removable by quick disconnect pins, as one complete unit including blade, lift assemblies and lights. Removal of lift shall also remove lights and electro-hydraulic lift unit. The vehicle bumper must remain in the same position as originally installed by the vehicle manufacturer.

3.4.12.4    Plow Control System:

Lift, lower and power angle shall be self-contained and consist of an electro-hydraulic pump, reservoir, electric solenoid control valves, lift cylinder, power angle cylinders, hoses, quick disconnects and wire harness.

Please note that the unit must have full hydraulic power for lift, lower and angle functions. No exceptions.

3.4.12.5    Hydraulically Operated Mechanical Chain Lift System: 

The hydraulically operated mechanical chain lift system shall provide float and short chain capabilities to transport the plow in case of inoperable condition.

[bookmark: _3.4.13_OPTION:_IN-CAB][bookmark: _Toc448401114][bookmark: _Toc467160948][bookmark: _Toc475717200]3.4.13    IN-CAB CONTROLler FOR HERBICIDE SPRAYER (PRICE LINE: 13)

3.4.13.1 This section and price line item is for the purchase and installation of an in-cab controller for the herbicide sprayer specified in Section 3.4.8 of the Bid Solicitation {RFP}. The in-cab controller shall be compatible with herbicide sprayer and applicable components. Please note that this price line item is for an in-cab control only and not for the actual herbicide sprayer. Since the cab and chassis (Section 3.4.1 of the Bid Solicitation {RFP}) and Hook Lift System (Section 3.4.2 of the Bid Solicitaion {RFP}) allow for the interchangeability of various bodies between trucks, the DOT intends to have this in-cab control installed in most of its trucks. 

[bookmark: _3.4.14_OPTION:_IN-CAB][bookmark: _Toc448401115][bookmark: _Toc467160949][bookmark: _Toc475717201]3.4.14    IN-CAB CONTROLler FOR SALT SPREADER (PRICE LINE: 14)

3.4.14.1 This section and price line item is for the purchase and installation of an in-cab controller for the salt spreader specified in Section 3.4.11 of the Bid Solicitation {RFP}. The in-cab controller shall be compatible with salt spreader and applicable components. Please note that this price line item is for an in-cab control only and not for the actual salt spreader. Since the cab and chassis (Section 3.4.1 of the Bid Solicitation {RFP}) and Hook Lift System (Section 3.4.2 of the Bid Solicitaion {RFP}) allow for the interchangeability of various bodies between trucks, the DOT intends to have this in-cab control installed in most of its trucks. 

[bookmark: _3.4.6_OPTION:_ONE_SET_OF_PARTS,_SER][bookmark: _3.4.3_OPTION:_ONE][bookmark: threefourfive][bookmark: threefourseven][bookmark: _3.4.11_OPTION:_ONE][bookmark: _3.4.15_OPTION:_ONE][bookmark: _Toc133985135][bookmark: _Toc158707874][bookmark: _Toc284596769][bookmark: _Toc293045211][bookmark: _Toc448401116][bookmark: _Toc467160950][bookmark: _Toc475717202]3.4.15    ONE SET OF PARTS, SERVICE AND O&M MANUALS (PRICE LINE: 15)

3.4.15.1    Optional Manuals: 

One set of parts, service and operation and maintenance manuals for each and every assembly system and/or component that makes up the unit shall be provided as follows:

 1 - set of parts manuals (illustrations and text) bound or with binders, or on CD-ROM, if unavailable bound.

 1 - set of complete shop repair (factory service) manuals bound or with binders or on CD-ROM, if unavailable bound.

 1 - set of complete operation and routine maintenance manuals

 1 - set of electrical schematics

 1 - set of troubleshooting manuals for the gas engine on sprayer

Examples of assembly systems and/or components include, but are not necessarily limited to:

	a.
	Hydraulic pump and hydraulic systems

	b.
	Engine, drives and chassis

	c.
	Transmission

	d.
	Electrical system

	e.
	Lubrication system

	
	


The manuals shall be delivered directly to the Using Agency upon delivery. Failure to supply these manuals may delay approval of invoices for payment.

[bookmark: _Toc467160951][bookmark: _Toc475717203]3.4.16    TECHNICAL SUPPORT (PRICE LINE: 16)

3.4.16.1    Operator Training:

The Vendor {Contractor}, in cooperation with all aftermarket installers/subcontractors, shall provide training as described below. 

The Vendor {Contractor} shall collaborate with the Using Agency to provide a four (4) hour operator training session for every completed truck delivered with a maximum of 5 agency personnel. This training shall be made available throughout the duration of the Blanket P.O. {Contract} and any extensions thereof.

Complete instructions on the operation and maintenance of each unit and a demonstration on the operation of the unit shall be given by the Vendor {Bidder}. 

The training shall consist of, but is not limited to, operator training with instruction on proper operation of the unit, safety, preventive maintenance and repair.

The Vendor {Contractor} and the Using Agency shall agree on the content of this material, based on the differences between the trucks contained herein and any existing truck in the Using Agency’s fleet. 

This demonstration shall be a formal training session and shall be arranged with the Vendor {Contractor}, conducted within one (1) week of delivery of the first unit, at the convenience of the Using Agency. 

The training session shall be conducted at the location of delivery or at a field location within the State of New Jersey.

3.4.16.2    Mechanics Training:	

The Vendor {Contractor}, in cooperation with aftermarket installers/subcontractors, shall provide technical training for all components of the complete truck. 

The Vendor {Contractor} shall collaborate with the Using Agency to provide a one (1) eight (8) hour day mechanics training session for every 5 completed trucks delivered with a maximum of 5 agency personnel.

The Vendor {Contractor} shall provide training for the listed critical areas. 

This training shall consist of, but is not limited to, the same training as is provided to technicians employed by dealerships who sell these components, with the following exceptions:

Course content shall be tailored to meet the specific needs of the Using Agency mechanics, and shall not place emphasis on areas or components not specified in these specifications. Course shall also include as much hands-on content as needed to reinforce lecture content.

	Cab and Chassis Systems 
a. Engine diagnostics and repair, including electronic controls, fuel system and emissions system. 
b. Electrical system controllers, operation and diagnostics.
c. Automatic transmission diagnostics and repair.

Body Builder-Installed Components
a. Hydraulic system operation, diagnostics and repair. 
b. Electrical accessories operation, circuits, diagnostics and repair. 
c. Warning light system operation, diagnostics and repair.

This demonstration shall be a formal training session and shall be arranged with the Vendor {Contractor}, conducted within one (1) week of delivery of the first unit, at the convenience of the Using Agency. 

The training session shall be conducted at the location of delivery or at a field location, within the State of New Jersey.

If additional training is required, it shall be part of the line item for mechanics training and shall cover, but not be limited to the above topics. The training shall be scheduled with the Using Agency and shall be a one (1) eight (8) hour day mechanics training session with a maximum of 5 agency personnel. This training shall be made available throughout the duration of the Blanket P.O. {Contract} and any extensions thereof.

[bookmark: _Toc448401118][bookmark: _Toc467160952][bookmark: _Toc475717204]3.5     BLANKET P.O. {CONTRACT} IMPLEMENTATION

[bookmark: _Toc475717205]3.5.1  PLACING ORDERS FOR BLANKET P.O. {CONTRACT} UNITS

3.5.1.1  This term Blanket P.O. {Contract} does not permit Using Agencies to order any option that is not specified in this Bid Solicitation {RFP}.

3.5.1.1.1  The Vendor {Contractor} shall not substitute any item (part, component, equipment, feature, accessory, material, performance, capacity, rating, design or control), which is a part of the Blanket P.O. {Contract} unit, without written authorization to do so from the Procurement Bureau.

3.5.1.2  During the Blanket P.O. {Contract} period, no change is permitted in any terms or conditions unless the Vendor {Contractor} receives written approval from the Procurement Bureau.

3.5.1.3  No dealer's accessories or options, or any other purchases which are not specified in this Bid Solicitation {RFP} shall be offered. 

3.5.1.4  Trade-ins are not permitted under the term Blanket P.O. {Contract} established as a result of this Bid Solicitation {RFP}.

3.5.1.5  Leasing of units is not permitted under the term Blanket P.O. {Contract} resulting from this Bid Solicitation {RFP}.

3.5.1.6  An offer to sell a non-Blanket P.O. {Contract} unit against two or more purchase orders, one for the Blanket P.O. {Contract} unit and one or more for non-Blanket P.O. {Contract} items, constitutes a serious violation of the Blanket P.O. {Contract} and may be the basis for termination of the Blanket P.O. {Contract} and may disqualify the Vendor {Contractor} from award of future State Blanket P.O.s {Contracts}.

[bookmark: _Toc475717206]3.5.2  PRODUCT BROCHURE

3.5.2.1  Sales literature and color charts shall be made available to agencies and NJ State inspectors on an "as requested" basis.

3.5.2.2  The State reserves the right to communicate with the Vendor {Contractor} and request any information regarding Vendor {Contractors} obligations under the Blanket P.O. {Contract}, and require acknowledgement of such communication from the Vendor {Contractor} during the term of the Blanket P.O. {Contract} and any extension(s) thereof. Failure to acknowledge and provide the required information within twenty-four (24) hours constitutes a Blanket P.O. {Contract} violation which may result in Blanket P.O. {Contract} cancellation.



[bookmark: _Toc475717207]3.5.3  CONFIRMATION OF ORDERS

3.5.3.1  Purchase order confirmation must be submitted to each Using Agency for each order accepted, to the attention of the contact person stated in the purchase order.

3.5.3.2  The Vendor {Contractor} must provide the order confirmation promptly following factory order entry.

3.5.3.3  Order confirmation shall mean that the Vendor {Contractor} has received the purchase order, has reviewed it for compatibility with the unit currently on Blanket P.O. {Contract}, has resolved any non-compatibility problems with the Using Agency, has entered the order with the manufacturer and that the manufacturer has accepted the order and assigned an order number and anticipated build and delivery dates.

3.5.3.4  The Vendor {Contractor} shall not accept any purchase order after the vehicle manufacturer’s cut-off date, unless instructed otherwise by the Ordering Agency in writing. If an order is not accepted for production by the manufacturer, the Vendor {Contractor} shall return the purchase order with "canceled" marked on the purchase order with an authorized signature next to it. No exception shall be permitted.

[bookmark: _Toc475717208]3.5.4  INSPECTION OF UNITS

3.5.4.1 Pre-production/pre-installation meeting and inspection: The Vendor {Contractor} shall coordinate and attend a post-order pre-production meeting, if required by the Using Agency, at a location convenient to the Using Agency, to provide all necessary information prior to building any prototype unit or scheduling the production. Only after the post-order pre-production meeting, if required by the Using Agency, and subsequent approval from the Using Agency shall the Vendor {Contractor} begin the production. The Vendor {Contractor} shall coordinate with the Using Agency for a pre-paint inspection for each unit ordered, if required by the Using Agency.

3.5.4.2 The State reserves the right to inspect the Vendor {Bidder} and/or aftermarket installer(s)' and/or Vendor {Contractor}’s facility. This provision applies during the Quote {Proposal} evaluation period, the Blanket P.O. {Contract} term and any extension(s) thereof. 

3.5.4.3 Pre-acceptance Inspections: The State Using Agency reserves the right to inspect the unit at the Vendor’s {Contractor's} facility or require that the Vendor {Contractor} make the unit available for inspection at the agency site. If, during inspection at the agency site, it becomes apparent that corrections/alterations must be made to the unit to comply with the Blanket P.O. {Contract} specifications which cannot be accomplished at the State Using Agency facility, the unit will be rejected and the Vendor {Contractor} must transport the unit to its facility at no expense to the agency. After the Vendor {Contractor} corrects the deficiencies, the Vendor {Contractor} must re-deliver the unit to the State Using Agency for re-inspection at the expense of the Vendor {Contractor}. 

3.5.4.4 For all inspections performed at the Vendor’s {Contractor's} site, the Vendor {Contractor} must provide a bay in the repair shop to facilitate the inspection of the unit.

3.5.4.5 The final inspection and acceptance of the unit shall occur at the State Using Agency.

3.5.4.6 OEM Equipment/Parts: All of the standard and optional equipment/parts provided shall be original equipment manufacturers items when available.

3.5.4.7 The Vendor {Contractor} must make arrangements for the Using Agency’s inspection of each vehicle prior to the delivery and acceptance of the vehicle by the Using Agency. Prior to presentation for inspection, it shall be the Vendor’s {Contractor's} responsibility to pre-inspect each unit. Each unit presented for inspection shall be accompanied by an inspection package including, but not limited to, the following: purchase order, line set sheet (when available) - brief list of all features, items and accessories included in the unit, pre-delivery inspection (PDI), and dealer's pre-inspection prep checklist. The checklist will list the responsible prep mechanic and acknowledge that the vehicle conforms to pre-delivery specifications and that all added equipment and accessories have been properly installed.

3.5.4.8 The Vendor {Contractor} shall notify the State Using Agency by fax and email that the unit is ready for inspection.

3.5.4.9  Delivered units will be inspected within ten (10) working days. If a unit has been accepted, the warranty shall commence on the date of final acceptance, or if a unit has been rejected, the Vendor {Contractor} will be notified. The notice will indicate the reason(s) for rejection. If rejected, the Vendor {Contractor} shall try to rectify the problem(s) at the State Using Agency site. If the problem cannot be corrected at the agency site, the rejected unit must be removed by the Vendor {Contractor} at its own expense. The Vendor {Contractor} shall present the corrected unit for re-inspection within ten (10) working days. No additional freight or transportation charges are permitted.

3.5.4.10 Within five (5) working days of the Vendor’s {Contractor’s} notification, the State Using Agency will, if desired, send a team of qualified inspectors to the Vendor’s {Contractor's} facility to accomplish the inspection of the unit(s) before delivery to the agency. The Vendor {Contractor} must properly itemize, organize and segregate all units.  

3.5.4.11 Non-State Agencies authorized to purchase under this Blanket P.O. {Contract} will make arrangements for unit inspection directly with the Vendor {Contractor}. All units must be delivered to each Using Agency’s designated destination at no additional cost.

3.5.4.12 Inspected units which do not comply with the Blanket P.O. {Contract} requirements will be rejected. The Vendor {Contractor} must correct all rejected units and the corrected unit(s) must be presented for re-inspection within ten (10) working days. The Using Agency may cancel the purchase order if the Vendor {Contractor} fails to correct any problem.

3.5.4.13 No additional freight or transportation charges are permitted under this Blanket P.O. {Contract}.  

[bookmark: MANUFACTURERSCERTIFCATEOFORIGIN][bookmark: NEWCARINSPECTIONSTICKER][bookmark: _Toc475717209]3.5.5  DELIVERY AND FINAL ACCEPTANCE

3.5.5.1  The Vendor {Contractor} must make arrangements for delivery of unit(s) as instructed by the Using Agency within 15 calendar days of Vendor’s {Contractor's} receipt of unit(s) from the manufacturer. All units must be delivered within 30 calendar days of Vendor’s {Contractor's} receipt of unit(s) from the manufacturer. All units must be delivered to each Using Agency's designated destination at no additional cost.

3.5.5.2 All deliveries of units must be made upon approval and as instructed by the Using Agency, by prior arrangement only, during working hours, except on legal holidays.

3.5.5.3  No unit will be accepted at the final delivery point without all supporting documentation and paperwork completed and delivered with the unit, which include the certificate of origin, warranty, any specified manuals, invoice and key sets (if applicable). No unit will be considered accepted until it has undergone final inspection at the delivery point.

3.5.5.4 For purchases by State Agencies, the manufacturer's certificate of origin must be made out to the State of New Jersey, and presented at the time of delivery. Purchase order number and requisition number must be indicated on the upper left hand corner. The Vendor {Contractor} shall not furnish the New Jersey Certificate of Title (certificate of ownership). The State will title the unit upon receipt of the manufacturer's certificate of origin. Other governmental entities authorized to purchase under this Blanket P.O. {Contract} will make arrangements for titling units directly with the Vendor {Contractor}. 

3.5.5.5 No advertising shall appear on any unit delivered under the terms of the Blanket P.O. {Contract}. Further, the Vendor {Contractor} shall not affix the dealer name to the unit. Units delivered to final destinations with dealer's advertising will be rejected.

3.5.5.6 No more than ten (10) units per day and fifty (50) units per week (based on a 5-day work week) will be accepted at each delivery site. When necessary, and with the consent of both the agency and the Vendor {Contractor}, the number of units delivered per day may be increased.

3.5.5.7 All vehicles must be delivered with the manufacturer suggested retail price label affixed to the window. The label shall not be removed prior to delivery to the New Jersey agency.

3.5.5.8 All delivered units must be clean both inside and outside. Manufacturer's standard items, such as hubcaps, floor mats, jack and lug wrench and the like, shall be provided and installed by the Vendor {Contractor} prior to delivery.

3.5.5.9 Complete instructions on the care and maintenance of the unit and a demonstration of its operation shall be given by the Vendor {Contractor} at the time of delivery and acceptance to the agency, if so requested by the Using Agency.

3.5.5.10 The Vendor {Contractor} shall indicate the delivery location of the unit on the factory order, so that recall notices will indicate the delivery location for each unit.

3.5.5.11 The Vendor {Contractor} must deliver the units with an index card or other label/card, visible through the windshield, bearing the following information, in typed or printed form:

Vendor's {Contractor’s} name
Purchase order number (if applicable)
Requisition number
Stock number
Serial number

Note: Units without this information will not be accepted.

3.5.5.13 No unit will be accepted without a New Jersey Motor Vehicle new vehicle inspection sticker in place as prescribed by law, correctly punched to the month of delivery and acceptance or appropriate Diesel Emission Approval Sticker. Out of State Vendors {Contractors} must comply with this requirement without any additional cost or delay. Failure to comply with this provision will result in the rejection of the unit.

[bookmark: _3.5.6__WARRANTIES][bookmark: _Toc475717210]3.5.6  WARRANTIES

3.5.6.1 The manufacturer's standard warranty must be supplied with each unit at the time of delivery and shall be in typed form. The warranty commences with the acceptance of the unit at the delivery site, following the final inspection. 

[bookmark: _Toc475717211]3.5.7  WARRANTY REQUIREMENTS

3.5.7.1 The Vendor {Contractor} shall ensure that the manufacturer whose product is supplied has a servicing dealer or service location able to provide warranty and recall service and/or repair within twenty four (24) hours of notification by the Using Agency. Users of this Blanket P.O. {Contract} should contact the Vendor {Contractor} in cases where warranty service/repair is to be performed at a place other than the original place of purchase to arrange for a servicing dealer proximate to their location.

3.5.7.2 The Vendor {Contractor} must perform any warranty service/repair/recall, which will be at Vendor’s {Contractor's} own expense. Events beyond Vendor’s {Contractor's} control, such as lack of parts due to strikes and unforeseen acts of God, shall constitute valid reasons for delay in making necessary repairs. However, the State will make such determination.

3.5.7.3 Manufacturer's Warranty Form: The Vendor {Contractor} must provide the appropriate warranty forms.

[bookmark: _Toc475717212]3.5.8  PAYMENT

3.5.8.1 Invoices will be processed for payment only after final acceptance of the units by the Using Agency and the delivery ticket has been signed off by an authorized representative of the Using Agency. Partial payments may be made for unit(s) accepted, if billed separately. Timely payment discounts will be taken if offered by the Vendor {Contractor}. The State reserves the right to make payments directly or through a third party.

3.5.8.2 The State reserves the right to order units through a line of credit. For these orders, the Vendor {Contractor} will receive a letter from the State in lieu of a purchase order. Line of credit letters must be accepted by the Vendor {Contractor} on the same basis as regular purchase orders. All terms and conditions that apply to purchase orders will apply to line of credit letters. 

[bookmark: _Toc475717213]3.5.9  SUBSTITUTION OF DISCONTINUED PRODUCTS

The Vendor {Contractor} may offer a substitution for any product discontinued by the manufacturer in its Blanket P.O. {Contract}. The State may consider substituting the discontinued model with a new model provided that the unit offered meets or exceeds the Blanket P.O. {Contract} specifications. All substitutions must be approved by the State. 

The Vendor {Contractor} must notify the State immediately in writing to the Division’s assigned Procurement Specialist stating that an item has been discontinued by the manufacturer along with supporting documentation from that manufacturer that the item has been discontinued. The Vendor {Contractor} must provide in its letter the discontinued model number, model number of the new product being offered, detailed literature for the new product being offered, the price of the discontinued item and the price of the product being offered as a replacement. The State will not approve the substitution of a discontinued item without all of the above information.

The replacement product should be offered to the State at that same price as the discontinued product. 

[bookmark: _Toc475717214]3.5.10  MANUFACTURER’S CUT-OFF DATE

3.5.10.1 The Vendor {Contractor} must notify the Procurement Bureau of the manufacturer's order cut-off date, as soon as that date is made available by the vehicle manufacturer to the Vendor {Contractor}. Cut-off Date Notification must be emailed to the assigned Procurement Specialist, or faxed to the Fleet Unit at 609-292-1114. 

3.5.10.2 Should a potential awardee be notified by a vehicle manufacturer of a cut-off date after the Quote {Proposal} opening and after receiving a letter of intent to award, but before Blanket P.O. {Contract} award has been finalized, the awardee must immediately notify the Procurement Bureau in writing. 

3.5.10.3 Failure to fax the cut-off-date notification on time may be considered a violation of the Blanket P.O. {Contract} terms and conditions and may result in termination of the Blanket P.O. {Contract} for cause.

3.5.10.4 All orders placed by the published cut-off date from either the State or cooperative purchasing program participants must be accepted by the Vendor {Contractor}. These orders may be hand delivered, or faxed with hard-print purchase orders to follow. The State also reserves the right to order by means of "a letter of intent to purchase" with purchase order to follow.

3.5.10.5 The Vendor {Contractor} is encouraged to offer, during the Blanket P.O. {Contract} term and any extension thereof, the contracted or later model year vehicle of configuration meeting or exceeding the Blanket P.O. {Contract} specifications at the same Blanket P.O. {Contract} terms, conditions and pricing after the manufacturer’s cut-off date. 

3.5.10.6 If a manufacturer is unable to build a vehicle for which an order has been placed by the manufacturer's cut-off date, the Vendor {Contractor} must immediately notify the Procurement Bureau by fax or e-mail. At a minimum, the letter shall provide the following information. 

3.5.10.6.1  Purchase order number or line of credit letter date;

3.5.10.6.2  The make, model and quantity of vehicles ordered; and

3.5.10.6.3  Whether the manufacturer has offered to price-protect and build these vehicles for the next model year.
1.0 
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[bookmark: _Toc400531492][bookmark: _Toc428533963][bookmark: _Toc475717215] QUOTE {PROPOSAL} PREPARATION AND SUBMISSION

1. [bookmark: _Toc400531493][bookmark: _Toc428533964][bookmark: _Toc475717216]General

Quotes {Proposals} including Vendor {Bidder} proposed terms and conditions may be accepted, but Vendor {Bidder} proposed terms or conditions that conflict with those contained in the Bid Solicitation {RFP} as defined in Section 2.0 of this Bid Solicitation {RFP}, or that diminish the State’s rights under any Blanket P.O. {Contract} resulting from the Bid Solicitation {RFP}, will be considered null and void. The State is not responsible for identifying conflicting Vendor {Bidder} proposed terms and conditions before issuing a Blanket P.O. {Contract} award. It is incumbent upon the Vendor {Bidder} to identify and remove its conflicting proposed terms and conditions prior to Quote {Proposal} submission. In the event that a Vendor {Bidder} intends to propose terms and conditions contrary to the Bid Solicitation {RFP}, these Vendor {Bidder} proposed terms and conditions shall only be considered if submitted pursuant to the procedure set forth in Section 1.3.1 of this Bid Solicitation {RFP}. Vendors {Bidders} shall not submit exceptions on the “Terms and Conditions” Tab through NJSTART. Under no circumstance is the State required to accept a Vendor’s {Bidder’s} exception to the Bid Solicitation {RFP}. 

In the event that prior to Notice of Intent to Award, the Division notifies the Vendor {Bidder} of any such conflicting Vendor {Bidder} proposed term or condition and the conflict it poses, the Division may require the Vendor {Bidder} to either withdraw it or withdraw its Quote {Proposal}. 

After award of Blanket P.O. {Contract}:

a. if conflict arises between a Vendor {Bidder} proposed term or condition included in the Quote {Proposal} and a term or condition of the Bid Solicitation {RFP}, the term or condition of the Bid Solicitation {RFP} will prevail; and

b. if the result of the application of a Vendor {Bidder} proposed term or condition included in the Quote {Proposal} would diminish the State’s rights, the Vendor {Bidder} proposed term or condition will be considered null and void.

The Vendor {Bidder} is advised to thoroughly read and follow all instructions contained in this Bid Solicitation {RFP}, including the instructions on the Bid Solicitation’s {RFP’s} Offer and Acceptance Page {Signatory Page} and through all QRGs located on the NJSTART Vendor Support Page, in preparing and submitting its Quote {Proposal}.

Use of URLs in a Quote {Proposal} should be kept to a minimum and may not be used to satisfy any material term of a Bid Solicitation {RFP}. If a preprinted or other document included as part of the Quote {Proposal} contains a URL, a printed (or if a Quote {Proposal} is submitted electronically, electronic) copy of the URL page shall be provided and will be considered as part of the Quote {Proposal}. Additional URLs on the copy of the URL page shall not be considered as part of the Quote {Proposal} unless a copy of those URL pages are also provided. 

[bookmark: _Toc400531494]The forms discussed herein and required for submission of a Quote {Proposal} in response to this Bid Solicitation {RFP} are available on the Division’s website (http://www.state.nj.us/treasury/purchase/forms.shtml) unless noted otherwise.

1. [bookmark: _Toc428533965][bookmark: _Toc475717217]QUOTE {Proposal} Delivery and Identification

A Quote {Proposal} must arrive at the Division in accordance with this Bid Solicitation’s {RFP’s} instructions within the time frames noted on the Bid Solicitation {RFP} cover sheet and on the “Summary” page of the Bid Solicitation in NJSTART. Vendors {Bidders} submitting electronic Quotes {Proposals} via NJSTART are cautioned to allow adequate time to ensure timely uploads of all Quote {Proposal} documents to mitigate unforeseen delays or issues. Vendors {Bidders} submitting hard copy Quotes {Proposals} are cautioned to allow adequate delivery time to ensure timely delivery of Quotes {Proposals}. State regulation mandates that late Quotes {Proposals}, regardless of submission method, are ineligible for consideration. THE EXTERIOR OF ALL QUOTE {PROPOSAL} PACKAGES SHALL BE LABELED WITH THE BID SOLICITATION {RFP} IDENTIFICATION NUMBER AND THE FINAL QUOTE {PROPOSAL} SUBMISSION DATE OR RISK NOT BEING RECEIVED IN TIME.

1.2 [bookmark: _Toc428533966][bookmark: _Toc475717218]njstart electronic submission VS. hard copy SUBMISSION INSTRUCTION

1.2.1 [bookmark: _Toc428533967][bookmark: _Toc475717219]NJSTART SUBMISSION OF QUOTE {PROPOSAL}

If the Vendor {Bidder} is submitting a NJSTART Quote {Proposal}, hard copy submission is not required. If a Vendor {Bidder} is submitting a hard copy Quote {Proposal} please see Section 4.3.2 for number of complete and exact copies. Vendors {Bidders} may refer to the QRGs “Vendor Registration” and “Submit a Quote” for additional instructions detailing how to enroll in NJSTART and submit a NJSTART electronic Quote {Proposal}. QRGs are located on the NJSTART Vendor Support Page. If the Vendor {Bidder} submits both a NJSTART and a hard copy of the Vendor’s {Bidder’s} Quote {Proposal}, the NJSTART Quote {Proposal} will prevail in the event of a discrepancy between the electronic and paper versions. 

When submitting a NJSTART Quote {Proposal}, do not use any symbols (i.e., #, @, $, &, *) in the filename. In addition, the Vendor {Bidder} should name each uploaded electronic file and folder with the information in the brackets [] below as follows: 

[Vendor {Bidder} name][Bid Solicitation {RFP} number]. Example: vendornameXXDPPXXXXX

If the Vendor {Bidder} submits a Quote {Proposal} electronically through NJSTART, the Vendor {Bidder} should select the “Confidential” option in NJSTART for attachments on the “Attachments” Tab to request that the documents not be displayed publicly through NJSTART. 

Note: Marking an attachment as "Confidential" in NJSTART shall not constitute the Vendor's {Bidder's} designation of the attachment as exempt from public disclosure under OPRA and/or the common law as outlined in Section 1.4.4.

1.2.2 [bookmark: _Toc400531497][bookmark: _Toc428533968][bookmark: _Toc475717220]HARD COPY SUBMISSION

If the Vendor {Bidder} is submitting a hard copy Quote {Proposal}, the Vendor {Bidder} must submit the following:

a. One (1) complete Quote {Proposal}, comprising all volumes and including original, physical signature, clearly marked as the “ORIGINAL” Quote {Proposal}. 

b. One (1) complete and exact ELECTRONIC copy of the original Quote {Proposal} in PDF file format on disc (CD or DVD). These should be cover to cover copies, and should not be password protected. THE PRICE SCHEDULE SHALL NOT BE INCLUDED ON THIS DISC. 

c. One (1) complete and exact ELECTRONIC copy of the original price schedule in Microsoft Excel file format on disc (CD or DVD). This should be a cover to cover copy, and should not be password protected.

Copies are necessary in the evaluation of the Quote {Proposal} and for record retention purposes. A Vendor {Bidder} failing to provide the requested number of copies will be charged the cost incurred by the State in producing the requested number of copies. The Vendor {Bidder} should make and retain a copy of its Quote {Proposal}. 

1.3 [bookmark: _Toc400531498][bookmark: _Toc428533969][bookmark: _Toc475717221]QUOTE {Proposal} Content

The Quote {Proposal} should contain the State supplied price sheet/schedule(s) and all forms/documents required by the Bid Solicitation {RFP}. The Vendor {Bidder} is cautioned to carefully read the Bid Solicitation {RFP} to ensure that all required forms are submitted with the Vendor’s {Bidder’s} Quote {Proposal}. NOTE: Failure to submit required forms/documents may result in the Vendor’s {Bidder’s} Quote {Proposal} being deemed non-responsive.
	
A Vendor {Bidder} submitting a Quote {Proposal} through NJSTART must complete its Price Schedule as an attachment using the State-supplied price sheet/schedule(s) accompanying this Bid Solicitation {RFP} and located on the “Attachments” Tab (See Section 4.4.5 of this Bid Solicitation {RFP}). The Vendor {Bidder} must enter a Unit Cost of $1.00 for each price line item on the “Items” Tab in NJSTART. The Vendor {Bidder} is instructed to do so only as a mechanism to comply with Bid Solicitation {RFP} Section 6.8 and prevent all pricing from being publicly displayed in NJSTART. In the event that a Vendor {Bidder} using NJSTART to submit a Quote {Proposal} uploads a price sheet/schedule attachment and completes the Items Tab in NJSTART (instead of entering a Unit Cost of $1.00 as instructed), the price sheet/schedule attachment will govern. 

1.3.1 [bookmark: _Toc108508238][bookmark: _Toc428533970][bookmark: _Toc475717222] Forms, rEGISTRATIONS and CERTIFICATIONS required with QUOTE {Proposal}

Vendors {Bidders} should refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation {RFP} through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

In the event that a Vendor {Bidder} fails to attach a required form, or the attached form is deemed deficient, the Division may access the Primary Form to be considered as part of the Quote {Proposal}.

Vendors {Bidders} submitting forms through hard copy must complete the full version of the form and may refer to instructions included within the forms on the Division’s website.

Vendors {Bidders} are under a continuing obligation to report updates to the information contained in its required forms whether submitting through NJSTART or as a hard copy.

Unless otherwise specified, forms must contain an original, physical signature, or an electronic signature pursuant to Section 1.3.4 of this Bid Solicitation {RFP}.

1.3.1.1 [bookmark: _4.4.1.1_Ownership_Disclosure][bookmark: _4.4.1.1_Signatory_page]OFFER AND ACCEPTANCE PAGE {Signatory page}

[bookmark: OLE_LINK5][bookmark: OLE_LINK6]The Vendor {Bidder} shall complete, including signature of an authorized representative of the Vendor {Bidder}, and submit the Offer and Acceptance Page {Signatory Page} accompanying this Bid Solicitation {RFP} (whether submitted through NJSTART or as a hard copy). If the Vendor {Bidder} is a limited partnership, the Offer and Acceptance Page {Signatory Page} must be signed by a general partner. All information requested must be submitted. If the Vendor {Bidder} is a joint venture, the Offer and Acceptance Page {Signatory Page} must be signed by a principal of each party to the joint venture. Failure to comply will result in rejection of the Quote {Proposal}.

1.3.1.1.1  MACBRIDE PRINCIPLES CERTIFICATION

The Vendor {Bidder} must certify pursuant to N.J.S.A. 52:34-12.2 that it is in compliance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of its compliance with those principles. See Section 2.5 of the SSTC and N.J.S.A. 52:34-12.2 for additional information about the MacBride principles. 
 
By signing the Bid Solicitation {RFP} Offer and Acceptance Page {Signatory Page}, the Vendor {Bidder} is automatically certifying that either:

a. The Vendor {Bidder} has no operations in Northern Ireland; or

b. The Vendor {Bidder} has business operations in Northern Ireland and is committed to compliance with the MacBride principles.

A Vendor {Bidder} electing not to certify to the MacBride Principles must nonetheless sign the Bid Solicitation {RFP} Offer and Acceptance Page {Signatory Page} AND must include, as part of its Quote {Proposal}, a statement indicating its refusal to comply with the provisions of this Act.

1.3.1.1.2 No SUBCONTRACTOR CERTIFICATION 

For a Quote {Proposal} that does NOT include the use of any Subcontractors, by signing the Bid Solicitation {RFP} Offer and Acceptance Page {Signatory Page}, the Vendor {Bidder} is automatically certifying that:

a. In the event the award is granted to the Vendor’s {Bidder’s} firm and the Vendor {Bidder} later determines at any time during the term of the Blanket P.O. {Contract} to engage Subcontractors to provide certain goods and/or services, pursuant to Section 5.8 of the SSTC, the Vendor {Bidder} shall submit a Subcontractor Utilization Plan form for approval to the Division in advance of any such engagement of Subcontractors; and 

b. If the Blanket P.O. {Contract} is a small business subcontracting set-aside, the Vendor {Bidder} certifies that in engaging Subcontractors, it shall make a good faith effort to achieve the subcontracting set-aside goals, and shall attach to the Subcontractor Utilization Plan documentation of such efforts in accordance with N.J.A.C. 17:13-4 et seq.

1.3.1.1.3 NON-COLLUSION

By submitting a Quote {Proposal} and signing the Bid Solicitation {RFP} Offer and Acceptance Page {Signatory Page}, the Vendor {Bidder} certifies as follows:

a. The price(s) and amount of its Quote {Proposal} have been arrived at independently and without consultation, communication or agreement with any other Vendor {Contractor}, Vendor {Bidder} or any other party;

b. Neither the price(s) nor the amount of its Quote {Proposal}, and neither the approximate price(s) nor approximate amount of this Quote {Proposal}, have been disclosed to any other firm or person who is a Vendor {Bidder} or potential Vendor {Bidder}, and they will not be disclosed before the Quote {Proposal} submission;

c. No attempt has been made or will be made to induce any firm or person to refrain from bidding on this Blanket P.O. {Contract}, or to submit a Quote {Proposal} higher than this Quote {Proposal}, or to submit any intentionally high or noncompetitive Quote {Proposal} or other form of complementary Quote {Proposal};

d. The Quote {Proposal} of the firm is made in good faith and not pursuant to any agreement or discussion with, or inducement from, any firm or person to submit a complementary or other noncompetitive Quote {Proposal}; and

e. The Vendor {Bidder}, its affiliates, subsidiaries, officers, directors, and employees are not currently under investigation by any governmental agency and have not in the last five (5) years been convicted or found liable for any act prohibited by state or federal law in any jurisdiction, involving conspiracy or collusion with respect to bidding on any public Blanket P.O. {Contract}.

1.3.1.1.4 NEW JERSEY BUSINESS ETHICS GUIDE CERTIFICATION

The Treasurer has established a business ethics guide to be followed by Vendors {Bidders/Contractors} in its dealings with the State. The guide provides further information about compliance with Section 2.8 of the SSTC. The guide can be found at: 
http://www.state.nj.us/treasury/purchase/ethics_guide.shtml

By signing the Bid Solicitation {RFP} Offer and Acceptance Page {Signatory Page}, the Vendor {Bidder} is automatically certifying that it has complied with all applicable laws and regulations governing the provision of State goods and services, including the Conflicts of Interest Law, N.J.S.A. 52:13D-12 to -28. 

1.3.1.2 nj standard BID SOLICITATION {rfp} forms REQUIRED WITH THE QUOTE {PROPOSAL}
 
Vendor’s {Bidder’s} failure to complete, sign and submit the forms in Section 4.4.1.2 shall be cause to reject its Quote {Proposal} as non-responsive. 

1.3.1.2.1 Ownership Disclosure Form

Pursuant to N.J.S.A. 52:25-24.2, in the event the Vendor {Bidder} is a corporation, partnership or sole proprietorship limited liability company, the Vendor {Bidder} must complete an Ownership Disclosure Form. 

A current completed Ownership Disclosure Form must be received prior to or accompany the submitted Quote {Proposal}. A Vendor’s {Bidder’s} failure to submit the completed and signed form with its Quote {Proposal} will result in the rejection of the Quote {Proposal} as non-responsive and preclude the award of a Blanket P.O. {Contract} to said Vendor {Bidder} unless the Division has on file a signed and accurate Ownership Disclosure Form dated and received no more than six (6) months prior to the Quote {Proposal} submission deadline for this procurement. If any ownership change has occurred within the last six (6) months, a new Ownership Disclosure Form must be completed, signed and submitted with the Quote {Proposal}.

Vendors {Bidders} using NJSTART to submit a Quote {Proposal} shall make the appropriate certification on the “Maintain Terms and Categories” Tab within its profile by checking the applicable box and, if required, completing and attaching the shortened Ownership Disclosure Form. Vendors {Bidders} not using NJSTART to submit a Quote {Proposal} must complete the full Ownership Disclosure Form located on the Division’s website. This form is also available in NJSTART (www.njstart.gov).

Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation {RFP} through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

Vendors {Bidders} utilizing NJSTART should designate one version of the Ownership Disclosure Form as the Primary Form. In the event that a Vendor {Bidder} fails to attach an Ownership Disclosure Form, or the attached Ownership Disclosure Form is deemed deficient, the Division may access the Primary Form and consider it as part of the Quote {Proposal}. Note: The Primary Form must have a Date Created within six (6) months of the Quote {Proposal} submission deadline to be considered valid.

In the alternative, to comply with this section, a Vendor {Bidder} with any direct or indirect parent entity which is publicly traded may submit the name and address of each publicly traded entity and the name and address of each person that holds a 10 percent or greater beneficial interest in the publicly traded entity as of the last annual filing with the federal Securities and Exchange Commission or the foreign equivalent, and, if there is any person that holds a 10 percent or greater beneficial interest, also shall submit links to the websites containing the last annual filings with the federal Securities and Exchange Commission or the foreign equivalent and the relevant page numbers of the filings that contain the information on each person that holds a 10 percent or greater beneficial interest. N.J.S.A. 52:25-24.2.
 
1.3.1.2.2 DISCLOSURE OF INVESTMENT ACTIVITIES IN IRAN form
 
Pursuant to N.J.S.A. 52:32-58, the Vendor {Bidder} must utilize this Disclosure of Investment Activities in Iran form to certify that neither the Vendor {Bidder}, nor one of its parents, subsidiaries, and/or affiliates (as defined in N.J.S.A. 52:32-56(e)(3)), is listed on the Department of the Treasury’s List of Persons or Entities Engaging in Prohibited Investment Activities in Iran and that neither the Vendor {Bidder}, nor one of its parents, subsidiaries, and/or affiliates, is involved in any of the investment activities set forth in N.J.S.A. 52:32-56(f). If the Vendor {Bidder} is unable to so certify, the Vendor {Bidder} shall provide a detailed and precise description of such activities as directed on the form. A Vendor’s {Bidder’s} failure to submit the completed and signed form with its Quote {Proposal} will result in the rejection of the Quote {Proposal} as non-responsive and preclude the award of a Blanket P.O. {Contract} to said Vendor {Bidder}. 

Vendors {Bidders} using NJSTART to submit a Quote {Proposal} shall make the appropriate certification on the “Maintain Terms and Categories” Tab within its profile by checking the applicable box and, if required, completing and attaching the shortened Disclosure of Investment Activities in Iran form. Vendors {Bidders} not using NJSTART to submit a Quote {Proposal} must complete the full Disclosure of Investment Activities in Iran form located on the Division’s website. The full version of the form is also available in NJSTART (www.njstart.gov).

Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation {RFP} through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

Vendors {Bidders} utilizing NJSTART should designate the most current version of the Disclosure of Investment Activities in Iran form as the Primary Form. In the event that a Vendor {Bidder} fails to attach a Disclosure of Investment Activities in Iran form, or the attached Disclosure of Investment Activities in Iran form is deemed deficient, the Division may access the Primary Form, as designed in the Vendor {Bidder} profile, to be considered as part of the Quote {Proposal}.

1.3.1.3 subcontractor utilization plan

Please note that the State of New Jersey will not be utilizing the “Subcontractor” Tab in NJSTART. Vendors {Bidders} intending to use a Subcontractor shall submit a Subcontractor Utilization Plan form. 

The Subcontractor Utilization Plan form is located on the Division’s website. The form is also available in NJSTART. Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation {RFP} through NJSTART. QRGs are located on the NJSTART Vendor Support Page. 


SMALL BUSINESS SUBCONTRACTING SET-ASIDE BLANKET P.O. {CONTRACTS}

Not applicable to this procurement.



1.3.1.4 BID SECURITY

Not applicable to this procurement.

1.3.2 [bookmark: _Toc473708352][bookmark: _Toc473719960][bookmark: _Toc474153006][bookmark: _Toc474246509][bookmark: _Toc474741453][bookmark: _Toc473708353][bookmark: _Toc473719961][bookmark: _Toc474153007][bookmark: _Toc474246510][bookmark: _Toc474741454][bookmark: _Toc473708355][bookmark: _Toc473719963][bookmark: _Toc474153009][bookmark: _Toc474246512][bookmark: _Toc474741456][bookmark: _Toc473708357][bookmark: _Toc473719965][bookmark: _Toc474153011][bookmark: _Toc474246514][bookmark: _Toc474741458][bookmark: _Toc473708359][bookmark: _Toc473719967][bookmark: _Toc474153013][bookmark: _Toc474246516][bookmark: _Toc474741460][bookmark: _Toc473708360][bookmark: _Toc473719968][bookmark: _Toc474153014][bookmark: _Toc474246517][bookmark: _Toc474741461][bookmark: _Toc473708361][bookmark: _Toc473719969][bookmark: _Toc474153015][bookmark: _Toc474246518][bookmark: _Toc474741462][bookmark: _Toc473708363][bookmark: _Toc473719971][bookmark: _Toc474153017][bookmark: _Toc474246520][bookmark: _Toc474741464][bookmark: _Toc473708365][bookmark: _Toc473719973][bookmark: _Toc474153019][bookmark: _Toc474246522][bookmark: _Toc474741466][bookmark: _Toc473708366][bookmark: _Toc473719974][bookmark: _Toc474153020][bookmark: _Toc474246523][bookmark: _Toc474741467][bookmark: _Toc473708367][bookmark: _Toc473719975][bookmark: _Toc474153021][bookmark: _Toc474246524][bookmark: _Toc474741468][bookmark: _Toc473708369][bookmark: _Toc473719977][bookmark: _Toc474153023][bookmark: _Toc474246526][bookmark: _Toc474741470][bookmark: _Toc473708371][bookmark: _Toc473719979][bookmark: _Toc474153025][bookmark: _Toc474246528][bookmark: _Toc474741472][bookmark: _Toc473708372][bookmark: _Toc473719980][bookmark: _Toc474153026][bookmark: _Toc474246529][bookmark: _Toc474741473][bookmark: _Toc473708373][bookmark: _Toc473719981][bookmark: _Toc474153027][bookmark: _Toc474246530][bookmark: _Toc474741474][bookmark: _Toc473708375][bookmark: _Toc473719983][bookmark: _Toc474153029][bookmark: _Toc474246532][bookmark: _Toc474741476][bookmark: _Toc473708376][bookmark: _Toc473719984][bookmark: _Toc474153030][bookmark: _Toc474246533][bookmark: _Toc474741477][bookmark: _Toc473708377][bookmark: _Toc473719985][bookmark: _Toc474153031][bookmark: _Toc474246534][bookmark: _Toc474741478][bookmark: _Toc473708378][bookmark: _Toc473719986][bookmark: _Toc474153032][bookmark: _Toc474246535][bookmark: _Toc474741479][bookmark: _Toc473708380][bookmark: _Toc473719988][bookmark: _Toc474153034][bookmark: _Toc474246537][bookmark: _Toc474741481][bookmark: _Toc473708382][bookmark: _Toc473719990][bookmark: _Toc474153036][bookmark: _Toc474246539][bookmark: _Toc474741483][bookmark: _Toc473708384][bookmark: _Toc473719992][bookmark: _Toc474153038][bookmark: _Toc474246541][bookmark: _Toc474741485][bookmark: _Toc473708386][bookmark: _Toc473719994][bookmark: _Toc474153040][bookmark: _Toc474246543][bookmark: _Toc474741487][bookmark: _Toc473708387][bookmark: _Toc473719995][bookmark: _Toc474153041][bookmark: _Toc474246544][bookmark: _Toc474741488][bookmark: _Toc473708388][bookmark: _Toc473719996][bookmark: _Toc474153042][bookmark: _Toc474246545][bookmark: _Toc474741489][bookmark: _Toc473708390][bookmark: _Toc473719998][bookmark: _Toc474153044][bookmark: _Toc474246547][bookmark: _Toc474741491][bookmark: _Toc473708392][bookmark: _Toc473720000][bookmark: _Toc474153046][bookmark: _Toc474246549][bookmark: _Toc474741493][bookmark: _Toc473708394][bookmark: _Toc473720002][bookmark: _Toc474153048][bookmark: _Toc474246551][bookmark: _Toc474741495][bookmark: _Toc473708395][bookmark: _Toc473720003][bookmark: _Toc474153049][bookmark: _Toc474246552][bookmark: _Toc474741496][bookmark: _Toc473708396][bookmark: _Toc473720004][bookmark: _Toc474153050][bookmark: _Toc474246553][bookmark: _Toc474741497][bookmark: _Toc473708397][bookmark: _Toc473720005][bookmark: _Toc474153051][bookmark: _Toc474246554][bookmark: _Toc474741498][bookmark: _Toc473708398][bookmark: _Toc473720006][bookmark: _Toc474153052][bookmark: _Toc474246555][bookmark: _Toc474741499][bookmark: _Toc473708399][bookmark: _Toc473720007][bookmark: _Toc474153053][bookmark: _Toc474246556][bookmark: _Toc474741500][bookmark: _Toc473708400][bookmark: _Toc473720008][bookmark: _Toc474153054][bookmark: _Toc474246557][bookmark: _Toc474741501][bookmark: _Toc475717223][bookmark: _Toc449428257]Forms, REGISTRATIONS AND CERTIFICATIONS REQUIRED before BLANKET P.O. {contract} award and THAT SHOULD BE SUBMITTED with the QUOTE {Proposal}

Unless otherwise specified, forms must contain an original, physical signature, or an electronic signature pursuant to Section 1.3.4 of this Bid Solicitation {RFP}.

1.3.2.1 BUSINESS REGISTRATION

In accordance with N.J.S.A. 52:32-44(b), a Vendor {Bidder} and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Blanket P.O. {Contract}. To facilitate the Quote {Proposal} evaluation and Blanket P.O. {Contract} award process, the Vendor {Bidder} should submit a copy of its valid BRC and those of any named Subcontractors with its Quote {Proposal}. See Section 2.1 of the SSTC.

Any Vendor {Bidder}, inclusive of any named Subcontractors, not having a valid business registration at the time of the Quote {Proposal} opening, or whose BRC was revoked prior to the submission of the Quote {Proposal}, should proceed immediately to register its business or seek reinstatement of a revoked BRC. Vendors {Bidders} should verify its BRC status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} BRC, NJSTART provides a link to take corrective action. 

The Vendor {Bidder} is cautioned that it may require a significant amount of time to secure the reinstatement of a revoked BRC. The process can require actions by both the Division of Revenue and Enterprise Services and the Division of Taxation. For this reason, a Vendor’s {Bidder’s} early attention to this requirement is highly recommended. The Vendor {Bidder} and its named Subcontractors may register with the Division of Revenue and Enterprise Services, obtain a copy of an existing BRC or obtain information necessary to seek re-instatement of a revoked BRC online at http://www.state.nj.us/treasury/revenue/busregcert.shtml.

A Vendor {Bidder} otherwise identified by the Division as a responsive and responsible Vendor {Bidder}, inclusive of any named Subcontractors, but that was not business registered at the time of submission of its Quote {Proposal} must be so registered and in possession of a valid BRC by a deadline to be specified in writing by the Division. A Vendor {Bidder} failing to comply with this requirement by the deadline specified by the Division will be deemed ineligible for Blanket P.O. {Contract} award. Under any circumstance, the Division will rely upon information available from computerized systems maintained by the State as a basis to verify independently compliance with the requirement for business registration.

A Vendor {Bidder} receiving a Blanket P.O. {Contract} award as a result of this procurement and any Subcontractors named by that Vendor {Bidder} will be required to maintain a valid business registration with the Division of Revenue and Enterprise Services for the duration of the executed Blanket P.O. {Contract}, inclusive of any Blanket P.O. {Contract} extensions.  

1.3.2.2 Disclosure of Investigations AND OTHER Actions Involving Bidder form
 
The Vendor {Bidder} should submit the Disclosure of Investigations and Other Actions Involving Bidder Form, with its Quote {Proposal}, to provide a detailed description of any investigation, litigation, including administrative complaints or other administrative proceedings, involving any public sector clients during the past five (5) years, including the nature and status of the investigation, and, for any litigation, the caption of the action, a brief description of the action, the date of inception, current status, and, if applicable, disposition. If a Vendor {Bidder} does not submit the form with the Quote {Proposal}, the Vendor {Bidder} must comply within seven (7) business days of the State’s request or the State may deem the Quote {Proposal} non-responsive.

Vendors {Bidders} using NJSTART to submit a Quote {Proposal} shall make the appropriate certification on the “Maintain Terms and Categories” Tab within its profile by checking the applicable box and, if required, complete and attach the shortened NJSTART form. Vendors {Bidders} not using NJSTART to submit a Quote {Proposal} must complete the full version of the form located on the Division’s website. This form is also available in NJSTART.

Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation {RFP} through NJSTART. Vendors {Bidders} may also refer to the QRG “Vendor Categories and Certifications” for additional instructions on completing shortened versions of required forms by completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

1.3.2.3 Source Disclosure 

Not applicable to this procurement.

1.3.2.4 AFFIDAVIT OF APPAREL FORM

Not applicable to this procurement.

1.3.3 [bookmark: _Toc475717224]SUBmittals

Vendors {Bidders} may refer to the QRG “Submit a Quote” for instructions detailing how to submit a NJSTART electronic Quote {Proposal}. QRGs are located on the NJSTART Vendor Support Page. 

1.3.3.1 Vendor {BIDDER} Experience

The Vendor {Bidder} should complete ALL the information requested on the Vendor {Bidder} Data Sheet Form attached to this Bid Solicitation {RFP} so that the State is able to make a sound business judgment regarding the Vendor’s {Bidder’s} experience and capability to perform the Blanket P.O. {Contract} to the State's satisfaction. Vendor {Bidder} shall not list a Procurement Specialist as a reference on the Vendor {Bidder} Data Sheet Form.

The State may require a Vendor {Bidder} to provide additional information or documentation within five (5) business days of request by the State.

1.3.3.2 MANUFACTURER’S CERTIFICATION

Dealers or agents submitting a Quote {Proposal} may be required to submit a letter of certification from the manufacturer whose product is supplied, certifying that the Vendor {Bidder} is a dealer or agent, authorized by the manufacturer to supply the unit specified. The State reserves the right to request such certification and to require that such certification be delivered within five (5) business days from the time it is requested. 

1.3.3.3 PRODUCT LITERATURE/MANUFACTURER’S SPECIFICATIONS

The Vendor {Bidder} must submit manufacturer’s specification sheets for all items listed on price line items one (1) through fourteen (14). All submittals should be properly labeled, showing the Vendor’s {Bidder’s} name and Quote {Proposal} number. The Vendor {Bidder} should also provide manufacturer’s drawing, schematics and blueprints, if available. 

If a Vendor {Bidder} does not provide the manufacturer's specifications sheet for price line item one (1) through fourteen (14), the State reserves the right to request such information from the Vendor {Bidder}. The Vendor {Bidder} must respond to such request by providing all requested information within forty-eight (48) hours. If the information requested is not received within forty-eight (48) hours, the Quote {Proposal} shall be rejected. 

1.3.3.4 [bookmark: _Toc284596690][bookmark: _Toc407614861]LIST OF AFTERMARKET INSTALLERs

Please refer to Attachment #1 – List of Aftermarket Installers. 
[bookmark: fourfourthreetwothree]
1.3.4 [bookmark: _Toc470687292][bookmark: _Toc470687639][bookmark: _Toc470687873][bookmark: _Toc470688107][bookmark: _Toc470688341][bookmark: _Toc470688575][bookmark: _Toc470688809][bookmark: _Toc470689044][bookmark: _Toc470689277][bookmark: _Toc470689511][bookmark: _Toc470689745][bookmark: _Toc470689980][bookmark: _Toc470693006][bookmark: _Toc470687293][bookmark: _Toc470687640][bookmark: _Toc470687874][bookmark: _Toc470688108][bookmark: _Toc470688342][bookmark: _Toc470688576][bookmark: _Toc470688810][bookmark: _Toc470689045][bookmark: _Toc470689278][bookmark: _Toc470689512][bookmark: _Toc470689746][bookmark: _Toc470689981][bookmark: _Toc470693007][bookmark: _Toc470687294][bookmark: _Toc470687641][bookmark: _Toc470687875][bookmark: _Toc470688109][bookmark: _Toc470688343][bookmark: _Toc470688577][bookmark: _Toc470688811][bookmark: _Toc470689046][bookmark: _Toc470689279][bookmark: _Toc470689513][bookmark: _Toc470689747][bookmark: _Toc470689982][bookmark: _Toc470693008][bookmark: _Toc470687295][bookmark: _Toc470687642][bookmark: _Toc470687876][bookmark: _Toc470688110][bookmark: _Toc470688344][bookmark: _Toc470688578][bookmark: _Toc470688812][bookmark: _Toc470689047][bookmark: _Toc470689280][bookmark: _Toc470689514][bookmark: _Toc470689748][bookmark: _Toc470689983][bookmark: _Toc470693009][bookmark: _Toc470687296][bookmark: _Toc470687643][bookmark: _Toc470687877][bookmark: _Toc470688111][bookmark: _Toc470688345][bookmark: _Toc470688579][bookmark: _Toc470688813][bookmark: _Toc470689048][bookmark: _Toc470689281][bookmark: _Toc470689515][bookmark: _Toc470689749][bookmark: _Toc470689984][bookmark: _Toc470693010][bookmark: _Toc470687297][bookmark: _Toc470687644][bookmark: _Toc470687878][bookmark: _Toc470688112][bookmark: _Toc470688346][bookmark: _Toc470688580][bookmark: _Toc470688814][bookmark: _Toc470689049][bookmark: _Toc470689282][bookmark: _Toc470689516][bookmark: _Toc470689750][bookmark: _Toc470689985][bookmark: _Toc470693011][bookmark: _Toc470687298][bookmark: _Toc470687645][bookmark: _Toc470687879][bookmark: _Toc470688113][bookmark: _Toc470688347][bookmark: _Toc470688581][bookmark: _Toc470688815][bookmark: _Toc470689050][bookmark: _Toc470689283][bookmark: _Toc470689517][bookmark: _Toc470689751][bookmark: _Toc470689986][bookmark: _Toc470693012][bookmark: _Toc470687299][bookmark: _Toc470687646][bookmark: _Toc470687880][bookmark: _Toc470688114][bookmark: _Toc470688348][bookmark: _Toc470688582][bookmark: _Toc470688816][bookmark: _Toc470689051][bookmark: _Toc470689284][bookmark: _Toc470689518][bookmark: _Toc470689752][bookmark: _Toc470689987][bookmark: _Toc470693013][bookmark: _Toc470687300][bookmark: _Toc470687647][bookmark: _Toc470687881][bookmark: _Toc470688115][bookmark: _Toc470688349][bookmark: _Toc470688583][bookmark: _Toc470688817][bookmark: _Toc470689052][bookmark: _Toc470689285][bookmark: _Toc470689519][bookmark: _Toc470689753][bookmark: _Toc470689988][bookmark: _Toc470693014][bookmark: _Toc470687301][bookmark: _Toc470687648][bookmark: _Toc470687882][bookmark: _Toc470688116][bookmark: _Toc470688350][bookmark: _Toc470688584][bookmark: _Toc470688818][bookmark: _Toc470689053][bookmark: _Toc470689286][bookmark: _Toc470689520][bookmark: _Toc470689754][bookmark: _Toc470689989][bookmark: _Toc470693015][bookmark: _Toc470687302][bookmark: _Toc470687649][bookmark: _Toc470687883][bookmark: _Toc470688117][bookmark: _Toc470688351][bookmark: _Toc470688585][bookmark: _Toc470688819][bookmark: _Toc470689054][bookmark: _Toc470689287][bookmark: _Toc470689521][bookmark: _Toc470689755][bookmark: _Toc470689990][bookmark: _Toc470693016][bookmark: _Toc470687303][bookmark: _Toc470687650][bookmark: _Toc470687884][bookmark: _Toc470688118][bookmark: _Toc470688352][bookmark: _Toc470688586][bookmark: _Toc470688820][bookmark: _Toc470689055][bookmark: _Toc470689288][bookmark: _Toc470689522][bookmark: _Toc470689756][bookmark: _Toc470689991][bookmark: _Toc470693017][bookmark: _Toc470687304][bookmark: _Toc470687651][bookmark: _Toc470687885][bookmark: _Toc470688119][bookmark: _Toc470688353][bookmark: _Toc470688587][bookmark: _Toc470688821][bookmark: _Toc470689056][bookmark: _Toc470689289][bookmark: _Toc470689523][bookmark: _Toc470689757][bookmark: _Toc470689992][bookmark: _Toc470693018][bookmark: _Toc470687305][bookmark: _Toc470687652][bookmark: _Toc470687886][bookmark: _Toc470688120][bookmark: _Toc470688354][bookmark: _Toc470688588][bookmark: _Toc470688822][bookmark: _Toc470689057][bookmark: _Toc470689290][bookmark: _Toc470689524][bookmark: _Toc470689758][bookmark: _Toc470689993][bookmark: _Toc470693019][bookmark: _Toc470687306][bookmark: _Toc470687653][bookmark: _Toc470687887][bookmark: _Toc470688121][bookmark: _Toc470688355][bookmark: _Toc470688589][bookmark: _Toc470688823][bookmark: _Toc470689058][bookmark: _Toc470689291][bookmark: _Toc470689525][bookmark: _Toc470689759][bookmark: _Toc470689994][bookmark: _Toc470693020][bookmark: _Toc470687307][bookmark: _Toc470687654][bookmark: _Toc470687888][bookmark: _Toc470688122][bookmark: _Toc470688356][bookmark: _Toc470688590][bookmark: _Toc470688824][bookmark: _Toc470689059][bookmark: _Toc470689292][bookmark: _Toc470689526][bookmark: _Toc470689760][bookmark: _Toc470689995][bookmark: _Toc470693021][bookmark: _Toc470687308][bookmark: _Toc470687655][bookmark: _Toc470687889][bookmark: _Toc470688123][bookmark: _Toc470688357][bookmark: _Toc470688591][bookmark: _Toc470688825][bookmark: _Toc470689060][bookmark: _Toc470689293][bookmark: _Toc470689527][bookmark: _Toc470689761][bookmark: _Toc470689996][bookmark: _Toc470693022][bookmark: _Toc470687309][bookmark: _Toc470687656][bookmark: _Toc470687890][bookmark: _Toc470688124][bookmark: _Toc470688358][bookmark: _Toc470688592][bookmark: _Toc470688826][bookmark: _Toc470689061][bookmark: _Toc470689294][bookmark: _Toc470689528][bookmark: _Toc470689762][bookmark: _Toc470689997][bookmark: _Toc470693023][bookmark: _Toc470687310][bookmark: _Toc470687657][bookmark: _Toc470687891][bookmark: _Toc470688125][bookmark: _Toc470688359][bookmark: _Toc470688593][bookmark: _Toc470688827][bookmark: _Toc470689062][bookmark: _Toc470689295][bookmark: _Toc470689529][bookmark: _Toc470689763][bookmark: _Toc470689998][bookmark: _Toc470693024][bookmark: _Toc470687311][bookmark: _Toc470687658][bookmark: _Toc470687892][bookmark: _Toc470688126][bookmark: _Toc470688360][bookmark: _Toc470688594][bookmark: _Toc470688828][bookmark: _Toc470689063][bookmark: _Toc470689296][bookmark: _Toc470689530][bookmark: _Toc470689764][bookmark: _Toc470689999][bookmark: _Toc470693025][bookmark: _Toc470687312][bookmark: _Toc470687659][bookmark: _Toc470687893][bookmark: _Toc470688127][bookmark: _Toc470688361][bookmark: _Toc470688595][bookmark: _Toc470688829][bookmark: _Toc470689064][bookmark: _Toc470689297][bookmark: _Toc470689531][bookmark: _Toc470689765][bookmark: _Toc470690000][bookmark: _Toc470693026][bookmark: _Toc470687313][bookmark: _Toc470687660][bookmark: _Toc470687894][bookmark: _Toc470688128][bookmark: _Toc470688362][bookmark: _Toc470688596][bookmark: _Toc470688830][bookmark: _Toc470689065][bookmark: _Toc470689298][bookmark: _Toc470689532][bookmark: _Toc470689766][bookmark: _Toc470690001][bookmark: _Toc470693027][bookmark: _Toc470687314][bookmark: _Toc470687661][bookmark: _Toc470687895][bookmark: _Toc470688129][bookmark: _Toc470688363][bookmark: _Toc470688597][bookmark: _Toc470688831][bookmark: _Toc470689066][bookmark: _Toc470689299][bookmark: _Toc470689533][bookmark: _Toc470689767][bookmark: _Toc470690002][bookmark: _Toc470693028][bookmark: _Toc470687315][bookmark: _Toc470687662][bookmark: _Toc470687896][bookmark: _Toc470688130][bookmark: _Toc470688364][bookmark: _Toc470688598][bookmark: _Toc470688832][bookmark: _Toc470689067][bookmark: _Toc470689300][bookmark: _Toc470689534][bookmark: _Toc470689768][bookmark: _Toc470690003][bookmark: _Toc470693029][bookmark: _Toc470687316][bookmark: _Toc470687663][bookmark: _Toc470687897][bookmark: _Toc470688131][bookmark: _Toc470688365][bookmark: _Toc470688599][bookmark: _Toc470688833][bookmark: _Toc470689068][bookmark: _Toc470689301][bookmark: _Toc470689535][bookmark: _Toc470689769][bookmark: _Toc470690004][bookmark: _Toc470693030][bookmark: _Toc470687317][bookmark: _Toc470687664][bookmark: _Toc470687898][bookmark: _Toc470688132][bookmark: _Toc470688366][bookmark: _Toc470688600][bookmark: _Toc470688834][bookmark: _Toc470689069][bookmark: _Toc470689302][bookmark: _Toc470689536][bookmark: _Toc470689770][bookmark: _Toc470690005][bookmark: _Toc470693031][bookmark: _Toc470687318][bookmark: _Toc470687665][bookmark: _Toc470687899][bookmark: _Toc470688133][bookmark: _Toc470688367][bookmark: _Toc470688601][bookmark: _Toc470688835][bookmark: _Toc470689070][bookmark: _Toc470689303][bookmark: _Toc470689537][bookmark: _Toc470689771][bookmark: _Toc470690006][bookmark: _Toc470693032][bookmark: _Toc470687319][bookmark: _Toc470687666][bookmark: _Toc470687900][bookmark: _Toc470688134][bookmark: _Toc470688368][bookmark: _Toc470688602][bookmark: _Toc470688836][bookmark: _Toc470689071][bookmark: _Toc470689304][bookmark: _Toc470689538][bookmark: _Toc470689772][bookmark: _Toc470690007][bookmark: _Toc470693033][bookmark: _Toc470687320][bookmark: _Toc470687667][bookmark: _Toc470687901][bookmark: _Toc470688135][bookmark: _Toc470688369][bookmark: _Toc470688603][bookmark: _Toc470688837][bookmark: _Toc470689072][bookmark: _Toc470689305][bookmark: _Toc470689539][bookmark: _Toc470689773][bookmark: _Toc470690008][bookmark: _Toc470693034][bookmark: _Toc470687321][bookmark: _Toc470687668][bookmark: _Toc470687902][bookmark: _Toc470688136][bookmark: _Toc470688370][bookmark: _Toc470688604][bookmark: _Toc470688838][bookmark: _Toc470689073][bookmark: _Toc470689306][bookmark: _Toc470689540][bookmark: _Toc470689774][bookmark: _Toc470690009][bookmark: _Toc470693035][bookmark: _Toc470687322][bookmark: _Toc470687669][bookmark: _Toc470687903][bookmark: _Toc470688137][bookmark: _Toc470688371][bookmark: _Toc470688605][bookmark: _Toc470688839][bookmark: _Toc470689074][bookmark: _Toc470689307][bookmark: _Toc470689541][bookmark: _Toc470689775][bookmark: _Toc470690010][bookmark: _Toc470693036][bookmark: _Toc470687323][bookmark: _Toc470687670][bookmark: _Toc470687904][bookmark: _Toc470688138][bookmark: _Toc470688372][bookmark: _Toc470688606][bookmark: _Toc470688840][bookmark: _Toc470689075][bookmark: _Toc470689308][bookmark: _Toc470689542][bookmark: _Toc470689776][bookmark: _Toc470690011][bookmark: _Toc470693037][bookmark: _Toc470687324][bookmark: _Toc470687671][bookmark: _Toc470687905][bookmark: _Toc470688139][bookmark: _Toc470688373][bookmark: _Toc470688607][bookmark: _Toc470688841][bookmark: _Toc470689076][bookmark: _Toc470689309][bookmark: _Toc470689543][bookmark: _Toc470689777][bookmark: _Toc470690012][bookmark: _Toc470693038][bookmark: _Toc470687325][bookmark: _Toc470687672][bookmark: _Toc470687906][bookmark: _Toc470688140][bookmark: _Toc470688374][bookmark: _Toc470688608][bookmark: _Toc470688842][bookmark: _Toc470689077][bookmark: _Toc470689310][bookmark: _Toc470689544][bookmark: _Toc470689778][bookmark: _Toc470690013][bookmark: _Toc470693039][bookmark: _Toc470687326][bookmark: _Toc470687673][bookmark: _Toc470687907][bookmark: _Toc470688141][bookmark: _Toc470688375][bookmark: _Toc470688609][bookmark: _Toc470688843][bookmark: _Toc470689078][bookmark: _Toc470689311][bookmark: _Toc470689545][bookmark: _Toc470689779][bookmark: _Toc470690014][bookmark: _Toc470693040][bookmark: _Toc473528339][bookmark: _Toc475717225]Financial Capability of the Vendor {Bidder}

In order to provide the State with the ability to judge the Vendor’s {Bidder’s} financial capacity and capabilities to undertake and successfully complete the Blanket P.O. {Contract}, the Vendor {Bidder} should submit opined certified financial statements in accordance with applicable standards by a Certified Public Accountant which include a balance sheet, income statement, and statement of cash flow, and all applicable notes for the most recent calendar year or the Vendor’s {Bidder’s} most recent fiscal year. If certified financial statements are not available, the Vendor {Bidder} should provide either a reviewed or compiled statement from an independent accountant setting forth the same information required for the certified financial statements, together with a certification from the Chief Executive Officer and the Chief Financial Officer, that the financial statements and other information included in the statements fairly present in all material respects the financial condition, results of operations, and cash flows of the Vendor {Bidder} as of, and for, the periods presented in the statements. In addition, the Vendor {Bidder} should submit a bank reference.

If the information is not supplied with the Quote {Proposal}, the State may still require the Vendor {Bidder} to submit it. If the Vendor {Bidder} fails to comply with the request within seven (7) business days, the State may deem the Quote {Proposal} non-responsive.

A Vendor {Bidder} may designate specific financial information as not subject to disclosure when the Vendor {Bidder} has a good faith legal/factual basis for such assertion. A Vendor {Bidder} may submit specific financial documents in a separate, sealed package clearly marked “Confidential-Financial Information” along with the Quote {Proposal}.

The State reserves the right to make the determination to accept the assertion and shall so advise the Vendor {Bidder}.

1.3.5 [bookmark: _Toc474246562][bookmark: _Toc474741506][bookmark: _Toc474246563][bookmark: _Toc474741507][bookmark: _Toc474246564][bookmark: _Toc474741508][bookmark: _Toc474246565][bookmark: _Toc474741509][bookmark: _Toc474246566][bookmark: _Toc474741510][bookmark: _Toc474246567][bookmark: _Toc474741511][bookmark: _Toc474246568][bookmark: _Toc474741512][bookmark: _Toc474246569][bookmark: _Toc474741513][bookmark: _Toc474246570][bookmark: _Toc474741514][bookmark: _Toc474246571][bookmark: _Toc474741515][bookmark: _Toc474246573][bookmark: _Toc474741517][bookmark: _Toc474246574][bookmark: _Toc474741518][bookmark: _Toc474246575][bookmark: _Toc474741519][bookmark: _Toc474246577][bookmark: _Toc474741521][bookmark: _Toc474246578][bookmark: _Toc474741522][bookmark: _Toc474246579][bookmark: _Toc474741523][bookmark: _Toc474246580][bookmark: _Toc474741524][bookmark: _Toc474246581][bookmark: _Toc474741525][bookmark: _4.4.2.3_Contract_Schedule][bookmark: _4.4.2.4_mobilization_and][bookmark: _Toc474246582][bookmark: _Toc474741526][bookmark: _Toc474246583][bookmark: _Toc474741527][bookmark: _Toc474246584][bookmark: _Toc474741528][bookmark: _Toc474246585][bookmark: _Toc474741529][bookmark: _Toc474246586][bookmark: _Toc474741530][bookmark: _Toc474246587][bookmark: _Toc474741531][bookmark: _Toc474246589][bookmark: _Toc474741533][bookmark: _Toc474246591][bookmark: _Toc474741535][bookmark: _Toc474246592][bookmark: _Toc474741536][bookmark: _Toc474246593][bookmark: _Toc474741537][bookmark: _Toc400531503][bookmark: _Toc428533974][bookmark: _Toc475717226]PRICE schedule/SHEET

The Vendor {Bidder} must submit its pricing using the State-supplied price sheet/schedule(s) accompanying this Bid Solicitation {RFP} and located on the “Attachments” Tab. 

Vendors {Bidders} may refer to the QRG “Submit a Quote” for instructions detailing how to submit a NJSTART electronic Quote {Proposal}. QRGs are located on the NJSTART Vendor Support Page. 


In order for the State to make sound business judgments regarding products and prices offered in response to this Bid Solicitation {RFP}, the Vendor {Bidder} must supply, with its Quote {Proposal}, the information requested on the Bid Solicitation’s {RFP's} pricing lines in sufficient detail as to allow the State to determine the firm, fixed Quote {Proposal} pricing and the precise product or service being offered, i.e., with no possible misinterpretation of the price or product/service being offered by the Vendor {Bidder}. A Vendor’s {Bidder's} failure to provide, within its Quote {Proposal}, the information deemed by the State to be essential for product identification or price determination shall result in rejection of that Vendor’s {Bidder's} Quote {Proposal}. Notwithstanding the aforementioned material obligation, in order to support the State's decision-making process, the State may require a Vendor {Bidder} to provide additional information or documentation that has been deemed not to be material to product identification or price determination, in which case, the Vendor {Bidder} shall, within the time limit set forth in the written request, comply with said request. Each Vendor {Bidder} is required to hold its prices firm through issuance of Blanket P.O. {Contract}.

1.3.5.1 NJSTART pricing submission instructions

If the Vendor {Bidder} is submitting a NJSTART Quote {Proposal}, the Vendor {Bidder} must enter a Unit Cost of $1.00 for each price line item on the “Items” Tab in NJSTART. The Vendor {Bidder} is instructed to do so only as a mechanism to comply with Bid Solicitation {RFP} Section 6.8 and prevent all pricing from being publicly displayed in NJSTART. 

1.3.5.2 price sheet/schedule attachment instructions

4.4.5.2.1  While Vendors {Bidders} must bid on all sixteen (16) price lines, Using Agencies may order price line 1 item only or any price line item or combination of items listed on price lines 2 through 16.  
· Step 1 – The Vendor {Bidder} shall insert a firm, fixed price in US dollars in the Unit Price column on the price sheet for price lines one (1) through (16). 

In order for a Vendor {Bidder} to be considered responsive, it must bid on each price line 

The price lines are as follows:

	Price Lines
	Description

	1 
	19,500 lb. GVWR Crew Cab & Chassis, DRW, 4WD,

	2
	Hook Lift System

	3
	Stainless Steel Dump Body With Tilt/Dump Interlock

	4
	Stake Body

	5
	Landscape Box Body

	6
	Chipper Body

	7
	Enclosed Steel Storage Body

	8
	Platform Body With 300 -Gallon, Gasoline Powered Herbicide Sprayer 

	9
	Platform Body With Toolboxes

	10 
	Dump Body With Multi-Function Tailgate 

	11
	Salt Spreader

	12
	Snow Plow

	13
	In-Cab Controller For Herbicide Sprayer

	14
	In-Cab Controller For Salt Spreader

	15
	One Set Of Parts, Service and O&M Manuals

	16
	Technical Support


 
· Step 2 – For price line one (1), the Vendor {Bidder} shall enter the make of the item being offered in the column entitled “Make”. (e.g. Ford), the model of the item being offered in the column entitled “Model” (e.g. F-150), and the model year of the item being offered in the column entitled “Model Year” (e.g. 2017) on the Price Sheet. 


· Step 3 – For price line one (1), the Vendor {Bidder} shall enter the specific manufacturer’s body code, trim level, trim line or series being offered in the column entitled “Manufacturer’s Body Code/Trim Level/Trim Line/Series”. For example, in the case of Ford, a Vendor {Bidder} may enter: Manufacturer’s body code: WSH, Trim level: XL, Trim Line: The standard set of features on the particular vehicle, example: 6-speed automatic transmission, air conditioning, GVWR rating, etc., Series: Regular Cab, 141” WB, 8’ Box.

· Step 4 – For price line one (1), the Vendor {Bidder} shall provide manufacturer’s option code number and a detailed description for each option bid in the “Optional Package/Options Bid” column on each price line to avoid any misunderstanding. For example, if the vehicle bid comes with standard manual transmission and if the Vendor {Bidder} does not list automatic transmission in the manufacturer’s option space, its Quote {Proposal} shall be determined to be non-responsive. No exception shall be permitted. Vendors {Bidders} are cautioned to thoroughly review the information provided before submitting the Quote {Proposal}.

The examples listed above are for reference only and may not specifically apply to the vehicles specified in this Bid Solicitaton { RFP}.

In the event that a Vendor {Bidder} using NJSTART to submit a Quote {Proposal} uploads a price sheet/schedule attachment and completes the “Items” Tab in NJSTART (instead of entering a Unit Cost of $1.00 as instructed), the price sheet/schedule attachment will govern. 

· Step 5 – For price line one (1), the Vendor {Bidder} shall enter the days required to make delivery upon receipt of an order into the “Delivery Days ARO” column of the Price Sheet. If the “Delivery Days ARO” column is left blank, then the delivery days shall default to the delivery days set forth in Section 4.4.5.4. 

· Step 6 – For price lines two (2) through fourteen (14), the Vendor {Bidder} shall enter the make of the item being offered in the column entitled “Make” , the model of the item being offered in the column entitled “Model”  and the installer of the item being offered in the column entitled “Installer” (e.g. ABC Body Co.) on the Price Sheet .  

· Step 7 – For price lines (2) through fourteen (14), the Vendor {Bidder} shall enter the days required to make delivery upon receipt of an order into the “Delivery Days ARO” column of the Price Sheet. If the “Delivery Days ARO” column is left blank, then the delivery days shall default to the delivery days set forth in Section 4.4.5.4. 

· Step 8 – The Vendor {Bidder} should enter the cash discount for expedited payments into the “Cash Discount” field of the Price Sheet. If the Vendor {Bidder} leaves the “Cash Discount” field blank, it shall mean that the Vendor {Bidder} is not offering a cash discount as reference in Section 4.4.5.6. 

The examples listed above are for reference only and may not specifically apply to the vehicles specified in this Bid Solicitation {RFP}.

In the event that a Vendor {Bidder} using NJSTART to submit a Quote {Proposal} uploads a price sheet/schedule attachment and completes the “Items” Tab in NJSTART (instead of entering a Unit Cost of $1.00 as instructed), the price sheet/schedule attachment will govern. 

4.4.5.2.2 Each vehicle is specified in three parts of the technical specifications of this Bid Solicitation {RFP}: Blanket P.O.{Contract} Specific Requirements (Section 3.2) and Vehicle Specifications, General Provisions (Section 3.3) and Vehicle Specifications, Technical Provisions (Section 3.4). Thus, price bid for any vehicle shall include, among other items, such as delivery and inspection, costs of both the Common Specifications and all Vehicle Specific Requirements.
 
1.3.5.3 Use of “no bid” versus “no charge” on the price sheet/schedule

If the Vendor {Bidder} is not submitting a price for an item on a price line, the Vendor {Bidder} must indicate “No Bid” on the State-supplied price sheet/schedule(s) attachment accompanying this Bid Solicitation {RFP}. If the Vendor {Bidder} will supply an item on a price line free of charge, the Vendor {Bidder} must indicate “No Charge” on the State-supplied price sheet/schedule(s) attachment accompanying this Bid Solicitation {RFP}. The use of any other identifier may result in the Vendor’s {Bidder’s} Quote {Proposal} being deemed non-responsive. If the Vendor {Bidder} leaves a price line blank, this shall mean that it was the Vendor’s {Bidder’s} intent to not submit a price for that price line. 

1.3.5.4 DELIVERY TIME AND COSTS

Unless otherwise noted elsewhere in the Bid Solicitation {RFP}, or price sheet all delivery times are 180 calendar days after receipt of order (ARO) and prices for items in Quotes {Proposals} shall be submitted Freight On Board (F.O.B.) Destination (180 calendar days ARO/F.O.B.). Quotes {Proposals} submitted other than 180 calendar days ARO/F.O.B. may be deemed non-responsive. The Vendor {Contractor} shall assume all costs, liability and responsibility for the delivery of merchandise in good condition to the State's Using Agency or designated purchaser. 180 calendar days ARO/F.O.B. does not cover "spotting" but does include delivery on the receiving platform of the Using Agency at any destination in the State of New Jersey unless otherwise specified.

No additional charges will be allowed for any additional transportation costs resulting from partial shipments made at the Vendor’s {Contractor’s} convenience when a single shipment is ordered.

1.3.5.5 COLLECT ON DELIVERY (C.O.D.) TERMS

C.O.D. terms are not acceptable as part of a Quote {Proposal} and shall be deemed non-responsive.

1.3.5.6 CASH DISCOUNTS

The Vendor {Bidder} is encouraged to offer cash discounts based on expedited payment by the State. The State will make efforts to take advantage of discounts, but discounts will not be considered in determining the price rankings of Quotes {Proposals}.

Should the Vendor {Bidder} choose to offer cash discounts the following shall apply:

a. Discount periods shall be calculated starting from the next business day after the Using Agency has accepted the goods or services, received a properly signed and executed invoice and, when required, a properly executed performance security, whichever is latest.

b. The date on the check issued by the State in payment of that invoice shall be deemed the date of the State's response to that invoice.

1.3.6 [bookmark: _Toc400531504][bookmark: _Toc428533975][bookmark: _Toc475717227]COOPERATIVE PURCHASING PROGRAM

The Vendor {Bidder} should complete the Cooperative Purchasing Form indicating willingness or unwillingness to extend State Blanket P.O. {Contract} pricing and terms to Cooperative Purchasing Program participants.
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1. [bookmark: _Toc475717228] SPECIAL CONTRACTUAL TERMS AND CONDITIONS APPLICABLE TO THE BLANKET P.O. {CONTRACT}

2. [bookmark: _Toc400531506][bookmark: _Toc428533977][bookmark: _Toc475717229]PRECEDENCE OF SPECIAL CONTRACTUAL TERMS AND CONDITIONS
	
This Blanket P.O. {Contract} awarded, and the entire agreement between the parties, as a result of this Bid Solicitation {RFP} shall consist of this Bid Solicitation {RFP}, including the SSTC, Bid Amendment {Addendum} to this Bid Solicitation {RFP}, the Vendor’s {Contractor’s} Quote {Proposal}, any Best and Final Offer, and the Division's Notice of Award.

In the event of a conflict in the terms and conditions among the documents comprising this Blanket P.O. {Contract}, the order of precedence, for purposes of interpretation thereof, listed from highest ranking to lowest ranking, shall be:

a. Executed Offer and Acceptance Page {Signatory Page};

b. Bid Solicitation {RFP} Section 5, as may be amended by Bid Amendment {Addendum};

c. The State of NJ Standard Terms and Conditions (SSTC) accompanying this Bid Solicitation {RFP};

d. All remaining sections of the Bid Solicitation {RFP}, as may be amended by Bid Amendment {Addendum}; 

e. The Vendor’s {Contractor’s} final submitted Best and Final Offer; and

f. The Vendor’s {Contractor’s} Quote {Proposal} as accepted by the State.

Note: In the event of conflicting information between the Bid Solicitation {RFP} and fields contained in NJSTART, the Bid Solicitation {RFP} will govern and NJSTART will be updated via Bid Amendment {Addend} or Change Order {Contract Amendment}.
2. [bookmark: _Toc400531507][bookmark: _Toc428533978][bookmark: _Toc475717230]BLANKET P.O. {Contract} Term and Extension Option

The term of this Blanket P.O. {Contract} shall be for a period of three (3) years. The anticipated "Blanket P.O. {Contract} Effective Date" is provided on the “Summary” page of the Bid Solicitation {RFP} in NJSTART. If delays in the procurement process result in a change to the anticipated Blanket P.O. {Contract} Effective Date, the Vendor {Bidder} agrees to accept a Blanket P.O. {Contract} for the full term of this Blanket P.O. {Contract}. 

This Blanket P.O. {Contract} may be extended up to three (3) years with no single extension exceeding one (1) year, by the mutual written consent of the Vendor {Contractor} and the Director at the same terms, conditions, and pricing at the rates in effect in the last year of this Blanket P.O. {Contract} or rates more favorable to the State.

Purchase orders may be placed against the Blanket P.O. {Contract} up to and including the end of business on the last day of the Blanket P.O. {Contract}, for delivery no more than forty-five (45) days after Blanket P.O. {Contract} expiration.

2.1.1 [bookmark: _Toc473708414][bookmark: _Toc473720025][bookmark: _Toc474246609][bookmark: _Toc474741553][bookmark: _Toc475717231][bookmark: _Toc449007554][bookmark: _Toc459890939]Price Adjustment

The Blanket PO {Contract} price shall remain firm for the initial term and any extensions of the Blanket PO {Contract} unless pricing offered is more favorable to the State. Refer to section 6.1 of the SSTC. In an exceptional situation the State may consider a price adjustment.

Requests for price adjustments must include justification and documentation such as notice of an increase in the manufacturer’s price, new product literature or an increase in the industry (i.e. fuel, labor, equipment, material etc.). The Vendor {Contractor} must provide, as applicable, a revised Price Sheet to the Procurement Specialist in hard copy and electronic form as specified by the Division. The file name should contain the Blanket PO {Contract} number and date of the revised price list. The correspondence to the Division with the revised price list shall reference the location of the specific price line that has been revised.

The State reserves the right to negotiate any requested price increase determined to be excessive or deny any requests for price increase that are excessive and/or not properly justified by the Vendor {Contractor} and/or recommended by the Division.

Price adjustments shall only be valid when they have been reduced to writing and approved in writing at the sole discretion of the Director. No other changes or revisions to the Blanket P.O. {Contract} and/or price list shall be permitted. The State’s decision shall be final. 

All approved Blanket PO {Contract} price increases will be reflected in a revised Blanket PO {Contract} to the Vendor {Contractor} and the publication of a Change Order {Contract Amendment} on the Division’s NJSTART website.

The State reserves the right to request any information on price concessions, price reductions, monetary benefits, rebates, or any promotional programs offered by the manufacturer, and verify the information provided by the Vendor {Contractor} with the manufacturer or any third party at any time during the term of the Blanket P.O. {Contract}.
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In the event that a new Blanket P.O. {Contract} has not been awarded prior to this Blanket P.O. {Contract} expiration date, including any extensions exercised, and the State exercises this Blanket P.O. {Contract} transition, the Vendor {Contractor} shall continue this Blanket P.O. {Contract} under the same terms, conditions and pricing until a new Blanket P.O. {Contract} can be completely operational. At no time shall this transition period extend more than 180 days beyond the expiration date of this Blanket P.O. {Contract}, including any extensions exercised.

2.3 [bookmark: _Toc108508270][bookmark: _Toc428533980][bookmark: _Toc475717233]CHANGE ORDER {Contract AMENDMENT}

Any changes or modifications to the terms of this Blanket P.O. {Contract} shall be valid only when they have been reduced to writing and signed by the Vendor {Contractor} and the Director.

2.4 [bookmark: _Toc400531510][bookmark: _Toc428533981][bookmark: _Toc475717234]Vendor {contractor} Responsibilities

The Vendor {Contractor} shall have sole responsibility for the complete effort specified in this Blanket P.O. {Contract}. Payment will be made only to the Vendor {Contractor}. The Vendor {Contractor} shall have sole responsibility for all payments due any Subcontractor.

The Vendor {Contractor} is responsible for the professional quality, technical accuracy and timely completion and submission of all deliverables, services or commodities required to be provided under this Blanket P.O. {Contract}. The Vendor {Contractor} shall, without additional compensation, correct or revise any errors, omissions, or other deficiencies in its deliverables and other services. The approval of deliverables furnished under this Blanket P.O. {Contract} shall not in any way relieve the Vendor {Contractor} of responsibility for the technical adequacy of its work. The review, approval, acceptance or payment for any of the services shall not be construed as a waiver of any rights that the State may have arising out of the Vendor’s {Contractor’s} performance of this Blanket P.O. {Contract}.

2.5 [bookmark: _Toc449428269][bookmark: _Toc475717235]Claims and Remedies

2.5.1 [bookmark: _Toc449428270][bookmark: _Toc475717236]Claims

All claims asserted against the State by the Vendor {Contractor} shall be subject to the New Jersey Tort Claims Act, N.J.S.A. 59:1-1, et seq., and/or the New Jersey Contractual Liability Act, N.J.S.A. 59:13-1, et seq.

2.5.2 [bookmark: _Toc449428271][bookmark: _Toc475717237]Remedies

Nothing in the Blanket P.O. {Contract} shall be construed to be a waiver by the State of any warranty, expressed or implied, of any remedy at law or equity, except as specifically and expressly stated in a writing executed by the Director.

2.5.3 [bookmark: _Toc473708422][bookmark: _Toc473720033][bookmark: _Toc474153107][bookmark: _Toc474246647][bookmark: _Toc474741591][bookmark: _Toc473708423][bookmark: _Toc473720034][bookmark: _Toc474153108][bookmark: _Toc474246648][bookmark: _Toc474741592][bookmark: _Toc473708424][bookmark: _Toc473720035][bookmark: _Toc474153109][bookmark: _Toc474246649][bookmark: _Toc474741593][bookmark: _Toc473708425][bookmark: _Toc473720036][bookmark: _Toc474153110][bookmark: _Toc474246650][bookmark: _Toc474741594][bookmark: _Toc473708426][bookmark: _Toc473720037][bookmark: _Toc474153111][bookmark: _Toc474246651][bookmark: _Toc474741595][bookmark: _Toc473708427][bookmark: _Toc473720038][bookmark: _Toc474153112][bookmark: _Toc474246652][bookmark: _Toc474741596][bookmark: _Toc473708428][bookmark: _Toc473720039][bookmark: _Toc474153113][bookmark: _Toc474246653][bookmark: _Toc474741597][bookmark: _Toc449428272][bookmark: _Toc475717238]Remedies for failure to comply with material Blanket P.O. {contract} requirements

In the event that the Vendor {Contractor} fails to comply with any material Blanket P.O. {Contract} requirements, the Director may take steps to terminate the Blanket P.O. {Contract} in accordance with the SSTC, authorize the delivery of Blanket P.O. {Contract} items by any available means, with the difference between the price paid and the defaulting Vendor’s {Contractor’s} price either being deducted from any monies due the defaulting Vendor {Contractor} or being an obligation owed the State by the defaulting Vendor {Contractor} as provided for in the State administrative code, or take any other action or seek any other remedies available at law or in equity.

2.6 [bookmark: _Toc449428273][bookmark: _Toc475717239]Items Ordered and Delivered

The Blanket P.O. {Contract} involves items which are necessary for the continuation of ongoing critical State services. Any delay in delivery of these items would disrupt State services and would force the State to immediately seek alternative sources of supply on an emergency basis. Timely delivery is critical to meeting the State's ongoing needs. Refer to Section 6.3.a of the State of NJ Standard Terms and Conditions for additional information.

2.7 [bookmark: _Toc449428274][bookmark: _Toc475717240]MANUFACTURING/PACKAGING REQUIREMENTS

	All products must conform in every respect to the standards and regulations established by Federal and New Jersey State laws. 

 	All products shall be manufactured and packaged under modern sanitary conditions in accordance with federal and state law and standard industry practice.

	All products are to be packaged in sizes as specified in this Bid Solicitation {RFP} and shall be packaged in such a manner as to ensure delivery in first class condition and properly marked for identification. All shipments must be comprised of original cartons associated with the commercial industry represented by the actual product contained within each carton. Deliveries containing re-used, re-labeled, re-worked or alternate cartons are subject to rejection by the Using Agency at the Vendor’s {Contractor's} expense.

2.8 [bookmark: _Toc475717241]ELECTRONIC PAYMENTS	

With the award of this Blanket P.O. {Contract}, the successful Vendor(s) {Contractor(s)} will be required to receive its payment(s) electronically. In order to receive your payments via automatic deposit from the State of New Jersey, complete and return the “Credit Authorization Agreement for Automatic Deposits (ACH Credits)” Form with an original voided check or bank letter. The form must include ABA number (routing or transit number), bank account number, and if the bank account is a checking or savings account. The form and instructions are located on the Office of Management & Budget’s website at:  http://www.state.nj.us/treasury/omb/forms/index.shtml. The completed form along with the required voided check or bank letter should be mailed or faxed to: Department of the Treasury, Office of Management and Budget, PO Box 221, 6TH Floor – Room 674, Trenton, N.J. 08625-0221; fax: (609)-984-5210. To assist in identifying payments, the State offers Vendors {Contractors} access to the Vendor Payment Inquiry web application (VPI) which offers check stub information online. Contact the State of New Jersey at AAIUNIT@treas.nj.gov to request access to this application.

2.9 [bookmark: _Toc400531512][bookmark: _Toc428533983][bookmark: _Toc475717242]Substitution or Addition of SubCONTRACTOR(s)

This Section of the Bid Solicitation {RFP} serves to supplement but not to supersede Sections 5.8 and 5.9 of the SSTC accompanying this Bid Solicitation {RFP}.

The Vendor {Contractor} shall forward a written request to substitute or add a Subcontractor or to substitute its own staff for a Subcontractor to the Blanket P.O.’s {Contract’s} assigned Procurement Specialist for consideration. If the Procurement Specialist approves the request, the Procurement Specialist will forward the request to the Director for final approval. No substituted or additional Subcontractors are authorized to begin work until the Vendor {Contractor} has received written approval from the Director.

If it becomes necessary for the Vendor {Contractor} to substitute a Subcontractor, add a Subcontractor, or substitute its own staff for a Subcontractor, the Vendor {Contractor} will identify the proposed new Subcontractor or staff member(s) and the work to be performed. The Vendor {Contractor} must provide detailed justification documenting the necessity for the substitution or addition.

The Vendor {Contractor} must provide detailed information of its proposed replacement staff or of the proposed Subcontractor’s management, supervisory, and other key personnel that demonstrate knowledge, ability and experience relevant to that part of the work which the Subcontractor is to undertake.

The qualifications and experience of the replacement(s) must equal or exceed those of similar personnel proposed by the Vendor {Contractor} in its Quote {Proposal}.
[bookmark: _Toc400531518][bookmark: _Toc428533989]
2.10 [bookmark: _Toc400531538][bookmark: _Toc428534010][bookmark: _Toc475717243]BLANKET P.O. {Contract} Activity Report

The Vendor {Contractor} must provide, on a calendar quarterly basis, a record of all purchases made under this Blanket P.O. {Contract} resulting from this Bid Solicitation {RFP}. This reporting requirement includes sales to State Using Agencies, political sub-divisions thereof and, if permitted under the terms of this Blanket P.O. {Contract}, sales to counties, municipalities, school districts, volunteer fire departments, first aid squads and rescue squads, independent institutions of higher education, state and county colleges and quasi-state agencies. Quasi-state agencies include any agency, commission, board, authority or other such governmental entity which is established and is allocated to a State department or any bi-state governmental entity of which the State of New Jersey is a member.

This information must be provided in Microsoft excel such that an analysis can be made to determine the following:

a. Vendor’s {Contractor’s} total sales volume, with line item detail, to each purchaser under this Blanket P.O. {Contract};

b. Subtotals by product, including, if applicable, catalog number and description, price list with appropriate page reference, and/or Blanket P.O. {Contract} discount applied; and

c. Total dollars paid to Subcontractors.

Submission of purchase orders, confirmations, and/or invoices do not fulfill this Blanket P.O. {Contract} requirement for information. Failure to report this mandated information may be a factor in future award decisions.

The Vendor {Contractor} must submit the required information in Microsoft Excel format to NJSupplierReports@treas.nj.gov.
 
Reports are due:
	Quarter 1:	January 1st through March 31st – due by April 30th
	Quarter 2:	April 1st through June 30th – due by July 30th
	Quarter 3:	July 1st through September 30th – due by October 30th
	Quarter 4:	October 1st through December 31st – due by January 30th	

2.11 [bookmark: _Toc400531540][bookmark: _Toc428534012][bookmark: _Toc475717244]PROGRAM EFFICIENCY ASSESSMENT FOR STATE USING AGENCIES

The Program Efficiency Assessment shall not be charged against the winning Vendor(s) {Contractor(s)} and therefore is not to be included in the Vendor’s {Bidder’s} pricing. The State Using Agencies shall be charged an assessment equal to one-quarter of one percent (0.25%) of the value of all transactions under this Blanket P.O. {Contract}. This assessment is authorized by N.J.S.A. 52:27B-56 and N.J.A.C. 17:12-1.5, to maintain the State’s procurement system at a level to meet industry standards of efficiency.

For purposes of this section, “transaction” is defined as the payment or remuneration to the Vendor {Contractor} for services rendered or products provided to the State pursuant to the terms of this Blanket P.O. {Contract}, including but not limited to the following: purchase orders, invoices, hourly rates, firm fixed price, commission payments, progress payments and contingency payments.

2.12 [bookmark: _Toc449428280][bookmark: _Toc475717245]DISCLOSURE OF PRODUCT COMPOSITION

Not applicable to this procurement.

2.13 [bookmark: _Toc475717246]News Releases

The Vendor {Contractor} is not permitted to issue news releases pertaining to any aspect of the services being provided under this Blanket P.O. {Contract} without the prior written consent of the Director.

2.14 [bookmark: _Toc400531519][bookmark: _Toc428533990][bookmark: _Toc475717247]Advertising

The Vendor {Contractor} shall not use the State’s name, logos, images, or any data or results arising from this Blanket P.O. {Contract} as a part of any commercial advertising without first obtaining the prior written consent of the Director.




3.0 [bookmark: _Toc332803059][bookmark: _Toc324415444][bookmark: _5.17_Retainage][bookmark: _5.21_Additional_Work][bookmark: _5.22_Additional_Work][bookmark: _5.9_Substitution_of][bookmark: _5.19_requirements_of_Executive_orde][bookmark: _5.20_requirements_of_Executive_orde][bookmark: _Toc400531541][bookmark: _Toc428534013][bookmark: _Toc475717248] QUOTE {PROPOSAL} EVALUATION
[bookmark: _Toc118513836]
3. [bookmark: _Toc400531542][bookmark: _Toc428534014][bookmark: _Toc475717249]RIGHT TO WAIVE
The Director reserves the right to waive minor irregularities or omissions in a Quote {Proposal}. The Director also reserves the right to waive a requirement provided that the requirement does not materially affect the procurement or the State's interests associated with the procurement.
3.1 [bookmark: _Toc400531543][bookmark: _Toc428534015][bookmark: _Toc475717250]DIRECTOR’S RIGHT OF FINAL Quote {Proposal} ACCEPTANCE

The Director reserves the right to reject any or all Quotes {Proposals}, or to award in whole or in part if deemed to be in the best interest of the State to do so. The Director shall have authority to award orders or Blanket P.O.s {Contracts} in accordance with N.J.S.A. 52:34-12. Tie Quotes {Proposals} will be awarded by the Director in accordance with N.J.A.C. 17:12-2.10. 

3.2 [bookmark: _Toc400531544][bookmark: _Toc428534016][bookmark: _Toc475717251]STATE'S RIGHT TO INSPECT VENDOR {BIDDER} FACILITIES

The State reserves the right to inspect the Vendor’s {Bidder’s} establishment before making an award, for the purposes of ascertaining whether the Vendor {Bidder} has the necessary facilities for performing the Blanket P.O. {Contract}.

The State may also consult with clients of the Vendor {Bidder} during the evaluation of Quotes {Proposals}. Such consultation is intended to assist the State in making a Blanket P.O. {Contract} award that is most advantageous to the State.

3.3 [bookmark: _Toc400531545][bookmark: _Toc428534017][bookmark: _Toc475717252]STATE'S RIGHT TO REQUEST FURTHER INFORMATION

The Director reserves the right to request all information which may assist him or her in making a Blanket P.O. {Contract} award, including factors necessary to evaluate the Vendor’s {Bidder’s} financial capabilities to perform the Blanket P.O. {Contract}. Further, the Director reserves the right to request a Vendor {Bidder} to explain, in detail, how the Quote {Proposal} price was determined.

3.4 [bookmark: _Toc118513837][bookmark: _Toc400531547][bookmark: _Toc428534019][bookmark: _Toc475717253]Oral Presentation and/or Clarification of Quote {Proposal}

After the submission of Quotes {Proposals}, unless requested by the State as noted below, Vendor {Bidder} contact with the State is still not permitted. 

After the Quotes {Proposals} are reviewed, one, some or all of the Vendors {Bidders} may be asked to clarify certain aspects of its Quote {Proposal}. A request for clarification may be made in order to resolve minor ambiguities, irregularities, informalities or clerical errors. Clarifications cannot correct any deficiencies or material omissions, or revise or modify a Quote {Proposal}, except to the extent that correction of apparent clerical mistakes results in a modification.

The Vendor {Bidder} may be required to give an oral presentation to the State concerning its Quote {Proposal}. 

A Vendor {Bidder} may not attend the oral presentations of its competitors.

It is within the State’s discretion whether to require the Vendor {Bidder} to give an oral presentation or require the Vendor {Bidder} to submit written responses to questions regarding its Quote {Proposal}. Action by the State in this regard should not be construed to imply acceptance or rejection of a Quote {Proposal}. The Division will be the sole point of contact regarding any request for an oral presentation or clarification.

3.5 [bookmark: _Toc118513838][bookmark: _Toc400531548][bookmark: _Toc428534020][bookmark: _Toc475717254]Evaluation Criteria

The following criteria will be used to evaluate Quotes {Proposals} received in response to this Bid Solicitation {RFP}. The criteria are not necessarily listed in order of importance:

a. Group Price (The sum of price lines one (1) through fourteen (14).)
 
b. Experience of the Vendor {Bidder}

c. The Vendor’s {Bidder's} documented past performance under similar Blanket P.O.s {Contracts}, including, but not limited to, the Division's Vendor {Contractor} performance database.

3.5.1 [bookmark: _Toc118513841][bookmark: _Toc400531551][bookmark: _Toc428534023][bookmark: _Toc475717255]QUOTE {PROPOSAL} discrepancies

In evaluating Quotes {Proposals}, discrepancies between words and figures will be resolved in favor of words. Discrepancies between unit prices and totals of unit prices will be resolved in favor of unit prices. Discrepancies in the multiplication of units of work and unit prices will be resolved in favor of the unit prices. Discrepancies between the indicated total of multiplied unit prices and units of work and the actual total will be resolved in favor of the actual total. Discrepancies between the indicated sum of any column of figures and the correct sum thereof will be resolved in favor of the correct sum of the column of figures.

In the event that a Vendor {Bidder} using NJSTART to submit a Quote {Proposal} uploads a price sheet/schedule attachment and completes the “Items” Tab in NJSTART (instead of entering a Unit Cost of $1.00 as instructed), the price sheet/schedule attachment will govern.

3.5.2 [bookmark: _Toc400531552][bookmark: _Toc428534024][bookmark: _Toc475717256]Evaluation of the QUOTES {Proposals}

After the Evaluation Committee completes its evaluation, it recommends to the Director for award the responsible Vendor(s) {Bidder(s)} whose Quote {Proposal}, conforming to this Bid Solicitation {RFP}, is most advantageous to the State, price and other factors considered. The Evaluation Committee considers and assesses price, technical criteria, and other factors during the evaluation process and makes a recommendation to the Director. The Director may accept, reject or modify the recommendation of the Evaluation Committee. Whether or not there has been a negotiation process as outlined in Section 6.7 below, the Director reserves the right to negotiate price reductions with the selected Vendor(s) {Bidder(s)}.

3.6 [bookmark: _Toc118513842][bookmark: _Toc400531553][bookmark: _Toc428534025][bookmark: _Toc475717257]Negotiation and Best and Final Offer (BAFO) 

In accordance with N.J.S.A. 52:34-12(f) and N.J.A.C. 17:12-2-7, after evaluating Quotes {Proposals}, the Division may establish a competitive range and enter into negotiations with one Vendor {Bidder} or multiple Vendors {Bidders} within this competitive range. The primary purpose of negotiations is to maximize the State’s ability to obtain the best value based on the mandatory requirements, evaluation criteria, and cost.  Multiple rounds of negotiations may be conducted with one Vendor {Bidder} or multiple Vendors {Bidders}.  Negotiations will be structured by the Division to safeguard information and ensure that all Vendors {Bidders} are treated fairly.

Similarly, the Division may invite one Vendor {Bidder} or multiple Vendors {Bidders} to submit a Best and Final Offer (BAFO). Said invitation will establish the time and place for submission of the BAFO. Any BAFO that does not result in more advantageous pricing to the State will not be considered, and the State will evaluate the Vendor’s {Bidder’s} most advantageous previously submitted pricing.

If required, after review of the BAFO(s), clarification may be sought from the Vendor(s) {Bidder(s)}.  The Division may conduct more than one round of negotiation and/or BAFO in order to attain the best value for the State. 

After evaluation of Quotes {Proposals} and as applicable, negotiation(s), and/or BAFO(s), the Division will recommend, to the Director, the responsible Vendor(s) {Bidder(s)} whose Quote(s) {Proposal(s)}, conforming to the Bid Solicitation {RFP}, is/are most advantageous to the State, price, and other factors considered. The Director may accept, reject or modify the recommendation of the Division. The Director may initiate additional negotiation or BAFO procedures with the selected Vendor(s) {Bidder(s)}.

Negotiations will be conducted only in those circumstances where it is deemed by the Division or Director to be in the State’s best interests and to maximize the State’s ability to get the best value.  Therefore, the Vendor {Bidder} is advised to submit its best technical and price Quote {Proposal} in response to this Bid Solicitation {RFP} since the State may, after evaluation, make a Blanket P.O. {Contract} award based on the content of the initial submission, without further negotiation and/or BAFO with any Vendor {Bidder}.  

All contacts, records of initial evaluations, any correspondence with a Vendor {Bidder} related to any request for clarification, negotiation or BAFO, any revised technical and/or price Quotes {Proposals}, and related documents will remain confidential until a Notice of Intent to Award a Blanket P.O. {Contract} is issued.

If the Division contemplates negotiation, Quote {Proposal} prices will not be publicly read at the Quote {Proposal} opening.  Only the name and address of each Vendor {Bidder} will be publicly announced at the Quote {Proposal} opening.

3.7 [bookmark: _Toc475717258]“REQUEST FOR REVISION” WITHIN NJSTART

The State may request a revision of the Vendor’s {Bidder’s} Quote {Proposal} within NJSTART. The Vendor {Bidder} shall respond to the “Request for Revision” (e.g., to reduce pricing if a BAFO is requested) only for the reason(s) identified by the State. Any changes made by a Vendor {Bidder} to the Quote {Proposal} other than as requested by the State shall be considered null and void. 

3.8 [bookmark: _Toc400531554][bookmark: _Toc428534026][bookmark: _Toc475717259]POOR PERFORMANCE

A Vendor {Bidder} with a history of performance problems may be bypassed for consideration of an award issued as a result of this Bid Solicitation {RFP}.  The following materials may be reviewed to determine Vendor {Bidder} performance:  Blanket P.O. {Contract} cancellations for cause pursuant to Section 5.7(b) of the SSTC; information contained in Vendor performance records; information obtained from audits or investigations conducted by a local, state or federal agency of the Vendor’s {Bidder’s} work experience; current licensure, registration, and/or certification status and relevant history thereof; or its status or rating with established business/financial reporting services, as applicable.  Vendors {Bidders} should note that this list is not exhaustive.
4.0 [bookmark: _Toc220920713][bookmark: _Toc400531555][bookmark: _Toc428534027][bookmark: _Toc475717260]
 BLANKET P.O. {CONTRACT} AWARD

4. [bookmark: _Toc220920714][bookmark: _Toc400531556][bookmark: _Toc428534028][bookmark: _Toc475717261]DOCUMENTS REQUIRED BEFORE BLANKET P.O. {CONTRACT} AWARD

4.0.1 [bookmark: _Toc220920715][bookmark: _Toc400531557][bookmark: _Toc428534029][bookmark: _Toc475717262]Requirements of Public Law 2005, CHAPTER 51, N.J.S.A. 19:44A-20.13 - N.J.S.A. 19:44A-20.25 (Formerly Executive Order NO. 134), EXECUTIVE ORDER No. 117 (2008) and N.J.A.C. 17:12-5 et seq.

a. The State shall not enter into a Blanket P.O. {Contract} to procure services or any material, supplies or equipment, or to acquire, sell, or lease any land or building from any Business Entity, where the value of the transaction exceeds $17,500, if that Business Entity has solicited or made any contribution of money, or pledge of contribution, including in-kind contributions, to a candidate committee and/or election fund of any candidate for or holder of the public office of Governor or Lieutenant Governor, to any State, county, municipal political party committee, or to any legislative leadership committee during certain specified time periods. 

b. Prior to awarding any Blanket P.O. {Contract} or agreement to any Business Entity, the Business Entity proposed as the intended Vendor {Contractor} of the Blanket P.O. {Contract} shall submit the Two-Year Chapter 51/Executive Order 117 Vendor Certification and Disclosure of Political Contributions form, certifying that no contributions prohibited by either Chapter 51 or Executive Order No. 117  have been made by the Business Entity and reporting all contributions the Business Entity made during the preceding four (4) years to any political organization organized under 26 U.S.C.527 of the Internal Revenue Code that also meets the definition of a “continuing political committee” within the means of N.J.S.A. 19:44A-3(n) and N.J.A.C. 19:25-1.7. The required form and instructions, available for review on the Division’s website at http://www.state.nj.us/treasury/purchase/forms/eo134/Chapter51.pdf, shall be provided to the intended Vendor {Contractor} for completion and submission to the Division with the Notice of Intent to Award. Upon receipt of a Notice of Intent to Award a Blanket P.O. {Contract}, the intended Vendor {Contractor} shall submit to the Division, in care of the Division Procurement Specialist, the Certification and Disclosure(s) within five (5) business days of the State’s request. Failure to submit the required forms will preclude award of a Blanket P.O. {Contract} under this Bid Solicitation {RFP}, as well as future Blanket P.O. {Contract} opportunities. 

c. Further, the Vendor {Contractor} is required, on a continuing basis, to report any contributions it makes during the term of the Blanket P.O. {Contract}, and any extension(s) thereof, at the time any such contribution is made. The required form and instructions, available for review on the Division’s website at http://www.state.nj.us/treasury/purchase/forms/eo134/Chapter51.pdf, shall be provided to the intended Vendor {Contractor} with the Notice of Intent to Award. 

The Two-Year Chapter 51/Executive Order 117 Vendor Certification and Disclosure of Political Contributions form is located on the Division’s website. The form is also available in NJSTART.
Vendors {Bidders} may refer to the QRGs “Vendor Forms” and “Attaching Files” for instructions on submitting the forms required by this section of the Bid Solicitation {RFP} through NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

Vendors {Bidders} should verify its Chapter 51 Compliance status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Chapter 51 Compliance status, NJSTART provides a link to take corrective action.




4.0.2 [bookmark: _Toc400531558][bookmark: _Toc428534030][bookmark: _Toc475717263]SOURCE DISCLOSURE REQUIREMENTS

Not applicable to this procurement.

4.0.3 [bookmark: _Toc400531559][bookmark: _Toc428534031][bookmark: _Toc475717264]AFFIRMATIVE Action 

The intended Vendor {Contractor} must submit a copy of a New Jersey Certificate of Employee Information Report, or a copy of Federal Letter of Approval verifying it is operating under a federally approved or sanctioned Affirmative Action program.   Intended Vendors {Contractors} not in possession of either a New Jersey Certificate of Employee Information Report or a Federal Letter of Approval  must complete the Affirmative Action Employee Information Report (AA-302) located on the web at http://www.nj.gov/treasury/purchase/forms/AA_%20Supplement.pdf.

Vendors {Bidders} should verify its Affirmative Action Compliance status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Affirmative Action Compliance status, NJSTART provides a link to take corrective action.

4.0.4 [bookmark: _Toc261501847][bookmark: _Toc400531560][bookmark: _Toc428534032][bookmark: _Toc475717265]BUSINESS REGISTRATION

In accordance with N.J.S.A. 52:32-44(b), a Vendor {Bidder} and its named Subcontractors must have a valid Business Registration Certificate (“BRC”) issued by the Department of the Treasury, Division of Revenue and Enterprise Services prior to the award of a Blanket P.O. {Contract}.  See Section 4.4.2.1 of this Bid Solicitation {RFP} for further information.

Vendors {Bidders} should verify its Business Registration Certification Active status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Business Registration Certification Active status, NJSTART provides a link to take corrective action. Vendors {Bidders} may refer to the QRG “Vendor Categories and Certifications” for instructions on completing certifications on the “Maintain Terms and Categories” Tab within its profile in NJSTART. QRGs are located on the NJSTART Vendor Support Page. 

4.1 [bookmark: _Toc400531561][bookmark: _Toc428534033][bookmark: _Toc475717266]FINAL BLANKET P.O. {CONTRACT} AWARD

Blanket P.O. {Contract} award[s] will be made with reasonable promptness by written notice to that responsible Vendor(s) {Bidder(s)}, whose Quote(s) {Proposal(s)}, conforming to this Bid Solicitation {RFP}, is(are) most advantageous to the State, price, and other factors considered.  Any or all Quotes {Proposals} may be rejected when the State Treasurer or the Director determines that it is in the public interest to do so.

4.2 [bookmark: _Toc400531562][bookmark: _Toc428534034][bookmark: _Toc475717267]INSURANCE CERTIFICATES

The Vendor {Contractor} shall provide the State with current certificates of insurance for all coverages required by the terms of this Blanket P.O. {Contract}, naming the State as an Additional Insured.   See Section 4.2 of the SSTC accompanying this Bid Solicitation {RFP}.

Vendors {Bidders} should verify its Insurance Certification Compliance status on the “Maintain Terms and Categories” Tab within its profile in NJSTART. In the event of an issue with a Vendor’s {Bidder’s} Insurance Certification Compliance status, contact the Division Procurement Specialist.

[bookmark: _Toc475717268]Performance Security

Not applicable to this procurement.



5.0 [bookmark: _Toc473708459][bookmark: _Toc473720070][bookmark: _Toc474153144][bookmark: _Toc474246684][bookmark: _Toc474741628][bookmark: _Toc473708460][bookmark: _Toc473720071][bookmark: _Toc474153145][bookmark: _Toc474246685][bookmark: _Toc474741629][bookmark: _Toc473708461][bookmark: _Toc473720072][bookmark: _Toc474153146][bookmark: _Toc474246686][bookmark: _Toc474741630][bookmark: _Toc473708462][bookmark: _Toc473720073][bookmark: _Toc474153147][bookmark: _Toc474246687][bookmark: _Toc474741631][bookmark: _Toc473708463][bookmark: _Toc473720074][bookmark: _Toc474153148][bookmark: _Toc474246688][bookmark: _Toc474741632][bookmark: _Toc473708464][bookmark: _Toc473720075][bookmark: _Toc474153149][bookmark: _Toc474246689][bookmark: _Toc474741633][bookmark: _Toc473708465][bookmark: _Toc473720076][bookmark: _Toc474153150][bookmark: _Toc474246690][bookmark: _Toc474741634][bookmark: _Toc473708467][bookmark: _Toc473720078][bookmark: _Toc474153152][bookmark: _Toc474246692][bookmark: _Toc474741636][bookmark: _Toc473708469][bookmark: _Toc473720080][bookmark: _Toc474153154][bookmark: _Toc474246694][bookmark: _Toc474741638][bookmark: _Toc473708471][bookmark: _Toc473720082][bookmark: _Toc474153156][bookmark: _Toc474246696][bookmark: _Toc474741640][bookmark: _Toc473708472][bookmark: _Toc473720083][bookmark: _Toc474153157][bookmark: _Toc474246697][bookmark: _Toc474741641][bookmark: _Toc473708473][bookmark: _Toc473720084][bookmark: _Toc474153158][bookmark: _Toc474246698][bookmark: _Toc474741642][bookmark: _Toc473708475][bookmark: _Toc473720086][bookmark: _Toc474153160][bookmark: _Toc474246700][bookmark: _Toc474741644][bookmark: _Toc473708476][bookmark: _Toc473720087][bookmark: _Toc474153161][bookmark: _Toc474246701][bookmark: _Toc474741645][bookmark: _Toc473708477][bookmark: _Toc473720088][bookmark: _Toc474153162][bookmark: _Toc474246702][bookmark: _Toc474741646][bookmark: _Toc473708479][bookmark: _Toc473720090][bookmark: _Toc474153164][bookmark: _Toc474246704][bookmark: _Toc474741648][bookmark: _Toc473708481][bookmark: _Toc473720092][bookmark: _Toc474153166][bookmark: _Toc474246706][bookmark: _Toc474741650][bookmark: _Toc473708483][bookmark: _Toc473720094][bookmark: _Toc474153168][bookmark: _Toc474246708][bookmark: _Toc474741652][bookmark: _Toc473708485][bookmark: _Toc473720096][bookmark: _Toc474153170][bookmark: _Toc474246710][bookmark: _Toc474741654][bookmark: _Toc473708487][bookmark: _Toc473720098][bookmark: _Toc474153172][bookmark: _Toc474246712][bookmark: _Toc474741656][bookmark: _Toc400531564][bookmark: _Toc428534036][bookmark: _Toc475717269] BLANKET P.O. {CONTRACT} ADMINISTRATION

5. [bookmark: _Toc400531565][bookmark: _Toc428534037][bookmark: _Toc475717270]STATE CONTRACT MANAGER

The State Contract Manager (SCM) is the State employee responsible for the overall management and administration of the Blanket P.O. {Contract}. 

The State Contract Manager for this project will be identified at the time of execution of Blanket P.O. {Contract}.  At that time, the Vendor {Contractor} will be provided with the State Contract Manager’s name, department, division, agency, address, telephone number, fax phone number, and e-mail address.

5.0.1 [bookmark: _Toc400531566][bookmark: _Toc428534038][bookmark: _Toc475717271]state contract manager responsibilities

For an agency Blanket P.O. {Contract} where only one State office uses the Blanket P.O. {Contract}, the State Contract Manager will be responsible for engaging the Vendor {Contractor}, assuring that Purchase Orders are issued to the Vendor {Contractor}, directing the Vendor {Contractor} to perform the work of the Blanket P.O. {Contract}, approving the deliverables and approving payment vouchers.  The State Contract Manager is the person who the Vendor {Contractor} will contact after the Blanket P.O. {Contract} is executed for answers to any questions and concerns about any aspect of the Blanket P.O. {Contract}.  The State Contract Manager is responsible for coordinating the use of the Blanket P.O. {Contract} and resolving minor disputes between the Vendor {Contractor} and any component part of the State Contract Manager's Department.  The State Contract Manager is also responsible for notifying OIT and other appropriate parties of security and privacy violations or incidents.  The SCM cannot modify the Blanket P.O. {Contract}, direct or approve a Change Order {Contract Amendment}.  

If the Blanket P.O. {Contract} has multiple users, the State Contract Manager shall be the central coordinator of the use of the Blanket P.O. {Contract} for all Using Agencies, while other State employees engage and pay the Vendor {Contractor}.  All persons and agencies using the Blanket P.O. {Contract} must notify and coordinate the use of the Blanket P.O. {Contract} with the State Contract Manager.  

5.0.2 [bookmark: _Toc400531567][bookmark: _Toc428534039][bookmark: _Toc475717272]Coordination with the State Contract manager

Any Blanket P.O. {Contract} user that is unable to resolve disputes with a Vendor {Contractor} shall refer those disputes to the State Contract Manager for resolution.  Any questions related to performance of the work of the Blanket P.O. {Contract} by Blanket P.O. {Contract} users shall be directed to the State Contract Manager.  The Vendor {Contractor} may contact the State Contract Manager if the Vendor {Contractor} cannot resolve a dispute with Blanket P.O. {Contract} users.


6.0 [bookmark: _Toc475717273] State of New Jersey Standard Terms and Conditions
(Rev: 12/15/2016 ST&C)

1. STANDARD TERMS AND CONDITIONS APPLICABLE TO THE CONTRACT - Unless the bidder/offeror is specifically instructed otherwise in the Request for Proposals (RFP), the following terms and conditions shall apply to all contracts or purchase agreements made with the State of New Jersey. These terms are in addition to the terms and conditions set forth in the RFP and should be read in conjunction with same unless the RFP specifically indicates otherwise. In the event that the bidder/offeror would like to present terms and conditions that are in conflict with either these terms and conditions or those set forth in the RFP, the bidder/offeror must present those conflicts during the Question and Answer period for the State to consider. Any conflicting terms and conditions that the State is willing to accept will be reflected in an addendum to the RFP. The State's terms and conditions shall prevail over any conflicts set forth in a bidder/offeror's Proposal that were not submitted through the question and answer process and approved by the State. Nothing in these terms and conditions shall prohibit the Director of the Division of Purchase and Property (Director) from amending a contract when the Director determines it is in the best interests of the State. 

[bookmark: _Toc469579742]2. STATE LAW REQUIRING MANDATORY COMPLIANCE BY ALL CONTRACTORS - The statutes, laws or codes cited herein are available for review at the New Jersey State Library, 185 West State Street, Trenton, New Jersey 08625. 

[bookmark: _Toc469579743]2.1 BUSINESS REGISTRATION – Pursuant to N.J.S.A. 52:32-44, the State is prohibited from entering into a contract with an entity unless the bidder and each subcontractor named in the proposal have a valid Business Registration Certificate on file with the Division of Revenue and Enterprise Services. The contractor and any subcontractor providing goods or performing services under the contract, and each of their affiliates, shall, during the term of the contract, collect and remit to the Director of the Division of Taxation in the Department of the Treasury, the use tax due pursuant to the “Sales and Use Tax Act, P.L. 1966, c. 30 (N.J.S.A. 54:32B-1 et seq.) on all sales of tangible personal property delivered into the State. Any questions in this regard can be directed to the Division of Revenue at (609) 292-1730. Form NJ-REG can be filed online at http://www.state.nj.us/treasury/revenue/busregcert.shtml.

[bookmark: _Toc469579744]2.2 ANTI-DISCRIMINATION - All parties to any contract with the State agree not to discriminate in employment and agree to abide by all anti-discrimination laws including those contained within N.J.S.A. 10:2-1 through N.J.S.A. 10:2-4, N.J.S.A. 10:5-1 et seq. and N.J.S.A. 10:5-31 through 10:5-38, and all rules and regulations issued thereunder are hereby incorporated by reference. The agreement to abide by the provisions of N.J.S.A. 10:5-31 through 10:5-38 include those provisions indicated for Goods, Professional Service and General Service Contracts (Exhibit A, attached) and Constructions Contracts (Exhibit B and Executive Order 151, August 28, 2009, attached) as appropriate.

The contractor or subcontractor, where applicable, agrees to comply with any regulations promulgated by the Treasurer pursuant to N.J.S.A. 10:5-31 et seq., as amended and supplemented from time to time.

[bookmark: _Toc469579745]2.3 PREVAILING WAGE ACT - The New Jersey Prevailing Wage Act, N.J.S.A. 34: 11-56.265 et seq. is hereby made part of every contract entered into on behalf of the State of New Jersey through the Division of Purchase and Property, except those contracts which are not within the contemplation of the Act. The bidder's signature on [this proposal] is his guarantee that neither he nor any subcontractors he might employ to perform the work covered by [this proposal] has been suspended or debarred by the Commissioner, Department of Labor and Workforce Development for violation of the provisions of the Prevailing Wage Act and/or the Public Works Contractor Registration Acts; the bidder’s signature on the proposal is also his guarantee that he and any subcontractors he might employ to perform the work covered by [this proposal] shall comply with the provisions of the Prevailing Wage and Public Works Contractor Registration Acts, where required. 

2.4 AMERICANS WITH DISABILITIES ACT - The contractor must comply with all provisions of the Americans with Disabilities Act (ADA), P.L 101-336, in accordance with 42 U.S.C. 12101, et seq. 

[bookmark: _Toc469579746]2.5 MACBRIDE PRINCIPLES – The bidder must certify pursuant to N.J.S.A. 52:34-12.2 that it either has no ongoing business activities in Northern Ireland and does not maintain a physical presence therein or that it will take lawful steps in good faith to conduct any business operations it has in Northern Ireland in accordance with the MacBride principles of nondiscrimination in employment as set forth in N.J.S.A. 52:18A-89.5 and in conformance with the United Kingdom’s Fair Employment (Northern Ireland) Act of 1989, and permit independent monitoring of their compliance with those principles. 

[bookmark: _Toc469579747]2.6 PAY TO PLAY PROHIBITIONS – Pursuant to N.J.S.A. 19:44A-20.13 et seq. (L.2005, c. 51), and specifically, N.J.S.A. 19:44A-20.21, it shall be a breach of the terms of the contract for the business entity to: 

a. Make or solicit a contribution in violation of the statute; 
b. Knowingly conceal or misrepresent a contribution given or received; 
c. Make or solicit contributions through intermediaries for the purpose of concealing or misrepresenting the source of the contribution; 
d. Make or solicit any contribution on the condition or with the agreement that it will be contributed to a campaign committee or any candidate of holder of the public office of Governor, or to any State or county party committee; 
e. Engage or employ a lobbyist or consultant with the intent or understanding that such lobbyist or consultant would make or solicit any contribution, which if made or solicited by the business entity itself, would subject that entity to the restrictions of the Legislation; 
f. Fund contributions made by third parties, including consultants, attorneys, family members, and employees; 
g. Engage in any exchange of contributions to circumvent the intent of the Legislation; or 
h. Directly or indirectly through or by any other person or means, do any act which would subject that entity to the restrictions of the Legislation. 

[bookmark: _Toc469579748]2.7 POLITICAL CONTRIBUTION DISCLOSURE – The contractor is advised of its responsibility to file an annual disclosure statement on political contributions with the New Jersey Election Law Enforcement Commission (ELEC), pursuant to N.J.S.A. 19:44A-20.27 (P.L. 2005, c. 271, §3 as amended) if in a calendar year the contractor receives one or more contracts valued at $50,000.00 or more. It is the contractor’s responsibility to determine if filing is necessary. Failure to file can result in the imposition of penalties by ELEC. Additional information about this requirement is available from ELEC by calling 1(888)313-3532 or on the internet at http://www.elec.state.nj.us/.

[bookmark: _Toc469579749]2.8 STANDARDS PROHIBITING CONFLICTS OF INTEREST - The following prohibitions on contractor activities shall apply to all contracts or purchase agreements made with the State of New Jersey, pursuant to Executive Order No. 189 (1988). 

No vendor shall pay, offer to pay, or agree to pay, either directly or indirectly, any fee, commission, compensation, gift, gratuity, or other thing of value of any kind to any State officer or employee or special State officer or employee, as defined by N.J.S.A. 52:13D-13b. and e., in the Department of the Treasury or any other agency with which such vendor transacts or offers or proposes to transact business, or to any member of the immediate family, as defined by N.J.S.A. 52:13D-13i., of any such officer or employee, or partnership, firm or corporation with which they are employed or associated, or in which such officer or employee has an interest within the meaning of N.J.S.A. 52: 13D-13g;
 
The solicitation of any fee, commission, compensation, gift, gratuity or other thing of value by any State officer or employee or special State officer or employee from any State vendor shall be reported in writing forthwith by the vendor to the Attorney General and the Executive Commission on Ethical Standards;

[bookmark: _GoBack]No vendor may, directly or indirectly, undertake any private business, commercial or entrepreneurial relationship with, whether or not pursuant to employment, contract or other agreement, express or implied, or sell any interest in such vendor to, any State officer or employee or special State officer or employee having any duties or responsibilities in connection with the purchase, acquisition or sale of any property or services by or to any State agency or any instrumentality thereof, or with any person, firm or entity with which he is employed or associated or in which he has an interest within the meaning of N.J.S.A. 52:130-13g. Any relationships subject to this provision shall be reported in writing forthwith to the Executive Commission on Ethical Standards, which may grant a waiver of this restriction upon application of the State officer or employee or special State officer or employee upon a finding that the present or proposed relationship does not present the potential, actuality or appearance of a conflict of interest;

No vendor shall influence, or attempt to influence or cause to be influenced, any State officer or employee or special State officer or employee in his official capacity in any manner which might tend to impair the objectivity or independence of judgment of said officer or employee;

No vendor shall cause or influence, or attempt to cause or influence, any State officer or employee or special State officer or employee to use, or attempt to use, his official position to secure unwarranted privileges or advantages for the vendor or any other person; and
 
The provisions cited above in paragraphs 2.8a through 2.8e shall not be construed to prohibit a State officer or employee or Special State officer or employee from receiving gifts from or contracting with vendors under the same terms and conditions as are offered or made available to members of the general public subject to any guidelines the Executive Commission on Ethical Standards may promulgate under paragraph 3c of Executive Order No. 189. 

[bookmark: _Toc469579750]2.9 NOTICE TO ALL CONTRACTORS SET-OFF FOR STATE TAX NOTICE - Pursuant to P.L. 1995, c. 159, effective January 1, 1996, and notwithstanding any provision of the law to the contrary, whenever any taxpayer, partnership or S corporation under contract to provide goods or services or construction projects to the State of New Jersey or its agencies or instrumentalities, including the legislative and judicial branches of State government, is entitled to payment for those goods or services at the same time a taxpayer, partner or shareholder of that entity is indebted for any State tax, the Director of the Division of Taxation shall seek to set off that taxpayer’s or shareholder’s share of the payment due the taxpayer, partnership, or S corporation. The amount set off shall not allow for the deduction of any expenses or other deductions which might be attributable to the taxpayer, partner or shareholder subject to set-off under this act. 
The Director of the Division of Taxation shall give notice to the set-off to the taxpayer and provide an opportunity for a hearing within thirty (30) days of such notice under the procedures for protests established under R.S. 54:49-18. No requests for conference, protest, or subsequent appeal to the Tax Court from any protest under this section shall stay the collection of the indebtedness. Interest that may be payable by the State, pursuant to P.L. 1987, c.184 (c.52:32-32 et seq.), to the taxpayer shall be stayed. 

[bookmark: _Toc469579751]2.10 COMPLIANCE - LAWS - The contractor must comply with all local, State and Federal laws, rules and regulations applicable to this contract and to the goods delivered and/or services performed hereunder. 

[bookmark: _Toc469579752]2.11 COMPLIANCE - STATE LAWS - It is agreed and understood that any contracts and/or orders placed as a result of [this proposal] shall be governed and construed and the rights and obligations of the parties hereto shall be determined in accordance with the laws of the State of New Jersey.

3. STATE LAW REQUIRING MANDATORY COMPLIANCE BY CONTRACTORS UNDER CIRCUMSTANCES SET FORTH IN LAW OR BASED ON THE TYPE OF CONTRACT 

3.1 COMPLIANCE - CODES – The contractor must comply with NJUCC and the latest NEC70, B.O.C.A. Basic Building code, OSHA and all applicable codes for this requirement. The contractor shall be responsible for securing and paying all necessary permits, where applicable. 

3.2 PUBLIC WORKS CONTRACTOR REGISTRATION ACT - The New Jersey Public Works Contractor Registration Act requires all contractors, subcontractors and lower tier subcontractor(s) who engage in any contract for public work as defined in N.J.S.A. 34:11-56.26 be first registered with the New Jersey Department of Labor and Workforce Development. Any questions regarding the registration process should be directed to the Division of Wage and Hour Compliance at (609) 292-9464. 

3.3 PUBLIC WORKS CONTRACT - ADDITIONAL AFFIRMATIVE ACTION REQUIREMENTS - 
N.J.S.A. 10:2-1 requires that during the performance of this contract, the contractor must agree as follows: 

a. In the hiring of persons for the performance of work under this contract or any subcontract hereunder, or for the procurement, manufacture, assembling or furnishing of any such materials, equipment, supplies or services to be acquired under this contract, no contractor, nor any person acting on behalf of such contractor or subcontractor, shall, by reason of race, creed, color, national origin, ancestry, marital status, gender identity or expression, affectional or sexual orientation or sex, discriminate against any person who is qualified and available to perform the work to which the employment relates;

b. No contractor, subcontractor, nor any person on his behalf shall, in any manner, discriminate against or intimidate any employee engaged in the performance of work under this contract or any subcontract hereunder, or engaged in the procurement, manufacture, assembling or furnishing of any such materials, equipment, supplies or services to be acquired under such contract, on account of race, creed, color, national origin, ancestry, marital status, gender identity or expression, affectional or sexual orientation or sex;

c. There may be deducted from the amount payable to the contractor by the contracting public agency, under this contract, a penalty of $50.00 for each person for each calendar day during which such person is discriminated against or intimidated in violation of the provisions of the contract; and

d. This contract may be canceled or terminated by the contracting public agency, and all money due or to become due hereunder may be forfeited, for any violation of this section of the contract occurring after notice to the contractor from the contracting public agency of any prior violation of this section of the contract.

N.J.S.A. 10:5-33 and N.J.A.C. 17:27-3.5 require that during the performance of this contract, the contractor must agree as follows: 

a. The contractor or subcontractor, where applicable, will not discriminate against any employee or applicant for employment because of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Except with respect to affectional or sexual orientation and gender identity or expression, the contractor will take affirmative action to ensure that such applicants are recruited and employed, and that employees are treated during employment, without regard to their age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Such action shall include, but not be limited to the following: employment, upgrading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship. The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided by the contracting officer setting forth the provisions of this nondiscrimination clause; 

b. The contractor or subcontractor, where applicable will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex; 

c. The contractor or subcontractor where applicable, will send to each labor union or representative of workers with which it has a collective bargaining agreement or other contract or understanding, a notice, to be provided by the agency contracting officer, advising the labor union or workers' representative of the contractor's commitments under this act and shall post copies of the notice in conspicuous places available to employees and applicants for employment, N.J.A.C. 17:27-3.7 requires all contractors and subcontractors, if any, to further agree as follows: 

1. The contractor or subcontractor agrees to make good faith efforts to meet targeted county employment goals established in accordance with N.J.A.C. 17:27-5.2;

2. The contractor or subcontractor agrees to inform in writing its appropriate recruitment agencies including, but not limited to, employment agencies, placement bureaus, colleges, universities, and labor unions, that it does not discriminate on the basis of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, and that it will discontinue the use of any recruitment agency which engages in direct or indirect discriminatory practices;

3. The contractor or subcontractor agrees to revise any of its testing procedures, if necessary, to assure that all personnel testing conforms with the principles of job-related testing, as established by the statutes and court decisions of the State of New Jersey and as established by applicable Federal law and applicable Federal court decisions; and
 
4. In conforming with the targeted employment goals, the contractor or subcontractor agrees to review all procedures relating to transfer, upgrading, downgrading and layoff to ensure that all such actions are taken without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, consistent with the statutes and court decisions of the State of New Jersey, and applicable Federal law and applicable Federal court decisions. 

3.4 BUILDING SERVICE – Pursuant to N.J.S.A. 34:11-56.58 et seq., in any contract for building services, as defined in N.J.S.A. 34:11-56.59, the employees of the contractor or subcontractors shall be paid prevailing wage for building services rates, as defined in N.J.S.A. 34:11.56.59. The prevailing wage shall be adjusted annually during the term of the contract. 

3.5 THE WORKER AND COMMUNITY RIGHT TO KNOW ACT - The provisions of N.J.S.A. 34:5A-1 et seq. which require the labeling of all containers of hazardous substances are applicable to this contract. Therefore, all goods offered for purchase to the State must be labeled by the contractor in compliance with the provisions of the statute. 

3.6 SERVICE PERFORMANCE WITHIN U.S. – Under N.J.S.A. 52:34-13.2, all contracts primarily for services awarded by the Director shall be performed within the United States, except when the Director certifies in writing a finding that a required service cannot be provided by a contractor or subcontractor within the United States and the certification is approved by the State Treasurer. 
A shift to performance of services outside the United States during the term of the contract shall be deemed a breach of contract. If, during the term of the contract, the contractor or subcontractor, proceeds to shift the performance of any of the services outside the United States, the contractor shall be deemed to be in breach of its contract, which contract shall be subject to termination for cause pursuant to Section 5.7(b) (1) of the Standard Terms and Conditions, unless previously approved by the Director and the Treasurer. 

3.7 BUY AMERICAN – Pursuant to N.J.S.A. 52:32-1, if manufactured items or farm products will be provided under this contract to be used in a public work, they shall be manufactured or produced in the United States and the contractor shall be required to so certify. 

4. INDEMNIFICATION AND INSURANCE 

4.1 INDEMNIFICATION - The contractor’s liability to the State and its employees in third party suits shall be as follows: 

a. Indemnification for Third Party Claims - The contractor shall assume all risk of and responsibility for, and agrees to indemnify, defend, and save harmless the State of New Jersey and its employees from and against any and all claims, demands, suits, actions, recoveries, judgments and costs and expenses in connection therewith which shall arise from or result directly or indirectly from the work and/or materials supplied under this contract, including liability of any nature or kind for or on account of the use of any copyrighted or uncopyrighted composition, secret process, patented or unpatented invention, article or appliance furnished or used in the performance of this contract;

b. The contractor’s indemnification and liability under subsection (a) is not limited by, but is in addition to the insurance obligations contained in Section 4.2 of these Terms and Conditions; and

c. In the event of a patent and copyright claim or suit, the contractor, at its option, may: (1) procure for the State of New Jersey the legal right to continue the use of the product; (2) replace or modify the product to provide a non-infringing product that is the functional equivalent; or (3) refund the purchase price less a reasonable allowance for use that is agreed to by both parties.

4.2 INSURANCE - The contractor shall secure and maintain in force for the term of the contract insurance as provided herein. All required insurance shall be provided by insurance companies with an A- VIII or better rating by A.M. Best & Company. The contractor shall provide the State with current certificates of insurance for all coverages and renewals thereof, and the certificates shall reflect that the insurance policies shall not be canceled for any reason except after sixty (60) days written notice to the State. Certificates of renewals shall be provided within thirty (30) days of the expiration of the insurance. The contractor shall not begin to provide services or goods to the State until evidence of the required insurance is provided. The certificates of insurance shall indicate the contract number or purchase order number and title of the contract in the Description of Operations box and shall list the State of New Jersey, Department of the Treasury, Division of Purchase & Property, Contract Compliance & Audit Unit, P.O. Box 236, Trenton, New Jersey 08625 in the Certificate Holder box. The certificates and any notice of cancelation shall be emailed to the State at: 

ccau.certificate@treas.nj.gov

The insurance to be provided by the contractor shall be as follows: 

a. Occurrence Form Comprehensive General Liability Insurance or its equivalent: The minimum limit of liability shall be $1,000,000 per occurrence as a combined single limit for bodily injury and property damage. The above required Comprehensive General Liability Insurance policy or its equivalent shall name the State, its officers, and employees as “Additional Insureds” and include the blanket additional insured endorsement or its equivalent. The coverage to be provided under these policies shall be at least as broad as that provided by the standard basic, unamended, and unendorsed Comprehensive General Liability Insurance occurrence coverage forms or its equivalent currently in use in the State of New Jersey, which shall not be circumscribed by any endorsement limiting the breadth of coverage; 

b. Automobile Liability Insurance which shall be written to cover any automobile used by the insured. Limits of liability for bodily injury and property damage shall not be less than $1 million per occurrence as a combined single limit. The State must be named as an “Additional Insured” and a blanket additional insured endorsement or its equivalent must be provided when the services being procured involve vehicle use on the State’s behalf or on State controlled property;
 
c. Worker’s Compensation Insurance applicable to the laws of the State of New Jersey and Employers Liability Insurance with limits not less than: 

$1,000,000 BODILY INJURY, EACH OCCURRENCE 
$1,000,000 DISEASE EACH EMPLOYEE 
$1,000,000 DISEASE AGGREGATE LIMIT 

d. This $1 million amount may have been raised by the RFP when deemed necessary by the Director;

e. In the case of a contract entered into pursuant to N.J.S.A. 52:32-17 et seq., (small business set asides) the minimum amount of insurance coverage in subsections a., b., and c. above may have been lowered in the RFP for certain commodities when deemed in the best interests of the State by the Director. 

5. TERMS GOVERNING ALL CONTRACTS 

5.1 CONTRACTOR IS INDEPENDENT CONTRACTOR – The contractor's status shall be that of any independent contractor and not as an employee of the State. 

5.2 CONTRACT AMOUNT - The estimated amount of the contract(s), when stated on the RFP form, shall not be construed as either the maximum or minimum amount which the State shall be obliged to order as the result of the RFP or any contract entered into as a result of the RFP. 

5.3 CONTRACT TERM AND EXTENSION OPTION - If, in the opinion of the Director, it is in the best interest of the State to extend a contract, the contractor shall be so notified of the Director’s Intent at least thirty (30) days prior to the expiration date of the existing contract. The contractor shall have fifteen (15) calendar days to respond to the Director's request to extend the term and period of performance of the contract. If the contractor agrees to the extension, all terms and conditions including pricing of the original contract shall apply unless more favorable terms for the State have been negotiated. 

5.4 STATE’S OPTION TO REDUCE SCOPE OF WORK – The State has the option, in its sole discretion, to reduce the scope of work for any deliverable, task or subtask called for under this contract. In such an event, the Director shall provide to the contractor advance written notice of the change in scope of work and what the Director believes should be the corresponding adjusted contract price. Within five (5) business days of receipt of such written notice, if either is applicable: 

a. If the contractor does not agree with the Director’s proposed adjusted contract price, the contractor shall submit to the Director any additional information that the contractor believes impacts the adjusted contract price with a request that the Director reconsider the proposed adjusted contract price. The parties shall negotiate the adjusted contract price. If the parties are unable to agree on an adjusted contract price, the Director shall make a prompt decision taking all such information into account, and shall notify the contractor of the final adjusted contract price; and
 
b. If the contractor has undertaken any work effort toward a deliverable, task or subtask that is being changed or eliminated such that it would not be compensated under the adjusted contract, the contractor shall be compensated for such work effort according to the applicable portions of its price schedule and the contractor shall submit to the Director an itemization of the work effort already completed by deliverable, task or subtask within the scope of work, and any additional information the Director may request. The Director shall make a prompt decision taking all such information into account, and shall notify the contractor of the compensation to be paid for such work effort. 

5.5 CHANGE IN LAW– Whenever a change in applicable law or regulation affects the scope of work, the Director shall provide written notice to the contractor of the change and the Director’s determination as to the corresponding adjusted change in the scope of work and corresponding adjusted contract price. Within five (5) business days of receipt of such written notice, if either is applicable: 

a. If the contractor does not agree with the adjusted contract price, the contractor shall submit to the Director any additional information that the contractor believes impacts the adjusted contract price with a request that the Director reconsider the adjusted contract price. The Director shall make a prompt decision taking all such information into account, and shall notify the contractor of the final adjusted contract price;
 
b. If the contractor has undertaken any work effort toward a deliverable, task or subtask that is being changed or eliminated such that it would not be compensated under the adjusted contract, the contractor shall be compensated for such work effort according to the applicable portions of its price schedule and the contractor shall submit to the Director an itemization of the work effort already completed by deliverable, task or subtask within the scope of work, and any additional information the Director may request. The Director shall make a prompt decision taking all such information into account, and shall notify the contractor of the compensation to be paid for such work effort. 

5.6 SUSPENSION OF WORK - The State may, for valid reason, issue a stop order directing the contractor to suspend work under the contract for a specific time. The contractor shall be paid for goods ordered, goods delivered, or services requested and performed until the effective date of the stop order. The contractor shall resume work upon the date specified in the stop order, or upon such other date as the State Contract Manager may thereafter direct in writing. The period of suspension shall be deemed added to the contractor's approved schedule of performance. The Director shall make an equitable adjustment, if any is required, to the contract price. The contractor shall provide whatever information that Director may require related to the equitable adjustment. 

5.7 TERMINATION OF CONTRACT 

a. For Convenience: 

Notwithstanding any provision or language in this contract to the contrary, the Director may terminate this contract at any time, in whole or in part, for the convenience of the State, upon no less than thirty (30) days written notice to the contractor;

b. For Cause:
 
1. Where a contractor fails to perform or comply with a contract or a portion thereof, and/or fails to comply with the complaints procedure in N.J.A.C. 17:12-4.2 et seq., the Director may terminate the contract, in whole or in part, upon ten (10) days’ notice to the contractor with an opportunity to respond; and
 
2. Where in the reasonable opinion of the Director, a contractor continues to perform a contract poorly as demonstrated by e.g., formal complaints, late delivery, poor performance of service, short-shipping, so that the Director is required to use the complaints procedure in N.J.A.C. 17:12-4.2 et seq., and there has been a failure on the part of the contractor to make progress towards ameliorating the issue(s) or problem(s) set forth in the complaint, the Director may terminate the contract, in whole or in part, upon ten (10) days’ notice to the contractor with an opportunity to respond.
 
c. In cases of emergency the Director may shorten the time periods of notification and may dispense with an opportunity to respond; and

d. In the event of termination under this section, the contractor shall be compensated for work performed in accordance with the contract, up to the date of termination. Such compensation may be subject to adjustments. 

5.8 SUBCONTRACTING OR ASSIGNMENT – 

a. Subcontracting: The contractor may not subcontract other than as identified in the contractor’s proposal without the prior written consent of the Director. Such consent, if granted in part, shall not relieve the contractor of any of his responsibilities under the contract, nor shall it create privity of contract between the State and any subcontractor. If the contractor uses a subcontractor to fulfill any of its obligations, the contractor shall be responsible for the subcontractor’s: (a) performance; (b) compliance with all of the terms and conditions of the contract; and (c) compliance with the requirements of all applicable laws; and 

b. Assignment: The contractor may not assign its responsibilities under the contract, in whole or in part, without the prior written consent of the Director. 

5.9 NO CONTRACTUAL RELATIONSHIP BETWEEN SUBCONTRACTORS AND STATE - Nothing contained in any of the contract documents, including the RFP and vendor’s bid or proposal shall be construed as creating any contractual relationship between any subcontractor and the State. 

5.10 MERGERS, ACQUISITIONS - If, during the term of this contract, the contractor shall merge with or be acquired by another firm, the contractor shall give notice to the Director as soon as practicable and in no event longer than thirty (30) days after said merger or acquisition. The contractor shall provide such documents as may be requested by the Director, which may include but need not be limited to the following: corporate resolutions prepared by the awarded contractor and new entity ratifying acceptance of the original contract, terms, conditions and prices; updated information including ownership disclosure and Federal Employer Identification Number. The documents must be submitted within thirty (30) days of the request. Failure to do so may result in termination of the contract for cause. 

If, at any time during the term of the contract, the contractor's partnership, limited liability company, limited liability partnership, professional corporation, or corporation shall dissolve, the Director must be so notified. All responsible parties of the dissolved business entity must submit to the Director in writing, the names of the parties proposed to perform the contract, and the names of the parties to whom payment should be made. No payment shall be made until all parties to the dissolved business entity submit the required documents to the Director. 

5.11 PERFORMANCE GUARANTEE OF CONTRACTOR - The contractor hereby certifies that: 

a. The equipment offered is standard new equipment, and is the manufacturer's latest model in production, with parts regularly used for the type of equipment offered; that such parts are all in production and not likely to be discontinued; and that no attachment or part has been substituted or applied contrary to manufacturer's recommendations and standard practice;
 
b. All equipment supplied to the State and operated by electrical current is UL listed where applicable;
 
c. All new machines are to be guaranteed as fully operational for the period stated in the contract from time of written acceptance by the State. The contractor shall render prompt service without charge, regardless of geographic location;

d. Sufficient quantities of parts necessary for proper service to equipment shall be maintained at distribution points and service headquarters;

e. Trained mechanics are regularly employed to make necessary repairs to equipment in the territory from which the service request might emanate within a 48-hour period or within the time accepted as industry practice; 

f. During the warranty period the contractor shall replace immediately any material which is rejected for failure to meet the requirements of the contract; and

g. All services rendered to the State shall be performed in strict and full accordance with the specifications stated in the contract. The contract shall not be considered complete until final approval by the State's Using Agency is rendered. 

5.12 DELIVERY REQUIREMENTS- 

a. Deliveries shall be made at such time and in such quantities as ordered in strict accordance with conditions contained in the contract;

b. The contractor shall be responsible for the delivery of material in first class condition to the State's Using Agency or the purchaser under this contract and in accordance with good commercial practice;
 
c. Items delivered must be strictly in accordance with the contract; and

d. In the event delivery of goods or services is not made within the number of days stipulated or under the schedule defined in the contract, the Using Agency shall be authorized to obtain the material or service from any available source, the difference in price, if any, to be paid by the contractor. 

5.13 APPLICABLE LAW AND JURISDICTION - This contract and any and all litigation arising therefrom or related thereto shall be governed by the applicable laws, regulations and rules of evidence of the State of New Jersey without reference to conflict of laws principles and shall be filed in the appropriate Division of the New Jersey Superior Court. 

5.14. CONTRACT AMENDMENT – Except as provided herein, the contract may only be amended by written agreement of the State and the contractor. 

5.15 MAINTENANCE OF RECORDS - The contractor shall maintain records for products and/or services delivered against the contract for a period of five (5) years from the date of final payment unless otherwise specified in the RFP. Such records shall be made available to the State, including the Comptroller, for audit and review.

5.16 ASSIGNMENT OF ANTITRUST CLAIM(S) - The contractor recognizes that in actual economic practice, overcharges resulting from antitrust violations are in fact usually borne by the ultimate purchaser. Therefore, and as consideration for executing this contract, the contractor, acting herein by and through its duly authorized agent, hereby conveys, sells, assigns, and transfers to the State of New Jersey, for itself and on behalf of its political subdivisions and public agencies, all right, title and interest to all claims and causes of action it may now or hereafter acquire under the antitrust laws of the United States or the State of New Jersey, relating to the particular goods and services purchased or acquired by the State of New Jersey or any of its political subdivisions or public agencies pursuant to this contract. 
In connection with this assignment, the following are the express obligations of the contractor: 

a. It shall take no action that will in any way diminish the value of the rights conveyed or assigned hereunder; 
b. It shall advise the Attorney General of New Jersey: 
1. in advance of its intention to commence any action on its own behalf regarding any such claim or cause(s) of action; and
2. immediately upon becoming aware of the fact that an action has been commenced on its behalf by some other person(s) of the pendency of such action. 
c. It shall notify the defendants in any antitrust suit of the within assignment at the earliest practicable opportunity after the contractor has initiated an action on its own behalf or becomes aware that such an action has been filed on its behalf by another person. A copy of such notice shall be sent to the Attorney General of New Jersey; and 
d. It is understood and agreed that in the event any payment under any such claim or cause of action is made to the contractor, it shall promptly pay over to the State of New Jersey the allotted share thereof, if any, assigned to the State hereunder. 
6. TERMS RELATING TO PRICE AND PAYMENT 

6.1 PRICE FLUCTUATION DURING CONTRACT - Unless otherwise agreed to in writing by the State, all prices quoted shall be firm through issuance of contract or purchase order and shall not be subject to increase during the period of the contract. 
In the event of a manufacturer's or contractor's price decrease during the contract period, the State shall receive the full benefit of such price reduction on any undelivered purchase order and on any subsequent order placed during the contract period. The Director must be notified, in writing, of any price reduction within five (5) days of the effective date. 
Failure to report price reductions may result in cancellation of contract for cause, pursuant to provision 5.7(b)1. 

6.2 TAX CHARGES - The State of New Jersey is exempt from State sales or use taxes and Federal excise taxes. Therefore, price quotations must not include such taxes. The State's Federal Excise Tax Exemption number is 22-75-0050K. 



6.3 PAYMENT TO VENDORS - 

a. The Using Agency(ies) is (are) authorized to order and the contractor is authorized to ship only those items covered by the contract resulting from the RFP. If a review of orders placed by the Using Agency(ies) reveals that goods and/or services other than that covered by the contract have been ordered and delivered, such delivery shall be a violation of the terms of the contract and may be considered by the Director as a basis to terminate the contract and/or not award the contractor a subsequent contract. The Director may take such steps as are necessary to have the items returned by the agency, regardless of the time between the date of delivery and discovery of the violation. In such event, the contractor shall reimburse the State the full purchase price; 

b. The contractor must submit invoices to the Using Agency with supporting documentation evidencing that work or goods for which payment is sought has been satisfactorily completed or delivered. For commodity contracts, the invoice, together with the original Bill of Lading, express receipt and other related papers must be sent to the State Contract Manager or Using Agency on the date of each delivery. For contracts featuring services, invoices must reference the tasks or subtasks detailed in the Scope of Work section of the RFP and must be in strict accordance with the firm, fixed prices submitted for each task or subtask on the RFP pricing sheets. When applicable, invoices should reference the appropriate RFP price sheet line number from the contractor’s bid proposal. All invoices must be approved by the State Contract Manager or Using Agency before payment will be authorized; 

c. In all time and materials contracts, the State Contract Manager or designee shall monitor and approve the hours of work and the work accomplished by contractor and shall document both the work and the approval. Payment shall not be made without such documentation. A form of timekeeping record that should be adapted as appropriate for the Scope of Work being performed can be found at www.nj.gov/treasury/purchase/forms/Vendor_Timesheet.xls; and

d. The contractor shall provide, on a monthly and cumulative basis, a breakdown in accordance with the budget submitted, of all monies paid to any small business, minority or woman-owned subcontractor(s). This breakdown shall be sent to the Chief of Operations, Division of Revenue, P.O. Box 628, Trenton, NJ 08646. 

6.4 OPTIONAL PAYMENT METHOD: P-CARD - The State offers contractors the opportunity to be paid through the MasterCard procurement card (p-card). A contractor’s acceptance and a State agency’s use of the p-card are optional. P-card transactions do not require the submission of a contractor invoice; purchasing transactions using the p-card will usually result in payment to a contractor in three (3) days. A contractor should take note that there will be a transaction-processing fee for each p-card transaction. To participate, a contractor must be capable of accepting the MasterCard. Additional information can be obtained from banks or merchant service companies. 

6.5 NEW JERSEY PROMPT PAYMENT ACT - The New Jersey Prompt Payment Act, N.J.S.A. 52:32-32 et seq., requires state agencies to pay for goods and services within sixty (60) days of the agency's receipt of a properly executed State Payment Voucher or within sixty (60) days of receipt and acceptance of goods and services, whichever is later. Properly executed performance security, when required, must be received by the State prior to processing any payments for goods and services accepted by state agencies. Interest will be paid on delinquent accounts at a rate established by the State Treasurer. Interest shall not be paid until it exceeds $5.00 per properly executed invoice. 

Cash discounts and other payment terms included as part of the original agreement are not affected by the Prompt Payment Act. 

6.6 AVAILABILITY OF FUNDS – The State’s obligation to make payment under this contract is contingent upon the availability of appropriated funds and receipt of revenues from which payment for contract purposes can be made. No legal liability on the part of the State for payment of any money shall arise unless and until funds are appropriated each fiscal year to the Using Agency by the State Legislature and made available through receipt of revenue.


EXHIBIT A

MANDATORY EQUAL EMPLOYMENT OPPORTUNITY LANGUAGE
N.J.S.A. 10:5-31 et seq. (P.L. 1975, C. 127)
N.J.A.C. 17:27

GOODS, PROFESSIONAL SERVICE AND GENERAL SERVICE CONTRACTS

During the performance of this contract, the contractor agrees as follows:

	The contractor or subcontractor, where applicable, will not discriminate against any employee or applicant for employment because of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Except with respect to affectional or sexual orientation and gender identity or expression, the contractor will ensure that equal employment opportunity is afforded to such applicants in recruitment and employment, and that employees are treated during employment, without regard to their age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex.  Such equal employment opportunity shall include, but not be limited to the following: employment, upgrading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship.  The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided by the Public Agency Compliance Officer setting forth provisions of this nondiscrimination clause.
 
	The contractor or subcontractor, where applicable will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex.

	The contractor or subcontractor will send to each labor union, with which it has a collective bargaining agreement, a notice, to be provided by the agency contracting officer, advising the labor union of the contractor's commitments under this chapter and shall post copies of the notice in conspicuous places available to employees and applicants for employment.

The contractor or subcontractor, where applicable, agrees to comply with any regulations promulgated by the Treasurer pursuant to N.J.S.A. 10:5-31 et seq., as amended and supplemented from time to time and the Americans with Disabilities Act.

	The contractor or subcontractor agrees to make good faith efforts to meet targeted county employment goals established in accordance with N.J.A.C. 17:27 5.2.

	The contractor or subcontractor agrees to inform in writing its appropriate recruitment agencies including, but not limited to, employment agencies, placement bureaus, colleges, universities, and labor unions, that it does not discriminate on the basis of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, and that it will discontinue the use of any recruitment agency which engages in direct or indirect discriminatory practices.
	The contractor or subcontractor agrees to revise any of its testing procedures, if necessary, to assure that all personnel testing conforms with the principles of job related testing, as established by the statutes and court decisions of the State of New Jersey and as established by applicable Federal law and applicable Federal court decisions.

	In conforming with the targeted employment goals, the contractor or subcontractor agrees to review all procedures relating to transfer, upgrading, downgrading and layoff to ensure that all such actions are taken without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex, consistent with the statutes and court decisions of the State of New Jersey, and applicable Federal law and applicable Federal court decisions.

	The contractor shall submit to the public agency, after notification of award but prior to execution of a goods and services contract, one of the following three documents:

	Letter of Federal Affirmative Action Plan Approval

	Certificate of Employee Information Report

	Employee Information Report Form AA302 (electronically provided by the Division and distributed to the public agency through the Division’s website at www.state.nj.us/treasury/contract_compliance)

	The contractor and its subcontractors shall furnish such reports or other documents to the Division of Public Contracts Equal Employment Opportunity Compliance as may be requested by the office from time to time in order to carry out the purposes of these regulations, and public agencies shall furnish such information as may be requested by the Division of Public Contracts Equal Employment Opportunity Compliance for conducting a compliance investigation pursuant to Subchapter 10 of the Administrative Code at N.J.A.C. 17:27-1 et seq.


EXHIBIT B

MANDATORY EQUAL EMPLOYMENT OPPORTUNITY LANGUAGE
N.J.S.A. 10:5-31 et seq. (P.L. 1975, C. 127)
N.J.A.C. 17:27

CONSTRUCTION CONTRACTS

During the performance of this contract, the contractor agrees as follows:

The contractor or subcontractor, where applicable, will not 	discriminate against any employee or applicant for employment because of age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Except with respect to affectional or sexual orientation and gender identity or expression, the contractor will ensure that equal employment opportunity is afforded to such applicants in recruitment and employment, and that employees are treated during employment, without regard to their age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex. Such equal employment opportunity shall include, but not be limited to the following: employment, up grading, demotion, or transfer; recruitment or recruitment advertising; layoff or termination; rates of pay or other forms of compensation; and selection for training, including apprenticeship. The contractor agrees to post in conspicuous places, available to employees and applicants for employment, notices to be provided by the Public Agency Compliance Officer setting forth provisions of this nondiscrimination clause.

The contractor or subcontractor, where applicable will, in all solicitations or advertisements for employees placed by or on behalf of the contractor, state that all qualified applicants will receive consideration for employment without regard to age, race, creed, color, national origin, ancestry, marital status, affectional or sexual orientation, gender identity or expression, disability, nationality or sex.

The contractor or subcontractor will send 	to each labor union, with which it has a collective bargaining agreement, a notice, to be provided by the agency contracting officer, advising the labor union or workers' representative of the contractor's commitments under this act and shall post copies of the notice in conspicuous places available to employees and applicants for employment.

The contractor or subcontractor, where applicable, agrees to comply with any regulations promulgated by the Treasurer, pursuant to N.J.S.A. 10:5-31 et seq., as amended and supplemented from time to time and the Americans with Disabilities Act.

When hiring or scheduling workers in each construction trade, the contractor or subcontractor agrees to make good faith efforts to employ 	minority and women workers in each construction trade consistent with the targeted employment goal prescribed by N.J.A.C. 17:27-7.2; provided, however, that the Division may, in its discretion, exempt a contractor or subcontractor from compliance with the good faith procedures prescribed by the following provisions, A, B and C, as long as the Division is satisfied that the contractor or subcontractor is employing workers provided by a union which provides evidence, in accordance with standards prescribed by the Division, that its percentage of active "card carrying" members who are minority and women workers is equal to or greater than the targeted employment goal established in accordance with N.J.A.C. 17:27-7.2.  The contractor or subcontractor agrees that a good faith effort shall include compliance with the following procedures:

(A)	If the contractor or subcontractor has a referral agreement or arrangement with a union for a construction trade, the contractor or subcontractor shall, within three business days of the contract award, seek assurances from the union that it will cooperate with the contractor or subcontractor as it fulfills its affirmative action obligations under this contract and in accordance with the rules promulgated by the Treasurer pursuant to N.J.S.A. 10:5-31 et. seq., as supplemented and amended from time to time and the Americans with Disabilities Act.  If the contractor or subcontractor is unable to obtain said assurances from the construction trade union at least five business days prior to the commencement of construction work, the contractor or subcontractor agrees to afford equal employment opportunities minority and women workers directly, consistent with this chapter.  If the contractor's or subcontractor's prior experience with a construction trade union, regardless of whether the union has provided said assurances, indicates a significant possibility that the trade union will not refer sufficient minority and women workers consistent with affording equal employment opportunities as specified in this chapter, the contractor or subcontractor agrees to be prepared to provide such opportunities to minority and women workers directly, consistent with this chapter, by complying with the hiring or scheduling procedures prescribed under (B) below; and the contractor or subcontractor further agrees to take said action immediately if it determines that the union is not referring minority and women workers consistent with the equal employment opportunity goals set forth in this chapter.

(B)	If good faith efforts to meet targeted employment goals have not or cannot be met for each construction trade by adhering to the procedures of (A) above, or if the contractor does not have a referral agreement or arrangement with a union for a construction trade, the contractor or subcontractor agrees to take the following actions:

(1) To notify the public agency compliance officer, the Division, and minority and women referral organizations listed by the Division pursuant to N.J.A.C. 17:27-5.3, of its workforce needs, and request referral of minority and women workers;
		
(2) To notify any minority and women workers who have been listed with it as awaiting available vacancies;

(3) Prior to commencement of work, to request that the local construction 	trade union refer minority and women workers to fill job openings, provided the contractor or subcontractor has a referral agreement or arrangement with a union for the construction trade;

(4) To leave standing requests for additional referral to minority and women workers with the local construction trade union, provided the contractor or subcontractor has a referral agreement or arrangement with a union for the construction trade, the State Training and Employment Service and other approved referral sources in the area;

(5) If it is necessary to lay off some of the workers in a given trade on the construction site, layoffs shall be conducted in compliance with the equal employment opportunity and non-discrimination standards set forth in this regulation, as well as with applicable Federal and State court decisions;

(6) To adhere to the following procedure when minority and women workers apply or are referred to the contractor or subcontractor:

(i) The contactor or subcontractor shall interview the referred minority or women worker.

(ii) If said individuals have never previously received any document or certification signifying a level of qualification lower than that required in order to perform the work of the construction trade, the contractor or subcontractor shall in good faith determine the qualifications of such individuals. The contractor or subcontractor shall hire or schedule those individuals who satisfy appropriate qualification standards in conformity with the equal employment opportunity and non-discrimination principles set forth in this chapter. However, a contractor or subcontractor shall determine that the individual at least possesses the requisite skills, and experience recognized by a union, apprentice program or a referral agency, provided the referral agency is acceptable to the Division. If necessary, the contractor or subcontractor shall hire or schedule minority and women workers who qualify as trainees pursuant to these rules. All of the requirements, however, are limited by the provisions of (C) below.

(iii) The name of any interested women or minority individual shall be maintained on a waiting list, and shall be considered for employment as described in (i) above, whenever vacancies occur. At the request of the Division, the contractor or subcontractor shall provide evidence of its good faith efforts to employ women and minorities from the list to fill vacancies.

(iv) If, for any reason, said contractor or subcontractor determines that a minority individual or a woman is not qualified or if the individual qualifies as an advanced trainee or apprentice, the contractor or subcontractor shall inform the individual in writing of the reasons for the determination, maintain a copy of the determination in its files, and send a copy to the public agency compliance officer and to the Division.

(7) To keep a complete and accurate record of all requests made for the referral of workers in any trade covered by the contract, on forms made available by the Division and submitted promptly to the Division upon request.

(C) The contractor or subcontractor agrees that nothing contained in (B) above shall preclude the contractor or subcontractor from complying with the union hiring hall or apprenticeship policies in any applicable collective bargaining agreement or union hiring hall arrangement, and, where required by custom or agreement, it shall send journeymen and trainees to the union for referral, or to the apprenticeship program for admission, pursuant to such agreement or arrangement. However, where the practices of a union or apprenticeship program will result in the exclusion of minorities and women or the failure to refer minorities and women consistent with the targeted county employment goal, the contractor or subcontractor shall consider for employment persons referred pursuant to (B) above without regard to such agreement or	arrangement; provided further, however, that the contractor or subcontractor shall not be required to employ women and minority advanced trainees and trainees in numbers which result in the employment of advanced trainees and trainees as a percentage of the total workforce for the construction trade, which percentage significantly exceeds the 	apprentice to journey worker ratio specified in the applicable collective bargaining agreement, or in the absence of a collective bargaining agreement, exceeds the ratio established by practice in the area for said construction trade.  Also, the contractor or subcontractor agrees that, in implementing the procedures of (B) above, it shall, where applicable, employ minority and women workers residing within the geographical jurisdiction of the union.

After notification of award, but prior to signing a construction contract, the contractor shall submit to the public agency compliance officer and the Division an initial project workforce report (Form AA 201) electronically provided to the public agency by the Division, through its website, for distribution to and completion by the contractor, in accordance with N.J.A.C. 17:27-7. 

The contractor also agrees to submit a copy of the Monthly Project Workforce Report once a month thereafter for the duration of this contract to the Division and to the public agency compliance officer.

The contractor agrees to cooperate with the public agency in the payment of budgeted funds, as is necessary, for on the job and/or off the job programs for outreach and training of minorities and women.

(D)  The contractor and its subcontractors shall furnish such reports or other documents to the Division of Public Contracts Equal Employment Opportunity Compliance as may be requested by the Division from time to time in order to carry out the purposes of these regulations, and public agencies shall furnish such information as may be requested by the Division of Public Contracts Equal Employment Opportunity Compliance for conducting a compliance investigation pursuant to Subchapter 10 of the Administrative Code (N.J.A.C. 17:27-1 et seq.).


EXECUTIVE ORDER NO. 151 REQUIREMENTS

It is the policy of the Division of Purchase and Property that its contracts should create a workforce that reflects the diversity of the State of New Jersey. Therefore, contractors engaged by the Division of Purchase and Property to perform under a construction contract shall put forth a good faith effort to engage in recruitment and employment practices that further the goal of fostering equal opportunities to minorities and women. 

The contractor must demonstrate to the Division of Purchase and Property’s satisfaction that a good faith effort was made to ensure that minorities and women have been afforded equal opportunity to gain employment under the Division of Purchase and Property’s contract with the contractor. Payment may be withheld from a contractor’s contract for failure to comply with these provisions. 

Evidence of a “good faith effort” includes, but is not limited to:
 
1. The Contractor shall recruit prospective employees through the State Job bank website, managed by the Department of Labor and Workforce Development, available online at http://NJ.gov/JobCentralNJ; 
2. The Contractor shall keep specific records of its efforts, including records of all individuals interviewed and hired, including the specific numbers of minorities and women;
3. The Contractor shall actively solicit and shall provide the Division of Purchase and Property with proof of solicitations for employment, including but not limited to advertisements in general circulation media, professional service publications and electronic media; and 
4. The Contractor shall provide evidence of efforts described at 2 above to the Division of Purchase and Property no less frequently than once every 12 months. 
5. The Contractor shall comply with the requirements set forth at N.J.A.C. 17:27. 

This language is in addition to and does not replace good faith efforts requirements for construction contracts required by N.J.A.C. 17:27-3.6, 3.7 and 3.8, also known as Exhibit B.
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